<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="22.86" y2="0" width="0.254" layer="20"/>
<wire x1="22.86" y1="0" x2="22.86" y2="22.86" width="0.254" layer="20"/>
<wire x1="22.86" y1="22.86" x2="0" y2="22.86" width="0.254" layer="20"/>
<wire x1="0" y1="22.86" x2="0" y2="0" width="0.254" layer="20"/>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>NC</text>
<text>IV-3a VFD
Breakout w/ RGB LED v1.1</text>
<text>Filiment: 1.7V/AC 10mA
Grid/Segments: 30V/DC 50mA</text>
<text>LED1</text>
<text>Phantomic Labs 2018</text>
<text>LED_DI</text>
<text>LED_VDD</text>
<text>8/FIL+</text>
<text>7/FIL-</text>
<text>9</text>
<text>6</text>
<text>5</text>
<text>4</text>
<text>3</text>
<text>2</text>
<text>1</text>
<text>10</text>
<text>11</text>
<text>LED_DO</text>
<text>GND</text>
</plain>
<libraries>
<library name="VFD_tubes">
<packages>
<package name="VFD_IV-3A">
</package>
</packages>
</library>
<library name="Ai_Connectors">
<description>&lt;h3&gt;Ai Connectors&lt;/h3&gt;
&lt;p&gt;
This library includes USB, pin headers and sockets in different configurations (e.g., pad shapes, with or without silkscreen), SD cards, screw terminals, etc.
&lt;/p&gt;</description>
<packages>
<package name="1X08-NOFIRST">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="LED3535">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="VFD_tubes" package="VFD_IV-3A" value="VFD_IV-3A"/>
<element name="J1" library="Ai_Connectors" package="1X08-NOFIRST" value="1X08NOFIRST"/>
<element name="J2" library="Ai_Connectors" package="1X08-NOFIRST" value="1X08NOFIRST"/>
<element name="LED1" library="adafruit" package="LED3535" value="RGB_3535"/>
</elements>
<signals>
<signal name="9/GRID+">
<contactref element="U$1" pad="P$9"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="LED_VDD">
<contactref element="J1" pad="7"/>
<contactref element="LED1" pad="2"/>
</signal>
<signal name="LED_DI">
<contactref element="J1" pad="8"/>
<contactref element="LED1" pad="1"/>
</signal>
<signal name="LED_DO">
<contactref element="LED1" pad="3"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="7/FIL-">
<contactref element="U$1" pad="P$7"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="8/FIL+">
<contactref element="U$1" pad="P$8"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="P$1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="P$2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="P$3"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="P$4"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="P$5"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="P$6"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="N$10">
<contactref element="U$1" pad="P$10"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="P$11"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="GND">
<contactref element="LED1" pad="4"/>
<contactref element="J2" pad="2"/>
<contactref element="J2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
