<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<wire x1="3.5" y1="0" x2="4.5" y2="0" width="0.1524" layer="20"/>
<wire x1="4.5" y1="0" x2="40.5" y2="0" width="0.1524" layer="20"/>
<wire x1="0" y1="9.25" x2="0" y2="9" width="0.1524" layer="20"/>
<wire x1="0" y1="9" x2="0" y2="4.5" width="0.1524" layer="20"/>
<wire x1="0" y1="4.5" x2="0" y2="3.5" width="0.1524" layer="20"/>
<wire x1="4.5" y1="13.5" x2="40.5" y2="13.5" width="0.1524" layer="20"/>
<wire x1="45" y1="9" x2="45" y2="4.5" width="0.1524" layer="20"/>
<hole x="11.75" y="6.75" drill="8.5"/>
<hole x="33.25" y="6.75" drill="8.5"/>
<rectangle x1="4.65" y1="3.25" x2="9.25" y2="10.25" layer="20"/>
<rectangle x1="35.75" y1="3.25" x2="40.35" y2="10.25" layer="20"/>
<wire x1="4.5" y1="13.5" x2="0" y2="9" width="0.1524" layer="20" curve="90"/>
<wire x1="0" y1="4.5" x2="4.5" y2="0" width="0.1524" layer="20" curve="90"/>
<wire x1="40.5" y1="0" x2="45" y2="4.5" width="0.1524" layer="20" curve="90"/>
<wire x1="45" y1="9" x2="40.5" y2="13.5" width="0.1524" layer="20" curve="90"/>
</plain>
<libraries>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP12SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="0402">
<description>&lt;p&gt;&lt;b&gt;Generic 1005 (0402) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402">
<description>&lt;p&gt;&lt;b&gt;Generic 1005 (0402) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="2608011024000">
<packages>
<package name="XCVR_2608011024000">
</package>
</packages>
</library>
<library name="Adafruit LIS3DH">
<description>Generated from &lt;b&gt;Adafruit LIS3DH.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="MICROBUILDER_LGA16_3X3MM">
</package>
</packages>
</library>
<library name="TLV70033DSER">
<packages>
<package name="SON50P150X150X80-6N">
</package>
</packages>
</library>
<library name="wirepad_2">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMD1,27-2,54">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BATTNEG" library="testpad" package="TP12SQ" value="BattNeg">
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="BATTPOS" library="testpad" package="TP12SQ" value="BattPos">
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0402" value="1.0uF">
<attribute name="PROD_ID" value="CAP-12417"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0402" value="1.0uF">
<attribute name="PROD_ID" value="CAP-12417"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0402" value="4.7k">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0402" value="4.7k">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="U1" library="2608011024000" package="XCVR_2608011024000" value="2608011024000">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Bluetooth Bluetooth v4.2 Transceiver Module 2.4GHz Integrated, Chip Surface Mount "/>
<attribute name="MF" value="Wurth Electronics"/>
<attribute name="MP" value="2608011024000"/>
<attribute name="PACKAGE" value="Module Wurth Electronics Inc."/>
<attribute name="PRICE" value="None"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603" value="10uF">
<attribute name="PROD_ID" value="CAP-11015"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0402" value="0.1uF">
<attribute name="PROD_ID" value="CAP-12417"/>
</element>
<element name="U5" library="Adafruit LIS3DH" package="MICROBUILDER_LGA16_3X3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="U2" library="TLV70033DSER" package="SON50P150X150X80-6N" value="TLV70033DSER">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Linear Voltage Regulator IC 1 Output 200mA 6-WSON _1.5x1.5_ "/>
<attribute name="MF" value="Texas Instruments"/>
<attribute name="MP" value="TLV70033DSER"/>
<attribute name="PACKAGE" value="WFDFN-6 Texas Instruments"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="PAD1" library="wirepad_2" package="SMD1,27-2,54" value="">
<attribute name="POPULARITY" value="15"/>
<attribute name="VALUE"/>
</element>
<element name="PAD2" library="wirepad_2" package="SMD1,27-2,54" value="">
<attribute name="POPULARITY" value="15"/>
<attribute name="VALUE"/>
</element>
<element name="PAD3" library="wirepad_2" package="SMD1,27-2,54" value="">
<attribute name="POPULARITY" value="15"/>
<attribute name="VALUE"/>
</element>
<element name="PAD4" library="wirepad_2" package="SMD1,27-2,54" value="">
<attribute name="POPULARITY" value="15"/>
<attribute name="VALUE"/>
</element>
<element name="PAD5" library="wirepad_2" package="SMD1,27-2,54" value="">
<attribute name="POPULARITY" value="15"/>
<attribute name="VALUE"/>
</element>
<element name="PAD6" library="wirepad_2" package="SMD1,27-2,54" value="">
<attribute name="POPULARITY" value="15"/>
<attribute name="VALUE"/>
</element>
<element name="PAD7" library="wirepad_2" package="SMD1,27-2,54" value="">
<attribute name="POPULARITY" value="15"/>
<attribute name="VALUE"/>
</element>
<element name="PAD8" library="wirepad_2" package="SMD1,27-2,54" value="">
<attribute name="POPULARITY" value="15"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="17"/>
<contactref element="BATTNEG" pad="TP"/>
<contactref element="C3" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="U5" pad="8"/>
<contactref element="U5" pad="7"/>
<contactref element="U5" pad="5"/>
<contactref element="U5" pad="12"/>
<contactref element="U5" pad="10"/>
<contactref element="U2" pad="2"/>
<contactref element="PAD1" pad="1"/>
<contactref element="PAD5" pad="1"/>
</signal>
<signal name="3V3">
<contactref element="U1" pad="7"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="PAD2" pad="1"/>
<contactref element="PAD6" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="12"/>
<contactref element="R1" pad="2"/>
<contactref element="U5" pad="6"/>
<contactref element="PAD3" pad="1"/>
<contactref element="PAD7" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="14"/>
<contactref element="R2" pad="2"/>
<contactref element="U5" pad="4"/>
<contactref element="PAD4" pad="1"/>
<contactref element="PAD8" pad="1"/>
</signal>
<signal name="BATTPOS">
<contactref element="BATTPOS" pad="TP"/>
<contactref element="U2" pad="6"/>
<contactref element="U2" pad="1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="C2" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U5" pad="1"/>
<contactref element="U5" pad="14"/>
</signal>
<signal name="INT1">
<contactref element="U5" pad="11"/>
<contactref element="U1" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
