(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-2")
  (general
    (thickness 1.6)
    (drawings 42)
    (tracks 12)
    (zones 0)
    (modules 0)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers(double)/"))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (gr_text "+ makho -" (at -3.5 18.5 270) (layer B.Mask))
  (gr_text "+ makho -" (at 2.5 13 90) (layer B.Mask))
  (gr_line (start -1.5 31.5) (end -5 31.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -6 30.5) (end -6 1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -1.5 0) (end -5 0) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -1 31) (end -1 0.5) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start -5 1) (end -5 0) (angle -90) (layer Edge.Cuts) (width 0.12))
  (gr_text "+ makho -" (at -3.5 18.5 270) (layer B.Cu))
  (gr_arc (start -1.5 0.5) (end -1 0.5) (angle -90) (layer Edge.Cuts) (width 0.12))
  (gr_arc (start -5 30.5) (end -6 30.5) (angle -90) (layer Edge.Cuts) (width 0.12))
  (gr_arc (start -1.5 31) (end -1.5 31.5) (angle -90) (layer Edge.Cuts) (width 0.12))
  (gr_arc (start 0.5 31) (end 0 31) (angle -90) (layer Edge.Cuts) (width 0.12))
  (gr_arc (start 0.5 0.5) (end 0.5 0) (angle -90) (layer Edge.Cuts) (width 0.12))
  (gr_arc (start 4 1) (end 5 1) (angle -90) (layer Edge.Cuts) (width 0.12))
  (gr_arc (start 4 30.5) (end 4 31.5) (angle -90) (layer Edge.Cuts) (width 0.12))
  (gr_text "+ makho -" (at 2.5 13 90) (layer B.Cu))
  (gr_line (start 0.5 31.5) (end 4 31.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0.5 0) (end 4 0) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 5 1) (end 5 30.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0 0.5) (end 0 31) (layer Edge.Cuts) (width 0.05))
)
