<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="26.67" y1="35.179" x2="26.67" y2="3.175" width="0.1016" layer="20"/>
<wire x1="0" y1="3.175" x2="0" y2="35.179" width="0.1016" layer="20"/>
<wire x1="23.495" y1="33.909" x2="23.495" y2="31.877" width="0.1016" layer="46"/>
<wire x1="23.495" y1="31.877" x2="22.225" y2="30.607" width="0.1016" layer="46"/>
<wire x1="22.225" y1="30.607" x2="4.445" y2="30.607" width="0.1016" layer="46"/>
<wire x1="4.445" y1="30.607" x2="3.175" y2="31.877" width="0.1016" layer="46"/>
<wire x1="3.175" y1="31.877" x2="3.175" y2="33.909" width="0.1016" layer="46"/>
<wire x1="3.175" y1="33.909" x2="4.445" y2="35.179" width="0.1016" layer="46"/>
<wire x1="4.445" y1="35.179" x2="22.225" y2="35.179" width="0.1016" layer="46"/>
<wire x1="22.225" y1="35.179" x2="23.495" y2="33.909" width="0.1016" layer="46"/>
<wire x1="0" y1="35.179" x2="3.175" y2="38.354" width="0.1016" layer="20"/>
<wire x1="3.175" y1="38.354" x2="23.495" y2="38.354" width="0.1016" layer="20"/>
<wire x1="23.495" y1="38.354" x2="26.67" y2="35.179" width="0.1016" layer="20"/>
<wire x1="3.175" y1="4.445" x2="3.175" y2="6.477" width="0.1016" layer="46"/>
<wire x1="4.445" y1="7.747" x2="22.225" y2="7.747" width="0.1016" layer="46"/>
<wire x1="22.225" y1="7.747" x2="23.495" y2="6.477" width="0.1016" layer="46"/>
<wire x1="23.495" y1="6.477" x2="23.495" y2="4.445" width="0.1016" layer="46"/>
<wire x1="23.495" y1="4.445" x2="22.225" y2="3.175" width="0.1016" layer="46"/>
<wire x1="22.225" y1="3.175" x2="4.445" y2="3.175" width="0.1016" layer="46"/>
<wire x1="4.445" y1="3.175" x2="3.175" y2="4.445" width="0.1016" layer="46"/>
<wire x1="26.67" y1="3.175" x2="23.495" y2="0" width="0.1016" layer="20"/>
<wire x1="23.495" y1="0" x2="3.175" y2="0" width="0.1016" layer="20"/>
<wire x1="3.175" y1="0" x2="0" y2="3.175" width="0.1016" layer="20"/>
<wire x1="4.445" y1="7.747" x2="3.175" y2="6.477" width="0.1016" layer="46"/>
</plain>
<libraries>
<library name="MF_IC_Digital">
<packages>
<package name="EFM8SB10F(2/4/8)G-A-QFN20">
<description>&lt;b&gt;Description:&lt;/b&gt; Silicon Labs Sleepy Bee QFN20 Package.&lt;br/&gt;</description>
</package>
</packages>
</library>
<library name="MF_Aesthetics">
<packages>
<package name="MF_FRAME_DEFAULT">
<description>&lt;b&gt;Description:&lt;/b&gt; Footprint for adding Meta Data to the PCB.&lt;br/&gt;</description>
</package>
<package name="FIDUCIAL_0.5MM">
</package>
</packages>
</library>
<library name="MF_Connectors">
<packages>
<package name="BAT-HLD-001">
<description>&lt;b&gt;Description:&lt;/b&gt; Package for a CR2032 Battery Holder. Based on Linx Technologies BAT-HLD-001.&lt;br&gt;</description>
</package>
<package name="POGO_PIN_70-9150">
<description>&lt;b&gt;Description:&lt;/b&gt; Package for SMD mount Pogo Pin connectors. Based on AVX 70-9150 series Pogo Pins.&lt;br&gt;</description>
</package>
</packages>
</library>
<library name="MF_Passives">
<packages>
<package name="C0402">
<description>&lt;b&gt;Description:&lt;/b&gt; Standard 0402 Package for Capacitors&lt;br/&gt;</description>
</package>
<package name="R0402">
<description>&lt;b&gt;Description:&lt;/b&gt; Standard 0402 Package for Resistors&lt;br/&gt;</description>
</package>
</packages>
</library>
<library name="MF_Switches">
<packages>
<package name="TACT4.2MM">
<description>&lt;b&gt;Description:&lt;/b&gt; Standard 4.2MM Tact Switch Package.Based off C&amp;K PTS 810 Series Tact Switch.&lt;br/&gt;</description>
</package>
</packages>
</library>
<library name="MF_LEDs">
<packages>
<package name="LED0603">
<description>&lt;b&gt;Description:&lt;/b&gt; Footprint for Single LEDs in 0603&lt;br/&gt;</description>
</package>
</packages>
</library>
<library name="MF_Frequency_Control">
<packages>
<package name="ECX-31B_SERIES">
</package>
</packages>
</library>
<library name="PP_Aesthetics">
<packages>
<package name="MF_LOGO_SMALL">
</package>
</packages>
</library>
<library name="PP_Connectors">
<packages>
<package name="TC2030">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FRAME1" library="MF_Aesthetics" package="MF_FRAME_DEFAULT" value="MF_FRAMEDEFAULT">
<attribute name="REVNUM" value="REV: 2"/>
<attribute name="DNAME" value="Parker Dillmann"/>
<attribute name="DRAWING_NAME"/>
</element>
<element name="BATT1" library="MF_Connectors" package="BAT-HLD-001" value="BAT-HLD-001"/>
<element name="C1" library="MF_Passives" package="C0402" value="MF-CAP-0402-1uF">
<attribute name="TOLERANCE" value="N/A"/>
<attribute name="MFG#" value="N/A"/>
<attribute name="VOLTAGE" value="N/A"/>
<attribute name="TEMP_COF" value="N/A"/>
</element>
<element name="C2" library="MF_Passives" package="C0402" value="MF-CAP-0402-0.1uF">
<attribute name="TOLERANCE" value="N/A"/>
<attribute name="MFG#" value="N/A"/>
<attribute name="VOLTAGE" value="N/A"/>
<attribute name="TEMP_COF" value="N/A"/>
</element>
<element name="TIME?" library="MF_Switches" package="TACT4.2MM" value="MF-SW-TACT-4.2MM">
<attribute name="NAME"/>
</element>
<element name="R1" library="MF_Passives" package="R0402" value="MF-RES-0402-10K">
<attribute name="TOLERANCE" value="N/A"/>
<attribute name="MFG#" value="N/A"/>
<attribute name="VOLTAGE" value="N/A"/>
<attribute name="WATTAGE" value="N/A"/>
</element>
<element name="M1" library="MF_LEDs" package="LED0603" value="MF-LED-0603-RED">
<attribute name="MFG#" value="N/A"/>
<attribute name="NAME"/>
</element>
<element name="M2" library="MF_LEDs" package="LED0603" value="MF-LED-0603-RED">
<attribute name="MFG#" value="N/A"/>
<attribute name="NAME"/>
</element>
<element name="M4" library="MF_LEDs" package="LED0603" value="MF-LED-0603-RED">
<attribute name="MFG#" value="N/A"/>
<attribute name="NAME"/>
</element>
<element name="M8" library="MF_LEDs" package="LED0603" value="MF-LED-0603-RED">
<attribute name="MFG#" value="N/A"/>
<attribute name="NAME"/>
</element>
<element name="M16" library="MF_LEDs" package="LED0603" value="MF-LED-0603-RED">
<attribute name="MFG#" value="N/A"/>
<attribute name="NAME"/>
</element>
<element name="M32" library="MF_LEDs" package="LED0603" value="MF-LED-0603-RED">
<attribute name="MFG#" value="N/A"/>
<attribute name="NAME"/>
</element>
<element name="H1" library="MF_LEDs" package="LED0603" value="MF-LED-0603-GREEN">
<attribute name="NAME"/>
<attribute name="MFG#" value="N/A"/>
</element>
<element name="H2" library="MF_LEDs" package="LED0603" value="MF-LED-0603-GREEN">
<attribute name="NAME"/>
<attribute name="MFG#" value="N/A"/>
</element>
<element name="H4" library="MF_LEDs" package="LED0603" value="MF-LED-0603-GREEN">
<attribute name="NAME"/>
<attribute name="MFG#" value="N/A"/>
</element>
<element name="H8" library="MF_LEDs" package="LED0603" value="MF-LED-0603-GREEN">
<attribute name="NAME"/>
<attribute name="MFG#" value="N/A"/>
</element>
<element name="X1" library="MF_Frequency_Control" package="ECX-31B_SERIES" value="ECS-.327-12.5-34B-TR"/>
<element name="C4" library="MF_Passives" package="C0402" value="500R07S120KV4T">
<attribute name="TOLERANCE" value="N/A"/>
<attribute name="MFG#" value="N/A"/>
<attribute name="VOLTAGE" value="N/A"/>
<attribute name="TEMP_COF" value="N/A"/>
</element>
<element name="C5" library="MF_Passives" package="C0402" value="500R07S120KV4T">
<attribute name="TOLERANCE" value="N/A"/>
<attribute name="MFG#" value="N/A"/>
<attribute name="VOLTAGE" value="N/A"/>
<attribute name="TEMP_COF" value="N/A"/>
</element>
<element name="SEC" library="MF_LEDs" package="LED0603" value="MF-LED-0603-RED">
<attribute name="NAME"/>
<attribute name="MFG#" value="N/A"/>
</element>
<element name="FID1" library="MF_Aesthetics" package="FIDUCIAL_0.5MM" value="FIDUCIAL_0.5MM"/>
<element name="FID2" library="MF_Aesthetics" package="FIDUCIAL_0.5MM" value="FIDUCIAL_0.5MM"/>
<element name="FID3" library="MF_Aesthetics" package="FIDUCIAL_0.5MM" value="FIDUCIAL_0.5MM"/>
<element name="FID4" library="MF_Aesthetics" package="FIDUCIAL_0.5MM" value="FIDUCIAL_0.5MM"/>
<element name="U$1" library="PP_Aesthetics" package="MF_LOGO_SMALL" value="MF_LOGOLOGO_SMALL"/>
<element name="U1" library="MF_IC_Digital" package="EFM8SB10F(2/4/8)G-A-QFN20" value="EFM8SB10F2G-A-QFN20R"/>
<element name="R2" library="MF_Passives" package="R0402" value="MF-RES-0402-10K">
<attribute name="VOLTAGE" value="N/A"/>
<attribute name="TOLERANCE" value="N/A"/>
<attribute name="WATTAGE" value="N/A"/>
<attribute name="MFG#" value="N/A"/>
</element>
<element name="R3" library="MF_Passives" package="R0402" value="MF-RES-0402-75">
<attribute name="VOLTAGE" value="N/A"/>
<attribute name="TOLERANCE" value="N/A"/>
<attribute name="WATTAGE" value="N/A"/>
<attribute name="MFG#" value="N/A"/>
</element>
<element name="R4" library="MF_Passives" package="R0402" value="MF-RES-0402-75">
<attribute name="VOLTAGE" value="N/A"/>
<attribute name="TOLERANCE" value="N/A"/>
<attribute name="WATTAGE" value="N/A"/>
<attribute name="MFG#" value="N/A"/>
</element>
<element name="R5" library="MF_Passives" package="R0402" value="MF-RES-0402-75">
<attribute name="VOLTAGE" value="N/A"/>
<attribute name="TOLERANCE" value="N/A"/>
<attribute name="WATTAGE" value="N/A"/>
<attribute name="MFG#" value="N/A"/>
</element>
<element name="R6" library="MF_Passives" package="R0402" value="MF-RES-0402-75">
<attribute name="VOLTAGE" value="N/A"/>
<attribute name="TOLERANCE" value="N/A"/>
<attribute name="WATTAGE" value="N/A"/>
<attribute name="MFG#" value="N/A"/>
</element>
<element name="R7" library="MF_Passives" package="R0402" value="MF-RES-0402-75">
<attribute name="VOLTAGE" value="N/A"/>
<attribute name="TOLERANCE" value="N/A"/>
<attribute name="WATTAGE" value="N/A"/>
<attribute name="MFG#" value="N/A"/>
</element>
<element name="R8" library="MF_Passives" package="R0402" value="MF-RES-0402-75">
<attribute name="VOLTAGE" value="N/A"/>
<attribute name="TOLERANCE" value="N/A"/>
<attribute name="WATTAGE" value="N/A"/>
<attribute name="MFG#" value="N/A"/>
</element>
<element name="R9" library="MF_Passives" package="R0402" value="MF-RES-0402-75">
<attribute name="VOLTAGE" value="N/A"/>
<attribute name="TOLERANCE" value="N/A"/>
<attribute name="WATTAGE" value="N/A"/>
<attribute name="MFG#" value="N/A"/>
</element>
<element name="R10" library="MF_Passives" package="R0402" value="MF-RES-0402-75">
<attribute name="VOLTAGE" value="N/A"/>
<attribute name="TOLERANCE" value="N/A"/>
<attribute name="WATTAGE" value="N/A"/>
<attribute name="MFG#" value="N/A"/>
</element>
<element name="R11" library="MF_Passives" package="R0402" value="MF-RES-0402-75">
<attribute name="VOLTAGE" value="N/A"/>
<attribute name="TOLERANCE" value="N/A"/>
<attribute name="WATTAGE" value="N/A"/>
<attribute name="MFG#" value="N/A"/>
</element>
<element name="R12" library="MF_Passives" package="R0402" value="MF-RES-0402-75">
<attribute name="VOLTAGE" value="N/A"/>
<attribute name="TOLERANCE" value="N/A"/>
<attribute name="WATTAGE" value="N/A"/>
<attribute name="MFG#" value="N/A"/>
</element>
<element name="R13" library="MF_Passives" package="R0402" value="MF-RES-0402-75">
<attribute name="VOLTAGE" value="N/A"/>
<attribute name="TOLERANCE" value="N/A"/>
<attribute name="WATTAGE" value="N/A"/>
<attribute name="MFG#" value="N/A"/>
</element>
<element name="J1" library="PP_Connectors" package="TC2030" value="">
<attribute name="LABEL06" value=""/>
<attribute name="LABEL04" value="C2D"/>
<attribute name="LABEL03" value="C2CK"/>
<attribute name="LABEL01" value="GND"/>
<attribute name="LABEL02" value="3.0V"/>
<attribute name="LABEL05" value=""/>
</element>
<element name="PP1" library="MF_Connectors" package="POGO_PIN_70-9150" value="">
<attribute name="LABEL00" value="P0.7"/>
</element>
</elements>
<signals>
<signal name="3.0V">
<contactref element="BATT1" pad="POS_0"/>
<contactref element="BATT1" pad="POS_1"/>
<contactref element="R1" pad="P$2"/>
<contactref element="U1" pad="P$4"/>
<contactref element="C1" pad="P$1"/>
<contactref element="C2" pad="P$1"/>
<contactref element="R2" pad="P$1"/>
<contactref element="J1" pad="P$2"/>
</signal>
<signal name="GND">
<contactref element="TIME?" pad="P$4"/>
<contactref element="C4" pad="P$2"/>
<contactref element="C5" pad="P$2"/>
<contactref element="R13" pad="P$2"/>
<contactref element="R3" pad="P$2"/>
<contactref element="R4" pad="P$2"/>
<contactref element="R5" pad="P$2"/>
<contactref element="R6" pad="P$2"/>
<contactref element="R7" pad="P$2"/>
<contactref element="R8" pad="P$2"/>
<contactref element="R9" pad="P$2"/>
<contactref element="R10" pad="P$2"/>
<contactref element="R11" pad="P$2"/>
<contactref element="R12" pad="P$2"/>
<contactref element="J1" pad="P$1"/>
<contactref element="BATT1" pad="NEG_0"/>
<contactref element="U1" pad="P$3"/>
<contactref element="U1" pad="P$12"/>
<contactref element="U1" pad="PAD"/>
<contactref element="C1" pad="P$2"/>
<contactref element="C2" pad="P$2"/>
</signal>
<signal name="X1">
<contactref element="U1" pad="P$7"/>
<contactref element="X1" pad="P$2"/>
<contactref element="C5" pad="P$1"/>
</signal>
<signal name="H8">
<contactref element="H8" pad="ANODE"/>
<contactref element="U1" pad="P$9"/>
</signal>
<signal name="H4">
<contactref element="H4" pad="ANODE"/>
<contactref element="U1" pad="P$10"/>
</signal>
<signal name="H2">
<contactref element="H2" pad="ANODE"/>
<contactref element="U1" pad="P$11"/>
</signal>
<signal name="H1">
<contactref element="H1" pad="ANODE"/>
<contactref element="U1" pad="P$13"/>
</signal>
<signal name="M2">
<contactref element="M2" pad="ANODE"/>
<contactref element="U1" pad="P$18"/>
</signal>
<signal name="M4">
<contactref element="M4" pad="ANODE"/>
<contactref element="U1" pad="P$19"/>
</signal>
<signal name="M8">
<contactref element="M8" pad="ANODE"/>
<contactref element="U1" pad="P$20"/>
</signal>
<signal name="M16">
<contactref element="M16" pad="ANODE"/>
<contactref element="U1" pad="P$1"/>
</signal>
<signal name="M32">
<contactref element="M32" pad="ANODE"/>
<contactref element="U1" pad="P$2"/>
</signal>
<signal name="SEC">
<contactref element="SEC" pad="ANODE"/>
<contactref element="U1" pad="P$14"/>
</signal>
<signal name="SW">
<contactref element="TIME?" pad="P$1"/>
<contactref element="U1" pad="P$16"/>
</signal>
<signal name="M1">
<contactref element="M1" pad="ANODE"/>
<contactref element="U1" pad="P$17"/>
</signal>
<signal name="N$1">
<contactref element="TIME?" pad="P$2"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="M1" pad="CATHODE"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="N$7">
<contactref element="M2" pad="CATHODE"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="N$8">
<contactref element="M4" pad="CATHODE"/>
<contactref element="R5" pad="P$1"/>
</signal>
<signal name="N$9">
<contactref element="M8" pad="CATHODE"/>
<contactref element="R6" pad="P$1"/>
</signal>
<signal name="N$10">
<contactref element="M16" pad="CATHODE"/>
<contactref element="R7" pad="P$1"/>
</signal>
<signal name="N$11">
<contactref element="M32" pad="CATHODE"/>
<contactref element="R8" pad="P$1"/>
</signal>
<signal name="N$12">
<contactref element="H1" pad="CATHODE"/>
<contactref element="R9" pad="P$1"/>
</signal>
<signal name="N$13">
<contactref element="H2" pad="CATHODE"/>
<contactref element="R10" pad="P$1"/>
</signal>
<signal name="N$14">
<contactref element="H4" pad="CATHODE"/>
<contactref element="R11" pad="P$1"/>
</signal>
<signal name="N$15">
<contactref element="H8" pad="CATHODE"/>
<contactref element="R12" pad="P$1"/>
</signal>
<signal name="N$16">
<contactref element="SEC" pad="CATHODE"/>
<contactref element="R13" pad="P$1"/>
</signal>
<signal name="X0">
<contactref element="U1" pad="P$8"/>
<contactref element="C4" pad="P$1"/>
<contactref element="X1" pad="P$1"/>
</signal>
<signal name="C2D">
<contactref element="J1" pad="P$4"/>
<contactref element="U1" pad="P$6"/>
</signal>
<signal name="C2CK">
<contactref element="J1" pad="P$3"/>
<contactref element="U1" pad="P$5"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="EXTRA">
<contactref element="U1" pad="P$15"/>
<contactref element="PP1" pad="P$1"/>
</signal>
<signal name="N$2">
</signal>
</signals>
</board>
</drawing>
</eagle>
