<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="6.430415625" x2="6.430415625" y2="0" width="0" layer="20" curve="90"/>
<wire x1="6.430415625" y1="0" x2="38.1504625" y2="0" width="0" layer="20"/>
<wire x1="38.1504625" y1="0" x2="41.91" y2="3.81" width="0" layer="20" curve="90.763913"/>
<wire x1="41.91" y1="3.81" x2="41.91" y2="6.985" width="0" layer="20"/>
<wire x1="41.91" y1="6.985" x2="41.927359375" y2="8.96145" width="0" layer="20"/>
<wire x1="41.927359375" y1="8.96145" x2="38.130828125" y2="12.7807" width="0" layer="20" curve="90.666275"/>
<wire x1="38.130828125" y1="12.7807" x2="6.259584375" y2="12.69" width="0" layer="20"/>
<wire x1="6.259584375" y1="12.69" x2="0" y2="6.430415625" width="0" layer="20" curve="90"/>
<hole x="3.81" y="6.35" drill="2.8"/>
</plain>
<libraries>
<library name="capacitor-wima">
<description>&lt;b&gt;WIMA Capacitors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="C5B7.2">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 7.5 x 7.2 mm, grid 5.08 mm</description>
</package>
</packages>
</library>
<library name="inductors">
<description>&lt;b&gt;Inductors and Filters&lt;/b&gt;&lt;p&gt;
Based on the previous library ind-a.lbr&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DR74">
<description>&lt;b&gt;High Power Density, High Efficiency, Shielded Inductors&lt;/b&gt;&lt;p&gt;
Source: coiltronics_dr_series.pdf</description>
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="P1-20Y">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ALI-Express-Conn">
<packages>
<package name="PJ313D">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="capacitor-wima" package="C5B7.2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="inductors" package="DR74" value="DR74">
<attribute name="NAME"/>
</element>
<element name="T1" library="transistor" package="SOT23" value="BC846"/>
<element name="TP1" library="testpad" package="P1-20Y" value="TPPAD1-20Y">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP2" library="testpad" package="P1-20Y" value="TPPAD1-20Y">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="ALI-Express-Conn" package="PJ313D" value="PJ313D"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="T1" pad="3"/>
<contactref element="T1" pad="1"/>
<contactref element="L1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="TP1" pad="TP"/>
</signal>
<signal name="N$2">
<contactref element="T1" pad="2"/>
<contactref element="U$1" pad="S1"/>
<contactref element="U$1" pad="S2"/>
</signal>
<signal name="N$3">
<contactref element="C1" pad="2"/>
<contactref element="L1" pad="1"/>
<contactref element="U$1" pad="LEFT1"/>
<contactref element="U$1" pad="LEFT2"/>
<contactref element="TP2" pad="TP"/>
</signal>
<signal name="N$5">
</signal>
<signal name="N$6">
</signal>
<signal name="N$7">
</signal>
<signal name="N$8">
</signal>
<signal name="N$9">
</signal>
<signal name="N$10">
</signal>
<signal name="N$11">
</signal>
<signal name="N$4">
</signal>
<signal name="N$12">
</signal>
</signals>
</board>
</drawing>
</eagle>
