(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+5V")
  (net 2 "GND")
  (net 3 "/DIN_PAD")
  (net 4 "/DOUT_PAD")
  (net 5 "/DIN_LED")
  (net 6 "/DOUT_LED")
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 116.047185 91.209338 135)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.43 135) (layer "F.Fab"))
    (fp_text value "100nF" (at 0 1.43 135) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 135) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 135) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 117.124815 76.985338 45)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.43 45) (layer "F.Fab"))
    (fp_text value "22" (at 0 1.43 45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 45) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/DOUT_LED") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 45) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/DOUT_PAD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 111.736662 71.597185 45)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.43 45) (layer "F.Fab"))
    (fp_text value "100nF" (at 0 1.43 45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 45) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 45) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 116.586 86.36 135)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -3.5 135) (layer "F.Fab"))
    (fp_text value "WS2812B" (at 0 4 135) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.732843 -1.65 135) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -2.732843 1.65 135) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/DOUT_LED") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd roundrect (at 2.732843 1.65 135) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd roundrect (at 2.732843 -1.65 135) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/DIN_LED") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom_Library:Pin_Header_01x01" (layer "F.Cu")
    (tedit 56049531)
    (at 112.993898 89.952102 -135)
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 0 2.54 -315) (layer "F.Fab"))
    (fp_text value "DIN" (at 0 -2.54 -315) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 225) (size 2.2 2.2) (drill 1.2) (layers F&B.Cu *.Mask)
      (net 3 "/DIN_PAD") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Custom_Library:Mousebite_3x_D0.3_P0.8" (layer "F.Cu")
    (tedit 5D6B2A2B)
    (at 130.81 78.486 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0) (layer "F.Fab") hide)
    (fp_text value "Mousebite_3x_D0.3_P0.8" (at 0 -0.25) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -0.799999 0 180) (size 0.4 0.4) (drill 0.4) (layers *.Mask)
      (solder_mask_margin 0.001))
    (pad "" np_thru_hole circle locked (at 0.799999 0 180) (size 0.4 0.4) (drill 0.4) (layers *.Mask)
      (solder_mask_margin 0.001))
    (pad "" np_thru_hole circle locked (at 0 0 180) (size 0.4 0.4) (drill 0.4) (layers *.Mask)
      (solder_mask_margin 0.001))
  )
  (footprint "Custom_Library:Mousebite_3x_D0.3_P0.8" (layer "F.Cu")
    (tedit 5D6B2A2B)
    (at 130.81 80.01 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0) (layer "F.Fab") hide)
    (fp_text value "Mousebite_3x_D0.3_P0.8" (at 0 -0.25) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -0.799999 0 180) (size 0.4 0.4) (drill 0.4) (layers *.Mask)
      (solder_mask_margin 0.001))
    (pad "" np_thru_hole circle locked (at 0.799999 0 180) (size 0.4 0.4) (drill 0.4) (layers *.Mask)
      (solder_mask_margin 0.001))
    (pad "" np_thru_hole circle (at 0 0.1 180) (size 0.4 0.4) (drill 0.4) (layers *.Mask)
      (solder_mask_margin 0.001))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 135.659338 71.597185 -45)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.43 -225) (layer "F.Fab"))
    (fp_text value "22" (at 0 1.43 -225) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -225) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 315) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/DIN_PAD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 315) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/DIN_LED") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom_Library:Pin_Header_01x01" (layer "F.Cu")
    (tedit 56049531)
    (at 134.402102 89.952102 -45)
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 0 2.54 135) (layer "F.Fab"))
    (fp_text value "DIN" (at 0 -2.54 135) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 315) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "/DIN_PAD") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Custom_Library:Pin_Header_01x01" (layer "F.Cu")
    (tedit 56049531)
    (at 112.993898 82.767898 -135)
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 2.54 -315) (layer "F.Fab"))
    (fp_text value "-" (at 0 -2.54 -315) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 225) (size 2.2 2.2) (drill 1.2) (layers F&B.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 131.348815 91.209338 -135)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.43 -315) (layer "F.Fab"))
    (fp_text value "22" (at 0 1.43 -315) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -315) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 225) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/DIN_PAD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 225) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/DIN_LED") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 130.81 72.136 -45)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -3.5 -225) (layer "F.Fab"))
    (fp_text value "WS2812B" (at 0 4 -225) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6 -225) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -225) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.732843 -1.65 315) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -2.732843 1.65 315) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/DOUT_LED") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd roundrect (at 2.732843 1.65 315) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd roundrect (at 2.732843 -1.65 315) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/DIN_LED") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 130.271185 81.510662 -135)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.43 -315) (layer "F.Fab"))
    (fp_text value "22" (at 0 1.43 -315) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -315) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 225) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/DOUT_LED") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 225) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/DOUT_PAD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom_Library:Pin_Header_01x01" (layer "F.Cu")
    (tedit 56049531)
    (at 134.402102 82.767898 -45)
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 2.54 135) (layer "F.Fab"))
    (fp_text value "+" (at 0 -2.921 135) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 315) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "+5V") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 121.435338 85.821185 135)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.43 135) (layer "F.Fab"))
    (fp_text value "22" (at 0 1.43 135) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 135) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/DOUT_LED") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 135) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/DOUT_PAD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom_Library:Mousebite_3x_D0.3_P0.8" (layer "F.Cu")
    (tedit 5D6B2A2B)
    (at 116.586 78.486 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0) (layer "F.Fab") hide)
    (fp_text value "Mousebite_3x_D0.3_P0.8" (at 0 -0.25) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 -0.1 180) (size 0.4 0.4) (drill 0.4) (layers *.Mask)
      (solder_mask_margin 0.001))
    (pad "" np_thru_hole circle locked (at -0.799999 0 180) (size 0.4 0.4) (drill 0.4) (layers *.Mask)
      (solder_mask_margin 0.001))
    (pad "" np_thru_hole circle locked (at 0.799999 0 180) (size 0.4 0.4) (drill 0.4) (layers *.Mask)
      (solder_mask_margin 0.001))
  )
  (footprint "Custom_Library:Pin_Header_01x01" (layer "F.Cu")
    (tedit 56049531)
    (at 120.178102 68.543898 135)
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 2.54 135) (layer "F.Fab"))
    (fp_text value "-" (at 0 -2.54 135) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 135) (size 2.2 2.2) (drill 1.2) (layers F&B.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 111.736662 86.898815 135)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.43 135) (layer "F.Fab"))
    (fp_text value "22" (at 0 1.43 135) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 135) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/DIN_PAD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 135) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/DIN_LED") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 131.348815 67.286662 -45)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.43 -225) (layer "F.Fab"))
    (fp_text value "100nF" (at 0 1.43 -225) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -225) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 315) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 315) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 125.960662 72.674815 -45)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.43 -225) (layer "F.Fab"))
    (fp_text value "22" (at 0 1.43 -225) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -225) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 315) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/DOUT_LED") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 315) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/DOUT_PAD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom_Library:Mousebite_3x_D0.3_P0.8" (layer "F.Cu")
    (tedit 5D6B2A2B)
    (at 122.936 86.36 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0 90) (layer "F.Fab") hide)
    (fp_text value "Mousebite_3x_D0.3_P0.8" (at 0 -0.25 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0.799999 0 90) (size 0.4 0.4) (drill 0.4) (layers *.Mask)
      (solder_mask_margin 0.001))
    (pad "" np_thru_hole circle (at 0 0.1 90) (size 0.4 0.4) (drill 0.4) (layers *.Mask)
      (solder_mask_margin 0.001))
    (pad "" np_thru_hole circle locked (at -0.799999 0 90) (size 0.4 0.4) (drill 0.4) (layers *.Mask)
      (solder_mask_margin 0.001))
  )
  (footprint "Custom_Library:Pin_Header_01x01" (layer "F.Cu")
    (tedit 56049531)
    (at 134.402102 68.543898 45)
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 0 2.54 45) (layer "F.Fab"))
    (fp_text value "DIN" (at 0 -2.54 45) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 45) (size 2.2 2.2) (drill 1.2) (layers F&B.Cu *.Mask)
      (net 3 "/DIN_PAD") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Custom_Library:Pin_Header_01x01" (layer "F.Cu")
    (tedit 56049531)
    (at 134.402102 75.728102 45)
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 2.54 45) (layer "F.Fab"))
    (fp_text value "-" (at 0 -2.54 45) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 45) (size 2.2 2.2) (drill 1.2) (layers F&B.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Custom_Library:Pin_Header_01x01" (layer "F.Cu")
    (tedit 56049531)
    (at 112.993898 68.543898 135)
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 0 2.54 135) (layer "F.Fab"))
    (fp_text value "DIN" (at 0 -2.54 135) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 135) (size 2.2 2.2) (drill 1.2) (layers F&B.Cu *.Mask)
      (net 3 "/DIN_PAD") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Custom_Library:Mousebite_3x_D0.3_P0.8" (layer "F.Cu")
    (tedit 5D6B2A2B)
    (at 122.936 72.136 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0 90) (layer "F.Fab") hide)
    (fp_text value "Mousebite_3x_D0.3_P0.8" (at 0 -0.25 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0 90) (size 0.4 0.4) (drill 0.4) (layers *.Mask)
      (solder_mask_margin 0.001))
    (pad "" np_thru_hole circle locked (at 0.799999 0 90) (size 0.4 0.4) (drill 0.4) (layers *.Mask)
      (solder_mask_margin 0.001))
    (pad "" np_thru_hole circle locked (at -0.799999 0 90) (size 0.4 0.4) (drill 0.4) (layers *.Mask)
      (solder_mask_margin 0.001))
  )
  (footprint "Custom_Library:Mousebite_3x_D0.3_P0.8" (layer "F.Cu")
    (tedit 5D6B2A2B)
    (at 124.46 86.36 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0 90) (layer "F.Fab") hide)
    (fp_text value "Mousebite_3x_D0.3_P0.8" (at 0 -0.25 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0.799999 0 90) (size 0.4 0.4) (drill 0.4) (layers *.Mask)
      (solder_mask_margin 0.001))
    (pad "" np_thru_hole circle locked (at 0 0 90) (size 0.4 0.4) (drill 0.4) (layers *.Mask)
      (solder_mask_margin 0.001))
    (pad "" np_thru_hole circle locked (at -0.799999 0 90) (size 0.4 0.4) (drill 0.4) (layers *.Mask)
      (solder_mask_margin 0.001))
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 116.586 72.136 45)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -3.5 45) (layer "F.Fab"))
    (fp_text value "WS2812B" (at 0 4 45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6 45) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.732843 -1.65 45) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -2.732843 1.65 45) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/DOUT_LED") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd roundrect (at 2.732843 1.65 45) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd roundrect (at 2.732843 -1.65 45) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/DIN_LED") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom_Library:Pin_Header_01x01" (layer "F.Cu")
    (tedit 56049531)
    (at 127.217898 89.952102 -45)
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 2.54 135) (layer "F.Fab"))
    (fp_text value "-" (at 0 -2.54 135) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 315) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Custom_Library:Pin_Header_01x01" (layer "F.Cu")
    (tedit 56049531)
    (at 127.217898 68.543898 45)
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 2.54 45) (layer "F.Fab"))
    (fp_text value "+" (at 0 -2.921 45) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 45) (size 2.2 2.2) (drill 1.2) (layers F&B.Cu *.Mask)
      (net 1 "+5V") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Custom_Library:Pin_Header_01x01" (layer "F.Cu")
    (tedit 56049531)
    (at 120.178102 82.767898 -45)
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 2.54 135) (layer "F.Fab"))
    (fp_text value "DOUT" (at 0 -2.54 135) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 315) (size 2.2 2.2) (drill 1.2) (layers F&B.Cu *.Mask)
      (net 4 "/DOUT_PAD") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Custom_Library:Mousebite_3x_D0.3_P0.8" (layer "F.Cu")
    (tedit 5D6B2A2B)
    (at 116.586 80.01 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0) (layer "F.Fab") hide)
    (fp_text value "Mousebite_3x_D0.3_P0.8" (at 0 -0.25) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -0.799999 0 180) (size 0.4 0.4) (drill 0.4) (layers *.Mask)
      (solder_mask_margin 0.001))
    (pad "" np_thru_hole circle locked (at 0 0 180) (size 0.4 0.4) (drill 0.4) (layers *.Mask)
      (solder_mask_margin 0.001))
    (pad "" np_thru_hole circle locked (at 0.799999 0 180) (size 0.4 0.4) (drill 0.4) (layers *.Mask)
      (solder_mask_margin 0.001))
  )
  (footprint "Custom_Library:Pin_Header_01x01" (layer "F.Cu")
    (tedit 56049531)
    (at 112.993898 75.728102 135)
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 2.54 135) (layer "F.Fab"))
    (fp_text value "+" (at 0 -2.921 135) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 135) (size 2.2 2.2) (drill 1.2) (layers F&B.Cu *.Mask)
      (net 1 "+5V") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Custom_Library:Pin_Header_01x01" (layer "F.Cu")
    (tedit 56049531)
    (at 127.217898 75.728102 135)
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 2.54 135) (layer "F.Fab"))
    (fp_text value "DOUT" (at 0 -2.54 135) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 135) (size 2.2 2.2) (drill 1.2) (layers F&B.Cu *.Mask)
      (net 4 "/DOUT_PAD") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 116.047185 67.286662 45)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.43 45) (layer "F.Fab"))
    (fp_text value "22" (at 0 1.43 45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 45) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/DIN_PAD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 45) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/DIN_LED") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom_Library:Mousebite_3x_D0.3_P0.8" (layer "F.Cu")
    (tedit 5D6B2A2B)
    (at 124.46 72.136 90)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 0 90) (layer "F.Fab") hide)
    (fp_text value "Mousebite_3x_D0.3_P0.8" (at 0 -0.25 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -0.799999 0 90) (size 0.4 0.4) (drill 0.4) (layers *.Mask)
      (solder_mask_margin 0.001))
    (pad "" np_thru_hole circle (at 0 -0.1 90) (size 0.4 0.4) (drill 0.4) (layers *.Mask)
      (solder_mask_margin 0.001))
    (pad "" np_thru_hole circle locked (at 0.799999 0 90) (size 0.4 0.4) (drill 0.4) (layers *.Mask)
      (solder_mask_margin 0.001))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 135.659338 86.898815 -135)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.43 -315) (layer "F.Fab"))
    (fp_text value "100nF" (at 0 1.43 -315) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -315) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 225) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 225) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 130.81 86.36 -135)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -3.5 -315) (layer "F.Fab"))
    (fp_text value "WS2812B" (at 0 4 -315) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6 -315) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -315) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.732843 -1.65 225) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -2.732843 1.65 225) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/DOUT_LED") (pinfunction "DOUT") (pintype "output"))
    (pad "3" smd roundrect (at 2.732843 1.65 225) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd roundrect (at 2.732843 -1.65 225) (size 2 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/DIN_LED") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom_Library:Pin_Header_01x01" (layer "F.Cu")
    (tedit 56049531)
    (at 127.217898 82.767898 45)
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 2.54 45) (layer "F.Fab"))
    (fp_text value "DOUT" (at 0 -2.54 45) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 45) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "/DOUT_PAD") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Custom_Library:Pin_Header_01x01" (layer "F.Cu")
    (tedit 56049531)
    (at 120.178102 75.728102 -135)
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 2.54 -315) (layer "F.Fab"))
    (fp_text value "DOUT" (at 0 -2.54 -315) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 225) (size 2.2 2.2) (drill 1.2) (layers F&B.Cu *.Mask)
      (net 4 "/DOUT_PAD") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Custom_Library:Pin_Header_01x01" (layer "F.Cu")
    (tedit 56049531)
    (at 120.178102 89.952102 -135)
    (property "Sheetfile" "Sewable Neopixel.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 2.54 -315) (layer "F.Fab"))
    (fp_text value "+" (at 0 -2.921 -315) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 225) (size 2.2 2.2) (drill 1.2) (layers F&B.Cu *.Mask)
      (net 1 "+5V") (pinfunction "Pin_1") (pintype "passive"))
  )
  (gr_arc (start 129.285994 78.300406) (mid 126.319872 76.626128) (end 124.645594 73.660006) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 122.750406 73.660006) (mid 121.076128 76.626128) (end 118.110006 78.300406) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 115.061994 78.300406) (mid 112.095872 67.645872) (end 122.750406 70.611994) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 132.334006 80.195594) (mid 135.300128 90.850128) (end 124.645594 87.884006) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 122.750406 87.884006) (mid 112.095872 90.850128) (end 115.061994 80.195594) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 132.334 80.195594) (end 132.334 78.300406) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 129.286 80.195594) (end 129.286 78.300406) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 115.062 80.195594) (end 115.062 78.300406) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 118.110006 80.195594) (mid 121.076128 81.869872) (end 122.750406 84.835994) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 122.750406 70.612) (end 124.645594 70.612) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 118.11 80.195594) (end 118.11 78.300406) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 122.750406 84.836) (end 124.645594 84.836) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 122.750406 73.66) (end 124.645594 73.66) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 122.750406 87.884) (end 124.645594 87.884) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 124.645594 70.611994) (mid 135.300128 67.645872) (end 132.334006 78.300406) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 124.645594 84.835994) (mid 126.319872 81.869872) (end 129.285994 80.195594) (layer "Edge.Cuts") (width 0.1))
  (gr_text "Sewable\nNeopixel v1" (at 129.373159 73.572841 135) (layer "B.SilkS"))
  (gr_text "Sewable\nNeopixel v1" (at 118.022841 84.923159 315) (layer "B.SilkS"))
  (gr_text "Dec 2022" (at 114.969554 87.976446 315) (layer "B.SilkS"))
  (gr_text "Dec 2022" (at 132.426446 70.519554 135) (layer "B.SilkS"))
  (gr_text "Sewable\nNeopixel v1" (at 118.022841 73.572841 225) (layer "B.SilkS"))
  (gr_text "Dec 2022" (at 132.426446 87.976446 45) (layer "B.SilkS"))
  (gr_text "Dec 2022" (at 114.969554 70.519554 225) (layer "B.SilkS"))
  (gr_text "Sewable\nNeopixel v1" (at 129.373159 84.923159 45) (layer "B.SilkS"))
  (zone (net 1) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.5))
    (polygon
      (pts
        (xy 112.006069 90.939931)
        (xy 110.928439 89.682695)
        (xy 112.006069 88.964274)
        (xy 112.814292 88.694867)
        (xy 113.532713 88.982235)
        (xy 113.963765 89.413287)
        (xy 114.251133 90.131708)
        (xy 113.981726 90.939931)
        (xy 113.263305 92.017561)
      )
    )
  )
  (zone (net 1) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.5))
    (polygon
      (pts
        (xy 135.389931 67.556069)
        (xy 136.467561 68.813305)
        (xy 135.389931 69.531726)
        (xy 134.581708 69.801133)
        (xy 133.863287 69.513765)
        (xy 133.432235 69.082713)
        (xy 133.144867 68.364292)
        (xy 133.414274 67.556069)
        (xy 134.132695 66.478439)
      )
    )
  )
  (zone (net 1) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.5))
    (polygon
      (pts
        (xy 121.165931 67.556069)
        (xy 122.243561 68.813305)
        (xy 121.165931 69.531726)
        (xy 120.357708 69.801133)
        (xy 119.639287 69.513765)
        (xy 119.208235 69.082713)
        (xy 118.920867 68.364292)
        (xy 119.190274 67.556069)
        (xy 119.908695 66.478439)
      )
    )
  )
  (zone (net 1) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.5))
    (polygon
      (pts
        (xy 135.389931 76.715931)
        (xy 134.132695 77.793561)
        (xy 133.414274 76.715931)
        (xy 133.144867 75.907708)
        (xy 133.432235 75.189287)
        (xy 133.863287 74.758235)
        (xy 134.581708 74.470867)
        (xy 135.389931 74.740274)
        (xy 136.467561 75.458695)
      )
    )
  )
  (zone (net 1) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.5))
    (polygon
      (pts
        (xy 121.165931 81.780069)
        (xy 122.243561 83.037305)
        (xy 121.165931 83.755726)
        (xy 120.357708 84.025133)
        (xy 119.639287 83.737765)
        (xy 119.208235 83.306713)
        (xy 118.920867 82.588292)
        (xy 119.190274 81.780069)
        (xy 119.908695 80.702439)
      )
    )
  )
  (zone (net 1) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.5))
    (polygon
      (pts
        (xy 126.230069 67.556069)
        (xy 127.487305 66.478439)
        (xy 128.205726 67.556069)
        (xy 128.475133 68.364292)
        (xy 128.187765 69.082713)
        (xy 127.756713 69.513765)
        (xy 127.038292 69.801133)
        (xy 126.230069 69.531726)
        (xy 125.152439 68.813305)
      )
    )
  )
  (zone (net 1) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.5))
    (polygon
      (pts
        (xy 112.006069 76.715931)
        (xy 110.928439 75.458695)
        (xy 112.006069 74.740274)
        (xy 112.814292 74.470867)
        (xy 113.532713 74.758235)
        (xy 113.963765 75.189287)
        (xy 114.251133 75.907708)
        (xy 113.981726 76.715931)
        (xy 113.263305 77.793561)
      )
    )
  )
  (zone (net 1) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.5))
    (polygon
      (pts
        (xy 121.165931 76.715931)
        (xy 119.908695 77.793561)
        (xy 119.190274 76.715931)
        (xy 118.920867 75.907708)
        (xy 119.208235 75.189287)
        (xy 119.639287 74.758235)
        (xy 120.357708 74.470867)
        (xy 121.165931 74.740274)
        (xy 122.243561 75.458695)
      )
    )
  )
  (zone (net 1) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.5))
    (polygon
      (pts
        (xy 135.389931 81.780069)
        (xy 136.467561 83.037305)
        (xy 135.389931 83.755726)
        (xy 134.581708 84.025133)
        (xy 133.863287 83.737765)
        (xy 133.432235 83.306713)
        (xy 133.144867 82.588292)
        (xy 133.414274 81.780069)
        (xy 134.132695 80.702439)
      )
    )
  )
  (zone (net 1) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.5))
    (polygon
      (pts
        (xy 135.389931 90.939931)
        (xy 134.132695 92.017561)
        (xy 133.414274 90.939931)
        (xy 133.144867 90.131708)
        (xy 133.432235 89.413287)
        (xy 133.863287 88.982235)
        (xy 134.581708 88.694867)
        (xy 135.389931 88.964274)
        (xy 136.467561 89.682695)
      )
    )
  )
  (zone (net 1) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.5))
    (polygon
      (pts
        (xy 126.230069 81.780069)
        (xy 127.487305 80.702439)
        (xy 128.205726 81.780069)
        (xy 128.475133 82.588292)
        (xy 128.187765 83.306713)
        (xy 127.756713 83.737765)
        (xy 127.038292 84.025133)
        (xy 126.230069 83.755726)
        (xy 125.152439 83.037305)
      )
    )
  )
  (zone (net 1) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.5))
    (polygon
      (pts
        (xy 121.165931 90.939931)
        (xy 119.908695 92.017561)
        (xy 119.190274 90.939931)
        (xy 118.920867 90.131708)
        (xy 119.208235 89.413287)
        (xy 119.639287 88.982235)
        (xy 120.357708 88.694867)
        (xy 121.165931 88.964274)
        (xy 122.243561 89.682695)
      )
    )
  )
  (zone (net 1) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.5))
    (polygon
      (pts
        (xy 112.006069 67.556069)
        (xy 113.263305 66.478439)
        (xy 113.981726 67.556069)
        (xy 114.251133 68.364292)
        (xy 113.963765 69.082713)
        (xy 113.532713 69.513765)
        (xy 112.814292 69.801133)
        (xy 112.006069 69.531726)
        (xy 110.928439 68.813305)
      )
    )
  )
  (zone (net 1) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.5))
    (polygon
      (pts
        (xy 126.230069 76.715931)
        (xy 125.152439 75.458695)
        (xy 126.230069 74.740274)
        (xy 127.038292 74.470867)
        (xy 127.756713 74.758235)
        (xy 128.187765 75.189287)
        (xy 128.475133 75.907708)
        (xy 128.205726 76.715931)
        (xy 127.487305 77.793561)
      )
    )
  )
  (zone (net 1) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.5))
    (polygon
      (pts
        (xy 126.230069 90.939931)
        (xy 125.152439 89.682695)
        (xy 126.230069 88.964274)
        (xy 127.038292 88.694867)
        (xy 127.756713 88.982235)
        (xy 128.187765 89.413287)
        (xy 128.475133 90.131708)
        (xy 128.205726 90.939931)
        (xy 127.487305 92.017561)
      )
    )
  )
  (zone (net 1) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.5))
    (polygon
      (pts
        (xy 112.006069 81.780069)
        (xy 113.263305 80.702439)
        (xy 113.981726 81.780069)
        (xy 114.251133 82.588292)
        (xy 113.963765 83.306713)
        (xy 113.532713 83.737765)
        (xy 112.814292 84.025133)
        (xy 112.006069 83.755726)
        (xy 110.928439 83.037305)
      )
    )
  )
)
