(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 27)
    (no_connects 0)
    (area 134.956499 94.316499 185.083501 144.443501)
    (thickness 1.6002)
    (drawings 2)
    (tracks 119)
    (zones 0)
    (modules 10)
    (nets 23)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (grid_origin 160.02 119.38)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory CAM/))
  )
  (net 0 "")
  (net 1 "Net-(LED1-Pad1-DO)")
  (net 2 +5V)
  (net 3 GND)
  (net 4 /Anode)
  (net 5 /HV12)
  (net 6 /HV6)
  (net 7 /HV11)
  (net 8 /HV5)
  (net 9 /HV10)
  (net 10 /HV4)
  (net 11 /HV9)
  (net 12 /HV3)
  (net 13 /HV8)
  (net 14 /HV2)
  (net 15 /HV7)
  (net 16 /HV1)
  (net 17 "Net-(J1-Pad15)")
  (net 18 /Din)
  (net 19 "Net-(LED2-Pad1-DO)")
  (net 20 "Net-(NX1-PadA)")
  (net 21 "Net-(NX1-PadT)")
  (net 22 "Net-(NX1-PadB)")
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +5V)
    (add_net /Anode)
    (add_net /Din)
    (add_net /HV1)
    (add_net /HV10)
    (add_net /HV11)
    (add_net /HV12)
    (add_net /HV2)
    (add_net /HV3)
    (add_net /HV4)
    (add_net /HV5)
    (add_net /HV6)
    (add_net /HV7)
    (add_net /HV8)
    (add_net /HV9)
    (add_net GND)
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(LED1-Pad1-DO)")
    (add_net "Net-(LED2-Pad1-DO)")
    (add_net "Net-(NX1-PadA)")
    (add_net "Net-(NX1-PadB)")
    (add_net "Net-(NX1-PadT)")
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module Pin_Headers:Pin_Header_Straight_2x09_Pitch2.54mm (layer F.Cu) (tedit 5B664FF8)
    (at 170.18 99.38 270)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference J1 (at 1.27 -2.33 270) (layer F.SilkS) hide)
    (fp_text value Nixie (at 1.27 22.65 270) (layer F.Fab))
    (fp_text user %R (at 1.27 10.16 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /Anode))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /Anode))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /HV12))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /HV6))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /HV11))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /HV5))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /HV10))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /HV4))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /HV9))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /HV3))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /HV8))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /HV2))
    (pad 13 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /HV7))
    (pad 14 thru_hole oval (at 2.54 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /HV1))
    (pad 15 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /Din))
    (pad 17 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 18 thru_hole oval (at 2.54 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x09_Pitch2.54mm.wrl
      (at (xyz 0 0 -0.024))
      (scale (xyz 1 1 -1))
      (rotate (xyz 0 0 0))
    )
  )
  (module adafruit:adafruit-LED3535 (layer F.Cu) (tedit 5B664B35)
    (at 153.166475 112.462158 315)
    (attr smd)
    (fp_text reference LED1 (at 3.175 -0.254 405) (layer F.SilkS) hide)
    (fp_text value WS2812BSK6812MINI (at 0.127 2.54 315) (layer F.SilkS) hide)
    (pad 1-DO smd rect (at 1.74752 0.87376 45) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(LED1-Pad1-DO)"))
    (pad 2-GN smd rect (at 1.74752 -0.87376 45) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3-DI smd rect (at -1.74752 -0.87376 45) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 18 /Din))
    (pad 4-VD smd rect (at -1.74752 0.87376 45) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
  )
  (module adafruit:adafruit-LED3535 (layer F.Cu) (tedit 5B664B3B)
    (at 167.02 126.38 315)
    (attr smd)
    (fp_text reference LED2 (at 3.175 -0.254 405) (layer F.SilkS) hide)
    (fp_text value WS2812BSK6812MINI (at 0.127 2.54 315) (layer F.SilkS) hide)
    (pad 1-DO smd rect (at 1.74752 0.87376 45) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(LED2-Pad1-DO)"))
    (pad 2-GN smd rect (at 1.74752 -0.87376 45) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3-DI smd rect (at -1.74752 -0.87376 45) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(LED1-Pad1-DO)"))
    (pad 4-VD smd rect (at -1.74752 0.87376 45) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
  )
  (module mynixies:mynixies-CD11 (layer F.Cu) (tedit 5B664AA4)
    (at 160.02 119.38 315)
    (autoplace_cost90 10)
    (attr virtual)
    (fp_text reference NX1 (at 10.16 0 315) (layer F.SilkS) hide)
    (fp_text value CD11ALLPINS (at -10.16 0 315) (layer F.SilkS) hide)
    (fp_text user Top (at 0 -13.97 315) (layer F.SilkS) hide)
    (fp_text user Bottom (at 0 13.97 315) (layer F.SilkS) hide)
    (pad 0 thru_hole circle (at -3.82524 -9.23798 315) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 9 /HV10))
    (pad 1 thru_hole circle (at -9.23798 3.82524 315) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 16 /HV1))
    (pad 2 thru_hole circle (at -7.06882 7.06882 315) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 14 /HV2))
    (pad 3 thru_hole circle (at -3.82524 9.23798 315) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 12 /HV3))
    (pad 4 thru_hole circle (at 3.82524 9.23798 315) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 10 /HV4))
    (pad 5 thru_hole circle (at 7.06882 7.06882 315) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 8 /HV5))
    (pad 6 thru_hole circle (at 9.23798 3.82524 315) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 6 /HV6))
    (pad 7 thru_hole circle (at 9.23798 -3.82524 315) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 15 /HV7))
    (pad 8 thru_hole circle (at 7.06882 -7.06882 315) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 13 /HV8))
    (pad 9 thru_hole circle (at 3.82524 -9.23798 315) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 11 /HV9))
    (pad A thru_hole circle (at -9.23798 -3.82524 315) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 20 "Net-(NX1-PadA)"))
    (pad B thru_hole circle (at 0 9.99998 315) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 22 "Net-(NX1-PadB)"))
    (pad NC@1 thru_hole circle (at -7.06882 -7.06882 315) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask))
    (pad T thru_hole circle (at 0 -9.99998 315) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 21 "Net-(NX1-PadT)"))
    (pad "" np_thru_hole circle (at 0 0 315) (size 11.1125 11.1125) (drill 11.1125) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 5.08 315) (size 3.96748 3.96748) (drill 3.96748) (layers *.Cu *.Mask))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B66575A)
    (at 170.77 111.38)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.45) (layer F.SilkS) hide)
    (fp_text value 40K (at 0 1.55) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(NX1-PadT)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 /HV11))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B665744)
    (at 150.02 128.13 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.45 180) (layer F.SilkS) hide)
    (fp_text value 40K (at 0 1.55 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(NX1-PadB)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 /HV12))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module logos:mermaid_l (layer B.Cu) (tedit 0)
    (at 164.27 136.88 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B665717)
    (at 170.02 129.38 45)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.75 45) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 -1.414214 45) (layer F.SilkS))
    (fp_text user %R (at 0 -1.75 45) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 45) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.25 0 45) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B6656E8)
    (at 150.02 109.38 45)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -1.75 45) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.75 45) (layer F.SilkS))
    (fp_text user %R (at 0 -1.75 45) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 45) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.25 0 45) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer B.Cu) (tedit 5B6656C9)
    (at 160.11 105.88)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 2.31) (layer B.SilkS) hide)
    (fp_text value 6.2K (at 5.08 0) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(NX1-PadA)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /Anode))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "nixies.us\nRodan GR-211" (at 162.77 136.63) (layer B.Mask))
  (gr_circle (center 160.02 119.38) (end 135.02 119.38) (layer Edge.Cuts) (width 0.127))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 132.52 91.88) (xy 187.52 91.88) (xy 187.52 146.88) (xy 132.52 146.88)
      )
    )
  )
)
