(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4)
  (general
    (links 63)
    (no_connects 0)
    (area 104.064999 93.904999 188.035001 147.395001)
    (thickness 1.6)
    (drawings 8)
    (tracks 171)
    (zones 0)
    (modules 29)
    (nets 43)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 1)
    (trace_clearance 0.25)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(CX1-Pad1)")
  (net 5 "Net-(D1-Pad2)")
  (net 6 "Net-(D1-Pad1)")
  (net 7 "Net-(D2-Pad2)")
  (net 8 "Net-(D3-Pad2)")
  (net 9 "Net-(D4-Pad2)")
  (net 10 "Net-(L1-Pad1)")
  (net 11 VCC)
  (net 12 "Net-(P1-Pad2)")
  (net 13 "Net-(P1-Pad3)")
  (net 14 "Net-(P1-Pad4)")
  (net 15 "Net-(P1-Pad5)")
  (net 16 "Net-(P1-Pad6)")
  (net 17 "Net-(P2-Pad3)")
  (net 18 "Net-(P2-Pad5)")
  (net 19 "Net-(P2-Pad6)")
  (net 20 "Net-(P2-Pad7)")
  (net 21 "Net-(Q1-Pad3)")
  (net 22 "Net-(Q1-Pad1)")
  (net 23 "Net-(R1-Pad1)")
  (net 24 "Net-(R2-Pad1)")
  (net 25 "Net-(R2-Pad2)")
  (net 26 "Net-(R3-Pad1)")
  (net 27 "Net-(R3-Pad2)")
  (net 28 "Net-(R4-Pad1)")
  (net 29 "Net-(R4-Pad2)")
  (net 30 "Net-(R5-Pad1)")
  (net 31 "Net-(R5-Pad2)")
  (net 32 "Net-(R6-Pad1)")
  (net 33 "Net-(R6-Pad2)")
  (net 34 "Net-(RV1-Pad3)")
  (net 35 "Net-(RV2-Pad3)")
  (net 36 "Net-(RV3-Pad3)")
  (net 37 "Net-(RV4-Pad3)")
  (net 38 "Net-(RV5-Pad3)")
  (net 39 "Net-(U1-Pad3)")
  (net 40 "Net-(U1-Pad5)")
  (net 41 "Net-(U1-Pad7)")
  (net 42 SYNC)
  (net_class Default "This is the default net class."
    (clearance 0.25)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(CX1-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P2-Pad5)")
    (add_net "Net-(P2-Pad6)")
    (add_net "Net-(P2-Pad7)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(RV1-Pad3)")
    (add_net "Net-(RV2-Pad3)")
    (add_net "Net-(RV3-Pad3)")
    (add_net "Net-(RV4-Pad3)")
    (add_net "Net-(RV5-Pad3)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad7)")
    (add_net SYNC)
    (add_net VCC)
  )
  (net_class normal ""
    (clearance 0.4)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Capacitors_ThroughHole:C_Rect_L7.5_W6.5_P5 (layer Top) (tedit 0)
    (at 177.8 119.38 90)
    (descr "Film Capacitor Length 7.5mm x Width 6.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 2.5 -4.5 90) (layer F.SilkS))
    (fp_text value 10nF (at 2.5 4.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L7.5_W6.5_P5 (layer Top) (tedit 58F95E50)
    (at 175.26 109.22)
    (descr "Film Capacitor Length 7.5mm x Width 6.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C2 (at 2.54 -1.905) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 4.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
  )
  (module local:COAX-SHLD (layer Top) (tedit 58F95E80)
    (at 166.37 102.87)
    (fp_text reference CX1 (at 0 -6.35) (layer F.SilkS))
    (fp_text value COAX (at 0 -1.27) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -3.81) (size 2.5 2.5) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(CX1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 -3.81) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole circle (at -2.54 -3.81) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module Diodes_ThroughHole:Diode_DO-35_SOD27_Horizontal_RM10 (layer Top) (tedit 58F95F1F)
    (at 157.48 102.87 180)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference D1 (at 5.08 1.27 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 5.08 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16052 -0.00254) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0.00052 -0.00254) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_ThroughHole:Diode_DO-35_SOD27_Horizontal_RM10 (layer Top) (tedit 58F95F23)
    (at 157.48 106.68 180)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference D2 (at 5.08 1.27 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 5.08 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16052 -0.00254) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (pad 1 thru_hole rect (at 0.00052 -0.00254) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_ThroughHole:Diode_DO-35_SOD27_Horizontal_RM10 (layer Top) (tedit 58F95F29)
    (at 157.48 110.49 180)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference D3 (at 5.08 1.27 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 5.08 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16052 -0.00254) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask)
      (net 8 "Net-(D3-Pad2)"))
    (pad 1 thru_hole rect (at 0.00052 -0.00254) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_ThroughHole:Diode_DO-35_SOD27_Horizontal_RM10 (layer Top) (tedit 58F95F2D)
    (at 157.48 115.57 180)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference D4 (at 5.08 1.27 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 5.08 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16052 -0.00254) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask)
      (net 9 "Net-(D4-Pad2)"))
    (pad 1 thru_hole rect (at 0.00052 -0.00254) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Inductors:INDUCTOR_V (layer Top) (tedit 0)
    (at 167.64 120.65)
    (descr "Inductor (vertical)")
    (tags INDUCTOR)
    (fp_text reference L1 (at 0 1.99898) (layer F.SilkS))
    (fp_text value 20uH (at 0.09906 -1.99898) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.905 1.905) (drill 0.8128) (layers *.Cu *.Mask)
      (net 10 "Net-(L1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.905 1.905) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 VCC))
    (model Inductors.3dshapes/INDUCTOR_V.wrl
      (at (xyz 0 0 0))
      (scale (xyz 2 2 2))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x06 (layer Top) (tedit 58F95F5A)
    (at 107.95 118.11 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -2.54 180) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 2.54 6.985 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(P1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "Net-(P1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "Net-(P1-Pad6)"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module local:CONN-1x7-5mm-pitch (layer Top) (tedit 58F95F69)
    (at 184.15 109.22 270)
    (fp_text reference P2 (at 13.335 2.54 270) (layer F.SilkS))
    (fp_text value CONN_01X07 (at 15.24 -2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.6 2.6) (drill 1.85) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 2.6 2.6) (drill 1.85) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 3 thru_hole circle (at 10 0 270) (size 2.6 2.6) (drill 1.85) (layers *.Cu *.Mask)
      (net 17 "Net-(P2-Pad3)"))
    (pad 4 thru_hole circle (at 15 0 270) (size 2.6 2.6) (drill 1.85) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 20 0 270) (size 2.6 2.6) (drill 1.85) (layers *.Cu *.Mask)
      (net 18 "Net-(P2-Pad5)"))
    (pad 6 thru_hole circle (at 25 0 270) (size 2.6 2.6) (drill 1.85) (layers *.Cu *.Mask)
      (net 19 "Net-(P2-Pad6)"))
    (pad 7 thru_hole circle (at 30 0 270) (size 2.6 2.6) (drill 1.85) (layers *.Cu *.Mask)
      (net 20 "Net-(P2-Pad7)"))
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer Top) (tedit 58F95E9E)
    (at 170.18 113.03 180)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 7.62 -0.635 360) (layer F.SilkS))
    (fp_text value C5468 (at 2.54 2.54 360) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(L1-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(Q1-Pad3)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(Q1-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer Top) (tedit 58F95F15)
    (at 147.32 99.06)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R1 (at 5.08 -1.905) (layer F.SilkS))
    (fp_text value 680 (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 23 "Net-(R1-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer Top) (tedit 58F95ED4)
    (at 118.11 128.27 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R2 (at 8.255 -2.54 180) (layer F.SilkS))
    (fp_text value 4K (at 5.08 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 24 "Net-(R2-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 25 "Net-(R2-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer Top) (tedit 58F95EE8)
    (at 123.19 132.08 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R3 (at 6.35 -2.54 180) (layer F.SilkS))
    (fp_text value 1.8K (at 5.08 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 26 "Net-(R3-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 27 "Net-(R3-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer Top) (tedit 58F95EBA)
    (at 138.43 128.27 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R4 (at 5.715 -2.54 180) (layer F.SilkS))
    (fp_text value 1K (at 5.08 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 28 "Net-(R4-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 29 "Net-(R4-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer Top) (tedit 58F95EF8)
    (at 143.51 133.35 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R5 (at 5.08 -1.905 180) (layer F.SilkS))
    (fp_text value 460 (at 5.08 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 30 "Net-(R5-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 31 "Net-(R5-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer Top) (tedit 58F95EAE)
    (at 156.21 128.27 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R6 (at 5.08 -2.54 180) (layer F.SilkS))
    (fp_text value 620 (at 5.08 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 32 "Net-(R6-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 33 "Net-(R6-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer Top) (tedit 58F95E8D)
    (at 161.29 106.68)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R7 (at 5.08 1.905) (layer F.SilkS))
    (fp_text value 100 (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(CX1-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 22 "Net-(Q1-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer Top) (tedit 58F95EA9)
    (at 171.45 127 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R8 (at 5.08 -2.54 180) (layer F.SilkS))
    (fp_text value 1.2K (at 5.08 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 21 "Net-(Q1-Pad3)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer Top) (tedit 58F95E74)
    (at 184.15 99.06 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R9 (at 5.08 -1.905 180) (layer F.SilkS))
    (fp_text value 2.4K (at 5.08 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 22 "Net-(Q1-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer Top) (tedit 58F95E6A)
    (at 184.15 102.87 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R10 (at 5.08 -1.905 180) (layer F.SilkS))
    (fp_text value 2.4K (at 5.08 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 22 "Net-(Q1-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module local:Potentiometer_Cermet_CT-6EP (layer Top) (tedit 58F95EDE)
    (at 113.03 140.97 270)
    (fp_text reference RV1 (at -5.08 2.54 360) (layer F.SilkS))
    (fp_text value POT (at 0.5 -5.5 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.5 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(R2-Pad1)"))
    (pad 2 thru_hole circle (at 0 -2.5 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(Q1-Pad3)"))
    (pad 3 thru_hole circle (at 2.5 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(RV1-Pad3)"))
  )
  (module local:Potentiometer_Cermet_CT-6EP (layer Top) (tedit 58F95EE4)
    (at 123.19 140.97 270)
    (fp_text reference RV2 (at -5.08 3.175 360) (layer F.SilkS))
    (fp_text value POT (at 0.5 -5.5 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.5 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(R3-Pad1)"))
    (pad 2 thru_hole circle (at 0 -2.5 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(Q1-Pad3)"))
    (pad 3 thru_hole circle (at 2.5 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(RV2-Pad3)"))
  )
  (module local:Potentiometer_Cermet_CT-6EP (layer Top) (tedit 58F95EF1)
    (at 133.35 140.97 270)
    (fp_text reference RV3 (at -5.08 3.175 360) (layer F.SilkS))
    (fp_text value POT (at 0.5 -5.5 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.5 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(R4-Pad1)"))
    (pad 2 thru_hole circle (at 0 -2.5 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(Q1-Pad3)"))
    (pad 3 thru_hole circle (at 2.5 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(RV3-Pad3)"))
  )
  (module local:Potentiometer_Cermet_CT-6EP (layer Top) (tedit 58F95EF5)
    (at 143.51 140.97 270)
    (fp_text reference RV4 (at -5.08 1.905 360) (layer F.SilkS))
    (fp_text value POT (at 0.5 -5.5 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.5 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(R5-Pad1)"))
    (pad 2 thru_hole circle (at 0 -2.5 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(Q1-Pad3)"))
    (pad 3 thru_hole circle (at 2.5 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(RV4-Pad3)"))
  )
  (module local:Potentiometer_Cermet_CT-6EP (layer Top) (tedit 58F95F00)
    (at 153.67 140.97 270)
    (fp_text reference RV5 (at -5.08 2.54 360) (layer F.SilkS))
    (fp_text value POT (at 0.5 -5.5 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.5 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(R6-Pad1)"))
    (pad 2 thru_hole circle (at 0 -2.5 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(Q1-Pad3)"))
    (pad 3 thru_hole circle (at 2.5 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(RV5-Pad3)"))
  )
  (module Housings_DIP:DIP-20_W7.62mm (layer Top) (tedit 58F95F4F)
    (at 115.57 99.06)
    (descr "20-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U1 (at 0 -3.175) (layer F.SilkS))
    (fp_text value 74LS244 (at 4.445 10.16 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(P1-Pad6)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(U1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(P1-Pad5)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(U1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(P1-Pad4)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(U1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(P1-Pad3)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 SYNC))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole oval (at 7.62 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(P1-Pad2)"))
    (pad 12 thru_hole oval (at 7.62 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D4-Pad2)"))
    (pad 13 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D3-Pad2)"))
    (pad 15 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (pad 17 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 18 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 19 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 20 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 VCC))
    (model Housings_DIP.3dshapes/DIP-20_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-14_W7.62mm (layer Top) (tedit 58F95F48)
    (at 130.81 99.06)
    (descr "14-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U2 (at 4.445 -3.175) (layer F.SilkS))
    (fp_text value 74HC04 (at 4.445 7.62 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(R2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(R3-Pad2)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D3-Pad2)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(R4-Pad2)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(R5-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D4-Pad2)"))
    (pad 10 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(R6-Pad2)"))
    (pad 11 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R1-Pad1)"))
    (pad 12 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(P2-Pad3)"))
    (pad 13 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 SYNC))
    (pad 14 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 VCC))
    (model Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220_Neutral123_Vertical (layer Top) (tedit 58F95F5E)
    (at 176.53 133.35 90)
    (descr "TO-220, Neutral, Vertical,")
    (tags "TO-220, Neutral, Vertical,")
    (fp_text reference U3 (at 0 -4.445 90) (layer F.SilkS))
    (fp_text value 7805 (at 0 3.81 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 180) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 19 "Net-(P2-Pad6)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 11 VCC))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Minitel-1B US\nVideo Crapdapter" (at 144.78 121.92 1.2) (layer F.SilkS))
  (gr_text 1 (at 110.49 118.11) (layer F.SilkS))
  (gr_text 7 (at 186.69 142.24) (layer F.SilkS))
  (gr_text 1 (at 186.055 106.045) (layer F.SilkS))
  (gr_line (start 104.14 147.32) (end 104.14 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 187.96 147.32) (end 104.14 147.32) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 187.96 93.98) (end 187.96 147.32) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.14 93.98) (end 187.96 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 187.96 147.32) (xy 104.14 147.32) (xy 104.14 93.98) (xy 187.96 93.98)
      )
    )
  )
)
