(kicad_pcb (version 20171130) (host pcbnew 5.1.5)
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 23)
    (zones 0)
    (modules 5)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 2)
    (user_trace_width 0.25)
    (user_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.75)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad4)")
  (net 2 "Net-(D1-Pad3)")
  (net 3 "Net-(D1-Pad2)")
  (net 4 "Net-(D1-Pad1)")
  (net 5 "Net-(J1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(D1-Pad4)")
    (add_net "Net-(J1-Pad1)")
  )
  (net_class 24VDC ""
    (clearance 1)
    (trace_width 4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class 48VDC ""
    (clearance 1)
    (trace_width 4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module LocoBoard:PowerHeader2 (layer F.Cu) (tedit 5F144076)
    (at 178 109 270)
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn-NID35 (at 0 48.05 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 -0.04 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.5 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.04 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.58 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad1)"))
    (pad 5 thru_hole oval (at 0 10.12 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad4)"))
    (pad 6 thru_hole oval (at 0 35.52 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad4)"))
    (pad 7 thru_hole oval (at 0 38.06 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 8 thru_hole oval (at 0 40.6 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 9 thru_hole oval (at 0 43.14 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 0 45.68 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 48.22 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module 1935161:PHOENIX_1935161 (layer F.Cu) (tedit 5DF4B136)
    (at 162 96)
    (fp_text reference J3 (at 0 0) (layer F.SilkS))
    (fp_text value 1935161 (at 0 0) (layer F.SilkS))
    (fp_text user VALUE (at -5.09283 6.36604) (layer Eco2.User))
    (fp_text user NAME (at -5.08705 -5.08705) (layer Cmts.User))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad4)"))
    (pad 1 thru_hole rect (at -2.5 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model 1935161--3DModel-STEP-56544.STEP
      (offset (xyz -2.5 2.5 5.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module 1935161:PHOENIX_1935161 (layer F.Cu) (tedit 5DF4B136)
    (at 132 95 90)
    (fp_text reference J4 (at 0 0 90) (layer F.SilkS))
    (fp_text value 1935161 (at 0 0 90) (layer F.SilkS))
    (fp_text user VALUE (at -5.09283 6.36604 90) (layer Eco2.User))
    (fp_text user NAME (at -5.08705 -5.08705 90) (layer Cmts.User))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad3)"))
    (pad 1 thru_hole rect (at -2.5 0 90) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (model 1935161--3DModel-STEP-56544.STEP
      (offset (xyz -2.5 2.5 5.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module 1935161:PHOENIX_1935161 (layer F.Cu) (tedit 5DF4B136)
    (at 174 96)
    (fp_text reference J1 (at 0 0) (layer F.SilkS))
    (fp_text value 1935161 (at 0 0) (layer F.SilkS))
    (fp_text user VALUE (at -5.09283 6.36604) (layer Eco2.User))
    (fp_text user NAME (at -5.08705 -5.08705) (layer Cmts.User))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad4)"))
    (pad 1 thru_hole rect (at -2.5 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad1)"))
    (model 1935161--3DModel-STEP-56544.STEP
      (offset (xyz -2.5 2.5 5.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module LocoBoard:SIP-4 (layer F.Cu) (tedit 5DF4A046)
    (at 146.405 93.5 180)
    (fp_text reference D1 (at 0 2.5) (layer F.SilkS))
    (fp_text value D_Bridge_+AA- (at 0 -2.5) (layer F.Fab))
    (pad 4 thru_hole circle (at 5.715 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad4)"))
    (pad 3 thru_hole circle (at 1.905 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad3)"))
    (pad 2 thru_hole circle (at -1.905 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 1 thru_hole circle (at -5.715 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad1)"))
  )
  (gr_text V2 (at 154 101) (layer B.SilkS))
  (gr_text "Track Power" (at 132 101) (layer F.SilkS))
  (gr_text "- 24VDC +" (at 162 90 180) (layer F.SilkS))
  (gr_text "- 5VDC +" (at 174 90 180) (layer F.SilkS))
  (gr_line (start 181 111) (end 181 112) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 181 89) (end 181 111) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127 89) (end 181 89) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127 112) (end 127 89) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 181 112) (end 127 112) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name "Net-(D1-Pad4)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.75))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 181 112) (xy 127 112) (xy 127 89) (xy 181 89)
      )
    )
  )
)
