(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 19)
    (no_connects 0)
    (area 128.380618 98.367 162.271 115.083001)
    (thickness 1.6)
    (drawings 11)
    (tracks 102)
    (zones 0)
    (modules 7)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0762)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x000a8_00000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C2-Pad1)")
  (net 3 "Net-(C2-Pad2)")
  (net 4 +5V)
  (net 5 "Net-(J1-Pad6)")
  (net 6 "Net-(J1-Pad8)")
  (net 7 /Vin)
  (net 8 /RESET)
  (net 9 /RX)
  (net 10 /TX)
  (net 11 /SET)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /RESET)
    (add_net /RX)
    (add_net /SET)
    (add_net /TX)
    (add_net /Vin)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad8)")
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5ADFC49B)
    (at 149.86 108.204 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at -0.254 1.778 360) (layer F.SilkS))
    (fp_text value 10uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at -0.254 1.778 360) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /Vin))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 144.272 101.092 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5ADFC4B5)
    (at 144.272 110.49)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at -0.254 2.032) (layer F.SilkS))
    (fp_text value 10uF (at 0 2) (layer F.Fab))
    (fp_text user %R (at -0.254 2.032) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x05_Pitch1.27mm (layer F.Cu) (tedit 59650536)
    (at 136.398 100.33)
    (descr "Through hole straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 1.27mm double row")
    (fp_text reference J1 (at 0.508 7.112) (layer F.SilkS))
    (fp_text value Conn_02x05_Odd_Even (at 0.635 6.775) (layer F.Fab))
    (fp_text user %R (at 0.635 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 2 thru_hole oval (at 1.27 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 3 thru_hole oval (at 0 1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 1.27 1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 2.54) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 8 /RESET))
    (pad 6 thru_hole oval (at 1.27 2.54) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at 0 3.81) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 9 /RX))
    (pad 8 thru_hole oval (at 1.27 3.81) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad8)"))
    (pad 9 thru_hole oval (at 0 5.08) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 10 /TX))
    (pad 10 thru_hole oval (at 1.27 5.08) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 11 /SET))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x05_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLib:PinSocket_SMT_1.06_100mil_RightAngle (layer F.Cu) (tedit 5ADFA48D)
    (at 154.94 107.188)
    (tags PinSocket6x100mil)
    (fp_text reference J2 (at 3.81 -0.254) (layer F.SilkS) hide)
    (fp_text value Conn_01x06 (at 6.096 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0 -6.35 270) (size 1.778 3.048) (layers F.Cu F.Paste F.Mask)
      (net 8 /RESET))
    (pad 2 smd rect (at 0 -3.81 270) (size 1.778 3.048) (layers F.Cu F.Paste F.Mask)
      (net 7 /Vin))
    (pad 3 smd rect (at 0 -1.27 270) (size 1.778 3.048) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 1.27 270) (size 1.778 3.048) (layers F.Cu F.Paste F.Mask)
      (net 11 /SET))
    (pad 5 smd rect (at 0 3.81 270) (size 1.778 3.048) (layers F.Cu F.Paste F.Mask)
      (net 10 /TX))
    (pad 6 smd rect (at 0 6.35 270) (size 1.778 3.048) (layers F.Cu F.Paste F.Mask)
      (net 9 /RX))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5ADFC489)
    (at 149.86 102.382 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference JP1 (at 0 1.778 360) (layer F.SilkS))
    (fp_text value Jumper (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at -0.02 1.778 360) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /Vin))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6_Handsoldering (layer F.Cu) (tedit 58CE4E7E)
    (at 144.272 105.664 90)
    (descr "6-pin SOT-23 package, Handsoldering")
    (tags "SOT-23-6 Handsoldering")
    (attr smd)
    (fp_text reference U1 (at 0 -2.9 180) (layer F.SilkS))
    (fp_text value AP3602A (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 -0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at -1.35 0 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.35 0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 /Vin))
    (pad 4 smd rect (at 1.35 0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 6 smd rect (at 1.35 -0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 5 smd rect (at 1.35 0 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 /Vin))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 156.972 98.806) (end 134.874 98.806) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.972 115.062) (end 156.972 98.806) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.874 115.062) (end 156.972 115.062) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.874 98.806) (end 134.874 115.062) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text RX (at 151.892 113.538) (layer F.SilkS))
  (gr_text TX (at 151.892 110.998) (layer F.SilkS))
  (gr_text Set (at 151.892 108.458) (layer F.SilkS))
  (gr_text GND (at 151.892 105.918) (layer F.SilkS))
  (gr_text Vin (at 152.146 103.378) (layer F.SilkS))
  (gr_text RES (at 151.892 100.838) (layer F.SilkS))
  (gr_text 1 (at 142.24 108.204) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.7 103.886) (xy 140.208 104.14) (xy 140.208 110.49) (xy 141.478 111.76) (xy 144.272 111.76)
        (xy 144.272 109.728) (xy 143.764 108.966) (xy 143.764 107.696) (xy 144.526 107.696) (xy 144.526 108.204)
        (xy 147.066 108.204) (xy 147.3708 108.3056) (xy 147.32 108.204) (xy 150.114 108.204) (xy 152.654 105.664)
        (xy 153.67 105.664) (xy 153.67 106.934) (xy 153.162 106.934) (xy 153.162 107.188) (xy 152.654 107.696)
        (xy 152.654 108.712) (xy 151.384 109.982) (xy 151.384 112.776) (xy 141.224 112.776) (xy 138.684 110.236)
        (xy 138.684 102.108) (xy 136.398 102.108) (xy 136.398 101.092) (xy 139.7 101.092)
      )
    )
  )
  (zone (net 4) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.256 110.236) (xy 140.462 110.236) (xy 140.462 103.124) (xy 140.462 100.838) (xy 137.668 100.838)
        (xy 137.668 99.822) (xy 141.732 99.822) (xy 141.732 104.394) (xy 142.494 105.156) (xy 143.002 105.664)
        (xy 143.256 107.442)
      )
    )
  )
  (zone (net 7) (net_name /Vin) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.368 107.188) (xy 149.606 107.95) (xy 145.542 107.95) (xy 145.288 106.172) (xy 145.288 105.664)
        (xy 146.05 105.918) (xy 148.844 102.87) (xy 153.67 102.87) (xy 153.67 104.394) (xy 152.908 104.394)
      )
    )
  )
  (zone (net 4) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.574 99.822) (xy 147.574 99.314) (xy 152.654 99.568) (xy 152.654 102.616) (xy 148.59 102.616)
        (xy 146.812 103.378) (xy 146.812 99.822)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (mode segment) (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.382 99.314) (xy 135.382 114.554) (xy 156.464 114.554) (xy 156.464 99.314)
      )
    )
  )
)
