(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6256)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Purple")
				(thickness 0.0152)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.0356)
			)
			(layer "dielectric 1"
				(type "core")
				(color "FR4 natural")
				(thickness 1.524)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.0356)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Purple")
				(thickness 0.0152)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask yes)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "V")
	(net 2 "GND")
	(footprint "Xer_Library:22awg_Wire"
		(layer "F.Cu")
		(at 120.460684 100.888 180)
		(property "Reference" "V_Wire1"
			(at 3.2 -7 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 9.6 5 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Xer_Library:22awg_Wire"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 0.974 0.974)
			(drill 0.72)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "V")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(model "${KICAD8_USER_3DMODEL_DIR}/teflon_22awg.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 0)
			)
		)
	)
	(footprint "Xer_Library:22awg_Wire"
		(layer "F.Cu")
		(at 115.8 104.163084)
		(property "Reference" "V_Wire1"
			(at 3.2 -7 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 9.6 5 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Xer_Library:22awg_Wire"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.974 0.974)
			(drill 0.72)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "V")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(model "${KICAD8_USER_3DMODEL_DIR}/teflon_22awg.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 0)
			)
		)
	)
	(footprint "Xer_Library:22awg_Wire"
		(layer "F.Cu")
		(at 109.360684 100.888 180)
		(property "Reference" "GND_Wire1"
			(at -3.8 -7 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at -7.6 5 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Xer_Library:22awg_Wire"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 0.974 0.974)
			(drill 0.72)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(model "${KICAD8_USER_3DMODEL_DIR}/teflon_22awg.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 0)
			)
		)
	)
	(footprint "Xer_Library:22awg_Wire"
		(layer "F.Cu")
		(at 101.5 104.112)
		(property "Reference" "GND_Wire1"
			(at -3.8 -7 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at -7.6 5 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Xer_Library:22awg_Wire"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "BT0.2.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.974 0.974)
			(drill 0.72)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(model "${KICAD8_USER_3DMODEL_DIR}/teflon_22awg.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 0)
			)
		)
	)
	(footprint "Xer_Library:22awg_Wire"
		(layer "F.Cu")
		(at 114.2 104.163084)
		(property "Reference" "GND_Wire1"
			(at -3.8 -7 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at -7.6 5 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Xer_Library:22awg_Wire"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.974 0.974)
			(drill 0.72)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(model "${KICAD8_USER_3DMODEL_DIR}/teflon_22awg.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 0)
			)
		)
	)
	(footprint "Xer_Library:BT2.0"
		(layer "F.Cu")
		(at 121.260684 103.688 180)
		(property "Reference" "U1"
			(at 0 -4 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at 0 3 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Xer_Library:BT2.0"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -1 0 180)
			(size 1.854 1.854)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "2" thru_hole circle
			(at 1 0 180)
			(size 1.854 1.854)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "V")
			(pinfunction "V+")
			(pintype "input")
			(zone_connect 2)
		)
		(model "${KICAD8_USER_3DMODEL_DIR}/1S_300mah_Pack.stp"
			(offset
				(xyz 0 0.9 67.7)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 180 0 0)
			)
		)
		(model "${KICAD8_USER_3DMODEL_DIR}/BT2.0-M.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "Xer_Library:22awg_Wire"
		(layer "F.Cu")
		(at 103.1 104.112)
		(property "Reference" "V_Wire1"
			(at 3.2 -7 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 9.6 5 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Xer_Library:22awg_Wire"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "BT0.2.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.974 0.974)
			(drill 0.72)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "V")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(model "${KICAD8_USER_3DMODEL_DIR}/teflon_22awg.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 0)
			)
		)
	)
	(footprint "Xer_Library:22awg_Wire"
		(layer "F.Cu")
		(at 122.060684 100.888 180)
		(property "Reference" "GND_Wire1"
			(at -3.8 -7 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at -7.6 5 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Xer_Library:22awg_Wire"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 0.974 0.974)
			(drill 0.72)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(model "${KICAD8_USER_3DMODEL_DIR}/teflon_22awg.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 0)
			)
		)
	)
	(footprint "Xer_Library:BT2.0"
		(layer "F.Cu")
		(at 102.3 101.312)
		(property "Reference" "U1"
			(at 0 -4 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at 0 3 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Xer_Library:BT2.0"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "BT0.2.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -1 0)
			(size 1.854 1.854)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "2" thru_hole circle
			(at 1 0)
			(size 1.854 1.854)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "V")
			(pinfunction "V+")
			(pintype "input")
			(zone_connect 2)
		)
		(model "${KICAD8_USER_3DMODEL_DIR}/1S_300mah_Pack.stp"
			(offset
				(xyz 0 0.9 67.7)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 180 0 0)
			)
		)
		(model "${KICAD8_USER_3DMODEL_DIR}/BT2.0-M.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "Xer_Library:22awg_Wire"
		(layer "F.Cu")
		(at 107.760684 100.888 180)
		(property "Reference" "V_Wire1"
			(at 3.2 -7 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 9.6 5 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Xer_Library:22awg_Wire"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 0.974 0.974)
			(drill 0.72)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "V")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(model "${KICAD8_USER_3DMODEL_DIR}/teflon_22awg.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 0)
			)
		)
	)
	(footprint "Xer_Library:BT2.0"
		(layer "F.Cu")
		(at 108.560684 103.688 180)
		(property "Reference" "U1"
			(at 0 -4 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at 0 3 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Xer_Library:BT2.0"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -1 0 180)
			(size 1.854 1.854)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "2" thru_hole circle
			(at 1 0 180)
			(size 1.854 1.854)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "V")
			(pinfunction "V+")
			(pintype "input")
			(zone_connect 2)
		)
		(model "${KICAD8_USER_3DMODEL_DIR}/1S_300mah_Pack.stp"
			(offset
				(xyz 0 0.9 67.7)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 180 0 0)
			)
		)
		(model "${KICAD8_USER_3DMODEL_DIR}/BT2.0-M.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "Xer_Library:BT2.0"
		(layer "F.Cu")
		(at 115 101.363084)
		(property "Reference" "U1"
			(at 0 -4 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at 0 3 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Xer_Library:BT2.0"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -1 0)
			(size 1.854 1.854)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "2" thru_hole circle
			(at 1 0)
			(size 1.854 1.854)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "V")
			(pinfunction "V+")
			(pintype "input")
			(zone_connect 2)
		)
		(model "${KICAD8_USER_3DMODEL_DIR}/1S_300mah_Pack.stp"
			(offset
				(xyz 0 0.9 67.7)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 180 0 0)
			)
		)
		(model "${KICAD8_USER_3DMODEL_DIR}/BT2.0-M.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(gr_line
		(start 118.983385 103.38825)
		(end 119.616615 100.689918)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.8 105)
		(end 108.8 107)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 103.944069 104.310082)
		(mid 103.638494 104.791495)
		(end 103.1 104.979)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 101.3 100)
		(end 103.3 100)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 122.260684 105)
		(end 120.260684 105)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 102.6 105)
		(end 102.6 107)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 106.916615 100.689918)
		(mid 107.22219 100.208505)
		(end 107.760684 100.021)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 110.837983 103.38825)
		(mid 110.588939 104.502884)
		(end 109.560684 105)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 114.8 100)
		(end 114.8 98)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 115.4 100)
		(end 115.4 98)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 109.360684 100.021)
		(end 107.760684 100.021)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 109.360684 100.021)
		(mid 109.899178 100.208505)
		(end 110.204753 100.689918)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 110.837983 103.38825)
		(end 110.204753 100.689918)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 116.644069 104.361166)
		(mid 116.338494 104.842579)
		(end 115.8 105.030084)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 122.060684 100.021)
		(mid 122.599178 100.208505)
		(end 122.904753 100.689918)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 101.5 104.979)
		(end 103.1 104.979)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 114 100.051084)
		(end 116 100.051084)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.2 100)
		(end 108.2 98)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 101.5 104.979)
		(mid 100.961506 104.791495)
		(end 100.655931 104.310082)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 115.4 105)
		(end 115.4 107)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 106.283385 103.38825)
		(end 106.916615 100.689918)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 121.6 105)
		(end 121.6 107)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 103.3 100)
		(mid 104.328255 100.497116)
		(end 104.577299 101.61175)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 109.560684 105)
		(end 107.560684 105)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.722701 101.662834)
		(end 113.355931 104.361166)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 114.8 105)
		(end 114.8 107)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 119.616615 100.689918)
		(mid 119.92219 100.208505)
		(end 120.460684 100.021)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 100.022701 101.61175)
		(end 100.655931 104.310082)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 107.560684 105)
		(mid 106.532429 104.502884)
		(end 106.283385 103.38825)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 100.022701 101.61175)
		(mid 100.271745 100.497116)
		(end 101.3 100)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.8 100)
		(end 108.8 98)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 116 100.051084)
		(mid 117.028255 100.5482)
		(end 117.277299 101.662834)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 112.722701 101.662834)
		(mid 112.971745 100.5482)
		(end 114 100.051084)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 120.260684 105)
		(mid 119.232429 104.502884)
		(end 118.983385 103.38825)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 102 105)
		(end 102 107)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 121 105)
		(end 121 107)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 98 98)
		(end 125.6 107)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 114.2 105.030084)
		(end 115.8 105.030084)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.2 105)
		(end 108.2 107)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 121 100)
		(end 121 98)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.537983 103.38825)
		(end 122.904753 100.689918)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 117.277299 101.662834)
		(end 116.644069 104.361166)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 122.060684 100.021)
		(end 120.460684 100.021)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.577299 101.61175)
		(end 103.944069 104.310082)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 121.6 100)
		(end 121.6 98)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 123.537983 103.38825)
		(mid 123.288939 104.502884)
		(end 122.260684 105)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 96.6 96.2)
		(end 127.6 109)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 102.6 100)
		(end 102.6 98)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 102 100)
		(end 102 98)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 114.2 105.030084)
		(mid 113.661506 104.842579)
		(end 113.355931 104.361166)
		(layer "Edge.Cuts")
	)
	(zone
		(net 1)
		(net_name "V")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 115.3 100.863084) (xy 115.35 104.363084) (xy 116.5 104.363084) (xy 117.4 100.863084)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 110.960684 104.188) (xy 108.860684 104.188) (xy 108.910684 100.688) (xy 110.060684 100.688)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 112.6 100.863084) (xy 114.7 100.863084) (xy 114.65 104.363084) (xy 113.5 104.363084)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 123.660684 104.188) (xy 121.560684 104.188) (xy 121.610684 100.688) (xy 122.760684 100.688)
			)
		)
	)
	(zone
		(net 1)
		(net_name "V")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 102.6 100.812) (xy 102.65 104.312) (xy 103.8 104.312) (xy 104.7 100.812)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 99.9 100.812) (xy 102 100.812) (xy 101.95 104.312) (xy 100.8 104.312)
			)
		)
	)
	(zone
		(net 1)
		(net_name "V")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 120.960684 104.188) (xy 120.910684 100.688) (xy 119.760684 100.688) (xy 118.860684 104.188)
			)
		)
	)
	(zone
		(net 1)
		(net_name "V")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 108.260684 104.188) (xy 108.210684 100.688) (xy 107.060684 100.688) (xy 106.160684 104.188)
			)
		)
	)
)
