(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 174.5 97.71)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "17")
  (net 2 "Net-(R2-Pad2)")
  (net 3 "Net-(R3-Pad2)")
  (net 4 "Net-(R20-Pad1)")
  (net 5 "9")
  (net 6 "Net-(R19-Pad1)")
  (net 7 "10")
  (net 8 "Net-(R18-Pad1)")
  (net 9 "11")
  (net 10 "Net-(R17-Pad1)")
  (net 11 "12")
  (net 12 "Net-(R16-Pad1)")
  (net 13 "13")
  (net 14 "Net-(R15-Pad1)")
  (net 15 "14")
  (net 16 "Net-(R14-Pad1)")
  (net 17 "15")
  (net 18 "Net-(R13-Pad1)")
  (net 19 "16")
  (net 20 "Net-(R12-Pad1)")
  (net 21 "19")
  (net 22 "Net-(R11-Pad1)")
  (net 23 "20")
  (net 24 "1")
  (net 25 "Net-(R10-Pad2)")
  (net 26 "2")
  (net 27 "Net-(R9-Pad2)")
  (net 28 "3")
  (net 29 "Net-(R8-Pad2)")
  (net 30 "4")
  (net 31 "Net-(R7-Pad2)")
  (net 32 "5")
  (net 33 "Net-(R6-Pad2)")
  (net 34 "6")
  (net 35 "Net-(R5-Pad2)")
  (net 36 "18")
  (net 37 "Net-(R1-Pad2)")
  (net 38 "7")
  (net 39 "Net-(R4-Pad2)")
  (net 40 "Net-(C1-Pad1)")
  (net 41 "GND")
  (net 42 "Net-(C11-Pad2)")
  (footprint "lowpassfilter_fp:rb_rotator" (layer "F.Cu")
    (tedit 0)
    (at 143.78644 94.54994)
    (descr "503320-2560-3")
    (tags "Connector")
    (attr smd)
    (fp_text reference "ribbon_connector_rotator" (at 0.05 3.13) (layer "F.Fab"))
    (fp_text value "rb_rotator" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -2.75 -1.24) (size 0.25 0.57) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "Net-(R1-Pad2)"))
    (pad "2" smd rect (at -3 1.165) (size 0.25 0.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(R2-Pad2)"))
    (pad "3" smd rect (at -2.25 -1.24) (size 0.25 0.57) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(R3-Pad2)"))
    (pad "4" smd rect (at -2.5 1.165) (size 0.25 0.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "Net-(R4-Pad2)"))
    (pad "5" smd rect (at -1.25 -1.24) (size 0.25 0.57) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "Net-(R5-Pad2)"))
    (pad "6" smd rect (at -1.5 1.165) (size 0.25 0.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "Net-(R6-Pad2)"))
    (pad "7" smd rect (at -0.75 -1.24) (size 0.25 0.57) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "Net-(R7-Pad2)"))
    (pad "8" smd rect (at -1 1.165) (size 0.25 0.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "Net-(R8-Pad2)"))
    (pad "9" smd rect (at 2.75 -1.24) (size 0.25 0.57) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(R9-Pad2)"))
    (pad "10" smd rect (at 3 1.165) (size 0.25 0.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(R10-Pad2)"))
    (pad "11" smd rect (at 2.25 -1.24) (size 0.25 0.57) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "11"))
    (pad "12" smd rect (at 2.5 1.165) (size 0.25 0.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "12"))
    (pad "13" smd rect (at 1.25 -1.24) (size 0.25 0.57) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "13"))
    (pad "14" smd rect (at 1.5 1.165) (size 0.25 0.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "14"))
    (pad "15" smd rect (at 0.75 -1.24) (size 0.25 0.57) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "15"))
    (pad "16" smd rect (at 1 1.165) (size 0.25 0.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "16"))
    (pad "17" smd rect (at -0.25 -1.24) (size 0.25 0.57) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "17"))
    (pad "18" smd rect (at -0.5 1.165) (size 0.25 0.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "18"))
    (pad "19" smd rect (at 0.5 1.165) (size 0.25 0.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "19"))
    (pad "20" smd rect (at 0.25 -1.24) (size 0.25 0.57) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "20"))
    (pad "21" smd rect (at -1.75 -1.24) (size 0.25 0.57) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "Net-(C1-Pad1)"))
    (pad "22" smd rect (at -2 1.165) (size 0.25 0.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "Net-(C1-Pad1)"))
    (pad "23" smd rect (at 1.75 -1.24) (size 0.25 0.57) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "Net-(C11-Pad2)"))
    (pad "24" smd rect (at 2 1.165) (size 0.25 0.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "Net-(C11-Pad2)"))
    (pad "25" smd rect (at 0 1.165) (size 0.25 0.72) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "GND"))
    (pad "MP1" smd rect (at 3.67 0.9) (size 0.4 0.95) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "MP2" smd rect (at -3.67 0.9) (size 0.4 0.95) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "503320-2560.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.32644 64.72298 180)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05) (layer "F.SilkS") hide)
    (fp_text value "R_0201" (at 0.03042 -0.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68) (layer "F.Fab") hide)
    (pad "" smd roundrect (at -0.345 0 180) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 180) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 180) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "18"))
    (pad "2" smd roundrect (at 0.32 0 180) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(R18-Pad1)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "lowpassfilter_fp:custom DIP-22_wider-board" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 138.73478 65.46149)
    (descr "22-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (attr through_hole)
    (fp_text reference "REF**" (at 4.02144 -5.08851) (layer "F.SilkS"))
    (fp_text value "custom DIP-22_wider-board" (at 4.89644 11.56149 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 -3.8) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask "F.Paste")
      (net 24 "1"))
    (pad "2" thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask "F.Paste")
      (net 2 "Net-(R2-Pad2)"))
    (pad "3" thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask "F.Paste")
      (net 3 "Net-(R3-Pad2)"))
    (pad "4" thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask "F.Paste")
      (net 39 "Net-(R4-Pad2)"))
    (pad "5" thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask "F.Paste")
      (net 35 "Net-(R5-Pad2)"))
    (pad "6" thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask "F.Paste")
      (net 33 "Net-(R6-Pad2)"))
    (pad "7" thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask "F.Paste")
      (net 31 "Net-(R7-Pad2)"))
    (pad "8" thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask "F.Paste")
      (net 29 "Net-(R8-Pad2)"))
    (pad "9" thru_hole oval (at 10.05332 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask "F.Paste")
      (net 5 "9"))
    (pad "10" thru_hole oval (at 10.05332 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask "F.Paste")
      (net 7 "10"))
    (pad "11" thru_hole oval (at 10.05332 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask "F.Paste")
      (net 22 "Net-(R11-Pad1)"))
    (pad "12" thru_hole oval (at 10.05332 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask "F.Paste")
      (net 20 "Net-(R12-Pad1)"))
    (pad "13" thru_hole oval (at 10.05332 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask "F.Paste")
      (net 18 "Net-(R13-Pad1)"))
    (pad "14" thru_hole oval (at 10.05332 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask "F.Paste")
      (net 16 "Net-(R14-Pad1)"))
    (pad "15" thru_hole oval (at 10.05332 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask "F.Paste")
      (net 14 "Net-(R15-Pad1)"))
    (pad "16" thru_hole oval (at 10.05332 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask "F.Paste")
      (net 12 "Net-(R16-Pad1)"))
    (pad "17" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask "F.Paste")
      (net 10 "Net-(R17-Pad1)"))
    (pad "18" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask "F.Paste")
      (net 8 "Net-(R18-Pad1)"))
    (pad "19" thru_hole oval (at 10.05332 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask "F.Paste")
      (net 6 "Net-(R19-Pad1)"))
    (pad "20" thru_hole oval (at 10.05332 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask "F.Paste")
      (net 4 "Net-(R20-Pad1)"))
    (pad "SH" thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask "F.Paste")
      (net 40 "Net-(C1-Pad1)"))
    (pad "SH" thru_hole oval (at 10.05332 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask "F.Paste")
      (net 42 "Net-(C11-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-22_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.30144 85.27298 90)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "R_0201" (at 0.03042 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(R11-Pad1)"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "11"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.22644 70.34798 90)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "C_0201" (at 0 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(R8-Pad2)"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(R8-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.30144 90.92298 90)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "R_0201" (at 0.03042 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "9"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(R9-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.30144 88.12298 90)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "R_0201" (at 0.03042 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "10"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(R10-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.30144 89.50298 90)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "C_0201" (at 0 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(R9-Pad2)"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.22644 85.37298 90)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "R_0201" (at 0.03042 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "3"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(R3-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.22644 67.52298 90)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "C_0201" (at 0 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "17" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(R17-Pad1)"))
    (pad "17" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "17"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.22644 73.17298 90)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "C_0201" (at 0 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "7"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(R7-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.22644 88.22298 90)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "R_0201" (at 0.03042 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "2"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(R2-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.22644 89.60298 90)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "C_0201" (at 0 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(R1-Pad2)"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.30144 67.20298 90)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "C_0201" (at 0 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(R19-Pad1)"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "19"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.30144 68.62298 90)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "R_0201" (at 0.03042 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "16"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 146.00144 64.62298 180)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05) (layer "F.SilkS") hide)
    (fp_text value "C_0201" (at 0 -0.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68) (layer "F.Fab") hide)
    (pad "" smd roundrect (at -0.345 0 180) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 180) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 180) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "20"))
    (pad "2" smd roundrect (at 0.32 0 180) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.30144 77.09798 90)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "R_0201" (at 0.03042 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "13"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.30144 75.67798 90)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "C_0201" (at 0 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(R14-Pad1)"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "14"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.30144 81.02798 90)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "C_0201" (at 0 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "12"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 141.73144 64.72298 180)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05) (layer "F.SilkS") hide)
    (fp_text value "C_0201" (at 0 -0.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68) (layer "F.Fab") hide)
    (pad "" smd roundrect (at -0.345 0 180) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 180) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 180) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "GND"))
    (pad "2" smd roundrect (at 0.32 0 180) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "18"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.22644 66.11798 90)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "R_0201" (at 0.03042 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "GND"))
    (pad "17" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "17"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.30144 86.70298 90)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "C_0201" (at 0 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(R10-Pad2)"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.30144 83.85298 90)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "C_0201" (at 0 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "11"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.22644 71.76798 90)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "R_0201" (at 0.03042 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(R7-Pad2)"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.22644 74.59298 90)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "R_0201" (at 0.03042 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(R6-Pad2)"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.30144 74.27298 90)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "R_0201" (at 0.03042 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "14"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.30144 70.02798 90)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "C_0201" (at 0 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(R16-Pad1)"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "16"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.22644 91.02298 90)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "R_0201" (at 0.03042 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "1"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(R1-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.22644 83.95298 90)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "C_0201" (at 0 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(R3-Pad2)"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.22644 81.12798 90)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "C_0201" (at 0 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(R4-Pad2)"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.22644 77.41798 90)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "R_0201" (at 0.03042 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(R5-Pad2)"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.30144 71.44798 90)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "R_0201" (at 0.03042 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "15"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.22644 82.57298 90)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "R_0201" (at 0.03042 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "4"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(R4-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.22644 86.80298 90)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "C_0201" (at 0 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(R2-Pad2)"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.22644 68.94298 90)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "R_0201" (at 0.03042 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(R8-Pad2)"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.40144 64.62298 180)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05) (layer "F.SilkS") hide)
    (fp_text value "R_0201" (at 0.03042 -0.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68) (layer "F.Fab") hide)
    (pad "" smd roundrect (at 0.345 0 180) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 180) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 180) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(R20-Pad1)"))
    (pad "2" smd roundrect (at 0.32 0 180) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "20"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.22644 75.99798 90)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "C_0201" (at 0 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "6"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(R6-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.30144 78.50298 90)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "C_0201" (at 0 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(R13-Pad1)"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "13"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.22644 78.82298 90)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "C_0201" (at 0 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "5"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(R5-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.30144 82.47298 90)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "R_0201" (at 0.03042 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(R12-Pad1)"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "12"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.30144 65.79798 90)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "R_0201" (at 0.03042 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "19"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "GND"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0201_0603Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.30144 72.85298 90)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -1.05 90) (layer "F.SilkS") hide)
    (fp_text value "C_0201" (at 0 -0.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.68 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(R15-Pad1)"))
    (pad "2" smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "15"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 136.75144 62.22298) (end 150.63 96.8) (layer "Edge.Cuts") (width 0.2) (fill none))
  (gr_text "SH1" (at 141.88 80.625) (layer "B.SilkS"))
  (gr_text "17" (at 141.38 67.625) (layer "B.SilkS"))
  (gr_text "14" (at 146.13 76.1) (layer "B.SilkS"))
  (gr_text "4" (at 141.455 83.2) (layer "B.SilkS"))
  (gr_text "2" (at 141.455 88.375) (layer "B.SilkS"))
  (gr_text "19" (at 146.08 67.9) (layer "B.SilkS"))
  (gr_text "13" (at 146.105 78.15) (layer "B.SilkS"))
  (gr_text "3" (at 141.38 85.8) (layer "B.SilkS"))
  (gr_text "15" (at 146.105 73.05) (layer "B.SilkS"))
  (gr_text "9" (at 146.205 90.825) (layer "B.SilkS"))
  (gr_text "12" (at 146.03 83.175) (layer "B.SilkS"))
  (gr_text "18" (at 142.43 65.8) (layer "B.SilkS"))
  (gr_text "8" (at 141.18 70.5) (layer "B.SilkS"))
  (gr_text "20" (at 145.48 65.725) (layer "B.SilkS"))
  (gr_text "5" (at 141.255 78.125) (layer "B.SilkS"))
  (gr_text "7" (at 141.205 73) (layer "B.SilkS"))
  (gr_text "10" (at 146.03 88.325) (layer "B.SilkS"))
  (gr_text "SH2" (at 145.68 80.575) (layer "B.SilkS"))
  (gr_text "11" (at 146.08 85.675) (layer "B.SilkS"))
  (gr_text "16" (at 146.03 70.425) (layer "B.SilkS"))
  (gr_text "6" (at 141.33 75.475) (layer "B.SilkS"))
  (gr_text "1" (at 141.455 90.9) (layer "B.SilkS"))
  (gr_text "18" (at 142.455 65.825) (layer "F.SilkS"))
  (gr_text "2" (at 141.455 88.4) (layer "F.SilkS"))
  (gr_text "17" (at 141.38 67.65) (layer "F.SilkS"))
  (gr_text "SH2" (at 145.68 80.575) (layer "F.SilkS"))
  (gr_text "19" (at 146.08 67.925) (layer "F.SilkS"))
  (gr_text "14" (at 146.18 76.125) (layer "F.SilkS"))
  (gr_text "10" (at 145.98 88.325) (layer "F.SilkS"))
  (gr_text "SH1" (at 141.905 80.65) (layer "F.SilkS"))
  (gr_text "1" (at 141.455 90.925) (layer "F.SilkS"))
  (gr_text "6" (at 141.355 75.525) (layer "F.SilkS"))
  (gr_text "13" (at 146.155 78.15) (layer "F.SilkS"))
  (gr_text "16" (at 146.08 70.475) (layer "F.SilkS"))
  (gr_text "20" (at 145.505 65.725) (layer "F.SilkS"))
  (gr_text "15" (at 146.13 73.075) (layer "F.SilkS"))
  (gr_text "4" (at 141.43 83.225) (layer "F.SilkS"))
  (gr_text "9" (at 146.23 90.9) (layer "F.SilkS"))
  (gr_text "3" (at 141.405 85.825) (layer "F.SilkS"))
  (gr_text "11" (at 146.155 85.675) (layer "F.SilkS"))
  (gr_text "8" (at 141.205 70.525) (layer "F.SilkS"))
  (gr_text "7" (at 141.23 73.025) (layer "F.SilkS"))
  (gr_text "12" (at 146.005 83.175) (layer "F.SilkS"))
  (gr_text "5" (at 141.28 78.15) (layer "F.SilkS"))
  (zone (net 41) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.405 96.475)
        (xy 137.08 96.5)
        (xy 137.03 62.5)
        (xy 150.33 62.5)
      )
    )
  )
)
