<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.0">
<drawing>
<board>
<plain>
<hole x="4.245" y="4.607" drill="1"/>
<hole x="0.181" y="4.607" drill="1"/>
<hole x="0.181" y="8.671" drill="0.4"/>
<hole x="7.266" y="4.307" drill="2.032"/>
<wire x1="0" y1="0" x2="0" y2="8.8" width="0.1" layer="20"/>
<wire x1="0" y1="8.8" x2="11.5" y2="8.8" width="0.1" layer="20"/>
<wire x1="11.5" y1="8.8" x2="11.5" y2="0" width="0.1" layer="20"/>
<wire x1="11.5" y1="0" x2="0" y2="0" width="0.1" layer="20"/>
</plain>
<libraries>
<library name="tcrt5000">
<packages>
<package name="TCRT5000">
</package>
</packages>
</library>
<library name="smd-ipc">
<description>&lt;b&gt;IPC Standard SMD Packages&lt;/b&gt;&lt;p&gt;
This is a package-only library, based on the Surface Mount Design and Land Pattern Standard developed by the 
Institute for Interconnecting and Packaging electronic Circuits (IPC).&lt;p&gt;
Source:&lt;p&gt;
IPC-SM-782&lt;br&gt;
Revision A, August 1993&lt;br&gt;
Includes Amendment 1, October 1996&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="R1206">
<description>&lt;b&gt;Chip RESISTOR, 1206 EIA (3216 Metric)&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1,6/0,9">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="TCRT5000" library="tcrt5000" package="TCRT5000" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="smd-ipc" package="R1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+5V" library="wirepad" package="1,6/0,9" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT" library="wirepad" package="1,6/0,9" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="wirepad" package="1,6/0,9" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="S$2">
<contactref element="R1" pad="2"/>
<contactref element="+5V" pad="1"/>
</signal>
<signal name="S$3">
<contactref element="TCRT5000" pad="K"/>
<contactref element="TCRT5000" pad="E"/>
</signal>
<signal name="S$4">
<contactref element="R1" pad="1"/>
<contactref element="TCRT5000" pad="A"/>
</signal>
<signal name="S$1">
<contactref element="TCRT5000" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
