(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 27)
    (no_connects 0)
    (area 124.672599 89.1 167.700001 109.400001)
    (thickness 1.6)
    (drawings 8)
    (tracks 91)
    (zones 0)
    (modules 16)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.3048)
    (user_trace_width 0.6096)
    (user_trace_width 1.2192)
    (user_trace_width 1.7)
    (user_trace_width 2.4384)
    (trace_clearance 0.1524)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.05)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (user_via 1.3716 0.6604)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.3 0.3)
    (mod_text_width 0.05)
    (pad_size 0.1 0.1)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /RUN_PD)
  (net 3 /LDO_VIN)
  (net 4 /V_OUT_CONN)
  (net 5 /LDO_VFB)
  (net 6 /LDO_SW)
  (net 7 /LABEL_NODE)
  (net 8 /LDO_MODE)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /LABEL_NODE)
    (add_net /LDO_MODE)
    (add_net /LDO_SW)
    (add_net /LDO_VFB)
    (add_net /LDO_VIN)
    (add_net /RUN_PD)
    (add_net /V_OUT_CONN)
    (add_net GND)
  )
  (module popsu_footprints:BARREL_JACK (layer F.Cu) (tedit 597E1490)
    (at 151.5 98.5 180)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference J2 (at -8.45 5.75 360) (layer F.SilkS))
    (fp_text value BARREL_JACK (at -8 -4.45 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 4.06 3.3) (layers F.Cu F.Mask)
      (net 4 /V_OUT_CONN))
    (pad 2 smd rect (at -9.14 -7.19 180) (size 6.35 3.81) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -9.14 6.1 180) (size 6.35 3.3) (layers F.Cu F.Mask)
      (net 2 /RUN_PD))
  )
  (module popsu_footprints:label_footprint2 (layer B.Cu) (tedit 597D49E9)
    (at 165.9 99.2)
    (fp_text reference "" (at 0 1.125) (layer B.SilkS))
    (fp_text value "" (at 0 -1.125) (layer B.Fab))
    (pad 1 smd oval (at 0 0.1) (size 0.1 0.1) (layers B.Cu B.Mask)
      (net 7 /LABEL_NODE))
    (pad 2 smd oval (at 0 -0.1) (size 0.1 0.1) (layers B.Cu B.Mask)
      (net 7 /LABEL_NODE))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 597E10AA)
    (at 141 101.4)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 2.1 0) (layer F.SilkS))
    (fp_text value 10kΩ (at 5.1 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 2 /RUN_PD))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 3 /LDO_VIN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module popsu_footprints:S6-TSOT-23 (layer F.Cu) (tedit 597D3704)
    (at 137.4 99.8 90)
    (fp_text reference U1 (at -1.74 0 180) (layer F.SilkS))
    (fp_text value LTC3405 (at 0 0 90) (layer F.Fab))
    (pad 6 smd rect (at -0.95 -1.31 90) (size 0.6 1.2) (layers F.Cu F.Mask)
      (net 8 /LDO_MODE))
    (pad 1 smd rect (at -0.95 1.31 90) (size 0.6 1.2) (layers F.Cu F.Mask)
      (net 2 /RUN_PD))
    (pad 5 smd rect (at 0 -1.31 90) (size 0.6 1.2) (layers F.Cu F.Mask)
      (net 5 /LDO_VFB))
    (pad 2 smd rect (at 0 1.31 90) (size 0.6 1.2) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.95 -1.31 90) (size 0.6 1.2) (layers F.Cu F.Mask)
      (net 3 /LDO_VIN))
    (pad 3 smd rect (at 0.95 1.31 90) (size 0.6 1.2) (layers F.Cu F.Mask)
      (net 6 /LDO_SW))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 597E10BE)
    (at 135.4 97.2)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.4) (layer F.SilkS))
    (fp_text value 4.7µF (at -0.5 -2.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Mask)
      (net 3 /LDO_VIN))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 597E10D2)
    (at 135.1 104.6 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -2.3 -0.1 180) (layer F.SilkS))
    (fp_text value 22pF (at -3.4 -1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Mask)
      (net 4 /V_OUT_CONN))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Mask)
      (net 5 /LDO_VFB))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 597E10C2)
    (at 139.4 97.2 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 1.4 180) (layer F.SilkS))
    (fp_text value 4.7µF (at -0.3 2.9 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Mask)
      (net 4 /V_OUT_CONN))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 597E1109)
    (at 135.1 102.9 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -2.2 0 180) (layer F.SilkS))
    (fp_text value 330kΩ (at 0.9 -3.2 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 6 /LDO_SW))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 5 /LDO_VFB))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 597E110F)
    (at 133.5 101.2)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 120kΩ (at -4.2 4.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 5 /LDO_VFB))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module popsu_footprints:5KT (layer F.Cu) (tedit 597D3C31)
    (at 145.4 97.6 180)
    (fp_text reference L1 (at -0.1 -0.1 180) (layer F.SilkS))
    (fp_text value 10µH (at 0 4.625 180) (layer F.Fab))
    (pad 1 smd rect (at 2.8 0 180) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 6 /LDO_SW))
    (pad 2 smd rect (at -2.8 0 180) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 4 /V_OUT_CONN))
  )
  (module popsu_footprints:USB_Micro-B-SMD (layer F.Cu) (tedit 59757E13)
    (at 129.4 99.9 270)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference J1 (at 0 -2.8 270) (layer F.SilkS))
    (fp_text value USB_OTG (at -0.1 2.2 270) (layer F.Fab))
    (pad 6 smd rect (at -3.8 1.45 90) (size 1.8 2.1) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 3.8 1.45 90) (size 1.8 2.1) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.15 -1.2) (size 1.6 2.1) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.3 -1.35) (size 1.35 0.4) (layers F.Cu F.Mask)
      (net 3 /LDO_VIN))
    (pad 2 smd rect (at -0.65 -1.35) (size 1.35 0.4) (layers F.Cu F.Mask))
    (pad 3 smd rect (at 0 -1.35) (size 1.35 0.4) (layers F.Cu F.Mask))
    (pad 4 smd rect (at 0.65 -1.35) (size 1.35 0.4) (layers F.Cu F.Mask))
    (pad 5 smd rect (at 1.3 -1.35) (size 1.35 0.4) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 3.15 -1.2) (size 1.6 2.1) (layers F.Cu F.Mask)
      (net 1 GND))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 597E10B6)
    (at 141 104.6)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 2.1 0) (layer F.SilkS))
    (fp_text value 0R (at 4.1 0.1) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 8 /LDO_MODE))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 3 /LDO_VIN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 597E10B0)
    (at 141 103)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 2.1 0) (layer F.SilkS))
    (fp_text value 0R (at 4.1 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 8 /LDO_MODE))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module popsu_footprints:pocket-operator-sm (layer B.Cu) (tedit 0)
    (at 143.25 107)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module popsu_footprints:nuts-bolts-osh-sm (layer B.Cu) (tedit 0)
    (at 158 92.75)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module popsu_footprints:power-ss (layer B.Cu) (tedit 0)
    (at 135.8 93.3)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (gr_line (start 165.25 109) (end 127.5 109) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 167.5 91.75) (end 167.5 106.75) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127.5 89.25) (end 165 89.25) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125 106.5) (end 125 91.75) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 127.5 91.75) (end 125 91.75) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 127.5 106.5) (end 127.5 109) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 165.25 106.75) (end 167.5 106.75) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 165 91.75) (end 165 89.25) (angle 90) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.5 109) (xy 125 109) (xy 125 89.25) (xy 167.5 89.25)
      )
    )
  )
  (zone (net 6) (net_name /LDO_SW) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.16))
    (min_thickness 0.16)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.5 99.25) (xy 138 99.25) (xy 138 98.5) (xy 139.5 98) (xy 140.75 98)
        (xy 140.75 96.75) (xy 143.5 96.75)
      )
    )
  )
  (zone (net 7) (net_name /LABEL_NODE) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.7 89.3) (xy 167.7 109) (xy 124.8 109.4) (xy 124.9 89.1)
      )
    )
  )
  (zone (net 3) (net_name /LDO_VIN) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.16))
    (min_thickness 0.16)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.4 97.842857) (xy 136.7 98.4) (xy 136.8 98.4) (xy 136.8 99.2) (xy 132.1 99.3)
        (xy 131.6 98.9) (xy 129.9 98.9) (xy 129.9 98.3) (xy 131.5 98.3) (xy 133.3 96.7)
        (xy 135.4 96.7)
      )
    )
  )
  (zone (net 4) (net_name /V_OUT_CONN) (layer F.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148 96.6) (xy 153.7 96.6) (xy 153.7 100.3) (xy 149.2 100.3) (xy 147.4 98.4)
        (xy 145.921739 96.4) (xy 140.9 96.4) (xy 140.9 96.385714) (xy 140.6 96.6) (xy 140.6 97.7)
        (xy 139.7 97.7) (xy 139.7 96.3) (xy 141.3 94.7) (xy 146.5 94.7)
      )
    )
  )
)
