(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.5448)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" mixed)
		(1 "In1.Cu" signal)
		(2 "In2.Cu" signal)
		(31 "B.Cu" mixed)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.0152)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.0432)
			)
			(layer "dielectric 1"
				(type "core")
				(color "FR4 natural")
				(thickness 0.2)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.0175)
			)
			(layer "dielectric 2"
				(type "prepreg")
				(color "FR4 natural")
				(thickness 0.991)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.0175)
			)
			(layer "dielectric 3"
				(type "core")
				(color "FR4 natural")
				(thickness 0.202)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.0432)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.0152)
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(aux_axis_origin 75 75)
		(pcbplotparams
			(layerselection 0x00010e8_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "plot/")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "/p3V3")
	(net 3 "/1V7_FIL")
	(net 4 "/BBIM")
	(net 5 "Net-(U1-BBIN)")
	(net 6 "Net-(U1-BBQN)")
	(net 7 "/BBQM")
	(net 8 "Net-(U1-BBIP)")
	(net 9 "/BBQP")
	(net 10 "Net-(U1-BBQP)")
	(net 11 "Net-(U2-VCON)")
	(net 12 "/p5VIN_FIL")
	(net 13 "/BBIP_WIRE")
	(net 14 "Net-(J3-Pin_3)")
	(net 15 "Net-(R10-Pad2)")
	(net 16 "Net-(R11-Pad2)")
	(net 17 "Net-(U2-VREF)")
	(net 18 "unconnected-(U2-EN-Pad1)")
	(net 19 "p5VIN")
	(net 20 "/r1")
	(net 21 "/r2")
	(net 22 "/r4")
	(net 23 "/r3")
	(net 24 "/rBBIP")
	(net 25 "/p5V0_3V3_FIL")
	(net 26 "/r6")
	(net 27 "/r5")
	(net 28 "Net-(T2-DC)")
	(net 29 "unconnected-(T2-ISO-Pad2)")
	(net 30 "/r7")
	(net 31 "/r9")
	(net 32 "/r8")
	(footprint "b_all:SOT-89-3"
		(layer "F.Cu")
		(at 209.85 104.225 90)
		(descr "SOT-89-3, http://ww1.microchip.com/downloads/en/DeviceDoc/3L_SOT-89_MB_C04-029C.pdf")
		(tags "SOT-89-3")
		(property "Reference" "U4"
			(at 0.375 3.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "PHA-1H"
			(at 0.3 3.5 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "b_all:SOT-89-3"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/PHA-1H+.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?89*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.5 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 -1.5 90)
			(size 1.3 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "/r7")
			(pintype "input")
		)
		(pad "2" smd custom
			(at -1.5625 0 90)
			(size 1.475 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.7375 -0.8665) (xy 3.8625 -0.8665) (xy 3.8625 0.8665) (xy 0.7375 0.8665)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "3" smd rect
			(at -1.65 1.5 90)
			(size 1.3 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "/r8")
			(pintype "output")
		)
		(model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 209.85 115.05 180)
		(property "Reference" "R2"
			(at 0 -2.2 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1"
			(at 0 1.9 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "/p5VIN_FIL")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "p5VIN")
			(pintype "passive")
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 203.7 113.1)
		(property "Reference" "R7"
			(at 0 -2.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "50"
			(at 0 1.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "/BBQP")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 218.05 115.1 180)
		(property "Reference" "R17"
			(at 0 -2.2 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "150k"
			(at 0 1.9 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "Net-(U2-VCON)")
			(pintype "passive")
		)
	)
	(footprint "b_all:C603"
		(layer "F.Cu")
		(at 201.8 100.6 90)
		(property "Reference" "C9"
			(at 0 -2.2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2u"
			(at 0 1.9 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:C603"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 90)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "Net-(U1-BBIN)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 90)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/BBIM")
			(pintype "passive")
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 196.6 104.9 90)
		(property "Reference" "R1"
			(at 0 -2.2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NU"
			(at 0 1.9 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 90)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "/r1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 90)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
	)
	(footprint "b_all:C603"
		(layer "F.Cu")
		(at 206.15 104.65 180)
		(property "Reference" "C13"
			(at 0 -2.2 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1n"
			(at 0 1.9 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:C603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "/p5V0_3V3_FIL")
			(pintype "passive")
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 200.2 112)
		(property "Reference" "R6"
			(at 0 -2.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "50"
			(at 0 1.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "/BBQM")
			(pintype "passive")
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 209.8 113.85)
		(property "Reference" "R20"
			(at 0 -2.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "/p3V3")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "/p5VIN_FIL")
			(pintype "passive")
		)
	)
	(footprint "b_all:C603"
		(layer "F.Cu")
		(at 217.7 106.2 180)
		(property "Reference" "C14"
			(at 0 -2.2 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ".01u"
			(at 0 1.9 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:C603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "/r6")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "/r9")
			(pintype "passive")
		)
	)
	(footprint "b_all:C603"
		(layer "F.Cu")
		(at 198.3 105.6 180)
		(property "Reference" "C1"
			(at 0 -2.2 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ".01u"
			(at 0 1.9 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:C603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "/r2")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "/r1")
			(pintype "passive")
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 207.4 110.8)
		(property "Reference" "R21"
			(at 0 -2.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "3k"
			(at 0 1.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/1V7_FIL")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "/p5VIN_FIL")
			(pintype "passive")
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 205.85 101.15)
		(property "Reference" "R16"
			(at 0 -2.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "Net-(R11-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/1V7_FIL")
			(pintype "passive")
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 203.5 102.3)
		(property "Reference" "R12"
			(at 0 -2.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100K"
			(at 0 1.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "Net-(U1-BBIP)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "Net-(R11-Pad2)")
			(pintype "passive")
		)
	)
	(footprint "b_all:C603"
		(layer "F.Cu")
		(at 203 111.3 90)
		(property "Reference" "C12"
			(at 0 -2.2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2u"
			(at 0 1.9 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:C603"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 90)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "/BBQP")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 90)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "Net-(U1-BBQP)")
			(pintype "passive")
		)
	)
	(footprint "b_all:SMA_Edge_062_142_0701"
		(layer "F.Cu")
		(at 195.7 105.6 90)
		(property "Reference" "J2"
			(at -1.55 -1.25 180)
			(layer "F.SilkS")
		)
		(property "Value" "SMA_Edge"
			(at 0.2 -1.3 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "b_all:SMA_Edge_062_142_0701"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at 0 -1.4 90)
			(size 0.5 2.6)
			(layers "F.Cu" "F.Mask")
			(net 20 "/r1")
			(pinfunction "RF")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -4.2418 -0.1 90)
			(size 1.9 5.2)
			(layers "*.Mask" "F.Cu")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.25)
		)
		(pad "2" smd rect
			(at -4.2 -0.1 90)
			(size 1.9 5.2)
			(layers "*.Mask" "B.Cu")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.25)
		)
		(pad "2" smd rect
			(at 4.2 -0.1 90)
			(size 1.9 5.2)
			(layers "*.Mask" "B.Cu")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.25)
		)
		(pad "2" smd rect
			(at 4.2418 -0.1 90)
			(size 1.9 5.2)
			(layers "*.Mask" "F.Cu")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.25)
		)
		(model "${T_LIBS}/3d/t_RF_conn/SMA_Edge.wrl"
			(offset
				(xyz 0 3.174999952 0.3809999943)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 270 0 90)
			)
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 203.6 109.6)
		(property "Reference" "R9"
			(at 0 -2.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100K"
			(at 0 1.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "Net-(U1-BBQP)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "Net-(R10-Pad2)")
			(pintype "passive")
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 217.35 116.95 -90)
		(property "Reference" "R18"
			(at 0 -2.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "118k"
			(at 0 1.9 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 270)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "Net-(U2-VCON)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 270)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(U2-VREF)")
			(pintype "passive")
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 204.9 110.8)
		(property "Reference" "R14"
			(at 0 -2.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "Net-(R10-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/1V7_FIL")
			(pintype "passive")
		)
	)
	(footprint "Package_LGA:Texas_SIL0008D_MicroSiP-8-1EP_2.8x3mm_P0.65mm_EP1.1x1.9mm"
		(layer "F.Cu")
		(at 214.8 114.9 180)
		(descr "Texas SIL0008D MicroSiP, 8 Pin (http://www.ti.com/lit/ds/symlink/tps82130.pdf#page=19), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "Texas MicroSiP NoLead")
		(property "Reference" "U2"
			(at -1.05 2.35 180)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 2.45 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_LGA:Texas_SIL0008D_MicroSiP-8-1EP_2.8x3mm_P0.65mm_EP1.1x1.9mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at 0 -0.63 180)
			(size 0.89 0.51)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0 0 180)
			(size 0.89 0.51)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0 0.63 180)
			(size 0.89 0.51)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -1.0625 -0.975 180)
			(size 0.625 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "unconnected-(U2-EN-Pad1)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.0625 -0.325 180)
			(size 0.625 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "Net-(U2-VCON)")
			(pinfunction "VCON")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -1.0625 0.325 180)
			(size 0.625 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/p3V3")
			(pinfunction "FB")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -1.0625 0.975 180)
			(size 0.625 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "SGND")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at 1.0625 0.975 180)
			(size 0.625 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/p3V3")
			(pinfunction "VOUT")
			(pintype "output")
		)
		(pad "6" smd roundrect
			(at 1.0625 0.325 180)
			(size 0.625 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "PGND")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at 1.0625 -0.325 180)
			(size 0.625 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "/p5VIN_FIL")
			(pinfunction "VIN")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at 1.0625 -0.975 180)
			(size 0.625 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "Net-(U2-VREF)")
			(pinfunction "VREF")
			(pintype "output")
		)
		(pad "9" smd rect
			(at 0 0 180)
			(size 1.1 1.9)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
			(zone_connect 2)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_LGA.3dshapes/Texas_SIL0008D_MicroSiP-8-1EP_2.8x3mm_P0.65mm_EP1.1x1.9mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "b_all:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
		(layer "F.Cu")
		(at 202.4 106.1)
		(descr "QFN, 24 Pin (http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf#page=278), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "QFN NoLead")
		(property "Reference" "U1"
			(at 3.1 2.6 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 3.3 0)
			(layer "F.Fab")
		)
		(property "Footprint" "b_all:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.65 -0.65)
			(size 1.05 1.05)
			(layers "F.Paste")
			(roundrect_rratio 0.238095)
		)
		(pad "" smd roundrect
			(at -0.65 0.65)
			(size 1.05 1.05)
			(layers "F.Paste")
			(roundrect_rratio 0.238095)
		)
		(pad "" smd roundrect
			(at 0.65 -0.65)
			(size 1.05 1.05)
			(layers "F.Paste")
			(roundrect_rratio 0.238095)
		)
		(pad "" smd roundrect
			(at 0.65 0.65)
			(size 1.05 1.05)
			(layers "F.Paste")
			(roundrect_rratio 0.238095)
		)
		(pad "1" smd roundrect
			(at -1.9375 -1.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "NC_PD")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.9375 -0.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -1.9375 -0.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "/r2")
			(pinfunction "LOP")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -1.9375 0.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/r3")
			(pinfunction "LOM")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -1.9375 0.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at -1.9375 1.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "Net-(J3-Pin_3)")
			(pinfunction "NC_GC")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -1.25 1.9375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "NC_GND")
			(pintype "passive")
		)
		(pad "8" smd roundrect
			(at -0.75 1.9375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "9" smd roundrect
			(at -0.25 1.9375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U1-BBQN)")
			(pinfunction "BBQN")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at 0.25 1.9375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "Net-(U1-BBQP)")
			(pinfunction "BBQP")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 0.75 1.9375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "12" smd roundrect
			(at 1.25 1.9375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "13" smd roundrect
			(at 1.9375 1.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "NC_GND")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at 1.9375 0.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "15" smd roundrect
			(at 1.9375 0.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "NC_GND")
			(pintype "passive")
		)
		(pad "16" smd roundrect
			(at 1.9375 -0.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 27 "/r5")
			(pinfunction "RF_OUT")
			(pintype "output")
		)
		(pad "17" smd roundrect
			(at 1.9375 -0.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "18" smd roundrect
			(at 1.9375 -1.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "/p5V0_3V3_FIL")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "19" smd roundrect
			(at 1.25 -1.9375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "20" smd roundrect
			(at 0.75 -1.9375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "21" smd roundrect
			(at 0.25 -1.9375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(U1-BBIP)")
			(pinfunction "BBIP")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at -0.25 -1.9375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "Net-(U1-BBIN)")
			(pinfunction "BBIN")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at -0.75 -1.9375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "24" smd roundrect
			(at -1.25 -1.9375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "/p5V0_3V3_FIL")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "25" smd rect
			(at 0 0)
			(size 2.6 2.6)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
			(zone_connect 2)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "b_all:C603"
		(layer "F.Cu")
		(at 217.4 113.4 -90)
		(property "Reference" "C15"
			(at 0 -2.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "470p"
			(at 0 1.9 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:C603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 270)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 270)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "Net-(U2-VCON)")
			(pintype "passive")
		)
	)
	(footprint "b_all:SMA_Edge_062_142_0701"
		(layer "F.Cu")
		(at 218.75 106.2 -90)
		(property "Reference" "J11"
			(at -2.2 1.7 0)
			(layer "F.SilkS")
		)
		(property "Value" "SMA_Edge"
			(at 0.2 -1.3 90)
			(layer "F.Fab")
		)
		(property "Footprint" "b_all:SMA_Edge_062_142_0701"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at 0 -1.4 270)
			(size 0.5 2.6)
			(layers "F.Cu" "F.Mask")
			(net 26 "/r6")
			(pinfunction "RF")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -4.2418 -0.1 270)
			(size 1.9 5.2)
			(layers "*.Mask" "F.Cu")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.25)
		)
		(pad "2" smd rect
			(at -4.2 -0.1 270)
			(size 1.9 5.2)
			(layers "*.Mask" "B.Cu")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.25)
		)
		(pad "2" smd rect
			(at 4.2 -0.1 270)
			(size 1.9 5.2)
			(layers "*.Mask" "B.Cu")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.25)
		)
		(pad "2" smd rect
			(at 4.2418 -0.1 270)
			(size 1.9 5.2)
			(layers "*.Mask" "F.Cu")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.25)
		)
		(model "${T_LIBS}/3d/t_RF_conn/SMA_Edge.wrl"
			(offset
				(xyz 0 3.174999952 0.3809999943)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 270 0 90)
			)
		)
	)
	(footprint "b_all:C603"
		(layer "F.Cu")
		(at 201.9 111.3 90)
		(property "Reference" "C10"
			(at 0 -2.2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2u"
			(at 0 1.9 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:C603"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 90)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "/BBQM")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 90)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "Net-(U1-BBQN)")
			(pintype "passive")
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 201.3 109.6 180)
		(property "Reference" "R10"
			(at 0 -2.2 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100K"
			(at 0 1.9 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "Net-(U1-BBQN)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "Net-(R10-Pad2)")
			(pintype "passive")
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 200.1 99.9)
		(property "Reference" "R4"
			(at 0 -2.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "50"
			(at 0 1.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/BBIM")
			(pintype "passive")
		)
	)
	(footprint "b_all:C603"
		(layer "F.Cu")
		(at 206.15 103.45 180)
		(property "Reference" "C2"
			(at 0 -2.2 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2uF"
			(at 0 1.9 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:C603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "/p5V0_3V3_FIL")
			(pintype "passive")
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 207.4 109.65)
		(property "Reference" "R22"
			(at 0 -2.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/1V7_FIL")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
	)
	(footprint "b_all:C603"
		(layer "F.Cu")
		(at 206.7 99.5 -90)
		(property "Reference" "C5"
			(at 0 -2.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2u"
			(at 0 1.9 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:C603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 270)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 270)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/1V7_FIL")
			(pintype "passive")
		)
	)
	(footprint "b_all:C603"
		(layer "F.Cu")
		(at 207.4 108.5 180)
		(property "Reference" "C7"
			(at 0 -2.2 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2u"
			(at 0 1.9 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:C603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/1V7_FIL")
			(pintype "passive")
		)
	)
	(footprint "b_all:PinHeader_2x04_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 201.8 114.85 -90)
		(descr "Through hole angled pin header, 2x04, 2.54mm pitch, 6mm pin length, double rows")
		(tags "Through hole angled pin header THT 2x04 2.54mm double row")
		(property "Reference" "J4"
			(at -1.75 7.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x04_Odd_Even"
			(at 5.655 9.89 90)
			(layer "F.Fab")
		)
		(property "Footprint" "b_all:PinHeader_2x04_P2.54mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x04, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.31 3.81 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/BBIP_WIRE")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/BBIM")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/BBQP")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/BBQM")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 2.54 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "b_all:C805"
		(layer "F.Cu")
		(at 205.95 114.6)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at 0.2 -1.4 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10u"
			(at 0 1.6 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:C805"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "/p5V0_3V3_FIL")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "b_all:SMA_Edge_062"
		(layer "F.Cu")
		(at 202.7 95.2)
		(property "Reference" "J1"
			(at -4.445 4.064 90)
			(layer "F.SilkS")
		)
		(property "Value" "SMA_Edge"
			(at 0.2 -1.3 0)
			(layer "F.Fab")
		)
		(property "Footprint" "b_all:SMA_Edge_062"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0 -0.1)
			(size 1.4986 5.2)
			(layers "F.Cu" "F.Mask")
			(net 24 "/rBBIP")
			(pinfunction "RF")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -4.2418 -0.1)
			(size 1.6002 5.2)
			(layers "*.Mask" "F.Cu")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.25)
		)
		(pad "2" smd rect
			(at 4.2418 -0.1)
			(size 1.6002 5.2)
			(layers "*.Mask" "F.Cu")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.25)
		)
		(model "${T_LIBS}/3d/t_RF_conn/SMA_Edge.wrl"
			(offset
				(xyz 0 3.174999952 0.3809999943)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 270 0 90)
			)
		)
	)
	(footprint "b_all:C603"
		(layer "F.Cu")
		(at 198.3 106.7 180)
		(property "Reference" "C3"
			(at 0 -2.2 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ".01u"
			(at 0 1.9 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:C603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/r3")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "/r4")
			(pintype "passive")
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 203.6 99)
		(property "Reference" "R8"
			(at 0 -2.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NU"
			(at 0 1.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "/rBBIP")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 205.85 102.3)
		(property "Reference" "R15"
			(at 0 -2.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "Net-(R11-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "/p5V0_3V3_FIL")
			(pintype "passive")
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 201.1 102.3 180)
		(property "Reference" "R11"
			(at 0 -2.2 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100K"
			(at 0 1.9 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "Net-(U1-BBIN)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "Net-(R11-Pad2)")
			(pintype "passive")
		)
	)
	(footprint "b_all:L805"
		(layer "F.Cu")
		(at 207.8 112.4)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "L1"
			(at 0.2 -1.4 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "L805"
			(at 0 1.6 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:L805"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "/p5V0_3V3_FIL")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/p3V3")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "b_all:GU1604"
		(layer "F.Cu")
		(at 214.1 107.7 180)
		(property "Reference" "T2"
			(at 2.6 3.3 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TCBT-2R5G"
			(at 0 -3 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:GU1604"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr through_hole)
		(fp_text user "REF**"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.27 -1.27 180)
			(size 0.762 1.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "Net-(T2-DC)")
			(pinfunction "DC")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 1.25 -1.25 180)
			(size 0.762 1.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "unconnected-(T2-ISO-Pad2)")
			(pinfunction "ISO")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 1.25 1.25 180)
			(size 0.762 1.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "/r8")
			(pinfunction "RF_DC")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -1.25 1.25 180)
			(size 0.762 1.27)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "/r9")
			(pinfunction "RF")
			(pintype "input")
		)
	)
	(footprint "b_all:PinHeader_1x04_P2.54mm_Vertical_SMD_Pin1Right"
		(layer "F.Cu")
		(at 209.05 118.85 -90)
		(descr "surface-mounted straight pin header, 1x04, 2.54mm pitch, single row, style 2 (pin 1 right)")
		(tags "Surface mounted pin header SMD 1x04 2.54mm single row style2 pin1 right")
		(property "Reference" "J3"
			(at 1.2 -6.15 -90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04"
			(at 0 6.14 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "b_all:PinHeader_1x04_P2.54mm_Vertical_SMD_Pin1Right"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.655 -3.81 270)
			(size 2.51 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.655 -1.27 270)
			(size 2.51 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "p5VIN")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.655 1.27 270)
			(size 2.51 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "Net-(J3-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.655 3.81 270)
			(size 2.51 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "/BBIP_WIRE")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical_SMD_Pin1Right.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "b_all:C805"
		(layer "F.Cu")
		(at 212.05 114.8 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at 0.2 -1.4 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10u"
			(at 0 1.6 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:C805"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "/p5VIN_FIL")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 196.9 107.8)
		(property "Reference" "R3"
			(at 0 -2.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "50"
			(at 0 1.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "/r4")
			(pintype "passive")
		)
	)
	(footprint "b_all:C603"
		(layer "F.Cu")
		(at 217.4 108.35 180)
		(property "Reference" "C19"
			(at 0 -2.2 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ".01uF"
			(at 0 1.9 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:C603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "25340-001"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "Net-(T2-DC)")
			(pintype "passive")
		)
	)
	(footprint "b_all:C603"
		(layer "F.Cu")
		(at 205.9 105.9 180)
		(property "Reference" "C6"
			(at 0 -2.2 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ".01u"
			(at 0 1.9 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:C603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "/r7")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "/r5")
			(pintype "passive")
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 213.2 110.6)
		(property "Reference" "R23"
			(at 0 -2.2 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NU"
			(at 0 1.9 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "/p5VIN_FIL")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "Net-(T2-DC)")
			(pintype "passive")
		)
	)
	(footprint "b_all:C603"
		(layer "F.Cu")
		(at 202.9 100.6 90)
		(property "Reference" "C11"
			(at 0 -2.2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2u"
			(at 0 1.9 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:C603"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 90)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "Net-(U1-BBIP)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 90)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "/rBBIP")
			(pintype "passive")
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 204 100.6 -90)
		(property "Reference" "R19"
			(at 0 -2.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.9 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 270)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "/rBBIP")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 270)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "/BBIP_WIRE")
			(pintype "passive")
		)
	)
	(footprint "b_all:R603"
		(layer "F.Cu")
		(at 204.9 111.9)
		(property "Reference" "R13"
			(at 0 -2.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:R603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "Net-(R10-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "/p5V0_3V3_FIL")
			(pintype "passive")
		)
	)
	(footprint "b_all:C805"
		(layer "F.Cu")
		(at 212.4 112.25)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 0.2 -1.4 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10u"
			(at 0 1.6 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:C805"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/p3V3")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "b_all:C603"
		(layer "F.Cu")
		(at 198.95 103.8)
		(property "Reference" "C4"
			(at 0 -2.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1n"
			(at 0 1.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "b_all:C603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "IQmod.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "/p5V0_3V3_FIL")
			(pintype "passive")
		)
	)
	(gr_line
		(start 192.6 122)
		(end 192.6 92.1)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 221.65 122)
		(end 192.6 122)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.6 92.1)
		(end 221.65 92.1)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 221.65 92.1)
		(end 221.65 122)
		(layer "Edge.Cuts")
	)
	(gr_text "IQmod"
		(at 194.1 95.45 90)
		(layer "F.SilkS")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.3)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 192.8 92.3) (xy 192.8 121.8) (xy 221.4 121.55) (xy 221.4 92.05)
			)
		)
	)
	(zone
		(net 2)
		(net_name "/p3V3")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.4)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 213.3 115) (xy 211.45 115) (xy 211.45 116.15) (xy 212.75 116.2) (xy 213.3 115.45)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 192.8 92.35) (xy 192.85 121.8) (xy 221.5 121.7) (xy 221.4 92.25)
			)
		)
	)
	(zone
		(net 2)
		(net_name "/p3V3")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.3)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 208.9 113.2) (xy 214.45 113.2) (xy 214.45 111.45) (xy 208.9 111.45)
			)
		)
	)
	(zone
		(net 25)
		(net_name "/p5V0_3V3_FIL")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads
			(clearance 0.3)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 205.2 103.7) (xy 204.2 103.7) (xy 199.4 103.7) (xy 199.4 104.6) (xy 204.65 104.6) (xy 205.75 114.2)
				(xy 208 114.2) (xy 206.9 104.35)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.153)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 221.45 121.45) (xy 192.9 121.6) (xy 192.85 92.4) (xy 221.4 92.25)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Mask")
		(hatch full 0.508)
		(priority 1)
		(connect_pads yes
			(clearance 0.22)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 217.5 116.5) (xy 217.5 117.5) (xy 220 117.5) (xy 220 116.5)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Mask")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads yes
			(clearance 0.22)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 221.4 97.3) (xy 208.6 97.3) (xy 208.6 92.3) (xy 221.4 92.3)
			)
		)
	)
)