(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu16.04.1)
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 1924)
    (zones 0)
    (modules 89)
    (nets 58)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.25)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.85)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C3-Pad1)")
  (net 3 "Net-(C5-Pad1)")
  (net 4 "Net-(C6-Pad1)")
  (net 5 +15V)
  (net 6 -5V)
  (net 7 "Net-(C12-Pad1)")
  (net 8 GNDA)
  (net 9 "Net-(C13-Pad1)")
  (net 10 "Net-(C14-Pad1)")
  (net 11 "Net-(C15-Pad1)")
  (net 12 GNDPWR)
  (net 13 +5V)
  (net 14 "Net-(D1-Pad1)")
  (net 15 "Net-(D2-Pad2)")
  (net 16 BUF_OUT)
  (net 17 KVD_OUT)
  (net 18 "Net-(Q1-Pad1)")
  (net 19 "Net-(Q1-Pad2)")
  (net 20 "Net-(Q3-Pad2)")
  (net 21 "Net-(Q4-Pad2)")
  (net 22 "Net-(R16-Pad2)")
  (net 23 "Net-(R18-Pad2)")
  (net 24 "Net-(U1-Pad5)")
  (net 25 "Net-(U2-Pad1)")
  (net 26 "Net-(R8-Pad2)")
  (net 27 Vreg)
  (net 28 /1052_IN)
  (net 29 /1052_FB)
  (net 30 /1052_OUT)
  (net 31 /KVD_IN)
  (net 32 "Net-(C3-Pad2)")
  (net 33 VOUT_NEG)
  (net 34 "Net-(C23-Pad1)")
  (net 35 "Net-(C26-Pad1)")
  (net 36 "Net-(C25-Pad1)")
  (net 37 VOUT_P)
  (net 38 "Net-(R22-Pad2)")
  (net 39 "Net-(C20-Pad1)")
  (net 40 "Net-(R20-Pad1)")
  (net 41 "Net-(R11-Pad2)")
  (net 42 "Net-(R10-Pad1)")
  (net 43 "Net-(U5-Pad4)")
  (net 44 "Net-(C27-Pad1)")
  (net 45 "Net-(U4-Pad7)")
  (net 46 "Net-(D3-Pad2)")
  (net 47 "Net-(L2-Pad1)")
  (net 48 "Net-(U3-Pad5)")
  (net 49 "Net-(U3-Pad6)")
  (net 50 "Net-(D4-Pad1)")
  (net 51 "Net-(C21-Pad1)")
  (net 52 "Net-(J3-Pad2)")
  (net 53 "Net-(J3-Pad3)")
  (net 54 "Net-(J3-Pad4)")
  (net 55 "Net-(D7-Pad2)")
  (net 56 "Net-(D6-Pad1)")
  (net 57 "Net-(D5-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +15V)
    (add_net +5V)
    (add_net -5V)
    (add_net /1052_FB)
    (add_net /1052_IN)
    (add_net /1052_OUT)
    (add_net /KVD_IN)
    (add_net BUF_OUT)
    (add_net GND)
    (add_net GNDA)
    (add_net GNDPWR)
    (add_net KVD_OUT)
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C23-Pad1)")
    (add_net "Net-(C25-Pad1)")
    (add_net "Net-(C26-Pad1)")
    (add_net "Net-(C27-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(L2-Pad1)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q3-Pad2)")
    (add_net "Net-(Q4-Pad2)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R16-Pad2)")
    (add_net "Net-(R18-Pad2)")
    (add_net "Net-(R20-Pad1)")
    (add_net "Net-(R22-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U4-Pad7)")
    (add_net "Net-(U5-Pad4)")
    (add_net VOUT_NEG)
    (add_net VOUT_P)
    (add_net Vreg)
  )
  (module Footprints:PCB_mount_banana (layer F.Cu) (tedit 5CE7AA7C)
    (at 180.89 98.48 90)
    (fp_text reference J4 (at 0 0.5 90) (layer F.SilkS))
    (fp_text value banana (at 0 -0.5 90) (layer F.Fab))
    (pad 5 thru_hole circle (at -5.08 6.36 90) (size 1.524 1.524) (drill 0.85) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -5.08 -3.8 90) (size 1.524 1.524) (drill 0.85) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 -3.8 90) (size 1.524 1.524) (drill 0.85) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 5.08 6.36 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0.01 90) (size 5 5) (drill 2.5) (layers *.Cu *.Mask)
      (net 16 BUF_OUT))
  )
  (module Footprints:PCB_mount_banana (layer F.Cu) (tedit 5CE7A97C)
    (at 180.925001 113.494999 90)
    (fp_text reference J5 (at 0 0.5 90) (layer F.SilkS))
    (fp_text value banana (at 0 -0.5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0.01 90) (size 5 5) (drill 2.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5.08 6.36 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 -3.8 90) (size 1.524 1.524) (drill 0.85) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -5.08 -3.8 90) (size 1.524 1.524) (drill 0.85) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -5.08 6.36 90) (size 1.524 1.524) (drill 0.85) (layers *.Cu *.Mask))
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 156.57 64.77 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 32 "Net-(C3-Pad2)"))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 133.12 57.89 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D7 (at -0.14 1.65 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 33 VOUT_NEG))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 55 "Net-(D7-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 142.38 113.09 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D6 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 37 VOUT_P))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 56 "Net-(D6-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 105.918 51.308 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D5 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 12 GNDPWR))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 57 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 136.93 118.04)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R19 (at 3.39 -0.14) (layer F.SilkS))
    (fp_text value 4.7R (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 37 VOUT_P))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 51 "Net-(C21-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 103.886 49.022)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R13 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 2K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 13 +5V))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 57 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 146.8 113.05)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R25 (at 0 1.76) (layer F.SilkS))
    (fp_text value 5K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 GNDA))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 56 "Net-(D6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 129.01 57.86 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R26 (at -0.1 1.76 180) (layer F.SilkS))
    (fp_text value 2K (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 55 "Net-(D7-Pad2)"))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 GNDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5005-5009_Compact (layer F.Cu) (tedit 5CE7AE53)
    (at 98.552 44.704)
    (descr "Keystone Miniature THM Test Point 5005-5009, http://www.keyelco.com/product-pdf.cfm?p=1314")
    (tags "Through Hole Mount Test Points")
    (fp_text reference TP2 (at 0.254 2.794) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.75) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 12 GNDPWR))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5005-5009_Compact.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5005-5009_Compact (layer F.Cu) (tedit 5CE7AE5C)
    (at 103.59 40.45)
    (descr "Keystone Miniature THM Test Point 5005-5009, http://www.keyelco.com/product-pdf.cfm?p=1314")
    (tags "Through Hole Mount Test Points")
    (fp_text reference TP1 (at 3.344 -0.064) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.75) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 13 +5V))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5005-5009_Compact.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5005-5009_Compact (layer F.Cu) (tedit 5CE7AE75)
    (at 98.552 40.386)
    (descr "Keystone Miniature THM Test Point 5005-5009, http://www.keyelco.com/product-pdf.cfm?p=1314")
    (tags "Through Hole Mount Test Points")
    (fp_text reference TP4 (at 0 -2.794) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.75) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 12 GNDPWR))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5005-5009_Compact.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5005-5009_Compact (layer F.Cu) (tedit 5CE7AE44)
    (at 103.59 44.76)
    (descr "Keystone Miniature THM Test Point 5005-5009, http://www.keyelco.com/product-pdf.cfm?p=1314")
    (tags "Through Hole Mount Test Points")
    (fp_text reference TP3 (at 3.598 0.198) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 13 +5V))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5005-5009_Compact.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 103.28 35.72)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C30 (at 0.04 1.97) (layer F.SilkS))
    (fp_text value .01uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 13 +5V))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 12 GNDPWR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_USB:USB_Micro-B_Wuerth-629105150521 (layer F.Cu) (tedit 59E3D6C4)
    (at 103.58 29.41)
    (descr "USB Micro-B receptacle, http://www.mouser.com/ds/2/445/629105150521-469306.pdf")
    (tags "usb micro receptacle")
    (attr smd)
    (fp_text reference J3 (at 6.88 -2.06) (layer F.SilkS))
    (fp_text value USB_B_Micro (at 0 5.6) (layer F.Fab))
    (fp_text user %R (at 0 1.05) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 3.75) (layer Dwgs.User))
    (pad 1 smd rect (at -1.3 -1.9) (size 0.45 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (pad 2 smd rect (at -0.65 -1.9) (size 0.45 1.3) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(J3-Pad2)"))
    (pad 3 smd rect (at 0 -1.9) (size 0.45 1.3) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(J3-Pad3)"))
    (pad 4 smd rect (at 0.65 -1.9) (size 0.45 1.3) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(J3-Pad4)"))
    (pad 5 smd rect (at 1.3 -1.9) (size 0.45 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 GNDPWR))
    (pad 6 thru_hole oval (at -3.725 -1.85) (size 1.45 2) (drill oval 0.85 1.4) (layers *.Cu *.Mask)
      (net 12 GNDPWR))
    (pad 6 thru_hole oval (at 3.725 -1.85) (size 1.45 2) (drill oval 0.85 1.4) (layers *.Cu *.Mask)
      (net 12 GNDPWR))
    (pad 6 thru_hole oval (at -3.875 1.95) (size 1.15 1.8) (drill oval 0.55 1.2) (layers *.Cu *.Mask)
      (net 12 GNDPWR))
    (pad 6 thru_hole oval (at 3.875 1.95) (size 1.15 1.8) (drill oval 0.55 1.2) (layers *.Cu *.Mask)
      (net 12 GNDPWR))
    (pad "" np_thru_hole oval (at -2.5 -0.8) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at 2.5 -0.8) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connectors_USB.3dshapes/USB_Micro-B_Wuerth-629105150521.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_Wuerth_HCM-7050 (layer F.Cu) (tedit 5CE4E975)
    (at 129.98 115.22)
    (descr "Inductor, Wuerth Elektronik, Wuerth_HCM-7050, 7.2mmx7.0mm")
    (tags "inductor Wuerth hcm smd")
    (attr smd)
    (fp_text reference L3 (at -4.82 -2.23 270) (layer F.SilkS))
    (fp_text value 1.5uH (at 0 5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 2.65 0) (size 2 3.1) (layers F.Cu F.Paste F.Mask)
      (net 37 VOUT_P))
    (pad 1 smd rect (at -2.65 0) (size 2 3.1) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(C21-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Wuerth_HCM-7050.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_Wuerth_HCM-7050 (layer F.Cu) (tedit 5CE4E8C5)
    (at 132.84 66.25 90)
    (descr "Inductor, Wuerth Elektronik, Wuerth_HCM-7050, 7.2mmx7.0mm")
    (tags "inductor Wuerth hcm smd")
    (attr smd)
    (fp_text reference L5 (at -5.04 -0.05 180) (layer F.SilkS))
    (fp_text value 2.2uH (at 0 5 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.65 0 90) (size 2 3.1) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C23-Pad1)"))
    (pad 2 smd rect (at 2.65 0 90) (size 2 3.1) (layers F.Cu F.Paste F.Mask)
      (net 33 VOUT_NEG))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Wuerth_HCM-7050.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_Wuerth_WE-PD-Typ-LS_Handsoldering (layer F.Cu) (tedit 5990349D)
    (at 109.223804 101.397287 180)
    (descr "Choke, Drossel, WE-PD Typ LS, Wuerth, SMD, Handsoldering,")
    (tags "Choke Drossel WE-PDTypLS Wuerth SMD Handsoldering ")
    (attr smd)
    (fp_text reference L2 (at 8.063804 5.167287 180) (layer F.SilkS))
    (fp_text value 15uH (at 0 7.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 5.9 0 180) (size 4.9 5.4) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -5.9 0 180) (size 4.9 5.4) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(L2-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Wuerth_WE-PD-Typ-LS.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_Wuerth_WE-PD-Typ-LS_Handsoldering (layer F.Cu) (tedit 5CE77B89)
    (at 105.853804 78.927287 90)
    (descr "Choke, Drossel, WE-PD Typ LS, Wuerth, SMD, Handsoldering,")
    (tags "Choke Drossel WE-PDTypLS Wuerth SMD Handsoldering ")
    (attr smd)
    (fp_text reference L4 (at 0 -7.2 90) (layer F.SilkS))
    (fp_text value 15uH (at 0 7.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -5.9 0 90) (size 4.9 5.4) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 5.9 0 90) (size 4.9 5.4) (layers F.Cu F.Paste F.Mask)
      (net 8 GNDA))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Wuerth_WE-PD-Typ-LS.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D12.5mm_P5.00mm (layer F.Cu) (tedit 5CE4E920)
    (at 119.76 63.91 90)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=12.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 12.5mm Electrolytic Capacitor")
    (fp_text reference C18 (at 9.66 -4.56 90) (layer F.SilkS))
    (fp_text value 47uF (at 2.5 7.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 +5V))
    (pad 2 thru_hole circle (at 5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 GNDPWR))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D12.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-7343-15_Kemet-W_Pad2.25x2.55mm_HandSolder (layer F.Cu) (tedit 5CE4E2EB)
    (at 131.963804 104.457287 90)
    (descr "Tantalum Capacitor SMD Kemet-W (7343-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C22 (at 6.31 -0.1 90) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 3.1 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -3.2 0 90) (size 2.25 2.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.111111)
      (net 37 VOUT_P))
    (pad 2 smd roundrect (at 3.2 0 90) (size 2.25 2.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.111111)
      (net 8 GNDA))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-7343-15_Kemet-W.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Files:B3100_Schottky" (layer F.Cu) (tedit 5CE3B48D)
    (at 109.643804 110.227287 180)
    (descr "Diode MELF Handsoldering")
    (tags "Diode MELF Handsoldering")
    (attr smd)
    (fp_text reference D3 (at 0 -2.25 180) (layer F.SilkS))
    (fp_text value B3100 (at 3.99034 2.64922 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.25 180) (layer F.Fab))
    (pad 2 smd rect (at 3.85 0 180) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -3.85 0 180) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(C21-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_MELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE3AD4A)
    (at 126.793804 82.432287 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R15 (at -3.375 0.1 90) (layer F.SilkS))
    (fp_text value 15K (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 11 "Net-(C15-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 10 "Net-(C14-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE3AD91)
    (at 122.383804 82.447287)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C19 (at 0 -1.86) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 27 Vreg))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE3B15C)
    (at 123.293804 78.187287 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C20 (at 0.09 -1.74 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 GNDA))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 39 "Net-(C20-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE3B30E)
    (at 122.253804 73.767287 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C23 (at -0.16 2.19 180) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.65 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 34 "Net-(C23-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE3B879)
    (at 129.043804 60.587287 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C24 (at -3.546196 -0.002713 180) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.65 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 GNDA))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 33 VOUT_NEG))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE3A71E)
    (at 137.393527 90.804409 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C27 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 44 "Net-(C27-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-7343-43_Kemet-X_Pad2.25x2.55mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 146.783527 96.624409 270)
    (descr "Tantalum Capacitor SMD Kemet-X (7343-43 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C29 (at 0.26 -3.51 270) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 3.1 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 3.2 0 270) (size 2.25 2.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.111111)
      (net 8 GNDA))
    (pad 1 smd roundrect (at -3.2 0 270) (size 2.25 2.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.111111)
      (net 5 +15V))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-7343-43_Kemet-X.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-7343-43_Kemet-X_Pad2.25x2.55mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 160.93 112.29)
    (descr "Tantalum Capacitor SMD Kemet-X (7343-43 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C28 (at 0 -3.1) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 3.1) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -3.2 0) (size 2.25 2.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.111111)
      (net 6 -5V))
    (pad 2 smd roundrect (at 3.2 0) (size 2.25 2.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.111111)
      (net 8 GNDA))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-7343-43_Kemet-X.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-7343-43_Kemet-X_Pad2.25x2.55mm_HandSolder (layer F.Cu) (tedit 5CE3A86E)
    (at 160.05 101.05)
    (descr "Tantalum Capacitor SMD Kemet-X (7343-43 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C26 (at 0 -3.1) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 3.1) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 3.2 0) (size 2.25 2.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.111111)
      (net 8 GNDA))
    (pad 1 smd roundrect (at -3.2 0) (size 2.25 2.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.111111)
      (net 35 "Net-(C26-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-7343-43_Kemet-X.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-7343-43_Kemet-X_Pad2.25x2.55mm_HandSolder (layer F.Cu) (tedit 5CE4EDE6)
    (at 119.033804 114.807287 270)
    (descr "Tantalum Capacitor SMD Kemet-X (7343-43 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C21 (at 0.032713 3.153804 270) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 3.1 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 3.2 0 270) (size 2.25 2.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.111111)
      (net 8 GNDA))
    (pad 1 smd roundrect (at -3.2 0 270) (size 2.25 2.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.111111)
      (net 51 "Net-(C21-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-7343-43_Kemet-X.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-7343-43_Kemet-X_Pad2.25x2.55mm_HandSolder (layer F.Cu) (tedit 5CE3A681)
    (at 144.553527 104.864409)
    (descr "Tantalum Capacitor SMD Kemet-X (7343-43 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C25 (at 0 -3.1) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 3.1) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -3.2 0) (size 2.25 2.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.111111)
      (net 36 "Net-(C25-Pad1)"))
    (pad 2 smd roundrect (at 3.2 0) (size 2.25 2.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.111111)
      (net 8 GNDA))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-7343-43_Kemet-X.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Files:B3100_Schottky" (layer F.Cu) (tedit 5CE3B714)
    (at 112.703804 78.577287 90)
    (descr "Diode MELF Handsoldering")
    (tags "Diode MELF Handsoldering")
    (attr smd)
    (fp_text reference D4 (at 7.01 -0.02 90) (layer F.SilkS))
    (fp_text value B3100 (at 3.99034 2.64922 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.25 90) (layer F.Fab))
    (pad 2 smd rect (at 3.85 0 90) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C23-Pad1)"))
    (pad 1 smd rect (at -3.85 0 90) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_MELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.35x2.35mm (layer F.Cu) (tedit 5A65EC84)
    (at 139.413527 97.324409 270)
    (descr "8-Lead Thermally Enhanced Plastic Small Outline (SE) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U4 (at 0 -3.5 270) (layer F.SilkS))
    (fp_text value ADP7105 (at 0 3.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +15V))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R11-Pad2)"))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 GNDA))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C27-Pad1)"))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R10-Pad1)"))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U4-Pad7)"))
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C25-Pad1)"))
    (pad "" smd rect (at 0.5875 0.5875 270) (size 0.95 0.95) (layers F.Paste))
    (pad 9 smd rect (at 0 0 270) (size 2.35 2.35) (layers F.Cu F.Mask)
      (net 8 GNDA))
    (pad "" smd rect (at -0.5875 0.5875 270) (size 0.95 0.95) (layers F.Paste))
    (pad "" smd rect (at -0.5875 -0.5875 270) (size 0.95 0.95) (layers F.Paste))
    (pad "" smd rect (at 0.5875 -0.5875 270) (size 0.95 0.95) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.35x2.35mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TSOT-23-5 (layer F.Cu) (tedit 5CE3A939)
    (at 156.76 106.71 270)
    (descr "5-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_5_05-08-1635.pdf")
    (tags TSOT-23-5)
    (attr smd)
    (fp_text reference U5 (at 0 -2.45 270) (layer F.SilkS))
    (fp_text value ADP7182 (at 0 2.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.31 -0.95 270) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 GNDA))
    (pad 2 smd rect (at -1.31 0 270) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C26-Pad1)"))
    (pad 3 smd rect (at -1.31 0.95 270) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R8-Pad2)"))
    (pad 4 smd rect (at 1.31 0.95 270) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U5-Pad4)"))
    (pad 5 smd rect (at 1.31 -0.95 270) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 -5V))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TSOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE3A68E)
    (at 137.673527 104.734409)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at -0.153527 1.795591) (layer F.SilkS))
    (fp_text value 2K (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 42 "Net-(R10-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 36 "Net-(C25-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE3A930)
    (at 153.21 105.11 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at -0.01 1.85 270) (layer F.SilkS))
    (fp_text value 2K (at 0 1.65 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 GNDA))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 26 "Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE3A92C)
    (at 153.16 100.96 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at -0.13 1.88 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 +15V))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 26 "Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE3A749)
    (at 138.313527 87.154409 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R12 (at 3.39 0.08 180) (layer F.SilkS))
    (fp_text value 11.5K (at 0 1.65 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 GNDA))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 41 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE3A760)
    (at 141.733527 88.024409 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at 3.38 0.07 90) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 +15V))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 41 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE3AF7A)
    (at 123.803804 97.197287 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R14 (at -0.02 1.63 270) (layer F.SilkS))
    (fp_text value 14K (at 0 1.65 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 "Net-(C12-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 9 "Net-(C13-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE4E290)
    (at 122.983804 107.667287)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R20 (at 2.59 -0.04 90) (layer F.SilkS))
    (fp_text value 2.15M (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 40 "Net-(R20-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 37 VOUT_P))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE4E267)
    (at 122.993804 104.747287)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R21 (at 2.58 -0.35 90) (layer F.SilkS))
    (fp_text value 100K (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 GNDA))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 40 "Net-(R20-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE3B229)
    (at 126.403804 77.257287)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R22 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 133K (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 39 "Net-(C20-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 38 "Net-(R22-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE3B2E1)
    (at 126.408804 73.757287 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R23 (at -3.49 -0.08 180) (layer F.SilkS))
    (fp_text value 1.62M (at 0 1.65 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 34 "Net-(C23-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 38 "Net-(R22-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE3A66A)
    (at 141.343527 109.744409 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference FB1 (at 0 -1.65 270) (layer F.SilkS))
    (fp_text value Ferrite_Bead (at 0 1.65 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 36 "Net-(C25-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 37 VOUT_P))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE3A5B8)
    (at 156.75 95.74 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference FB2 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value Ferrite_Bead (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 33 VOUT_NEG))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 35 "Net-(C26-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE3B8A4)
    (at 138.523804 66.187287 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R24 (at 0 -1.65 270) (layer F.SilkS))
    (fp_text value 10R (at 0 1.65 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 33 VOUT_NEG))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 34 "Net-(C23-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE1FCFA)
    (at 169.61 85.56)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0.07 1.84) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 16 BUF_OUT))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 29 /1052_FB))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:SMB_Jack_Vertical (layer F.Cu) (tedit 5A1DBFC1)
    (at 154.33 38.74)
    (descr "SMB pcb mounting jack")
    (tags "SMB Jack  Striaght")
    (fp_text reference J2 (at 0 -4.85) (layer F.SilkS))
    (fp_text value "SMB Jack" (at 0 5.05) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.24 2.24) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 BUF_OUT))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMB_Jack_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE1DC63)
    (at 164.38 51.39 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 2.99 0.01 180) (layer F.SilkS))
    (fp_text value 1nF (at 0 1.65 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 31 /KVD_IN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE1DC9F)
    (at 164.1 61.49 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 3.27 0.03 180) (layer F.SilkS))
    (fp_text value 400pF (at 0 1.65 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 28 /1052_IN))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE1DED3)
    (at 177.55 68.03 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at -0.085 -2.11 270) (layer F.SilkS))
    (fp_text value 680n (at 0 1.65 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 32 "Net-(C3-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE1E05D)
    (at 172.26 77.85)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 3.18 0.14) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 "Net-(C5-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE1DEF4)
    (at 177.47 72.95 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at -0.09 2.11 90) (layer F.SilkS))
    (fp_text value 680n (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 "Net-(C6-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 32 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE1F65E)
    (at 169.7 80.49)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at 3.03 0.14) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 30 /1052_OUT))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 29 /1052_FB))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE1DDA8)
    (at 150.917221 84.451095 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C8 (at 3.36 0.12 270) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.65 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 +15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 151.35 72.49 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C9 (at 3.06 -0.12 180) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 -5V))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5CE1DDB5)
    (at 147.847221 84.471095 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C10 (at 4.3 0.03 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.82 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 5 +15V))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE1FB44)
    (at 151.32 74.92 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C11 (at 3.36 -0.08 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.65 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 -5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE3AF7D)
    (at 123.803804 101.397287 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C12 (at -0.14 1.68 270) (layer F.SilkS))
    (fp_text value 47nF (at 0 1.65 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 "Net-(C12-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE3AB86)
    (at 127.043804 101.477287 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C13 (at 0 -1.65 270) (layer F.SilkS))
    (fp_text value 27pF (at 0 1.65 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 GNDA))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 9 "Net-(C13-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE3AD42)
    (at 129.433804 79.552287 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C14 (at 0 -1.65 270) (layer F.SilkS))
    (fp_text value 47nF (at 0 1.65 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 10 "Net-(C14-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE3AD46)
    (at 129.433804 83.817287 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C15 (at -0.12 1.96 90) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 GNDA))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 11 "Net-(C15-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE3AE14)
    (at 118.213804 82.417287 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C16 (at -0.05 -1.75) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.65 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 12 GNDPWR))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 13 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5CE3AE9E)
    (at 117.673804 79.357287 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C17 (at 0.38 1.99 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.82 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 12 GNDPWR))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 13 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323_HandSoldering (layer F.Cu) (tedit 5CE1E092)
    (at 179.82 82.53 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value BZX84-A6V2,215 (at 0.1 1.9 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.85 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 30 /1052_OUT))
    (pad 1 smd rect (at -1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323_HandSoldering (layer F.Cu) (tedit 5CE1F911)
    (at 160.06 72.39 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D2 (at -0.12 1.93 180) (layer F.SilkS))
    (fp_text value BZX84-A6V2,215 (at 0.1 1.9 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.85 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 30 /1052_OUT))
    (pad 2 smd rect (at 1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 10V_Supply:KVD_studs (layer F.Cu) (tedit 5CE8AF7D)
    (at 183.81 39.21)
    (descr "Mounting Hole 5mm")
    (tags "mounting hole 5mm")
    (attr virtual)
    (fp_text reference J1 (at -73.82 -0.42) (layer F.SilkS) hide)
    (fp_text value KVD_Studs (at -62.29 8.06) (layer F.Fab))
    (fp_text user %R (at -62.1 0) (layer F.Fab))
    (fp_text user HI (at 2.3 -9.93) (layer F.SilkS))
    (fp_text user MountingHole_4.8mm_Pad_Via (at 2.64 7.62) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -62.4 0) (size 13.5 13.5) (drill 4.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -58.65 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -59.74835 2.65165) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -62.4 3.75) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -65.05165 2.65165) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -66.15 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -65.05165 -2.65165) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -62.4 -3.75) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -59.74835 -2.65165) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.4 0) (size 13.5 13.5) (drill 4.8) (layers *.Cu *.Mask)
      (net 17 KVD_OUT))
    (pad 2 thru_hole circle (at 6.2 -0.01) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 17 KVD_OUT))
    (pad 2 thru_hole circle (at 5.57 -2.52) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 17 KVD_OUT))
    (pad 2 thru_hole circle (at 2.5 -3.8) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 17 KVD_OUT))
    (pad 2 thru_hole circle (at -1.4 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 17 KVD_OUT))
    (pad 2 thru_hole circle (at -0.46 -2.41) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 17 KVD_OUT))
    (pad 2 thru_hole circle (at -0.53 2.48) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 17 KVD_OUT))
    (pad 2 thru_hole circle (at 2.28 3.8) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 17 KVD_OUT))
    (pad 2 thru_hole circle (at 5.15 2.57) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask)
      (net 17 KVD_OUT))
  )
  (module Inductor_SMD:L_Taiyo-Yuden_MD-2020 (layer F.Cu) (tedit 5990349C)
    (at 168.8 48.87 270)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L1 (at -0.29 2.38) (layer F.SilkS))
    (fp_text value 15uH (at -2.87 0.63) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 17 KVD_OUT))
    (pad 2 smd rect (at 0.675 0 270) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 31 /KVD_IN))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 168.77 53.28 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value NJFET (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(Q1-Pad2)"))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 31 /KVD_IN))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5CE1DC03)
    (at 168.74 60.69 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at -0.1 -2.92) (layer F.SilkS))
    (fp_text value NJFET (at 0 2.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 28 /1052_IN))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Q1-Pad1)"))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5CE1F972)
    (at 152.76 68.62 90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q3 (at 1.27 -3.56 90) (layer F.SilkS))
    (fp_text value 2N3906 (at 1.27 2.79 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 -5V))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 32 "Net-(C3-Pad2)"))
    (pad 2 thru_hole oval (at 1.27 0 90) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 20 "Net-(Q3-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5CE1F54C)
    (at 185.42 76.6 270)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q4 (at -2.77 1.21 270) (layer F.SilkS))
    (fp_text value 2N3904 (at 1.27 2.79 270) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 -3.56 270) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 1.27 0 270) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 21 "Net-(Q4-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 +15V))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 172.93 49.26 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at -0.12 2.22 180) (layer F.SilkS))
    (fp_text value 100R (at 2.8 -0.04 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 17 KVD_OUT))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 31 /KVD_IN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE1DBE7)
    (at 168.73 57.09 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 3.09 0.11 180) (layer F.SilkS))
    (fp_text value 20K (at 0 1.65 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 19 "Net-(Q1-Pad2)"))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 18 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE1F51A)
    (at 181.76 78.94 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 21 "Net-(Q4-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 14 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE1E1AC)
    (at 156.59 68.87 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 3.03 -0.05 90) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 15 "Net-(D2-Pad2)"))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 20 "Net-(Q3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE1F4D0)
    (at 184.42 82.48 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value 15K (at 0 1.65 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 +15V))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 14 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE1F643)
    (at 155.54 72.35 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value 15K (at 0 1.65 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 -5V))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 15 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE3B05F)
    (at 127.998804 95.417287 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R16 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value 30.1K (at 0 1.65 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 22 "Net-(R16-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 13 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE3B001)
    (at 130.783804 89.527287 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R17 (at -0.1 -1.865 90) (layer F.SilkS))
    (fp_text value 18.7K (at 0 1.65 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 22 "Net-(R16-Pad2)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 GNDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CE3AB8A)
    (at 127.193804 91.557287 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R18 (at 0 -1.65 270) (layer F.SilkS))
    (fp_text value 49.9K (at 1.05 -2.31 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 GNDA))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 23 "Net-(R18-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-8_W7.62mm_LongPads (layer F.Cu) (tedit 5A02E8C5)
    (at 173.76 66.36 270)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference U1 (at 8.15 10.24 270) (layer F.SilkS))
    (fp_text value LTC1052 (at 3.81 9.95 270) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C3-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(U1-Pad5)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /1052_FB))
    (pad 6 thru_hole oval (at 7.62 5.08 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /1052_OUT))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /1052_IN))
    (pad 7 thru_hole oval (at 7.62 2.54 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C5-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(C3-Pad2)"))
    (pad 8 thru_hole oval (at 7.62 0 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-8_W7.62mm_LongPads (layer F.Cu) (tedit 5A02E8C5)
    (at 161.907221 85.691095 180)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference U2 (at 3.81 -2.33 180) (layer F.SilkS))
    (fp_text value BUF634 (at 3.81 9.95 180) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 180) (layer F.Fab))
    (pad 8 thru_hole oval (at 7.62 0 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 -5V))
    (pad 7 thru_hole oval (at 7.62 2.54 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 +15V))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /1052_OUT))
    (pad 6 thru_hole oval (at 7.62 5.08 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 BUF_OUT))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 7.62 7.62 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(U2-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:ETSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3x4.2mm (layer F.Cu) (tedit 5CE3AC4E)
    (at 122.143804 89.457287 90)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body with Exposed Pad [eTSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U3 (at 0 -4.3 90) (layer F.SilkS))
    (fp_text value ADP5071 (at 0 4.4 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -2.925 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 12 GNDPWR))
    (pad 2 smd rect (at -2.95 -2.275 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D3-Pad2)"))
    (pad 3 smd rect (at -2.95 -1.625 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(L2-Pad1)"))
    (pad 4 smd rect (at -2.95 -0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 8 GNDA))
    (pad 5 smd rect (at -2.95 -0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U3-Pad5)"))
    (pad 6 smd rect (at -2.95 0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U3-Pad6)"))
    (pad 7 smd rect (at -2.95 0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R20-Pad1)"))
    (pad 8 smd rect (at -2.95 1.625 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C13-Pad1)"))
    (pad 9 smd rect (at -2.95 2.275 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R16-Pad2)"))
    (pad 10 smd rect (at -2.95 2.925 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R18-Pad2)"))
    (pad 11 smd rect (at 2.95 2.925 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R16-Pad2)"))
    (pad 12 smd rect (at 2.95 2.275 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C15-Pad1)"))
    (pad 13 smd rect (at 2.95 1.625 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R22-Pad2)"))
    (pad 14 smd rect (at 2.95 0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C20-Pad1)"))
    (pad 15 smd rect (at 2.95 0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 8 GNDA))
    (pad 16 smd rect (at 2.95 -0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 27 Vreg))
    (pad 17 smd rect (at 2.95 -0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (pad 18 smd rect (at 2.95 -1.625 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (pad 19 smd rect (at 2.95 -2.275 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (pad 20 smd rect (at 2.95 -2.925 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(D4-Pad1)"))
    (pad 21 smd rect (at 0 0 90) (size 3 4.2) (layers F.Cu F.Paste F.Mask)
      (net 8 GNDA))
    (pad "" smd rect (at 0.75 -1.4 90) (size 1.2 1.14) (layers F.Paste))
    (pad "" smd rect (at -0.75 -1.4 90) (size 1.2 1.14) (layers F.Paste))
    (pad "" smd rect (at -0.75 0 90) (size 1.2 1.14) (layers F.Paste))
    (pad "" smd rect (at 0.75 0 90) (size 1.2 1.14) (layers F.Paste))
    (pad "" smd rect (at -0.75 1.4 90) (size 1.2 1.14) (layers F.Paste))
    (pad "" smd rect (at 0.75 1.4 90) (size 1.2 1.14) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/ETSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3x4.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Footprints:jop (layer F.Cu) (tedit 0)
    (at 139.45 39.14)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text GND (at 172.42 113.28) (layer F.SilkS))
  (gr_text BUF_OUT (at 170.95 97.93) (layer F.SilkS))
  (gr_text VIN (at 101.27 51.46) (layer F.SilkS))
  (gr_line (start 97.44 26.12) (end 96.56 26.12) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 96.56 26.25) (end 96.56 26.14) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 96.56 121.84) (end 96.56 26.25) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 196.41 121.84) (end 96.56 121.84) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 196.76 26.08) (end 196.41 121.84) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97.44 26.12) (end 196.76 26.08) (layer Edge.Cuts) (width 0.15))
  (gr_text 2N3906 (at 147.58 66.98 90) (layer F.SilkS))
  (gr_text 2N3904 (at 189.62 77.98 90) (layer F.SilkS))
  (gr_text LO (at 121.93 29.23) (layer F.SilkS))
  (zone (net 29) (net_name /1052_FB) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.99 50.51) (xy 166.07 50.04) (xy 164.9 49.99) (xy 164.91 48.18) (xy 165.08 45.82)
        (xy 165.98 44.63) (xy 167.36 44.11) (xy 170.165 44.195) (xy 172.15 43.78) (xy 173.52 42.23)
        (xy 176.08 39.24) (xy 177.5 36.04) (xy 178.88 38.82) (xy 179.03 40.65) (xy 173.01 46.63)
        (xy 167.32 46.62) (xy 167 50.25) (xy 166.98 50.25)
      )
    )
  )
  (zone (net 29) (net_name /1052_FB) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172.59 63.79) (xy 169.22 63.87) (xy 169.24 62.84) (xy 170.12 62.21) (xy 170.78 61.47)
        (xy 170.91 53.06) (xy 172.42 52.96) (xy 174.14 51.25) (xy 174.18 47.95) (xy 179.35 42.87)
        (xy 180.85 44.39) (xy 182.11 45.65) (xy 183 46) (xy 184.66 46.35) (xy 187.19 46.5)
        (xy 188.93 46.41) (xy 188.07 47.78) (xy 185.56 47.78) (xy 183.12 47.54) (xy 182.25 47.31)
        (xy 181.12 47.24) (xy 180.41 47.34) (xy 179.7 47.79) (xy 178.79 48.66) (xy 177.79 49.62)
        (xy 176.24 51.51) (xy 175.37 53.51) (xy 174.16 54.53) (xy 173.55 55.05) (xy 173.56 57.15)
        (xy 173.53 61.68)
      )
    )
  )
  (zone (net 29) (net_name /1052_FB) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 164.11 59.93) (xy 166.48 60.29) (xy 166.55 58.11) (xy 166.55 55.4) (xy 166.6 53.5)
        (xy 166.81 52.87) (xy 163.99 52.73) (xy 164.04 57.6)
      )
    )
  )
  (zone (net 29) (net_name /1052_FB) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 166.31 63.01) (xy 172.81 62.98) (xy 173.54 61.67) (xy 173.59 54.89) (xy 175.29 53.42)
        (xy 176.18 51.41) (xy 176.05 48.59) (xy 178.83 45.58) (xy 180.56 44.17) (xy 179.08 41.05)
        (xy 178.67 38.78) (xy 173.06 44.27) (xy 167.07 44.05) (xy 165.95 44.63) (xy 165.17 45.69)
        (xy 164.84 48.23) (xy 164.81 52.05) (xy 164.98 62.21)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.75))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 159.66 71.6) (xy 162.65 71.75) (xy 161.39 60.85) (xy 161.32 56.1) (xy 161.29 48.28)
        (xy 161.34 40.67) (xy 161.16 31.78) (xy 160.53 29.81) (xy 158.59 28.85) (xy 149.11 28.89)
        (xy 131.21 28.55) (xy 122.15 28.22) (xy 114.65 28.13) (xy 112.47 28.99) (xy 111.25 30.91)
        (xy 111.27 31.61) (xy 111.56 47.5) (xy 116.58 49.8) (xy 130.74 51.21) (xy 144.05 54.51)
        (xy 143.935 63.765) (xy 143.8775 68.3925) (xy 143.94 77.84) (xy 145.72 80.07) (xy 151.32 84.53)
        (xy 151.34 80.82) (xy 151.21 78.78) (xy 150.92 70.98)
      )
    )
  )
  (zone (net 29) (net_name /1052_FB) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.75))
    (polygon
      (pts
        (xy 177.24 48.29) (xy 176.74 48.97) (xy 177.8 49.51) (xy 178.27 49.33) (xy 178.87 48.94)
        (xy 179.93 48.46) (xy 180.97 48.23) (xy 182.75 48.77) (xy 184.63 49.12) (xy 188.6 49.1)
        (xy 190.3 48.51) (xy 191.72 47.66) (xy 192.79 46.73) (xy 193.51 45.92) (xy 193.93 45.19)
        (xy 194.77 43.61) (xy 195.29 42.26) (xy 195.55 40.46) (xy 195.64 37.32) (xy 194.86 34.57)
        (xy 193.48 32.57) (xy 191.03 30.52) (xy 189.58 29.66) (xy 187.24 29.36) (xy 185.35 29.43)
        (xy 183.84 29.43) (xy 182.85 29.69) (xy 181.58 30.42) (xy 180.09 31.65) (xy 179.1 32.67)
        (xy 178.25 34.02) (xy 177.4 36.21) (xy 177.75 39.96) (xy 179.02 39.71) (xy 179.12 37.47)
        (xy 181 34.29) (xy 182.66 33.02) (xy 183.94 32.41) (xy 185.45 32.14) (xy 187.1 32.02)
        (xy 188.4 32.18) (xy 189.67 32.82) (xy 190.78 33.53) (xy 191.82 34.47) (xy 192.71 35.94)
        (xy 193.07 37.06) (xy 193.39 38.7) (xy 193.31 39.91) (xy 193.27 41.09) (xy 192.64 42.47)
        (xy 192.32 43.03) (xy 191.51 44.04) (xy 190.81 44.82) (xy 189.68 45.52) (xy 188.23 46.21)
        (xy 186.5 46.36) (xy 184.44 46.21) (xy 183.14 45.73) (xy 181.53 44.74)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.45))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.75))
    (polygon
      (pts
        (xy 112.39 29.08) (xy 111.27 30.97) (xy 111.21 33.47) (xy 111.21 46.51) (xy 112.45 48.9)
        (xy 113.41 49.97) (xy 115.49 50.51) (xy 118.93 50.75) (xy 123.81 50.91) (xy 129.01 51.11)
        (xy 132.88 51.52) (xy 138.5 52.67) (xy 141.54 53.8) (xy 142.82 54.45) (xy 143.55 55.14)
        (xy 143.95 57.03) (xy 144.12 58.79) (xy 144 64.11) (xy 151.98 55.99) (xy 151.9 42.78)
        (xy 149.82 39.18) (xy 151.26 35.39) (xy 153.27 34.81) (xy 157.22 34.88) (xy 158.44 36.46)
        (xy 158.3 41.35) (xy 157.08 43.15) (xy 155.57 44.51) (xy 155.57 57.37) (xy 150.11 62.95)
        (xy 163.25 63.81) (xy 163.4 61.58) (xy 163.4 51.31) (xy 161.39 48.72) (xy 161.46 36.37)
        (xy 161.24 32.4) (xy 160.88 30.68) (xy 160.59 29.89) (xy 159.3 29.24) (xy 158.22 28.81)
        (xy 114.7 28.09)
      )
    )
  )
  (zone (net 12) (net_name GNDPWR) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.75))
    (polygon
      (pts
        (xy 116.14 62.53) (xy 112.96 63.08) (xy 104.72 62.96) (xy 97.63 62.71) (xy 97.62 40.5)
        (xy 97.49 28.19) (xy 98.52 28.245) (xy 100.33 28.194) (xy 100.33 30.734) (xy 100.33 32.258)
        (xy 100.584 40.894) (xy 100.584 46.99) (xy 100.584 50.292) (xy 100.584 50.8) (xy 101.092 51.308)
        (xy 102.108 51.562) (xy 102.87 52.07) (xy 103.378 52.832) (xy 104.648 52.832) (xy 106.426 52.832)
        (xy 106.305 50.45875) (xy 106.28 47.4075) (xy 106.255 44.35625) (xy 106.23 41.305) (xy 106.13 29.1)
        (xy 107.02 28.25) (xy 110.15 28.44) (xy 109.25 31.15) (xy 109.04 46.89) (xy 111.05 50.5)
        (xy 114.66 52.3) (xy 120.21 52.58) (xy 124.3 52.65) (xy 128.4 52.72) (xy 131.93 53.07)
        (xy 136.14 53.72) (xy 139.65 55.05) (xy 141.06 55.96) (xy 142.07 57.17) (xy 142.52 59.18)
        (xy 142.521368 59.206197) (xy 142.91 61.72) (xy 140.97 61.92) (xy 138.8 61.81) (xy 137.86 60.3)
        (xy 137.44 59.625) (xy 136.52 57.86) (xy 135.74 56.83) (xy 130.46 56.65) (xy 123.64 56.6)
        (xy 123.72 58) (xy 123.43 59.27) (xy 122.6 60.01) (xy 118.93 60.37) (xy 117.26 61.71)
      )
    )
  )
  (zone (net 8) (net_name GNDA) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.75))
    (polygon
      (pts
        (xy 129.39 80) (xy 130.78 79.94) (xy 130.78 77.39) (xy 130.74 77.08) (xy 128.78 77.09)
        (xy 128.8 72.82) (xy 128.41 71.87) (xy 130.12 70.96) (xy 135.83 71.01) (xy 135.54 82.58)
        (xy 137.87 84.8) (xy 137.63 89.84) (xy 135.66 90.32) (xy 135.78 98.57) (xy 134.47 99.99)
        (xy 133.13 100.27) (xy 132.3 101.23) (xy 131.13 102.06) (xy 130.45 102.63) (xy 128.6 102.55)
        (xy 128.58 99.1) (xy 129.83 98.74) (xy 130.49 97.96) (xy 130.74 96.4) (xy 130.53 93.13)
        (xy 130.21 92.75) (xy 129.36 92.53) (xy 128.53 92.62) (xy 128.55 90.58) (xy 132.55 90.46)
        (xy 132.3 86.51) (xy 130.97 86.69) (xy 130.74 83.66) (xy 129.52 82.73)
      )
    )
  )
  (zone (net 8) (net_name GNDA) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.75))
    (polygon
      (pts
        (xy 116.59 88.38) (xy 116.66 90.72) (xy 115.36 92.28) (xy 97.91 91.82) (xy 97.69 67.38)
        (xy 101.5 65.18) (xy 111.94 65.28) (xy 111.94 68.6) (xy 106.33 68.65) (xy 105.94 74.51)
        (xy 103.3 75.34) (xy 100.38 78.61) (xy 100.33 87.2) (xy 101.94 88.76) (xy 113.51 88.71)
      )
    )
  )
  (zone (net 8) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.75))
    (polygon
      (pts
        (xy 115.15 90.07) (xy 114.9 94.07) (xy 117.71 95.76) (xy 125.27 96.13) (xy 124.83 100.57)
        (xy 129.01 104.25) (xy 135.76 104.5) (xy 135.2 120.99) (xy 97.35 120.13) (xy 97.48 64.73)
        (xy 113.06 64.28) (xy 113.06 68.85) (xy 110.29 68.92) (xy 110.37 74.47) (xy 114.64 78.81)
        (xy 115.09 85.33)
      )
    )
  )
  (zone (net 8) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.75))
    (polygon
      (pts
        (xy 134.88 112.85) (xy 134.52 120.66) (xy 152.03 120.54) (xy 151.81 114.44) (xy 151.87 110.16)
        (xy 159.5 109.44) (xy 161.15 107.63) (xy 161.09 101.26) (xy 158.68 98.08) (xy 151.79 98.32)
        (xy 134.46 81.12) (xy 133.66 80.21) (xy 133.11 63.29) (xy 123.5 62.47) (xy 123.56 68.4)
        (xy 127.02 68.62) (xy 131.25 72.63) (xy 131.19 80.98) (xy 127.84 81.14) (xy 128.23 83.78)
        (xy 128.39 95.44) (xy 130.81 96.61) (xy 130.59 99.03) (xy 124.33 98.87) (xy 124.6 102.98)
        (xy 129.21 104.85) (xy 135.42 105.84) (xy 135.14 108.95)
      )
    )
  )
  (zone (net 8) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.75))
    (polygon
      (pts
        (xy 110.27 73.19) (xy 110.71 75.88) (xy 115.21 82.62) (xy 131.73 83.5) (xy 131.73 73.01)
        (xy 128.7 73.17) (xy 113.36 73.15)
      )
    )
  )
  (zone (net 8) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.75))
    (polygon
      (pts
        (xy 118.96 96.03) (xy 118.87 93.45) (xy 119.02 86.49) (xy 125.74 86.51) (xy 125.48 99.51)
      )
    )
  )
  (zone (net 12) (net_name GNDPWR) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.75))
    (polygon
      (pts
        (xy 106.16 28.2) (xy 106.31 53.34) (xy 109.46 56.11) (xy 113.77 59.18) (xy 115.64 59.99)
        (xy 118.63 60.17) (xy 121.23 60.12) (xy 123.11 59.15) (xy 131.23 58.99) (xy 137.2 58.95)
        (xy 138.83 61.96) (xy 143.1 61.95) (xy 142.64 59.98) (xy 142.25 57.93) (xy 141.27 56.14)
        (xy 139.53 54.96) (xy 135.97 53.79) (xy 128.8 53.03) (xy 114.72 52.37) (xy 110.72 50.62)
        (xy 108.87 46.91) (xy 108.995 38.93) (xy 109.06 29.44) (xy 108.37 28.51)
      )
    )
  )
  (zone (net 13) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.75))
    (polygon
      (pts
        (xy 122.09 65.36) (xy 122.78 64.19) (xy 122.3 62.38) (xy 117.29 62.36) (xy 116.93 65.29)
        (xy 120.15 65.94)
      )
    )
  )
  (zone (net 12) (net_name GNDPWR) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.75))
    (polygon
      (pts
        (xy 138.01 71.62) (xy 139.81 69.12) (xy 139.82 61.5) (xy 142.83 60.95) (xy 142.69 70.53)
        (xy 142.68 77.88) (xy 143.9 80.41) (xy 145.82 82.02) (xy 145.75 86.98) (xy 145.74 88.34)
        (xy 145.78 90.03) (xy 144.77 90.05) (xy 144.35 89.3) (xy 144.35 85.87) (xy 142.62 84.2)
        (xy 140.25 84.11) (xy 136.73 80.59) (xy 136.56 73.16)
      )
    )
  )
  (zone (net 29) (net_name /1052_FB) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.75))
    (polygon
      (pts
        (xy 180.69 45.88) (xy 182.81 48.1) (xy 187.05 48.44) (xy 190.33 48.06) (xy 193.1 45.99)
        (xy 194.61 43.55) (xy 195.54 40.38) (xy 195.4 37.25) (xy 194.48 34.59) (xy 192.78 32.71)
        (xy 190.34 30.66) (xy 188.44 30.11) (xy 185.86 30.11) (xy 183.54 30.16) (xy 182.5 30.98)
        (xy 181.13 32.29) (xy 179.52 33.91) (xy 177.92 35.92) (xy 177.74 39.88) (xy 179.01 39.63)
        (xy 179.11 37.39) (xy 180.99 34.21) (xy 182.65 32.94) (xy 183.93 32.33) (xy 185.44 32.06)
        (xy 187.09 31.94) (xy 188.39 32.1) (xy 189.66 32.74) (xy 190.77 33.45) (xy 191.81 34.39)
        (xy 192.7 35.86) (xy 193.06 36.98) (xy 193.38 38.62) (xy 193.3 39.83) (xy 193.26 41.01)
        (xy 192.63 42.39) (xy 192.31 42.95) (xy 191.5 43.96) (xy 190.8 44.74) (xy 189.67 45.44)
        (xy 188.22 46.13) (xy 186.49 46.28) (xy 184.43 46.13) (xy 183.13 45.65) (xy 181.52 44.66)
      )
    )
  )
  (zone (net 13) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.75))
    (polygon
      (pts
        (xy 101.78 29.34) (xy 101.78 59.73) (xy 105.52 62.98) (xy 118.17 62.89) (xy 118.24 61.83)
        (xy 114.55 61.86) (xy 104.87 54.57) (xy 104.94 53.58) (xy 104.78 31.23) (xy 103.54 29.31)
      )
    )
  )
  (zone (net 13) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.75))
    (polygon
      (pts
        (xy 101.71 49.95) (xy 102.17 50.41) (xy 102.75 50.54) (xy 103.45 50.47) (xy 103.62 50.11)
        (xy 103.585 48.915) (xy 103.63 47.26) (xy 104.83 46.71) (xy 105.4 46.4) (xy 105.45 45.93)
        (xy 105.45 44.94) (xy 105.31 38.55) (xy 103.06 36.63) (xy 103.16 29.41) (xy 101.58 29.87)
        (xy 101.7 48.22)
      )
    )
  )
  (zone (net 8) (net_name GNDA) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.75))
    (polygon
      (pts
        (xy 102.26 81.63) (xy 109.32 81.4) (xy 109.57 82.26) (xy 109.41 85.03) (xy 110.72 84.96)
        (xy 110.81 80.29) (xy 99.68 79.85) (xy 99.14 90.02) (xy 116.12 89.38) (xy 117.97 88.68)
        (xy 117.9 87.76) (xy 109.19 87.67) (xy 108.49 87.95) (xy 102.96 87.95) (xy 102.26 86.65)
      )
    )
  )
  (zone (net 16) (net_name BUF_OUT) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 179.01 72.72) (xy 181.05 72.69) (xy 181.11 64.72) (xy 179.67 63.29) (xy 176.94 63.29)
        (xy 176.16 62.59) (xy 175.04 62.54) (xy 174.42 63.01) (xy 174.43 63.59) (xy 175.19 64.26)
        (xy 177.75 64.27) (xy 179.04 65.54) (xy 179.02 72.43)
      )
    )
  )
  (zone (net 8) (net_name GNDA) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 158.68 105.39) (xy 162.56 109.53) (xy 163.43 109.48) (xy 164.24 110.51) (xy 164.38 101.85)
        (xy 162.09 101.86) (xy 162.14 103.36) (xy 161.69 104.05) (xy 159.67 104.19)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.3))
    (polygon
      (pts
        (xy 176.98 116.21) (xy 172.98 116.15) (xy 170.78 112.11) (xy 170.59 100.6) (xy 165.82 95.45)
        (xy 165.86 93.33) (xy 168.86 93.39) (xy 169.26 93.88) (xy 169.44 94.73) (xy 174.3 100.27)
        (xy 174.04 111.42) (xy 177.32 111.76)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.3))
    (polygon
      (pts
        (xy 177.02 116.19) (xy 173.02 116.13) (xy 170.82 112.09) (xy 170.63 100.58) (xy 165.86 95.43)
        (xy 165.9 93.31) (xy 168.9 93.37) (xy 169.3 93.86) (xy 169.48 94.71) (xy 174.34 100.25)
        (xy 174.73 111.14) (xy 176.8 113.58)
      )
    )
  )
  (zone (net 8) (net_name GNDA) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.3))
    (polygon
      (pts
        (xy 144.16 118.49) (xy 144 121.84) (xy 171.23 121.67) (xy 171.25 116.68) (xy 168.85 112.3)
        (xy 168.29 101.12) (xy 164.21 96.26) (xy 162.1 96.22) (xy 162.06 99.91) (xy 162.53 114.05)
        (xy 161.8 115.03) (xy 160.09 115.85) (xy 152.05 116.28) (xy 146.77 116.45) (xy 145.57 116.58)
        (xy 144.92 116.71) (xy 144.58 117.1) (xy 144.26 117.7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.3))
    (polygon
      (pts
        (xy 187.35 32.34) (xy 189.67 33.06) (xy 191.94 34.97) (xy 193.14 37.52) (xy 193.14 40.76)
        (xy 192.36 42.86) (xy 190.58 44.68) (xy 189.45 45.44) (xy 188.16 46.1) (xy 186.77 46.23)
        (xy 185.51 46.16) (xy 184.35 46.09) (xy 182.87 45.51) (xy 181.98 44.93) (xy 181.17 44.53)
        (xy 180.09 43.48) (xy 179.8 43.13) (xy 179.51 42.87) (xy 179.09 42.91) (xy 178.48 43.49)
        (xy 176.27 45.72) (xy 174.05 47.92) (xy 174.02 51.21) (xy 173.295 51.925) (xy 172.52 52.69)
        (xy 172.33 52.85) (xy 170.86 53.02) (xy 170.805 57.24) (xy 170.76 61.43) (xy 170.47 61.66)
        (xy 170.17 61.83) (xy 170.04 62.17) (xy 169.79 62.4) (xy 169.18 62.77) (xy 169.21 64.15)
        (xy 169.18 64.89) (xy 169.73 65.44) (xy 169.73 67.19) (xy 169.14 67.8) (xy 168.22 67.8)
        (xy 167.53 67.06) (xy 167.53 65.62) (xy 167.66 65.26) (xy 167.73 64.5) (xy 168.21 64.13)
        (xy 168.16 62.7) (xy 165.25 62.6) (xy 164.4 62.53) (xy 164.36 61.73) (xy 164.35 60.75)
        (xy 164.75 60.06) (xy 165.82 60.22) (xy 166 60.35) (xy 166.3 60.44) (xy 166.61 60.28)
        (xy 166.67 60.05) (xy 166.7 58.71) (xy 166.68 57.03) (xy 166.74 55.7) (xy 166.73 54.49)
        (xy 166.75 53.47) (xy 166.98 53.29) (xy 167.02 53.05) (xy 166.95 52.75) (xy 166.61 52.61)
        (xy 166.24 52.76) (xy 165.42 52.77) (xy 165.55 50.41) (xy 166.1 50.11) (xy 166.52 50.51)
        (xy 167.06 50.57) (xy 167.2 50.12) (xy 167.22 48.96) (xy 167.49 48.64) (xy 167.39 47.74)
        (xy 167.4 47.52) (xy 167.56 47.31) (xy 167.57 46.64) (xy 168.31 46.64) (xy 173.03 46.69)
        (xy 174.8075 44.8625) (xy 176.56 43.16) (xy 177.51 42.24) (xy 177.97 41.73) (xy 179.07 40.68)
        (xy 179.18 40.35) (xy 179.24 38.73) (xy 179.53 37.11) (xy 180.75 34.87) (xy 182.8 33.12)
        (xy 185.06 32.34)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.3))
    (polygon
      (pts
        (xy 153.83 80.11) (xy 152.81 80.01) (xy 150.94 77.76) (xy 148.34 77.73) (xy 147.1 76.36)
        (xy 147.1 65.01) (xy 154.92 57.26) (xy 154.93 44.43) (xy 156.25 43.07) (xy 156.16 42.21)
        (xy 157.24 40.32) (xy 157.14 35.45) (xy 154.37 34.88) (xy 151.69 35.74) (xy 151.31 37.41)
        (xy 151.43 41.33) (xy 152.38 42.64) (xy 152.33 56.31) (xy 152.25 56.44) (xy 152.1 56.63)
        (xy 145.02 63.72) (xy 144.99 65.08) (xy 144.94 65.23) (xy 144.87 65.31) (xy 144.88 77.42)
        (xy 148.22 80.78) (xy 148.85 81.4) (xy 153.88 81.38) (xy 153.87 80.63)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.3))
    (polygon
      (pts
        (xy 156.97 83.17) (xy 156.97 91.65) (xy 174.4 91.62) (xy 174.44 92.24) (xy 174.28 93.15)
        (xy 173.32 93.52) (xy 171.22 93.61) (xy 169.76 94.85) (xy 174.94 100.73) (xy 176.65 100.69)
        (xy 176.5 92.5) (xy 183.7 92.22) (xy 183.54 90.1) (xy 181.04 87.55) (xy 174.445 87.515)
        (xy 167.85 87.48) (xy 165.7 87.49) (xy 165.68 88.76) (xy 163.92 88.76) (xy 163.93 88.12)
        (xy 163.91 87.47) (xy 163.33 87.48) (xy 159.4 87.49) (xy 159.43 85.75) (xy 159.41 82.94)
        (xy 159.4 81.01) (xy 156.68 79.36) (xy 154.64 79.34) (xy 152.01 79.33) (xy 149.02 80.75)
        (xy 148.93 81.59) (xy 155.39 81.96)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.3))
    (polygon
      (pts
        (xy 174.9 100.77) (xy 174.98 107.38) (xy 191.87 107.39) (xy 191.8 90.63) (xy 188.13 87.53)
        (xy 180.34 87.46) (xy 180.17 92.28) (xy 188.1 92.38) (xy 188.13 104.7) (xy 176.21 104.54)
        (xy 176.54 101.04) (xy 176.41 99.35) (xy 174.89 99.05)
      )
    )
  )
)
