(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4)
  (general
    (links 35)
    (no_connects 0)
    (area 120.649499 69.849499 146.050501 115.570501)
    (thickness 1.6)
    (drawings 10)
    (tracks 52)
    (zones 0)
    (modules 16)
    (nets 18)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4064)
    (user_trace_width 0.254)
    (user_trace_width 0.4064)
    (user_trace_width 0.6096)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.001)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad2)")
  (net 2 +5V)
  (net 3 GND)
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(P1-Pad2)")
  (net 7 "Net-(P1-Pad4)")
  (net 8 "Net-(P1-Pad8)")
  (net 9 ANT)
  (net 10 ANT_RX)
  (net 11 ANT_TX)
  (net 12 ANT_SWITCH)
  (net 13 TX)
  (net 14 RX)
  (net 15 "Net-(P3-Pad2)")
  (net 16 "Net-(C7-Pad1)")
  (net 17 "Net-(P1-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net ANT_SWITCH)
    (add_net GND)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(P3-Pad2)")
    (add_net RX)
    (add_net TX)
  )
  (net_class Antennas ""
    (clearance 0.2)
    (trace_width 0.4064)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net ANT)
    (add_net ANT_RX)
    (add_net ANT_TX)
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 58A73EFD)
    (at 123.19 77.47)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 20.955) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 2.54 8.89 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(P1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(P1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 ANT_SWITCH))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 TX))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(P1-Pad8)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58A74441)
    (at 135.255 102.87 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 2.286 -0.254 360) (layer F.SilkS))
    (fp_text value 10K (at 0.254 -1.778 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 ANT_SWITCH))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 58A73ECC)
    (at 132.08 96.52)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U1 (at 3.81 -3.175) (layer F.SilkS))
    (fp_text value SA630 (at 0 1.27) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 7 smd rect (at -0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C7-Pad1)"))
    (pad 6 smd rect (at 0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 5 smd rect (at 1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 4 smd rect (at 1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 12 ANT_SWITCH))
    (pad 3 smd rect (at 0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at -0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 58A73EF3)
    (at 133.35 80.01 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -2.54 180) (layer F.SilkS))
    (fp_text value RF_TX (at -2.54 0.635 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 ANT_TX))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 TX))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 58A73E8F)
    (at 143.51 80.01 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 -2.54 180) (layer F.SilkS))
    (fp_text value RF_RX1 (at 2.54 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "Net-(P3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 RX))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 58A73E8D)
    (at 143.51 113.03 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 0 10.16 180) (layer F.SilkS))
    (fp_text value RF_RX2 (at 2.54 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 ANT_RX))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58A7442A)
    (at 128.27 99.06 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 2.54 -0.254 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 -2.286 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58A73EE3)
    (at 127 78.74 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Michels_Library:U.FL-Coax (layer F.Cu) (tedit 55FA0B94)
    (at 133.145 111.76 90)
    (fp_text reference P5 (at 0 2.9 90) (layer F.SilkS))
    (fp_text value BNC (at 0 -2.8 90) (layer F.Fab))
    (pad 2 smd rect (at -1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 9 ANT))
    (pad 2 smd rect (at 0 -1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 132.715 89.535 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value 10nF (at 0.52 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 138.43 74.295 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 0 -1.9 90) (layer F.SilkS))
    (fp_text value 10pF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 RX))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 138.43 78.105 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 2.54 1.27 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 RX))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(P1-Pad8)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 128.27 102.87 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 132.715 102.87 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.9 90) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 ANT))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 137.795 97.79 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 ANT_RX))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 130.175 89.535 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 -1.9 90) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 ANT_TX))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 121.92 114.3) (end 121.92 115.57) (angle 90) (layer Edge.Cuts) (width 0.001))
  (gr_arc (start 144.78 114.3) (end 146.05 114.3) (angle 90) (layer Edge.Cuts) (width 0.001))
  (gr_text "(C) BusError Dynamics, LTD" (at 140.335 90.17 90) (layer F.SilkS))
  (gr_text "rf_bridge 1.1" (at 143.51 92.075 90) (layer F.SilkS))
  (gr_arc (start 144.78 71.12) (end 144.78 69.85) (angle 90) (layer Edge.Cuts) (width 0.001))
  (gr_arc (start 121.92 71.12) (end 120.65 71.12) (angle 90) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 120.65 114.3) (end 120.65 71.12) (angle 90) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 144.78 115.57) (end 121.92 115.57) (angle 90) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 146.05 71.12) (end 146.05 114.3) (angle 90) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 121.92 69.85) (end 144.78 69.85) (angle 90) (layer Edge.Cuts) (width 0.001))
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.2))
    (polygon
      (pts
        (xy 145.415 114.935) (xy 121.285 114.935) (xy 121.285 70.485) (xy 145.415 70.485)
      )
    )
  )
  (zone (net 2) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1.2))
    (polygon
      (pts
        (xy 145.415 114.935) (xy 121.285 114.935) (xy 121.285 70.485) (xy 145.415 70.485)
      )
    )
  )
)
