(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 397)
    (zones 0)
    (modules 53)
    (nets 39)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.6)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "/home/rick/Nextcloud/Endless Torch V2.2/gerber/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 Vin)
  (net 3 Vout)
  (net 4 "Net-(D2-Pad1)")
  (net 5 "Net-(R1-Pad1)")
  (net 6 "Net-(R3-Pad1)")
  (net 7 "Net-(C1-Pad1)")
  (net 8 "Net-(C2-Pad1)")
  (net 9 "Net-(C2-Pad2)")
  (net 10 "Net-(C3-Pad2)")
  (net 11 "Net-(C4-Pad2)")
  (net 12 "Net-(C9-Pad1)")
  (net 13 "Net-(D3-Pad1)")
  (net 14 "Net-(J1-PadA2)")
  (net 15 "Net-(J1-PadA3)")
  (net 16 "Net-(J1-PadA5)")
  (net 17 "Net-(J1-PadA6)")
  (net 18 "Net-(J1-PadA7)")
  (net 19 "Net-(J1-PadA10)")
  (net 20 "Net-(J1-PadA8)")
  (net 21 "Net-(J1-PadA11)")
  (net 22 "Net-(J1-PadB2)")
  (net 23 "Net-(J1-PadB3)")
  (net 24 "Net-(J1-PadB5)")
  (net 25 "Net-(J1-PadB6)")
  (net 26 "Net-(J1-PadB7)")
  (net 27 "Net-(J1-PadB8)")
  (net 28 "Net-(J1-PadB10)")
  (net 29 "Net-(J1-PadB11)")
  (net 30 "Net-(L2-Pad2)")
  (net 31 "Net-(R4-Pad2)")
  (net 32 "Net-(R9-Pad1)")
  (net 33 "Net-(R11-Pad2)")
  (net 34 "Net-(U1-Pad3)")
  (net 35 "Net-(U1-Pad5)")
  (net 36 "Net-(C5-Pad2)")
  (net 37 "Net-(Q1-Pad4)")
  (net 38 "Net-(Q2-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(J1-PadA10)")
    (add_net "Net-(J1-PadA11)")
    (add_net "Net-(J1-PadA2)")
    (add_net "Net-(J1-PadA3)")
    (add_net "Net-(J1-PadA5)")
    (add_net "Net-(J1-PadA6)")
    (add_net "Net-(J1-PadA7)")
    (add_net "Net-(J1-PadA8)")
    (add_net "Net-(J1-PadB10)")
    (add_net "Net-(J1-PadB11)")
    (add_net "Net-(J1-PadB2)")
    (add_net "Net-(J1-PadB3)")
    (add_net "Net-(J1-PadB5)")
    (add_net "Net-(J1-PadB6)")
    (add_net "Net-(J1-PadB7)")
    (add_net "Net-(J1-PadB8)")
    (add_net "Net-(L2-Pad2)")
    (add_net "Net-(Q1-Pad4)")
    (add_net "Net-(Q2-Pad4)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R9-Pad1)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad5)")
    (add_net Vin)
    (add_net Vout)
  )
  (module "Rick's Custom:VIA-0.6mm" (layer F.Cu) (tedit 5E83D8F7)
    (at 131.286 60.5978)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.016) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 11 "Net-(C4-Pad2)") (zone_connect 2))
  )
  (module "Rick's Custom:VIA-0.6mm" (layer F.Cu) (tedit 5E83D8F7)
    (at 130.286 60.5978)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.016) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 11 "Net-(C4-Pad2)") (zone_connect 2))
  )
  (module "Rick's Custom:VIA-0.6mm" (layer F.Cu) (tedit 5E83D8F7)
    (at 129.286 60.5978)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.016) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 11 "Net-(C4-Pad2)") (zone_connect 2))
  )
  (module "Rick's Custom:VIA-0.6mm" (layer F.Cu) (tedit 5E83D8F7)
    (at 131.286 59.5978)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.016) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 11 "Net-(C4-Pad2)") (zone_connect 2))
  )
  (module "Rick's Custom:VIA-0.6mm" (layer F.Cu) (tedit 5E83D8F7)
    (at 130.286 59.5978)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.016) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 11 "Net-(C4-Pad2)") (zone_connect 2))
  )
  (module "Rick's Custom:VIA-0.6mm" (layer F.Cu) (tedit 5E83D8F7)
    (at 129.286 59.5978)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.016) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 11 "Net-(C4-Pad2)") (zone_connect 2))
  )
  (module "Rick's Custom:VIA-0.6mm" (layer F.Cu) (tedit 5E83D8F7)
    (at 131.286 58.5978)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.016) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 11 "Net-(C4-Pad2)") (zone_connect 2))
  )
  (module "Rick's Custom:VIA-0.6mm" (layer F.Cu) (tedit 5E83D8F7)
    (at 130.286 58.5978)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.016) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 11 "Net-(C4-Pad2)") (zone_connect 2))
  )
  (module "Rick's Custom:VIA-0.6mm" (layer F.Cu) (tedit 5E83D787)
    (at 134.7658 55.467)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.016) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 "Net-(C2-Pad1)") (zone_connect 2))
  )
  (module "Rick's Custom:VIA-0.6mm" (layer F.Cu) (tedit 5E83D787)
    (at 133.7658 55.467)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.016) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 "Net-(C2-Pad1)") (zone_connect 2))
  )
  (module "Rick's Custom:VIA-0.6mm" (layer F.Cu) (tedit 5E83D787)
    (at 132.7658 55.467)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.016) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 "Net-(C2-Pad1)") (zone_connect 2))
  )
  (module "Rick's Custom:VIA-0.6mm" (layer F.Cu) (tedit 5E83D787)
    (at 134.7658 54.467)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.016) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 "Net-(C2-Pad1)") (zone_connect 2))
  )
  (module "Rick's Custom:VIA-0.6mm" (layer F.Cu) (tedit 5E83D787)
    (at 133.7658 54.467)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.016) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 "Net-(C2-Pad1)") (zone_connect 2))
  )
  (module "Rick's Custom:VIA-0.6mm" (layer F.Cu) (tedit 5E83D787)
    (at 132.7658 54.467)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.016) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 "Net-(C2-Pad1)") (zone_connect 2))
  )
  (module "Rick's Custom:VIA-0.6mm" (layer F.Cu) (tedit 5E83D787)
    (at 134.7658 53.467)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.016) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 "Net-(C2-Pad1)") (zone_connect 2))
  )
  (module "Rick's Custom:VIA-0.6mm" (layer F.Cu) (tedit 5E83D787)
    (at 133.7658 53.467)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.016) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 "Net-(C2-Pad1)") (zone_connect 2))
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5E278CC9)
    (at 131.2164 41.0718 325)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 1.789528 -0.012734 235) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.43 325) (layer F.Fab))
    (fp_text user %R (at 0 0 325) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 325) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 325) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 Vin))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5E278C81)
    (at 130.937 42.7228 145)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at -1.951836 0.002353 235) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.43 145) (layer F.Fab))
    (fp_text user %R (at 0 0 145) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 145) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0 145) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 Vout))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 5E278D0E)
    (at 115.2144 50.3428 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1 (at 0.003106 -0.0221) (layer F.SilkS))
    (fp_text value BAT54 (at 0.1 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 270) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at 1.05 0 270) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5E278CFB)
    (at 138.6332 47.2186 285)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D2 (at 0 0 15) (layer F.SilkS))
    (fp_text value GREEN (at 0 1.65 285) (layer F.Fab))
    (fp_text user %R (at 0 0 285) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 285) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(D2-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 285) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Rick's Custom:3014_led" (layer B.Cu) (tedit 5DEC37D2)
    (at 124.2568 51.0032)
    (fp_text reference D3 (at 0 -1.651) (layer B.SilkS) hide)
    (fp_text value 3014 (at 0 1.524) (layer B.Fab))
    (pad 1 smd rect (at -1.11 0) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 0.695 0) (size 1.61 0.72) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module Connector_USB:USB_C_Receptacle_Amphenol_12401610E4-2A (layer F.Cu) (tedit 5DF15557)
    (at 115.6208 60.833 315)
    (descr "USB TYPE C, RA RCPT PCB, SMT, https://www.amphenolcanada.com/StockAvailabilityPrice.aspx?From=&PartNum=12401610E4%7e2A")
    (tags "USB C Type-C Receptacle SMD")
    (solder_paste_ratio -0.2)
    (attr smd)
    (fp_text reference J1 (at 0 -6.36 315) (layer F.SilkS) hide)
    (fp_text value 12401610E4#2A (at 0 6.14 315) (layer F.Fab))
    (fp_text user %R (at 0 0 315) (layer F.Fab))
    (pad S1 thru_hole oval (at -4.13 -3.11 315) (size 0.8 1.4) (drill oval 0.5 1.1) (layers *.Cu *.Mask F.Paste)
      (net 1 GND))
    (pad A1 smd rect (at -2.75 -5.019999 315) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A2 smd rect (at -2.250001 -5.02 315) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J1-PadA2)"))
    (pad A3 smd rect (at -1.75 -5.02 315) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J1-PadA3)"))
    (pad A4 smd rect (at -1.25 -5.020001 315) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C4-Pad2)"))
    (pad A5 smd rect (at -0.75 -5.02 315) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J1-PadA5)"))
    (pad A6 smd rect (at -0.25 -5.02 315) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J1-PadA6)"))
    (pad A7 smd rect (at 0.25 -5.02 315) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J1-PadA7)"))
    (pad A12 smd rect (at 2.749999 -5.02 315) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A10 smd rect (at 1.75 -5.019999 315) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J1-PadA10)"))
    (pad A9 smd rect (at 1.25 -5.020001 315) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C4-Pad2)"))
    (pad A8 smd rect (at 0.75 -5.02 315) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J1-PadA8)"))
    (pad A11 smd rect (at 2.25 -5.02 315) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J1-PadA11)"))
    (pad B1 smd rect (at 2.499999 -3.32 315) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at 4.13 -3.11 315) (size 0.8 1.4) (drill oval 0.5 1.1) (layers *.Cu *.Mask F.Paste)
      (net 1 GND))
    (pad S1 thru_hole oval (at 4.49 2.84 315) (size 0.8 1.4) (drill oval 0.5 1.1) (layers *.Cu *.Mask F.Paste)
      (net 1 GND))
    (pad S1 thru_hole oval (at -4.49 2.84 315) (size 0.8 1.4) (drill oval 0.5 1.1) (layers *.Cu *.Mask F.Paste)
      (net 1 GND))
    (pad "" np_thru_hole oval (at 3.6 -4.36 315) (size 0.95 0.65) (drill oval 0.95 0.65) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.6 -4.36 315) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad B2 smd rect (at 2 -3.32 315) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J1-PadB2)"))
    (pad B3 smd rect (at 1.5 -3.32 315) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J1-PadB3)"))
    (pad B4 smd rect (at 1 -3.32 315) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C4-Pad2)"))
    (pad B5 smd rect (at 0.5 -3.32 315) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J1-PadB5)"))
    (pad B6 smd rect (at 0 -3.320001 315) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J1-PadB6)"))
    (pad B7 smd rect (at -0.5 -3.32 315) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J1-PadB7)"))
    (pad B8 smd rect (at -1 -3.32 315) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J1-PadB8)"))
    (pad B9 smd rect (at -1.5 -3.320001 315) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C4-Pad2)"))
    (pad B10 smd rect (at -2 -3.319999 315) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J1-PadB10)"))
    (pad B11 smd rect (at -2.499999 -3.32 315) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J1-PadB11)"))
    (pad B12 smd rect (at -2.999997 -3.32 315) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_C_Receptacle_Amphenol_12401610E4-2A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Rick's Custom:ETQ-P3M6R8KVP" (layer F.Cu) (tedit 5DE4367D)
    (at 126.6952 51.6382 135)
    (fp_text reference L1 (at 0.046722 0.020076 225) (layer F.SilkS))
    (fp_text value 6.8uH (at -0.1016 -3.81 135) (layer F.Fab))
    (pad 1 smd roundrect (at -2.429999 0 135) (size 1.9 2.79) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C2-Pad1)"))
    (pad 2 smd roundrect (at 2.429999 0 135) (size 1.9 2.79) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(C5-Pad2)"))
  )
  (module "Rick's Custom:LPS3015-472MRC" (layer F.Cu) (tedit 5B144F5C)
    (at 126.873 42.2148 145)
    (fp_text reference L2 (at -0.026292 -0.005898 235) (layer F.SilkS))
    (fp_text value 4.7uH (at 0 -2.667 145) (layer F.Fab))
    (pad 2 smd rect (at 1.27 0 145) (size 0.76 3.05) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(L2-Pad2)"))
    (pad 1 smd rect (at -1.27 0 145) (size 0.76 3.05) (layers F.Cu F.Paste F.Mask)
      (net 2 Vin))
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5E278D40)
    (at 113.1824 42.799 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -1.9812 0.0033) (layer F.SilkS))
    (fp_text value 100Kohm (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(R1-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5E278D60)
    (at 111.633 42.799 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 1.9812 0.0254 -180) (layer F.SilkS))
    (fp_text value 100Kohm (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(R1-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5E278D59)
    (at 114.7318 42.799 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 1.9812 -0.0254 -180) (layer F.SilkS))
    (fp_text value 100ohm (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(R1-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5E278D48)
    (at 108.3564 50.0126 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 0.9906 90) (layer F.SilkS))
    (fp_text value 100Kohm (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5E278D4F)
    (at 108.3564 53.1114 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 1.0414 90) (layer F.SilkS))
    (fp_text value 13.8Kohm (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(R4-Pad2)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5E278D87)
    (at 120.142 40.513 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at -1.8796 0 -90) (layer F.SilkS))
    (fp_text value 30Kohm (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 Vin))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5E278D73)
    (at 117.8306 39.751 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 1.8288 -0.0254 -180) (layer F.SilkS))
    (fp_text value 105Kohm (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5E278CE9)
    (at 136.4742 45.5931 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at -0.8637 1.0922 90) (layer F.SilkS))
    (fp_text value 340Ohm (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(R9-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5E278CA6)
    (at 129.0574 45.212 145)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at -1.84571 0.021066 235) (layer F.SilkS))
    (fp_text value 340Ohm (at 0 1.43 145) (layer F.Fab))
    (fp_text user %R (at 0 0 145) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 145) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 Vout))
    (pad 1 smd roundrect (at -0.7875 0 145) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5E278C8D)
    (at 129.9972 43.9674 325)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 2.403384 0.022555 55) (layer F.SilkS))
    (fp_text value 536Kohm (at 0 1.43 325) (layer F.Fab))
    (fp_text user %R (at 0 0 325) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 325) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(R11-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 325) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 Vout))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5E278CBA)
    (at 132.3848 39.497 325)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 0 -1.1176 145) (layer F.SilkS))
    (fp_text value 309Kohm (at 0 1.43 325) (layer F.Fab))
    (fp_text user %R (at 0 0 325) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 325) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(R11-Pad2)"))
    (pad 2 smd roundrect (at 0.7875 0 325) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Rick's Custom:Texas_RGV_S-PVQFN-N16_EP2.1x2.1mm_ThermalVias" (layer F.Cu) (tedit 5E278D20)
    (at 111.6076 49.784 270)
    (descr "QFN, 16 Pin (http://www.ti.com/lit/ds/symlink/ina3221.pdf#page=44), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (solder_paste_ratio -0.2)
    (attr smd)
    (fp_text reference U1 (at -1.5748 1.524) (layer F.SilkS))
    (fp_text value BQ24640 (at 0 3.32 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 17 smd roundrect (at 0 0 270) (size 2.14 2.14) (layers F.Cu F.Mask) (roundrect_rratio 0.119)
      (net 1 GND))
    (pad 17 thru_hole circle (at -0.8 -0.8 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 17 thru_hole circle (at 0 -0.8 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 17 thru_hole circle (at 0.8 -0.8 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 17 thru_hole circle (at -0.8 0 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 17 thru_hole circle (at 0 0 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 17 thru_hole circle (at 0.8 0 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 17 thru_hole circle (at -0.8 0.8 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 17 thru_hole circle (at 0 0.8 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 17 thru_hole circle (at 0.8 0.8 270) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 17 smd roundrect (at 0 0 270) (size 2.1 2.1) (layers B.Cu) (roundrect_rratio 0.119048)
      (net 1 GND))
    (pad "" smd roundrect (at -0.525 -0.525 270) (size 0.91 0.91) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.525 0.525 270) (size 0.91 0.91) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.525 -0.525 270) (size 0.91 0.91) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.525 0.525 270) (size 0.91 0.91) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -1.65 -0.75 270) (size 0.7 0.28) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C4-Pad2)"))
    (pad 2 smd roundrect (at -1.65 -0.25 270) (size 0.7 0.28) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C1-Pad1)"))
    (pad 3 smd roundrect (at -1.65 0.25 270) (size 0.7 0.28) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(U1-Pad3)"))
    (pad 4 smd roundrect (at -1.65 0.75 270) (size 0.7 0.28) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(R3-Pad1)"))
    (pad 5 smd roundrect (at -0.75 1.65 270) (size 0.28 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(U1-Pad5)"))
    (pad 6 smd roundrect (at -0.25 1.65 270) (size 0.28 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C1-Pad1)"))
    (pad 7 smd roundrect (at 0.25 1.65 270) (size 0.28 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(R4-Pad2)"))
    (pad 8 smd roundrect (at 0.75 1.65 270) (size 0.28 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C9-Pad1)"))
    (pad 9 smd roundrect (at 1.65 0.75 270) (size 0.7 0.28) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 Vin))
    (pad 10 smd roundrect (at 1.65 0.25 270) (size 0.7 0.28) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(C5-Pad2)"))
    (pad 11 smd roundrect (at 1.65 -0.25 270) (size 0.7 0.28) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 12 smd roundrect (at 1.65 -0.75 270) (size 0.7 0.28) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C3-Pad2)"))
    (pad 13 smd roundrect (at 0.75 -1.65 270) (size 0.28 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.119)
      (net 38 "Net-(Q2-Pad4)"))
    (pad 14 smd roundrect (at 0.25 -1.65 270) (size 0.26 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.119)
      (net 8 "Net-(C2-Pad1)"))
    (pad 15 smd roundrect (at -0.25 -1.65 270) (size 0.26 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(Q1-Pad4)"))
    (pad 16 smd roundrect (at -0.75 -1.65 270) (size 0.28 0.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Texas_RGV_S-PVQFN-N16_EP2.1x2.1mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "/home/rick/Nextcloud/Kicad/Rick's Custom.pretty/bq24640.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5DF14677)
    (at 135.1534 42.2148 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U2 (at -0.0467 -0.026383 180) (layer F.SilkS))
    (fp_text value TPS3809L30DBVR (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R9-Pad1)"))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 Vin))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.75x1.45mm (layer F.Cu) (tedit 5E278CB0)
    (at 129.2606 38.862 235)
    (descr "8-Lead Plastic Dual Flat, No Lead Package (MC) - 2x3x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.5")
    (solder_paste_ratio -0.2)
    (attr smd)
    (fp_text reference U3 (at 0.005898 1.548508 235) (layer F.SilkS))
    (fp_text value MCP1624-DFN (at 0 2.05 235) (layer F.Fab))
    (fp_text user %R (at 0 0 235) (layer F.Fab))
    (pad 1 smd rect (at -1.45 -0.75 235) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R11-Pad2)"))
    (pad 2 smd rect (at -1.45 -0.25 235) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.45 0.25 235) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -1.45 0.75 235) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 Vin))
    (pad 5 smd rect (at 1.45 0.75 235) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(L2-Pad2)"))
    (pad 6 smd rect (at 1.45 0.25 235) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 Vout))
    (pad 7 smd rect (at 1.45 -0.25 235) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 Vout))
    (pad 8 smd rect (at 1.45 -0.75 235) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 Vin))
    (pad "" smd rect (at -0.4375 0.3625 235) (size 0.71 0.58) (layers F.Paste))
    (pad 9 smd rect (at 0 0 235) (size 1.75 1.45) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad "" smd rect (at 0.4375 0.362499 235) (size 0.71 0.58) (layers F.Paste))
    (pad "" smd rect (at 0.4375 -0.3625 235) (size 0.71 0.58) (layers F.Paste))
    (pad "" smd rect (at -0.4375 -0.362499 235) (size 0.71 0.58) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-8-1EP_3x2mm_P0.5mm_EP1.75x1.45mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Rick's Custom:400F_Supercap_4Pin" (layer F.Cu) (tedit 5E38AC7D)
    (at 123.7996 51.9176)
    (fp_text reference C8 (at 0 -15.875) (layer F.SilkS) hide)
    (fp_text value 400F (at 0.0254 -14.5288) (layer F.Fab))
    (fp_text user + (at 0 -10.287) (layer F.SilkS))
    (fp_text user - (at 0 10.16) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 -11.8) (size 2 2) (drill 1.25) (layers *.Cu *.Mask)
      (net 2 Vin))
    (pad 3 thru_hole circle (at -10.214 -5.996) (size 2 2) (drill 1.25) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 10.214 -5.996) (size 2 2) (drill 1.25) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 11.8) (size 2 2) (drill 1.25) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module "Rick's Custom:logo_6mm" (layer B.Cu) (tedit 0)
    (at 115.6208 60.6298)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5E39532E)
    (at 109.855 45.9994 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.0414 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5E395316)
    (at 115.3668 48.006 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 1.0414 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C2-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5E3952D4)
    (at 113.157 53.5432 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0.1016 -0.9906 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C3-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5E395359)
    (at 116.6368 42.799 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0.1016 -1.0668 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C4-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5E3952E4)
    (at 110.0582 53.5686 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at -0.127 -1.0922 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 Vin))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5E3952B6)
    (at 110.0582 56.6166 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0 -1.0414 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(C5-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5E3953D5)
    (at 120.142 38.9636)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 0 -1.0414) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 Vin))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5E3953BF)
    (at 120.142 42.0878)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 1.905 0 270 unlocked) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C9-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 Vin))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5E395378)
    (at 120.904 45.5422 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0.0762 0) (layer F.SilkS))
    (fp_text value 10mOhm (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 Vin))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 36 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TDSON-8-1 (layer F.Cu) (tedit 5A70FA3B)
    (at 129.921 59.4106 315)
    (descr "Power MOSFET package, TDSON-8-1, SuperS08, SON-8_5x6mm")
    (tags "tdson ")
    (solder_paste_ratio -0.2)
    (attr smd)
    (fp_text reference Q1 (at 0 4 315) (layer F.SilkS))
    (fp_text value BSC020N03MS (at 0 -4 315) (layer F.Fab))
    (fp_text user %R (at 0 -1 315) (layer F.Fab))
    (pad "" smd rect (at -0.75 1.089999 225) (size 1.55 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.75 -1.089999 225) (size 1.55 1.2) (layers F.Paste))
    (pad "" smd rect (at 1.25 1.09 225) (size 1.55 1.6) (layers F.Paste))
    (pad "" smd rect (at 1.25 -1.09 225) (size 1.55 1.6) (layers F.Paste))
    (pad 5 smd rect (at 0.499999 0 225) (size 4.5 4.29) (layers F.Cu F.Mask)
      (net 11 "Net-(C4-Pad2)"))
    (pad 5 smd rect (at 2.75 -1.91 225) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C4-Pad2)"))
    (pad 5 smd rect (at 2.75 -0.64 225) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C4-Pad2)"))
    (pad 5 smd rect (at 2.75 0.64 225) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C4-Pad2)"))
    (pad 5 smd rect (at 2.75 1.91 225) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C4-Pad2)"))
    (pad 4 smd rect (at -2.75 1.91 225) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(Q1-Pad4)"))
    (pad 3 smd rect (at -2.75 0.64 225) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at -2.75 -0.64 225) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C2-Pad1)"))
    (pad 1 smd rect (at -2.75 -1.91 225) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TDSON-8-1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TDSON-8-1 (layer F.Cu) (tedit 5A70FA3B)
    (at 134.103194 54.866022 135)
    (descr "Power MOSFET package, TDSON-8-1, SuperS08, SON-8_5x6mm")
    (tags "tdson ")
    (solder_paste_ratio -0.2)
    (attr smd)
    (fp_text reference Q2 (at 0 4 135) (layer F.SilkS))
    (fp_text value BSC020N03MS (at 0 -4 135) (layer F.Fab))
    (fp_text user %R (at 0 -1 135) (layer F.Fab))
    (pad 1 smd rect (at -2.75 -1.91 45) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.75 -0.64 45) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.75 0.64 45) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -2.75 1.91 45) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(Q2-Pad4)"))
    (pad 5 smd rect (at 2.75 1.91 45) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C2-Pad1)"))
    (pad 5 smd rect (at 2.75 0.64 45) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C2-Pad1)"))
    (pad 5 smd rect (at 2.75 -0.64 45) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C2-Pad1)"))
    (pad 5 smd rect (at 2.75 -1.91 45) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C2-Pad1)"))
    (pad 5 smd rect (at 0.499999 0 45) (size 4.5 4.29) (layers F.Cu F.Mask)
      (net 8 "Net-(C2-Pad1)"))
    (pad "" smd rect (at 1.25 -1.09 45) (size 1.55 1.6) (layers F.Paste))
    (pad "" smd rect (at 1.25 1.09 45) (size 1.55 1.6) (layers F.Paste))
    (pad "" smd rect (at -0.75 -1.089999 45) (size 1.55 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.75 1.089999 45) (size 1.55 1.2) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TDSON-8-1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Rick's Custom:VIA-0.6mm" (layer F.Cu) (tedit 5E83D787)
    (at 132.7658 53.467)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.016) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 8 "Net-(C2-Pad1)") (zone_connect 2))
  )
  (module "Rick's Custom:VIA-0.6mm" (layer F.Cu) (tedit 5E83D8F7)
    (at 129.286 58.5978)
    (fp_text reference REF** (at 0 1.27) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.016) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 11 "Net-(C4-Pad2)") (zone_connect 2))
  )
  (gr_text "DANGER!\nHot While Charging" (at 131.0132 64.4144 30) (layer B.Mask))
  (gr_text "Endless Torch\nV2.31 2020\nMadElectronEngineering.com" (at 123.6726 37.0332) (layer B.Mask))
  (gr_text "Green LED\n95% Charged" (at 137.9728 46.5074 110) (layer B.Mask))
  (gr_circle (center 123.6472 51.7398) (end 140.7922 51.7398) (layer Edge.Cuts) (width 0.15))
  (zone (net 8) (net_name "Net-(C2-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 133.1468 49.53) (xy 129.8956 49.53) (xy 122.174 56.7944) (xy 123.698 58.3438) (xy 125.8062 58.3438)
        (xy 126.5174 57.7088) (xy 127.6096 58.7502) (xy 130.6322 55.7784) (xy 133.2738 58.3692) (xy 137.6934 54.102)
      )
    )
  )
  (zone (net 11) (net_name "Net-(C4-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 130.6322 56.1848) (xy 134.62 60.1218) (xy 130.2258 64.2112) (xy 127.2286 63.9572) (xy 122.0724 59.0296)
        (xy 121.5136 58.4962) (xy 121.0354 58.923472) (xy 117.1448 55.1434) (xy 117.3734 54.8894) (xy 116.0272 53.6194)
        (xy 113.8682 53.6448) (xy 114.7318 52.4764) (xy 115.7732 51.4858) (xy 123.4186 58.9788) (xy 123.571 59.1312)
        (xy 125.8824 59.1566) (xy 126.7968 60.0202)
      )
    )
  )
  (zone (net 36) (net_name "Net-(C5-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 126.2634 51.3588) (xy 121.9708 55.372) (xy 118.11 51.3842) (xy 114.935 47.1678) (xy 116.3066 45.847)
        (xy 118.11 45.847) (xy 127.4064 45.847) (xy 128.3716 45.847) (xy 129.7686 46.7614) (xy 129.7686 48.0822)
      )
    )
  )
  (zone (net 2) (net_name Vin) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 120.904 45.6438) (xy 128.0922 45.6438) (xy 125.3744 44.196) (xy 125.3744 41.7576) (xy 128.8796 37.0586)
        (xy 125.3744 37.0586) (xy 125.3744 37.8714) (xy 120.1928 37.8714) (xy 120.1928 42.9006) (xy 117.6782 42.9006)
        (xy 116.7384 45.6438) (xy 117.6782 45.6438)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 106.9086 56.515) (xy 106.426 47.3456) (xy 112.6236 50.7238) (xy 116.5098 54.483) (xy 122.682 60.2996)
        (xy 123.1646 60.6806) (xy 127.0508 64.3128) (xy 130.4036 64.5414) (xy 130.4544 71.628) (xy 107.1626 71.2724)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 130.3274 64.4906) (xy 135.1026 60.071) (xy 133.5278 58.3692) (xy 136.525 55.5498) (xy 137.4902 56.4642)
        (xy 138.9634 55.0164) (xy 143.9164 56.9722) (xy 129.9972 72.3646)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 138.43 55.499) (xy 137.795 53.1114) (xy 133.2738 48.7172) (xy 130.2258 48.6918) (xy 130.2004 46.4312)
        (xy 132.3594 44.5008) (xy 130.683 43.3832) (xy 131.6228 42.1132) (xy 130.8862 41.5544) (xy 132.9944 38.7604)
        (xy 134.493 40.2844) (xy 134.493 42.2148) (xy 135.4836 42.2148) (xy 135.4582 46.7106) (xy 136.4488 47.6504)
        (xy 141.5288 46.5074) (xy 142.3924 56.5658)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 126.2634 58.5216) (xy 130.81 54.8894) (xy 131.826 51.2826) (xy 131.6736 49.2252) (xy 145.6182 41.6814)
        (xy 128.0414 32.2326) (xy 103.9114 34.2646) (xy 103.8352 69.215) (xy 124.9172 70.0532)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 131.0386 34.163) (xy 128.778 36.9062) (xy 125.1839 36.9062) (xy 125.1966 37.6428) (xy 119.8372 37.6428)
        (xy 119.8372 39.751) (xy 117.5512 39.7764) (xy 117.1956 40.0558) (xy 117.221 42.8244) (xy 116.4082 42.8244)
        (xy 115.9764 43.3832) (xy 115.9764 45.1866) (xy 114.2238 46.99) (xy 112.903 47.9044) (xy 111.9124 47.498)
        (xy 110.998 46.4566) (xy 109.22 46.4058) (xy 109.601 39.1922) (xy 118.5926 32.8168)
      )
    )
  )
  (zone (net 11) (net_name "Net-(C4-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.0226 55.372) (xy 137.5664 62.6618) (xy 129.6924 69.7484) (xy 125.5268 69.596) (xy 118.237 68.58)
        (xy 118.237 65.2018) (xy 125.516652 65.201824) (xy 125.5268 58.2676) (xy 128.3716 57.1246)
      )
    )
  )
  (zone (net 8) (net_name "Net-(C2-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.1242 55.2704) (xy 137.668 62.484) (xy 140.3858 57.1754) (xy 141.2494 52.5272) (xy 140.843 43.9928)
        (xy 135.9916 38.989) (xy 132.6642 40.8432) (xy 136.1186 46.4312) (xy 131.2926 49.149) (xy 131.4196 51.1556)
        (xy 131.191 53.3654)
      )
    )
  )
)
