(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (date "mar. 31 mars 2015")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 103.378 121.666)
    (pcbplotparams
      (layerselection 0x00010f0_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "../../Documents/Xe Level Sensor/official-level-sensor-gerbers")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "/A10")
  (net 3 "/A11")
  (net 4 "/A12")
  (net 5 "/A13")
  (net 6 "/A14")
  (net 7 "/A15")
  (net 8 "Net-(C1-Pad2)")
  (net 9 "unconnected-(U1-Pad8)")
  (net 10 "unconnected-(U1-Pad5)")
  (net 11 "unconnected-(U1-Pad3)")
  (net 12 "unconnected-(Teensy_Ethernet1-Pad7)")
  (net 13 "unconnected-(Teensy_Ethernet1-Pad12)")
  (net 14 "unconnected-(Teensy_Ethernet1-Pad11)")
  (net 15 "Net-(C7-Pad1)")
  (net 16 "Net-(J1-Pad1)")
  (net 17 "Net-(J1-Pad3)")
  (net 18 "Net-(J1-Pad4)")
  (net 19 "Net-(J1-Pad5)")
  (net 20 "Net-(MCU1-Pad2)")
  (net 21 "Net-(MCU1-Pad3)")
  (net 22 "Net-(MCU1-Pad33)")
  (net 23 "Net-(U1-Pad7)")
  (net 24 "Net-(J1-Pad2)")
  (net 25 "Net-(C3-Pad1)")
  (net 26 "Net-(MCU1-Pad65)")
  (net 27 "Net-(MCU1-Pad63)")
  (net 28 "Net-(MCU1-Pad62)")
  (net 29 "Net-(MCU1-Pad61)")
  (net 30 "Net-(MCU1-Pad60)")
  (net 31 "Net-(MCU1-Pad41)")
  (net 32 "Net-(MCU1-Pad40)")
  (net 33 "Net-(C2-Pad1)")
  (net 34 "Net-(C1-Pad1)")
  (net 35 "unconnected-(U2-Pad11)")
  (net 36 "unconnected-(U2-Pad12)")
  (net 37 "Net-(J5-Pad1)")
  (net 38 "Net-(J5-Pad2)")
  (net 39 "Net-(J5-Pad3)")
  (net 40 "Net-(J5-Pad4)")
  (net 41 "+3.3V")
  (net 42 "unconnected-(MCU1-Pad49)")
  (net 43 "Net-(MCU1-Pad48)")
  (net 44 "unconnected-(MCU1-Pad45)")
  (net 45 "unconnected-(MCU1-Pad44)")
  (net 46 "unconnected-(MCU1-Pad43)")
  (net 47 "unconnected-(MCU1-Pad42)")
  (net 48 "unconnected-(MCU1-Pad39)")
  (net 49 "unconnected-(MCU1-Pad38)")
  (net 50 "unconnected-(MCU1-Pad37)")
  (net 51 "unconnected-(MCU1-Pad36)")
  (net 52 "unconnected-(MCU1-Pad35)")
  (net 53 "Net-(MCU1-Pad4)")
  (net 54 "Net-(MCU1-Pad5)")
  (net 55 "Net-(MCU1-Pad6)")
  (net 56 "Net-(MCU1-Pad7)")
  (net 57 "Net-(MCU1-Pad8)")
  (net 58 "Net-(MCU1-Pad9)")
  (net 59 "Net-(MCU1-Pad10)")
  (net 60 "Net-(MCU1-Pad11)")
  (net 61 "Net-(MCU1-Pad12)")
  (net 62 "Net-(MCU1-Pad13)")
  (net 63 "unconnected-(MCU1-Pad32)")
  (net 64 "unconnected-(MCU1-Pad29)")
  (net 65 "unconnected-(MCU1-Pad28)")
  (net 66 "unconnected-(MCU1-Pad27)")
  (net 67 "unconnected-(MCU1-Pad26)")
  (net 68 "unconnected-(MCU1-Pad25)")
  (net 69 "unconnected-(MCU1-Pad24)")
  (net 70 "unconnected-(MCU1-Pad23)")
  (net 71 "unconnected-(MCU1-Pad22)")
  (net 72 "Net-(MCU1-Pad14)")
  (net 73 "Net-(C6-Pad1)")
  (net 74 "Net-(J2-Pad1)")
  (net 75 "Net-(J2-Pad4)")
  (net 76 "unconnected-(MCU1-Pad31)")
  (net 77 "unconnected-(MCU1-Pad30)")
  (footprint "Connector_Molex:Molex_SL_171971-0004_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5DA36613)
    (at 184.8 95 -90)
    (descr "Molex Stackable Linear Connector, 171971-0004 (compatible alternatives: 171971-0104, 171971-0204), 4 Pins per row (https://www.molex.com/pdm_docs/sd/1719710002_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex SL vertical")
    (property "Description" "2.54mm,Cgrid,header,shrouded,vert,4w Molex SL Series, Series Number 70543, 2.54mm Pitch 4 Way 1 Row Straight PCB Header, Solder Termination, 3A")
    (property "Height" "11.43")
    (property "Manufacturer_Name" "Molex")
    (property "Manufacturer_Part_Number" "70543-0003")
    (property "Mouser Part Number" "538-70543-0003")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Molex/70543-0003?qs=tYx%252BZc2nXqp%2Fu7bSTX42XQ%3D%3D")
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J6" (at 3.81 -3.75 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x04" (at 3.81 5.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 1.85 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 1.74 1.74) (drill 1.09) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 37 "Net-(J5-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.74 1.74) (drill 1.09) (layers *.Cu *.Mask)
      (net 38 "Net-(J5-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.08 0 270) (size 1.74 1.74) (drill 1.09) (layers *.Cu *.Mask)
      (net 39 "Net-(J5-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 7.62 0 270) (size 1.74 1.74) (drill 1.09) (layers *.Cu *.Mask)
      (net 40 "Net-(J5-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_SL_171971-0004_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Molex:Molex_SL_171971-0004_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5DA36613)
    (at 184.75 110.73 -90)
    (descr "Molex Stackable Linear Connector, 171971-0004 (compatible alternatives: 171971-0104, 171971-0204), 4 Pins per row (https://www.molex.com/pdm_docs/sd/1719710002_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex SL vertical")
    (property "Description" "2.54mm,Cgrid,header,shrouded,vert,4w Molex SL Series, Series Number 70543, 2.54mm Pitch 4 Way 1 Row Straight PCB Header, Solder Termination, 3A")
    (property "Height" "11.43")
    (property "Manufacturer_Name" "Molex")
    (property "Manufacturer_Part_Number" "70543-0003")
    (property "Mouser Part Number" "538-70543-0003")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Molex/70543-0003?qs=tYx%252BZc2nXqp%2Fu7bSTX42XQ%3D%3D")
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J8" (at 3.81 -3.75 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x04" (at 3.81 5.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 1.85 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 1.74 1.74) (drill 1.09) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 37 "Net-(J5-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.74 1.74) (drill 1.09) (layers *.Cu *.Mask)
      (net 38 "Net-(J5-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.08 0 270) (size 1.74 1.74) (drill 1.09) (layers *.Cu *.Mask)
      (net 39 "Net-(J5-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 7.62 0 270) (size 1.74 1.74) (drill 1.09) (layers *.Cu *.Mask)
      (net 40 "Net-(J5-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_SL_171971-0004_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:ScrewTerm 4p 3.5mm" (layer "F.Cu")
    (tedit 0)
    (at 174.6 70.45 90)
    (property "DigikeyPN" "609-3920-ND")
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 5.8 -4.7 90 unlocked) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Female" (at 0 1 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 74 "Net-(J2-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5 0 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 7 0 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 10.5 0 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 75 "Net-(J2-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
  )
  (footprint "Library:break" (layer "F.Cu")
    (tedit 0)
    (at 178.8 98.4)
    (fp_text reference "REF**" (at -1.6 -0.5 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "break" (at 3.5 0.8 unlocked) (layer "F.Fab"))
    (pad "" np_thru_hole oval (at 0 0) (size 1 4) (drill oval 1 4) (layers *.Mask))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 163.5625 66.8)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "68pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 73 "Net-(C6-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 126 64.044888 -90)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C7" (at 1 3.8 90) (layer "F.SilkS"))
    (fp_text value "47uF" (at 1 3.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C7-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:ScrewTerm 5p 3.5mm" (layer "F.Cu")
    (tedit 0)
    (at 148.1 117.1)
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 3.7 unlocked) (layer "F.SilkS"))
    (fp_text value "Conn_01x05" (at 0 7.62 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -7 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at -3.5 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 3.5 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 7 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 158 67.6)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 33 "Net-(C2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 75 "Net-(J2-Pad4)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:mechanical 4-40" (layer "F.Cu")
    (tedit 0)
    (at 154.8 106.4)
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H2" (at 1.8 2.4 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 1 unlocked) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.048 3.048) (drill 3.048) (layers *.Mask))
  )
  (footprint "Connector_BarrelJack:BarrelJack_Horizontal" (layer "F.Cu")
    (tedit 5A1DBF6A)
    (at 117.6 63.8)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at -8.45 5.75) (layer "F.SilkS"))
    (fp_text value "Barrel_Jack" (at -6.2 -5.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3 -2.95) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 15 "Net-(C7-Pad1)") (pintype "passive"))
    (pad "2" thru_hole roundrect (at -6 0) (size 3 3.5) (drill oval 1 3) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "3" thru_hole roundrect (at -3 4.7) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
    (model "${KICAD6_3DMODEL_DIR}/Connector_BarrelJack.3dshapes/BarrelJack_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:loadcell_mechanical" (layer "F.Cu")
    (tedit 0)
    (at 208.4 113.75 90)
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H1" (at 3.9 -1.5 90 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 1 90 unlocked) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3.048 3.048) (drill 3.048) (layers *.Mask))
    (pad "" np_thru_hole circle (at 12.7 0 90) (size 3.048 3.048) (drill 3.048) (layers *.Mask))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 127.8 70.8 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 41 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 32 "Net-(MCU1-Pad40)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:mechanical 4-40" (layer "F.Cu")
    (tedit 0)
    (at 122.5 60)
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H3" (at 0 -1.4 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 1 unlocked) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.048 3.048) (drill 3.048) (layers *.Mask))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 149 69.0375 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "22pF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 25 "Net-(C3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:break" (layer "F.Cu")
    (tedit 0)
    (at 178.8 116)
    (fp_text reference "REF**" (at -1.6 -0.5 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "break" (at 3.5 0.8 unlocked) (layer "F.Fab"))
    (pad "" np_thru_hole oval (at 0 0) (size 1 4) (drill oval 1 4) (layers *.Mask))
  )
  (footprint "Library:mechanical 4-40" (layer "F.Cu")
    (tedit 0)
    (at 161.6 60)
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "H5" (at 0 -1.4 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 1 unlocked) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.048 3.048) (drill 3.048) (layers *.Mask))
  )
  (footprint "Connector_Molex:Molex_SL_171971-0004_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5DA36613)
    (at 201.6 96.54 180)
    (descr "Molex Stackable Linear Connector, 171971-0004 (compatible alternatives: 171971-0104, 171971-0204), 4 Pins per row (https://www.molex.com/pdm_docs/sd/1719710002_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex SL vertical")
    (property "Description" "2.54mm,Cgrid,header,shrouded,vert,4w Molex SL Series, Series Number 70543, 2.54mm Pitch 4 Way 1 Row Straight PCB Header, Solder Termination, 3A")
    (property "Height" "11.43")
    (property "Manufacturer_Name" "Molex")
    (property "Manufacturer_Part_Number" "70543-0003")
    (property "Mouser Part Number" "538-70543-0003")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Molex/70543-0003?qs=tYx%252BZc2nXqp%2Fu7bSTX42XQ%3D%3D")
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J9" (at -4 0.54) (layer "F.SilkS"))
    (fp_text value "Conn_01x04" (at 3.81 5.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 1.85) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 180) (size 1.74 1.74) (drill 1.09) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 37 "Net-(J5-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.74 1.74) (drill 1.09) (layers *.Cu *.Mask)
      (net 38 "Net-(J5-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.08 0 180) (size 1.74 1.74) (drill 1.09) (layers *.Cu *.Mask)
      (net 39 "Net-(J5-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 7.62 0 180) (size 1.74 1.74) (drill 1.09) (layers *.Cu *.Mask)
      (net 40 "Net-(J5-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_SL_171971-0004_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:break" (layer "F.Cu")
    (tedit 0)
    (at 178.8 120.4)
    (fp_text reference "REF**" (at -1.6 -0.5 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "break" (at 3.5 0.8 unlocked) (layer "F.Fab"))
    (pad "" np_thru_hole oval (at 0 0) (size 1 4) (drill oval 1 4) (layers *.Mask))
  )
  (footprint "Teensy41:Teensy41" (layer "F.Cu")
    (tedit 5FD6DEAD)
    (at 136.01 83.52)
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "MCU1" (at 0 -10.16) (layer "F.SilkS"))
    (fp_text value "Teensy4.1" (at 0 10.16) (layer "F.Fab"))
    (fp_text user "USB" (at -26.67 0 270) (layer "F.SilkS"))
    (fp_text user "MIMXRT1062" (at -1.27 0 -90) (layer "F.SilkS"))
    (fp_text user "DVJ6A" (at -2.54 -0.18 -90) (layer "F.SilkS"))
    (fp_text user "Ethernet" (at -12.065 -3.2766 90) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -29.21 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" thru_hole circle (at -26.67 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 20 "Net-(MCU1-Pad2)") (pinfunction "0_RX1_CRX2_CS1") (pintype "bidirectional"))
    (pad "3" thru_hole circle (at -24.13 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 21 "Net-(MCU1-Pad3)") (pinfunction "1_TX1_CTX2_MISO1") (pintype "bidirectional"))
    (pad "4" thru_hole circle (at -21.59 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 53 "Net-(MCU1-Pad4)") (pinfunction "2_OUT2") (pintype "bidirectional"))
    (pad "5" thru_hole circle (at -19.05 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 54 "Net-(MCU1-Pad5)") (pinfunction "3_LRCLK2") (pintype "bidirectional"))
    (pad "6" thru_hole circle (at -16.51 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 55 "Net-(MCU1-Pad6)") (pinfunction "4_BCLK2") (pintype "bidirectional"))
    (pad "7" thru_hole circle (at -13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 56 "Net-(MCU1-Pad7)") (pinfunction "5_IN2") (pintype "bidirectional"))
    (pad "8" thru_hole circle (at -11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 57 "Net-(MCU1-Pad8)") (pinfunction "6_OUT1D") (pintype "bidirectional"))
    (pad "9" thru_hole circle (at -8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 58 "Net-(MCU1-Pad9)") (pinfunction "7_RX2_OUT1A") (pintype "bidirectional"))
    (pad "10" thru_hole circle (at -6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 59 "Net-(MCU1-Pad10)") (pinfunction "8_TX2_IN1") (pintype "bidirectional"))
    (pad "11" thru_hole circle (at -3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 60 "Net-(MCU1-Pad11)") (pinfunction "9_OUT1C") (pintype "bidirectional"))
    (pad "12" thru_hole circle (at -1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 61 "Net-(MCU1-Pad12)") (pinfunction "10_CS_MQSR") (pintype "bidirectional"))
    (pad "13" thru_hole circle (at 1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 62 "Net-(MCU1-Pad13)") (pinfunction "11_MOSI_CTX1") (pintype "bidirectional"))
    (pad "14" thru_hole circle (at 3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 72 "Net-(MCU1-Pad14)") (pinfunction "12_MISO_MQSL") (pintype "bidirectional"))
    (pad "15" thru_hole circle (at 6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 41 "+3.3V") (pinfunction "3V3") (pintype "power_in"))
    (pad "16" thru_hole circle (at 8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "/A10") (pinfunction "24_A10_TX6_SCL2") (pintype "bidirectional"))
    (pad "17" thru_hole circle (at 11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "/A11") (pinfunction "25_A11_RX6_SDA2") (pintype "bidirectional"))
    (pad "18" thru_hole circle (at 13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 "/A12") (pinfunction "26_A12_MOSI1") (pintype "bidirectional"))
    (pad "19" thru_hole circle (at 16.51 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "/A13") (pinfunction "27_A13_SCK1") (pintype "bidirectional"))
    (pad "20" thru_hole circle (at 19.05 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "/A14") (pinfunction "28_RX7") (pintype "bidirectional"))
    (pad "21" thru_hole circle (at 21.59 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "/A15") (pinfunction "29_TX7") (pintype "bidirectional"))
    (pad "22" thru_hole circle (at 24.13 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 71 "unconnected-(MCU1-Pad22)") (pinfunction "30_CRX3") (pintype "bidirectional"))
    (pad "23" thru_hole circle (at 26.67 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 70 "unconnected-(MCU1-Pad23)") (pinfunction "31_CTX3") (pintype "bidirectional"))
    (pad "24" thru_hole circle (at 29.21 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 69 "unconnected-(MCU1-Pad24)") (pinfunction "32_OUT1B") (pintype "bidirectional"))
    (pad "25" thru_hole circle (at 29.21 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 68 "unconnected-(MCU1-Pad25)") (pinfunction "33_MCLK2") (pintype "bidirectional"))
    (pad "26" thru_hole circle (at 26.67 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 67 "unconnected-(MCU1-Pad26)") (pinfunction "34_RX8") (pintype "bidirectional"))
    (pad "27" thru_hole circle (at 24.13 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 66 "unconnected-(MCU1-Pad27)") (pinfunction "35_TX8") (pintype "bidirectional"))
    (pad "28" thru_hole circle (at 21.59 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 65 "unconnected-(MCU1-Pad28)") (pinfunction "36_CS") (pintype "bidirectional"))
    (pad "29" thru_hole circle (at 19.05 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 64 "unconnected-(MCU1-Pad29)") (pinfunction "37_CS") (pintype "bidirectional"))
    (pad "30" thru_hole circle (at 16.51 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 77 "unconnected-(MCU1-Pad30)") (pinfunction "38_CS1_IN1") (pintype "bidirectional"))
    (pad "31" thru_hole circle (at 13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 76 "unconnected-(MCU1-Pad31)") (pinfunction "39_MISO1_OUT1A") (pintype "bidirectional"))
    (pad "32" thru_hole circle (at 11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 63 "unconnected-(MCU1-Pad32)") (pinfunction "40_A16") (pintype "bidirectional"))
    (pad "33" thru_hole circle (at 8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 22 "Net-(MCU1-Pad33)") (pinfunction "41_A17") (pintype "bidirectional"))
    (pad "34" thru_hole circle (at 6.35 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "35" thru_hole circle (at 3.81 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 52 "unconnected-(MCU1-Pad35)") (pinfunction "13_SCK_LED") (pintype "bidirectional"))
    (pad "36" thru_hole circle (at 1.27 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 51 "unconnected-(MCU1-Pad36)") (pinfunction "14_A0_TX3_SPDIF_OUT") (pintype "bidirectional"))
    (pad "37" thru_hole circle (at -1.27 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 50 "unconnected-(MCU1-Pad37)") (pinfunction "15_A1_RX3_SPDIF_IN") (pintype "bidirectional"))
    (pad "38" thru_hole circle (at -3.81 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 49 "unconnected-(MCU1-Pad38)") (pinfunction "16_A2_RX4_SCL1") (pintype "bidirectional"))
    (pad "39" thru_hole circle (at -6.35 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 48 "unconnected-(MCU1-Pad39)") (pinfunction "17_A3_TX4_SDA1") (pintype "bidirectional"))
    (pad "40" thru_hole circle (at -8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 32 "Net-(MCU1-Pad40)") (pinfunction "18_A4_SDA") (pintype "bidirectional"))
    (pad "41" thru_hole circle (at -11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 31 "Net-(MCU1-Pad41)") (pinfunction "19_A5_SCL") (pintype "bidirectional"))
    (pad "42" thru_hole circle (at -13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 47 "unconnected-(MCU1-Pad42)") (pinfunction "20_A6_TX5_LRCLK1") (pintype "bidirectional"))
    (pad "43" thru_hole circle (at -16.51 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 46 "unconnected-(MCU1-Pad43)") (pinfunction "21_A7_RX5_BCLK1") (pintype "bidirectional"))
    (pad "44" thru_hole circle (at -19.05 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 45 "unconnected-(MCU1-Pad44)") (pinfunction "22_A8_CTX1") (pintype "bidirectional"))
    (pad "45" thru_hole circle (at -21.59 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 44 "unconnected-(MCU1-Pad45)") (pinfunction "23_A9_CRX1_MCLK1") (pintype "bidirectional"))
    (pad "46" thru_hole circle (at -24.13 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 41 "+3.3V") (pinfunction "3V3") (pintype "output"))
    (pad "47" thru_hole circle (at -26.67 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "output"))
    (pad "48" thru_hole circle (at -29.21 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 43 "Net-(MCU1-Pad48)") (pinfunction "VIN") (pintype "power_in"))
    (pad "49" thru_hole circle (at -26.67 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 42 "unconnected-(MCU1-Pad49)") (pinfunction "VUSB") (pintype "power_out"))
    (pad "60" thru_hole rect (at -16.24 -5.1816) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(MCU1-Pad60)") (pinfunction "R+") (pintype "bidirectional"))
    (pad "61" thru_hole circle (at -16.24 -3.1816) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(MCU1-Pad61)") (pinfunction "LED") (pintype "bidirectional"))
    (pad "62" thru_hole circle (at -16.24 -1.1816) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(MCU1-Pad62)") (pinfunction "T-") (pintype "bidirectional"))
    (pad "63" thru_hole circle (at -14.24 -1.1816) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(MCU1-Pad63)") (pinfunction "T+") (pintype "bidirectional"))
    (pad "64" thru_hole circle (at -14.24 -3.1816) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C1-Pad2)") (pinfunction "GND") (pintype "power_in"))
    (pad "65" thru_hole circle (at -14.24 -5.1816) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(MCU1-Pad65)") (pinfunction "R-") (pintype "bidirectional"))
    (model "${KICAD_USER_DIR}/teensy.pretty/Teensy_4.1_Assembly.STEP"
      (offset (xyz 0 0 0.762))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:Fuse" (layer "F.Cu")
    (tedit 0)
    (at 134.52 64.75 -90)
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "F1" (at 0 -0.5 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "Fuse_Small" (at 0 1 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -3.75 0 270) (size 4.5 3.81) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(C7-Pad1)") (pintype "passive"))
    (pad "2" smd rect (at 3.75 0 270) (size 4.5 3.81) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "Net-(MCU1-Pad48)") (pintype "passive"))
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Bridged2Bar_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (tedit 5C74525F)
    (at 130.8 64.6 -90)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 2 copper strips")
    (tags "net tie solder jumper bridged")
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "JP4" (at 0 -1.8 90) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Bridged" (at 0 1.9 90) (layer "F.Fab"))
    (pad "1" smd custom (at -0.65 0 270) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 15 "Net-(C7-Pad1)") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0.5 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0 270) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 43 "Net-(MCU1-Pad48)") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0 -0.75)
          ) (width 0) (fill yes))
      ))
  )
  (footprint "Library:break" (layer "F.Cu")
    (tedit 0)
    (at 178.8 94)
    (fp_text reference "REF**" (at -1.6 -0.5 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "break" (at 3.5 0.8 unlocked) (layer "F.Fab"))
    (pad "" np_thru_hole oval (at 0 0) (size 1 4) (drill oval 1 4) (layers *.Mask))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 124.4 70.8 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 41 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 31 "Net-(MCU1-Pad41)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 173 95.2)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C1" (at 1.25 -2.05) (layer "F.SilkS"))
    (fp_text value "0.1uF1" (at 1.25 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:break" (layer "F.Cu")
    (tedit 0)
    (at 178.8 107.2)
    (fp_text reference "REF**" (at -1.6 -0.5 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "break" (at 3.5 0.8 unlocked) (layer "F.Fab"))
    (pad "" np_thru_hole oval (at 0 0) (size 1 4) (drill oval 1 4) (layers *.Mask))
  )
  (footprint "Library:break" (layer "F.Cu")
    (tedit 0)
    (at 178.8 102.8)
    (fp_text reference "REF**" (at -1.6 -0.5 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "break" (at 3.5 0.8 unlocked) (layer "F.Fab"))
    (pad "" np_thru_hole oval (at 0 0) (size 1 4) (drill oval 1 4) (layers *.Mask))
  )
  (footprint "Connector_Molex:Molex_SL_171971-0004_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5DA36613)
    (at 201.8 118.14 180)
    (descr "Molex Stackable Linear Connector, 171971-0004 (compatible alternatives: 171971-0104, 171971-0204), 4 Pins per row (https://www.molex.com/pdm_docs/sd/1719710002_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex SL vertical")
    (property "Description" "2.54mm,Cgrid,header,shrouded,vert,4w Molex SL Series, Series Number 70543, 2.54mm Pitch 4 Way 1 Row Straight PCB Header, Solder Termination, 3A")
    (property "Height" "11.43")
    (property "Manufacturer_Name" "Molex")
    (property "Manufacturer_Part_Number" "70543-0003")
    (property "Mouser Part Number" "538-70543-0003")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Molex/70543-0003?qs=tYx%252BZc2nXqp%2Fu7bSTX42XQ%3D%3D")
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at -4.2 0.14) (layer "F.SilkS"))
    (fp_text value "Conn_01x04" (at 3.81 5.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 1.85) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 180) (size 1.74 1.74) (drill 1.09) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 37 "Net-(J5-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.74 1.74) (drill 1.09) (layers *.Cu *.Mask)
      (net 38 "Net-(J5-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.08 0 180) (size 1.74 1.74) (drill 1.09) (layers *.Cu *.Mask)
      (net 39 "Net-(J5-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 7.62 0 180) (size 1.74 1.74) (drill 1.09) (layers *.Cu *.Mask)
      (net 40 "Net-(J5-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_SL_171971-0004_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Bridged2Bar_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (tedit 5C74525F)
    (at 144.9 72.05 90)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 2 copper strips")
    (tags "net tie solder jumper bridged")
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "JP3" (at 0 -1.8 90) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Bridged" (at 0 1.9 90) (layer "F.Fab"))
    (pad "1" smd custom (at -0.65 0 90) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 22 "Net-(MCU1-Pad33)") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0.5 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0 90) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 23 "Net-(U1-Pad7)") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0 -0.75)
          ) (width 0) (fill yes))
      ))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 158 64.2)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "47pF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 33 "Net-(C2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 153.4 70)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "82k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 25 "Net-(C3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 73 "Net-(C6-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:MSOP-10_3x3mm_P0.5mm" (layer "F.Cu")
    (tedit 5A02F25C)
    (at 151.2 64.4)
    (descr "10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.5")
    (property "DigikeyPN" "AD7151BRMZ-ND")
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -2.6) (layer "F.SilkS"))
    (fp_text value "AD7151" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.2 -1) (size 1.4 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (pad "2" smd rect (at -2.2 -0.5) (size 1.4 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "+3.3V") (pinfunction "VDD") (pintype "input"))
    (pad "3" smd rect (at -2.2 0) (size 1.4 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "unconnected-(U1-Pad3)") (pinfunction "NC") (pintype "no_connect"))
    (pad "4" smd rect (at -2.2 0.5) (size 1.4 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(C3-Pad1)") (pinfunction "CIN") (pintype "input"))
    (pad "5" smd rect (at -2.2 1) (size 1.4 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "unconnected-(U1-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd rect (at 2.2 1) (size 1.4 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "Net-(C2-Pad1)") (pinfunction "EXC") (pintype "output"))
    (pad "7" smd rect (at 2.2 0.5) (size 1.4 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(U1-Pad7)") (pinfunction "OUT") (pintype "output"))
    (pad "8" smd rect (at 2.2 0) (size 1.4 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "unconnected-(U1-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (pad "9" smd rect (at 2.2 -0.5) (size 1.4 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "Net-(MCU1-Pad41)") (pinfunction "SCL") (pintype "input"))
    (pad "10" smd rect (at 2.2 -1) (size 1.4 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "Net-(MCU1-Pad40)") (pinfunction "SDA") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/MSOP-10_3x3mm_P0.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SEN-13879:SPARKFUN_SEN-13879" (layer "F.Cu")
    (tedit 62D764EA)
    (at 120.8895 106.205 180)
    (property "MANUFACTURER" "SparkFun")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at -11.2657 -12.35574 180) (layer "F.SilkS"))
    (fp_text value "SEN-13879" (at -3.6171 12.56965 180) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at -13.97 -5.08 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad1)") (pinfunction "RED") (pintype "bidirectional"))
    (pad "2" thru_hole circle locked (at -13.97 -2.54 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad2)") (pinfunction "BLK") (pintype "bidirectional"))
    (pad "3" thru_hole circle locked (at -13.97 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad3)") (pinfunction "WHT") (pintype "input"))
    (pad "4" thru_hole circle locked (at -13.97 2.54 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad4)") (pinfunction "GRN") (pintype "input"))
    (pad "5" thru_hole circle locked (at -13.97 5.08 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad5)") (pinfunction "YLW") (pintype "bidirectional"))
    (pad "6" thru_hole circle locked (at 13.97 5.08 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "7" thru_hole circle locked (at 13.97 2.54 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "Net-(MCU1-Pad3)") (pinfunction "CLK") (pintype "input"))
    (pad "8" thru_hole circle locked (at 13.97 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(MCU1-Pad2)") (pinfunction "DAT") (pintype "output"))
    (pad "9" thru_hole circle locked (at 13.97 -2.54 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 "+3.3V") (pinfunction "VCC") (pintype "power_in"))
    (pad "10" thru_hole circle locked (at 13.97 -5.08 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 "+3.3V") (pinfunction "VDD") (pintype "power_in"))
    (pad "11" thru_hole circle locked (at 6.35 2.54 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 "unconnected-(U2-Pad11)") (pinfunction "B+") (pintype "input"))
    (pad "12" thru_hole circle locked (at 6.35 5.08 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 "unconnected-(U2-Pad12)") (pinfunction "B-") (pintype "input"))
  )
  (footprint "Connector_Molex:Molex_SL_171971-0004_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5DA36613)
    (at 201.6 107.14 180)
    (descr "Molex Stackable Linear Connector, 171971-0004 (compatible alternatives: 171971-0104, 171971-0204), 4 Pins per row (https://www.molex.com/pdm_docs/sd/1719710002_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex SL vertical")
    (property "Description" "2.54mm,Cgrid,header,shrouded,vert,4w Molex SL Series, Series Number 70543, 2.54mm Pitch 4 Way 1 Row Straight PCB Header, Solder Termination, 3A")
    (property "Height" "11.43")
    (property "Manufacturer_Name" "Molex")
    (property "Manufacturer_Part_Number" "70543-0003")
    (property "Mouser Part Number" "538-70543-0003")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Molex/70543-0003?qs=tYx%252BZc2nXqp%2Fu7bSTX42XQ%3D%3D")
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J7" (at -4 0.94) (layer "F.SilkS"))
    (fp_text value "Conn_01x04" (at 3.81 5.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 1.85) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 180) (size 1.74 1.74) (drill 1.09) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 37 "Net-(J5-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.74 1.74) (drill 1.09) (layers *.Cu *.Mask)
      (net 38 "Net-(J5-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.08 0 180) (size 1.74 1.74) (drill 1.09) (layers *.Cu *.Mask)
      (net 39 "Net-(J5-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 7.62 0 180) (size 1.74 1.74) (drill 1.09) (layers *.Cu *.Mask)
      (net 40 "Net-(J5-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_SL_171971-0004_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:break" (layer "F.Cu")
    (tedit 0)
    (at 178.8 111.6)
    (fp_text reference "REF**" (at -1.6 -0.5 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "break" (at 3.5 0.8 unlocked) (layer "F.Fab"))
    (pad "" np_thru_hole oval (at 0 0) (size 1 4) (drill oval 1 4) (layers *.Mask))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 157.675 96.4 -90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P4" (at 0 -2.33 90) (layer "F.SilkS"))
    (fp_text value "Analog" (at 0 20.11 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "/A15") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "/A14") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "/A13") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/A12") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/A11") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "/A10") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "+3.3V") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_RJ:RJ45_Cetus_J1B1211CCD_Horizontal" (layer "F.Cu")
    (tedit 5BBCB15F)
    (at 163.755 104.05)
    (descr "1 Port RJ45 Magjack Connector Through Hole 10/100 Base-T, Cetus, used and distributed by WIZnet (https://wizwiki.net/wiki/lib/exe/fetch.php?media=products:wiz550web:wiz550webds_kr:j1b1211ccd.pdf)")
    (tags "RJ45 Magjack")
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Teensy_Ethernet1" (at 4.645 -5.65) (layer "F.SilkS"))
    (fp_text value "RJ45_LED" (at 4.445 18) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4 16) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -1.27 6.35) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 10.16 6.35) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.167)
      (net 27 "Net-(MCU1-Pad63)") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.27 -2.54) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 34 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "3" thru_hole circle (at 2.54 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 28 "Net-(MCU1-Pad62)") (pintype "passive"))
    (pad "4" thru_hole circle (at 3.81 -2.54) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 30 "Net-(MCU1-Pad60)") (pintype "passive"))
    (pad "5" thru_hole circle (at 5.08 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 34 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "6" thru_hole circle (at 6.35 -2.54) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 26 "Net-(MCU1-Pad65)") (pintype "passive"))
    (pad "7" thru_hole circle (at 7.62 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "unconnected-(Teensy_Ethernet1-Pad7)") (pintype "passive"))
    (pad "8" thru_hole circle (at 8.89 -2.54) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(C1-Pad2)") (pintype "passive"))
    (pad "9" thru_hole circle (at -1.88 11.43) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 8 "Net-(C1-Pad2)") (pintype "passive"))
    (pad "10" thru_hole circle (at 0.66 9.73) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 29 "Net-(MCU1-Pad61)") (pintype "passive"))
    (pad "11" thru_hole circle (at 8.23 11.43) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 14 "unconnected-(Teensy_Ethernet1-Pad11)") (pintype "passive"))
    (pad "12" thru_hole circle (at 10.77 9.73) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 13 "unconnected-(Teensy_Ethernet1-Pad12)") (pintype "passive"))
    (pad "13" thru_hole circle (at 12.32 3.3) (size 2.5 2.5) (drill 1.6) (layers *.Cu *.Mask))
    (pad "13" thru_hole circle (at -3.43 3.3) (size 2.5 2.5) (drill 1.6) (layers *.Cu *.Mask))
    (model "${KICAD6_3DMODEL_DIR}/Connector_RJ.3dshapes/RJ45_Cetus_J1B1211CCD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:ScrewTerm 4p 3.5mm" (layer "F.Cu")
    (tedit 0)
    (at 174.6 88 90)
    (property "DigikeyPN" "609-3920-ND")
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J10" (at 5.6 2.8 90 unlocked) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Female" (at 0 1 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5 0 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 41 "+3.3V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 7 0 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 41 "+3.3V") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 10.5 0 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 163.4 70.4)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "R_Small_US" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 73 "Net-(C6-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 74 "Net-(J2-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 144.6 65.2625 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 41 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 141.1 65.2625 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Official level sensorV2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 41 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 178.4 91.6) (end 178.4 57.6) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 211.6 121.6) (end 211.6 91.6) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 211.6 91.6) (end 178.4 91.6) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 178.4 57.6) (end 103.4 57.6) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 103.4 121.6) (end 211.6 121.6) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 103.4 57.6) (end 103.4 121.6) (layer "Edge.Cuts") (width 0.15))
  (gr_text "A15" (at 157.8 99.2 90) (layer "F.SilkS"))
  (gr_text "AD7151" (at 151.4 60) (layer "F.SilkS"))
  (gr_text "Cin" (at 169.4 70.4) (layer "F.SilkS"))
  (gr_text "Sparkfun HX711\n" (at 122.4 119.2) (layer "F.SilkS"))
  (gr_text "10k" (at 122.4 70.6 90) (layer "F.SilkS"))
  (gr_text "A10" (at 145 99.2 90) (layer "F.SilkS"))
  (gr_text "A14" (at 155.2 99.2 90) (layer "F.SilkS"))
  (gr_text "bung@slac\nTeensy LevelSensor V01" (at 148.6 103) (layer "F.SilkS"))
  (gr_text "A11" (at 147.6 99.2 90) (layer "F.SilkS"))
  (gr_text "3.6-5.5 VDC\nCenter Hot" (at 110 72.6) (layer "F.SilkS"))
  (gr_text "Exc" (at 169.4 59.8) (layer "F.SilkS"))
  (gr_text "G +3 +3 G" (at 169.6 82.6 90) (layer "F.SilkS"))
  (gr_text "A12" (at 150.2 99.2 90) (layer "F.SilkS"))
  (gr_text "Grn" (at 151.6 111.4 90) (layer "F.SilkS"))
  (gr_text "1A" (at 137.8 60.4) (layer "F.SilkS"))
  (gr_text "Wht" (at 148.2 111.4 90) (layer "F.SilkS"))
  (gr_text "LoadCell" (at 148 108.6) (layer "F.SilkS"))
  (gr_text "A13\n" (at 152.6 99.2 90) (layer "F.SilkS"))
  (gr_text "Ylw" (at 155.2 111.2 90) (layer "F.SilkS"))
  (gr_text "47uF" (at 126.4 61.4) (layer "F.SilkS"))
  (gr_text "Blk" (at 144.6 111.6 90) (layer "F.SilkS"))
  (gr_text "Red" (at 141 111.4 90) (layer "F.SilkS"))
  (gr_text "Gnd" (at 139.8 99.4 90) (layer "F.SilkS"))
  (gr_text "3v3" (at 142.6 99.4 90) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layer "B.Cu") (name "GND") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178.6 121.6)
        (xy 103.4 121.6)
        (xy 103.4 57.8)
        (xy 103.6 57.6)
        (xy 178.4 57.6)
      )
    )
  )
)
