(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 36)
    (no_connects 0)
    (area 147.624999 100.074999 166.075001 130.15)
    (thickness 1.6)
    (drawings 11)
    (tracks 126)
    (zones 0)
    (modules 15)
    (nets 54)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.127)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(R1-Pad1)")
  (net 5 /D+)
  (net 6 "Net-(R2-Pad1)")
  (net 7 /D-)
  (net 8 "Net-(R3-Pad1)")
  (net 9 /VCC)
  (net 10 "Net-(R4-Pad1)")
  (net 11 "Net-(R5-Pad1)")
  (net 12 "Net-(U1-Pad1)")
  (net 13 "Net-(U1-Pad6)")
  (net 14 "Net-(U1-Pad9)")
  (net 15 "Net-(U1-Pad10)")
  (net 16 "Net-(U1-Pad11)")
  (net 17 "Net-(U1-Pad12)")
  (net 18 "Net-(U1-Pad13)")
  (net 19 "Net-(U1-Pad18)")
  (net 20 "Net-(U1-Pad19)")
  (net 21 "Net-(U1-Pad20)")
  (net 22 "Net-(U1-Pad21)")
  (net 23 "Net-(U1-Pad22)")
  (net 24 "Net-(U1-Pad25)")
  (net 25 "Net-(U1-Pad26)")
  (net 26 "Net-(U1-Pad27)")
  (net 27 "Net-(U1-Pad28)")
  (net 28 "Net-(U1-Pad29)")
  (net 29 "Net-(U1-Pad30)")
  (net 30 "Net-(U1-Pad31)")
  (net 31 "Net-(U1-Pad32)")
  (net 32 "Net-(U1-Pad33)")
  (net 33 "Net-(U1-Pad36)")
  (net 34 "Net-(U1-Pad37)")
  (net 35 "Net-(U1-Pad38)")
  (net 36 "Net-(U1-Pad39)")
  (net 37 "Net-(U1-Pad40)")
  (net 38 "Net-(U1-Pad41)")
  (net 39 "Net-(U1-Pad42)")
  (net 40 "Net-(U2-PadA2)")
  (net 41 "Net-(U2-PadA3)")
  (net 42 "Net-(U2-PadA8)")
  (net 43 "Net-(U2-PadA10)")
  (net 44 "Net-(U2-PadA11)")
  (net 45 "Net-(U2-PadB2)")
  (net 46 "Net-(U2-PadB3)")
  (net 47 "Net-(U2-PadB6)")
  (net 48 "Net-(U2-PadB7)")
  (net 49 "Net-(U2-PadB8)")
  (net 50 "Net-(U2-PadB10)")
  (net 51 "Net-(U2-PadB11)")
  (net 52 "Net-(W1-Pad1)")
  (net 53 "Net-(X1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /D+)
    (add_net /D-)
    (add_net /VCC)
    (add_net GND)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad33)")
    (add_net "Net-(U1-Pad36)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad38)")
    (add_net "Net-(U1-Pad39)")
    (add_net "Net-(U1-Pad40)")
    (add_net "Net-(U1-Pad41)")
    (add_net "Net-(U1-Pad42)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-PadA10)")
    (add_net "Net-(U2-PadA11)")
    (add_net "Net-(U2-PadA2)")
    (add_net "Net-(U2-PadA3)")
    (add_net "Net-(U2-PadA8)")
    (add_net "Net-(U2-PadB10)")
    (add_net "Net-(U2-PadB11)")
    (add_net "Net-(U2-PadB2)")
    (add_net "Net-(U2-PadB3)")
    (add_net "Net-(U2-PadB6)")
    (add_net "Net-(U2-PadB7)")
    (add_net "Net-(U2-PadB8)")
    (add_net "Net-(W1-Pad1)")
    (add_net "Net-(X1-Pad2)")
  )
  (module Mounting_Holes:MountingHole_4mm (layer F.Cu) (tedit 5811039A)
    (at 0 0)
    (descr "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -5.4991) (layer F.SilkS))
    (fp_text value MountingHole_3mm (at 0 5.99948) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_4mm (layer F.Cu) (tedit 5811039A)
    (at 0 0)
    (descr "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -5.4991) (layer F.SilkS))
    (fp_text value MountingHole_3mm (at 0 5.99948) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module usb-type-c:12401548E4#2A-usb-c (layer F.Cu) (tedit 58104CFB)
    (at 157.8 129.7)
    (fp_text reference U2 (at 0 -1.9685) (layer F.SilkS) hide)
    (fp_text value USB_TYPE_C (at 0 -7.366) (layer F.Fab) hide)
    (pad A1 smd rect (at -2.7715 -0.795) (size 0.27 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A2 smd rect (at -2.2715 -0.795) (size 0.27 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U2-PadA2)"))
    (pad A3 smd rect (at -1.7715 -0.795) (size 0.27 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U2-PadA3)"))
    (pad A4 smd rect (at -1.2715 -0.795) (size 0.27 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 /VCC))
    (pad A5 smd rect (at -0.7715 -0.795) (size 0.27 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R4-Pad1)"))
    (pad A6 smd rect (at -0.2715 -0.795) (size 0.27 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 /D+))
    (pad A7 smd rect (at 0.2285 -0.795) (size 0.27 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 /D-))
    (pad A8 smd rect (at 0.7285 -0.795) (size 0.27 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U2-PadA8)"))
    (pad A9 smd rect (at 1.2285 -0.795) (size 0.27 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 /VCC))
    (pad A10 smd rect (at 1.7285 -0.795) (size 0.27 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U2-PadA10)"))
    (pad A11 smd rect (at 2.2285 -0.795) (size 0.27 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U2-PadA11)"))
    (pad A12 smd rect (at 2.7285 -0.795) (size 0.27 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B1 smd rect (at 2.7275 -0.7825) (size 0.27 0.8) (layers B.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B2 smd rect (at 2.2275 -0.7825) (size 0.27 0.8) (layers B.Cu F.Paste F.Mask)
      (net 45 "Net-(U2-PadB2)"))
    (pad B3 smd rect (at 1.7275 -0.7825) (size 0.27 0.8) (layers B.Cu F.Paste F.Mask)
      (net 46 "Net-(U2-PadB3)"))
    (pad B4 smd rect (at 1.2275 -0.7825) (size 0.27 0.8) (layers B.Cu F.Paste F.Mask)
      (net 9 /VCC))
    (pad B5 smd rect (at 0.7275 -0.7825) (size 0.27 0.8) (layers B.Cu F.Paste F.Mask)
      (net 11 "Net-(R5-Pad1)"))
    (pad B6 smd rect (at 0.2275 -0.7825) (size 0.27 0.8) (layers B.Cu F.Paste F.Mask)
      (net 47 "Net-(U2-PadB6)"))
    (pad B7 smd rect (at -0.2725 -0.7825) (size 0.27 0.8) (layers B.Cu F.Paste F.Mask)
      (net 48 "Net-(U2-PadB7)"))
    (pad B8 smd rect (at -0.7725 -0.7825) (size 0.27 0.8) (layers B.Cu F.Paste F.Mask)
      (net 49 "Net-(U2-PadB8)"))
    (pad B9 smd rect (at -1.2725 -0.7825) (size 0.27 0.8) (layers B.Cu F.Paste F.Mask)
      (net 9 /VCC))
    (pad B10 smd rect (at -1.7725 -0.7825) (size 0.27 0.8) (layers B.Cu F.Paste F.Mask)
      (net 50 "Net-(U2-PadB10)"))
    (pad B11 smd rect (at -2.2725 -0.7825) (size 0.27 0.8) (layers B.Cu F.Paste F.Mask)
      (net 51 "Net-(U2-PadB11)"))
    (pad B12 smd rect (at -2.7725 -0.7825) (size 0.27 0.8) (layers B.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad "" smd rect (at -3.2385 -0.8255) (size 0.27 0.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 3.175 -0.8255) (size 0.27 0.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 3.175 -0.8255) (size 0.27 0.8) (layers B.Cu F.Paste F.Mask))
    (pad "" smd rect (at -3.2385 -0.762) (size 0.27 0.8) (layers B.Cu F.Paste F.Mask))
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58104BC4)
    (at 160.9 113.2 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 1.9 180) (layer B.SilkS) hide)
    (fp_text value 22p (at 0 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58104B43)
    (at 157 110.5 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 1.9 180) (layer B.SilkS) hide)
    (fp_text value 22p (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58104CB5)
    (at 149.2 122.2 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.9 270) (layer F.SilkS) hide)
    (fp_text value 22 (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 /D+))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58104CAC)
    (at 151.9 122.3 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.9 270) (layer F.SilkS) hide)
    (fp_text value 22 (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 /D-))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58104C3A)
    (at 150.3 117.2 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 1.9 180) (layer B.SilkS) hide)
    (fp_text value 10m (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 9 /VCC))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5810FFF0)
    (at 151.7 126.65 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value 56k (at -0.05 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 /VCC))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58104D20)
    (at 159.35 126.2)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 1.9) (layer B.SilkS) hide)
    (fp_text value 56k (at 0 0 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 9 /VCC))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_Matias_Quiet (layer F.Cu) (tedit 545FEB3B)
    (at 154.3 107.4)
    (descr http://matias.ca/switches/quiet/)
    (tags "Matias, quiet, keyboard, key, switch")
    (fp_text reference SW1 (at 2.5 4) (layer F.SilkS))
    (fp_text value SPST (at 2.5 6.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5 -0.5) (size 3 3) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(R3-Pad1)"))
  )
  (module Housings_DFN_QFN:QFN-44-1EP_7x7mm_Pitch0.5mm (layer B.Cu) (tedit 58104CE2)
    (at 157.4 119.9)
    (descr "UK Package; 44-Lead Plastic QFN (7mm x 7mm); (see Linear Technology QFN_44_05-08-1763.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 4.75) (layer B.SilkS) hide)
    (fp_text value ATMEGA32U4-M (at 4.6 -1.6 90) (layer B.SilkS))
    (pad 1 smd rect (at -3.4 2.5) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(U1-Pad1)"))
    (pad 2 smd rect (at -3.4 2) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 9 /VCC))
    (pad 3 smd rect (at -3.4 1.5) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(R2-Pad1)"))
    (pad 4 smd rect (at -3.4 1) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(R1-Pad1)"))
    (pad 5 smd rect (at -3.4 0.5) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.4 0) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at -3.4 -0.5) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 9 /VCC))
    (pad 8 smd rect (at -3.4 -1) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(R3-Pad1)"))
    (pad 9 smd rect (at -3.4 -1.5) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(U1-Pad9)"))
    (pad 10 smd rect (at -3.4 -2) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(U1-Pad10)"))
    (pad 11 smd rect (at -3.4 -2.5) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(U1-Pad11)"))
    (pad 12 smd rect (at -2.5 -3.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(U1-Pad12)"))
    (pad 13 smd rect (at -2 -3.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(U1-Pad13)"))
    (pad 14 smd rect (at -1.5 -3.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 9 /VCC))
    (pad 15 smd rect (at -1 -3.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 16 smd rect (at -0.5 -3.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 17 smd rect (at 0 -3.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 18 smd rect (at 0.5 -3.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(U1-Pad18)"))
    (pad 19 smd rect (at 1 -3.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(U1-Pad19)"))
    (pad 20 smd rect (at 1.5 -3.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(U1-Pad20)"))
    (pad 21 smd rect (at 2 -3.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(U1-Pad21)"))
    (pad 22 smd rect (at 2.5 -3.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(U1-Pad22)"))
    (pad 23 smd rect (at 3.4 -2.5) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 3.4 -2) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 9 /VCC))
    (pad 25 smd rect (at 3.4 -1.5) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(U1-Pad25)"))
    (pad 26 smd rect (at 3.4 -1) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(U1-Pad26)"))
    (pad 27 smd rect (at 3.4 -0.5) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(U1-Pad27)"))
    (pad 28 smd rect (at 3.4 0) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(U1-Pad28)"))
    (pad 29 smd rect (at 3.4 0.5) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(U1-Pad29)"))
    (pad 30 smd rect (at 3.4 1) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(U1-Pad30)"))
    (pad 31 smd rect (at 3.4 1.5) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(U1-Pad31)"))
    (pad 32 smd rect (at 3.4 2) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(U1-Pad32)"))
    (pad 33 smd rect (at 3.4 2.5) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(U1-Pad33)"))
    (pad 34 smd rect (at 2.5 3.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 9 /VCC))
    (pad 35 smd rect (at 2 3.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 1.5 3.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(U1-Pad36)"))
    (pad 37 smd rect (at 1 3.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(U1-Pad37)"))
    (pad 38 smd rect (at 0.5 3.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(U1-Pad38)"))
    (pad 39 smd rect (at 0 3.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(U1-Pad39)"))
    (pad 40 smd rect (at -0.5 3.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(U1-Pad40)"))
    (pad 41 smd rect (at -1 3.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(U1-Pad41)"))
    (pad 42 smd rect (at -1.5 3.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(U1-Pad42)"))
    (pad 43 smd rect (at -2 3.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 44 smd rect (at -2.5 3.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 9 /VCC))
    (pad 45 smd rect (at 1.93125 -1.93125) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at 1.93125 -0.64375) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at 1.93125 0.64375) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at 1.93125 1.93125) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at 0.64375 -1.93125) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at 0.64375 -0.64375) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at 0.64375 0.64375) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at 0.64375 1.93125) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at -0.64375 -1.93125) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at -0.64375 -0.64375) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at -0.64375 0.64375) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at -0.64375 1.93125) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at -1.93125 -1.93125) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at -1.93125 -0.64375) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at -1.93125 0.64375) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 45 smd rect (at -1.93125 1.93125) (size 1.2875 1.2875) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-44-1EP_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58104C20)
    (at 150.45 114.8)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference W1 (at 0 1.9) (layer B.SilkS) hide)
    (fp_text value TEST (at 2.5 0.1) (layer B.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 52 "Net-(W1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(U1-Pad13)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Res_kyocera (layer B.Cu) (tedit 581037EA)
    (at 157 112.8 180)
    (descr "Murata CSTCC8M00G53-R0; 8MHz resonator, SMD, 0.5+0.3%; Farnell (Element 14) #1170435")
    (tags resonator)
    (attr smd)
    (fp_text reference X1 (at 0.127 1.3335 180) (layer B.SilkS))
    (fp_text value XTAL (at 0 -1.143 180) (layer B.Fab))
    (pad 1 smd rect (at -1.2 0 180) (size 0.4 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at 0 0 180) (size 0.4 1.3) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(X1-Pad2)"))
    (pad 3 smd rect (at 1.2 0 180) (size 0.4 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad2)"))
  )
  (module Mounting_Holes:MountingHole3mm (layer F.Cu) (tedit 58110484)
    (at 156.9 101.3)
    (descr "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 4mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -5.4991) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0 5.99948) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_line (start 166 100.1) (end 166 98.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.7 98.25) (end 147.7 98.15) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.7 100.2) (end 147.7 98.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166 100.15) (end 166 107.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 165.65 98.1) (end 166.05 98.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.7 98.1) (end 165.6 98.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.7 107.05) (end 147.7 100.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.7 129.4) (end 147.7 107.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166 129.4) (end 147.7 129.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166 119.1) (end 166 129.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166 107.2) (end 166 119.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.128) (thermal_bridge_width 0.128))
    (polygon
      (pts
        (xy 147.85 100.35) (xy 165.8 100.35) (xy 165.7 129.15) (xy 147.85 129) (xy 147.95 100.45)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.128) (thermal_bridge_width 0.128))
    (polygon
      (pts
        (xy 147.85 100.35) (xy 165.8 100.35) (xy 165.7 129.15) (xy 147.85 129) (xy 147.95 100.45)
      )
    )
  )
)
