(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 115)
    (no_connects 0)
    (area 130.474999 94.174999 210.65613 129.325001)
    (thickness 1.6)
    (drawings 34)
    (tracks 299)
    (zones 0)
    (modules 39)
    (nets 55)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3048)
    (trace_clearance 0.0508)
    (zone_clearance 0.762)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4 4)
    (pad_drill 4)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 129.65 129.95)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VMOT)
  (net 2 GND)
  (net 3 VCC)
  (net 4 "Net-(D1-Pad1)")
  (net 5 "Net-(D2-Pad1)")
  (net 6 "Net-(FAN1-Pad2)")
  (net 7 "Net-(FAN2-Pad2)")
  (net 8 D5)
  (net 9 D4)
  (net 10 "Net-(J7-Pad1)")
  (net 11 "Net-(J7-Pad2)")
  (net 12 "Net-(J7-Pad3)")
  (net 13 "Net-(J7-Pad4)")
  (net 14 "Net-(J8-Pad1)")
  (net 15 "Net-(J8-Pad2)")
  (net 16 "Net-(J8-Pad3)")
  (net 17 "Net-(J8-Pad4)")
  (net 18 "Net-(J9-Pad1)")
  (net 19 "Net-(J9-Pad2)")
  (net 20 "Net-(J9-Pad3)")
  (net 21 "Net-(J9-Pad4)")
  (net 22 "Net-(Q1-Pad2)")
  (net 23 "Net-(Q1-Pad4)")
  (net 24 "Net-(Stepstick1-Pad5)")
  (net 25 "Net-(Stepstick2-Pad5)")
  (net 26 "Net-(Stepstick3-Pad5)")
  (net 27 "Net-(J4-Pad1)")
  (net 28 "Net-(J4-Pad3)")
  (net 29 "Net-(J4-Pad5)")
  (net 30 "Net-(J5-Pad1)")
  (net 31 "Net-(J5-Pad3)")
  (net 32 "Net-(J5-Pad5)")
  (net 33 "Net-(J6-Pad1)")
  (net 34 "Net-(J6-Pad3)")
  (net 35 "Net-(J6-Pad5)")
  (net 36 "FAN1(D11)")
  (net 37 "FAN2(D6)")
  (net 38 "EN_1(D44)")
  (net 39 "EN_2(D42)")
  (net 40 "EN_3(A4/D58)")
  (net 41 "STEP_1(A10/D64)")
  (net 42 "DIR_1(A5/D59)")
  (net 43 "STEP_2(D48)")
  (net 44 "DIR_2(A9/D63)")
  (net 45 "STEP_3(A3/D57)")
  (net 46 "DIR_3(A12/D66)")
  (net 47 "Net-(P1-Pad4)")
  (net 48 "Net-(P1-Pad7)")
  (net 49 "Net-(P1-Pad9)")
  (net 50 "Net-(P1-Pad11)")
  (net 51 "Net-(P1-Pad13)")
  (net 52 "Net-(P1-Pad15)")
  (net 53 "Z_PROBE(A11/D65)")
  (net 54 "Net-(D3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.0508)
    (trace_width 0.3048)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net D4)
    (add_net D5)
    (add_net "DIR_1(A5/D59)")
    (add_net "DIR_2(A9/D63)")
    (add_net "DIR_3(A12/D66)")
    (add_net "EN_1(D44)")
    (add_net "EN_2(D42)")
    (add_net "EN_3(A4/D58)")
    (add_net "FAN1(D11)")
    (add_net "FAN2(D6)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J5-Pad5)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(J6-Pad5)")
    (add_net "Net-(P1-Pad11)")
    (add_net "Net-(P1-Pad13)")
    (add_net "Net-(P1-Pad15)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P1-Pad9)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q1-Pad4)")
    (add_net "Net-(Stepstick1-Pad5)")
    (add_net "Net-(Stepstick2-Pad5)")
    (add_net "Net-(Stepstick3-Pad5)")
    (add_net "STEP_1(A10/D64)")
    (add_net "STEP_2(D48)")
    (add_net "STEP_3(A3/D57)")
    (add_net "Z_PROBE(A11/D65)")
  )
  (net_class FAN ""
    (clearance 0.127)
    (trace_width 0.381)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(FAN1-Pad2)")
    (add_net "Net-(FAN2-Pad2)")
  )
  (net_class Motor ""
    (clearance 0.2)
    (trace_width 0.762)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(J7-Pad2)")
    (add_net "Net-(J7-Pad3)")
    (add_net "Net-(J7-Pad4)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(J8-Pad2)")
    (add_net "Net-(J8-Pad3)")
    (add_net "Net-(J8-Pad4)")
    (add_net "Net-(J9-Pad1)")
    (add_net "Net-(J9-Pad2)")
    (add_net "Net-(J9-Pad3)")
    (add_net "Net-(J9-Pad4)")
    (add_net VMOT)
  )
  (net_class Power ""
    (clearance 0.2032)
    (trace_width 0.254)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net VCC)
  )
  (module VORON_V2.0:PIN_HEADER_TOP_1X3 (layer F.Cu) (tedit 5A493C64)
    (at 172.6848 125.1466 270)
    (fp_text reference P3 (at 0 3.81 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.81 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VMOT))
    (pad 2 thru_hole circle (at 0 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(D3-Pad1)"))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/PIN_HEADER_TOP_1X3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:Steppers (layer F.Cu) (tedit 5A4937F3)
    (at 188.89 106.63 90)
    (fp_text reference Stepstick1 (at 0 -12.7 90) (layer Eco1.User) hide)
    (fp_text value Stepstick (at 0 11.43 270) (layer Eco1.User))
    (pad 1 thru_hole circle (at -6.35 -8.89 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 "EN_1(D44)"))
    (pad 2 thru_hole circle (at -6.35 -6.35 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(J4-Pad1)"))
    (pad 3 thru_hole circle (at -6.35 -3.81 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(J4-Pad3)"))
    (pad 4 thru_hole circle (at -6.35 -1.27 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(J4-Pad5)"))
    (pad 5 thru_hole circle (at -6.35 1.27 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(Stepstick1-Pad5)"))
    (pad 6 thru_hole circle (at -6.35 3.81 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(Stepstick1-Pad5)"))
    (pad 7 thru_hole circle (at -6.35 6.35 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 "STEP_1(A10/D64)"))
    (pad 8 thru_hole circle (at -6.35 8.89 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 "DIR_1(A5/D59)"))
    (pad 9 thru_hole circle (at 6.35 8.89 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 10 thru_hole circle (at 6.35 6.35 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 11 thru_hole circle (at 6.35 3.81 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J7-Pad4)"))
    (pad 12 thru_hole circle (at 6.35 1.27 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J7-Pad3)"))
    (pad 13 thru_hole circle (at 6.35 -1.27 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J7-Pad2)"))
    (pad 14 thru_hole circle (at 6.35 -3.81 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J7-Pad1)"))
    (pad 15 thru_hole circle (at 6.35 -6.35 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 16 thru_hole circle (at 6.35 -8.89 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VMOT))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/Steppers.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:Steppers (layer F.Cu) (tedit 5A4937EF)
    (at 168.57 106.63 90)
    (fp_text reference Stepstick2 (at 0 -12.7 90) (layer Eco1.User) hide)
    (fp_text value Stepstick (at 0 11.43 270) (layer Eco1.User))
    (pad 1 thru_hole circle (at -6.35 -8.89 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 "EN_2(D42)"))
    (pad 2 thru_hole circle (at -6.35 -6.35 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(J5-Pad1)"))
    (pad 3 thru_hole circle (at -6.35 -3.81 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(J5-Pad3)"))
    (pad 4 thru_hole circle (at -6.35 -1.27 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(J5-Pad5)"))
    (pad 5 thru_hole circle (at -6.35 1.27 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(Stepstick2-Pad5)"))
    (pad 6 thru_hole circle (at -6.35 3.81 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(Stepstick2-Pad5)"))
    (pad 7 thru_hole circle (at -6.35 6.35 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 "STEP_2(D48)"))
    (pad 8 thru_hole circle (at -6.35 8.89 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 "DIR_2(A9/D63)"))
    (pad 9 thru_hole circle (at 6.35 8.89 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 10 thru_hole circle (at 6.35 6.35 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 11 thru_hole circle (at 6.35 3.81 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J8-Pad4)"))
    (pad 12 thru_hole circle (at 6.35 1.27 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J8-Pad3)"))
    (pad 13 thru_hole circle (at 6.35 -1.27 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J8-Pad2)"))
    (pad 14 thru_hole circle (at 6.35 -3.81 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J8-Pad1)"))
    (pad 15 thru_hole circle (at 6.35 -6.35 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 16 thru_hole circle (at 6.35 -8.89 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VMOT))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/Steppers.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:LED_0805 (layer F.Cu) (tedit 5A493BF1)
    (at 200.45 126.15 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at -0.2 -1.45 450) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 270) (layer F.Fab) hide)
    (fp_text user %R (at 2.384 0.012 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module VORON_V2.0:LED_0805 (layer F.Cu) (tedit 5A493BF6)
    (at 205.3 126.15 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at -0.2 1.35 450) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 270) (layer F.Fab) hide)
    (fp_text user %R (at 2.0792 0.0252 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module VORON_V2.0:2X03_PIN_HEADER (layer F.Cu) (tedit 59B56E3A)
    (at 191.4 105)
    (descr "<b>PIN HEADER</b>")
    (fp_text reference J4 (at 2.4892 -3.3528) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0 3.175) (layer Eco1.User) hide)
    (pad 1 thru_hole oval (at -2.54 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 "Net-(J4-Pad1)"))
    (pad 2 thru_hole oval (at -2.54 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 3 thru_hole oval (at 0 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "Net-(J4-Pad3)"))
    (pad 4 thru_hole oval (at 0 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 5 thru_hole oval (at 2.54 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "Net-(J4-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/PIN_HEADER_TOP_2X3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:2X03_PIN_HEADER locked (layer F.Cu) (tedit 59B56FBE)
    (at 171.05 105)
    (descr "<b>PIN HEADER</b>")
    (fp_text reference J5 (at 2.4892 -3.3528) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0 3.175) (layer Eco1.User) hide)
    (pad 1 thru_hole oval (at -2.54 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "Net-(J5-Pad1)"))
    (pad 2 thru_hole oval (at -2.54 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 3 thru_hole oval (at 0 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 "Net-(J5-Pad3)"))
    (pad 4 thru_hole oval (at 0 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 5 thru_hole oval (at 2.54 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 "Net-(J5-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/PIN_HEADER_TOP_2X3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:2X03_PIN_HEADER (layer F.Cu) (tedit 59B5700D)
    (at 150.65 105)
    (descr "<b>PIN HEADER</b>")
    (fp_text reference J6 (at 2.5728 -3.4232) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0 3.175) (layer Eco1.User) hide)
    (pad 1 thru_hole oval (at -2.54 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 "Net-(J6-Pad1)"))
    (pad 2 thru_hole oval (at -2.54 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 3 thru_hole oval (at 0 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 "Net-(J6-Pad3)"))
    (pad 4 thru_hole oval (at 0 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 5 thru_hole oval (at 2.54 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 "Net-(J6-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/PIN_HEADER_TOP_2X3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:1X04_PIN_HEADER (layer F.Cu) (tedit 59B56E48)
    (at 185.08 96.851)
    (fp_text reference J7 (at -2.5084 0.0776) (layer F.SilkS))
    (fp_text value "Stepper 1" (at 0 1.9) (layer Eco1.User))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(J7-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(J7-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(J7-Pad3)"))
    (pad 4 thru_hole oval (at 7.62 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(J7-Pad4)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/PIN_HEADER_TOP_1X4.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:1X04_PIN_HEADER (layer F.Cu) (tedit 59B56E4B)
    (at 164.76 96.851)
    (fp_text reference J8 (at -2.4852 0.0268) (layer F.SilkS))
    (fp_text value "Stepper 2" (at 0 1.9) (layer Eco1.User))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(J8-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "Net-(J8-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "Net-(J8-Pad3)"))
    (pad 4 thru_hole oval (at 7.62 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(J8-Pad4)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/PIN_HEADER_TOP_1X4.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:1X04_PIN_HEADER (layer F.Cu) (tedit 59B56E71)
    (at 144.44 96.851)
    (fp_text reference J9 (at -2.5636 0.0268) (layer F.SilkS))
    (fp_text value "Stepper 3" (at 0 1.9) (layer Eco1.User))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "Net-(J9-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "Net-(J9-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(J9-Pad3)"))
    (pad 4 thru_hole oval (at 7.62 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "Net-(J9-Pad4)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/PIN_HEADER_TOP_1X4.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:R_0603 (layer F.Cu) (tedit 59CED595)
    (at 190.95 126.15 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 1.984 -0.411 360) (layer F.SilkS))
    (fp_text value 100 (at 0 1.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(Q1-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "FAN1(D11)") (clearance 0.2032))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:R_0603 (layer F.Cu) (tedit 59CED593)
    (at 189.2 126.15 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 1.984 0.1885 360) (layer F.SilkS))
    (fp_text value 100k (at 0 1.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "FAN1(D11)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:R_0603 (layer F.Cu) (tedit 59CED5A0)
    (at 190.95 123.15 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -2.3185 -0.03 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(Q1-Pad4)") (clearance 0.127))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "FAN2(D6)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:R_0603 (layer F.Cu) (tedit 59CED5AD)
    (at 189.2 123.15 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -2.3185 -0.0655 270) (layer F.SilkS))
    (fp_text value 100k (at 0 1.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "FAN2(D6)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:R_0603 (layer F.Cu) (tedit 5A493C00)
    (at 198.45 125.4 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 2.05 -0.05 270) (layer F.SilkS))
    (fp_text value 1.80k (at 0 1.5 270) (layer F.Fab) hide)
    (fp_text user %R (at -0.0036 -0.0168 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(FAN1-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:R_0603 (layer F.Cu) (tedit 5A493C17)
    (at 207.3 125.4 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 2.05 0 270) (layer F.SilkS))
    (fp_text value 1.80k (at 0 1.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(FAN2-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:R_0603 (layer F.Cu) (tedit 5A3AC56D)
    (at 181.9 110.45)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 2.3904 0.1044) (layer F.SilkS))
    (fp_text value 100k (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J4-Pad1)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:R_0603 (layer F.Cu) (tedit 59B8618A)
    (at 161.4 110.45)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 2.54 0.1552) (layer F.SilkS))
    (fp_text value 100k (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J5-Pad1)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:R_0603 (layer F.Cu) (tedit 59B86185)
    (at 141.15 110.45)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 2.4892 0.1552) (layer F.SilkS))
    (fp_text value 100k (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J6-Pad1)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:R_0603 (layer F.Cu) (tedit 5A4945BE)
    (at 178.9 115.45)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0 1.5) (layer F.SilkS))
    (fp_text value 10.0k (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "EN_1(D44)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:R_0603 (layer F.Cu) (tedit 5A4945B3)
    (at 158.65 115.45)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 0.05 1.45) (layer F.SilkS))
    (fp_text value 10.0k (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 "EN_2(D42)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:R_0603 (layer F.Cu) (tedit 5A4945AA)
    (at 138.4 115.45)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 0 1.45) (layer F.SilkS))
    (fp_text value 10.0k (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "EN_3(A4/D58)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 5A494026)
    (at 194.95 123.9 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference Q1 (at 4.7195 0.221 360) (layer F.SilkS))
    (fp_text value IRF8313PBF (at 0 3.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 1 -1 90) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (clearance 0.2032))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(Q1-Pad2)"))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(Q1-Pad4)"))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(FAN2-Pad2)"))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(FAN2-Pad2)"))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(FAN1-Pad2)"))
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(FAN1-Pad2)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/SOIC_8_3_9x4_9mm_Pitch1_27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:Steppers locked (layer F.Cu) (tedit 5A4937EA)
    (at 148.25 106.63 90)
    (fp_text reference Stepstick3 (at 0 -12.7 90) (layer Eco1.User) hide)
    (fp_text value Stepstick (at 0 11.43 270) (layer Eco1.User))
    (pad 1 thru_hole circle (at -6.35 -8.89 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 "EN_3(A4/D58)"))
    (pad 2 thru_hole circle (at -6.35 -6.35 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(J6-Pad1)"))
    (pad 3 thru_hole circle (at -6.35 -3.81 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(J6-Pad3)"))
    (pad 4 thru_hole circle (at -6.35 -1.27 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(J6-Pad5)"))
    (pad 5 thru_hole circle (at -6.35 1.27 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(Stepstick3-Pad5)"))
    (pad 6 thru_hole circle (at -6.35 3.81 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(Stepstick3-Pad5)"))
    (pad 7 thru_hole circle (at -6.35 6.35 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 "STEP_3(A3/D57)"))
    (pad 8 thru_hole circle (at -6.35 8.89 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 "DIR_3(A12/D66)"))
    (pad 9 thru_hole circle (at 6.35 8.89 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 10 thru_hole circle (at 6.35 6.35 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 11 thru_hole circle (at 6.35 3.81 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J9-Pad4)"))
    (pad 12 thru_hole circle (at 6.35 1.27 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(J9-Pad3)"))
    (pad 13 thru_hole circle (at 6.35 -1.27 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(J9-Pad2)"))
    (pad 14 thru_hole circle (at 6.35 -3.81 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(J9-Pad1)"))
    (pad 15 thru_hole circle (at 6.35 -6.35 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 16 thru_hole circle (at 6.35 -8.89 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VMOT))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/Steppers.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:c_elec_6.3x7.7 (layer F.Cu) (tedit 0)
    (at 181.65 105.2 180)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (fp_text reference C1 (at 0 -3.937 180) (layer F.SilkS))
    (fp_text value 100uF (at 0 3.81 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.75082 0 180) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 1 VMOT))
    (pad 2 smd rect (at -2.75082 0 180) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/c_elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:c_elec_6.3x7.7 (layer F.Cu) (tedit 0)
    (at 161.4 105.2 180)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (fp_text reference C2 (at 0 -3.937 180) (layer F.SilkS))
    (fp_text value 100uF (at 0 3.81 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.75082 0 180) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 1 VMOT))
    (pad 2 smd rect (at -2.75082 0 180) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/c_elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:c_elec_6.3x7.7 (layer F.Cu) (tedit 0)
    (at 141.15 105.2 180)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (fp_text reference C3 (at 0 -3.937 180) (layer F.SilkS))
    (fp_text value 100uF (at 0 3.81 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.75082 0 180) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 1 VMOT))
    (pad 2 smd rect (at -2.75082 0 180) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/c_elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:mkds_1,5-2 (layer F.Cu) (tedit 5A4943B5)
    (at 206.8 109 90)
    (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference PWRIN1 (at 0 -6.6 90) (layer F.SilkS) hide)
    (fp_text value PWRIN (at 0 5.9 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.5 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 VMOT))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/mkds_1,5-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:PIN_HEADER_TOP_2X12 (layer F.Cu) (tedit 5A493C6C)
    (at 150.917 126.442)
    (fp_text reference P1 (at -0.017 -3.292) (layer F.SilkS) hide)
    (fp_text value CONN_02X12 (at 0 -3.81) (layer F.Fab))
    (pad 2 thru_hole circle (at -13.97 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 1 thru_hole circle (at -13.97 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 3 thru_hole circle (at -11.43 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole circle (at -11.43 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(P1-Pad4)"))
    (pad 5 thru_hole circle (at -8.89 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole circle (at -8.89 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 40 "EN_3(A4/D58)"))
    (pad 7 thru_hole circle (at -6.35 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(P1-Pad7)"))
    (pad 8 thru_hole circle (at -6.35 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 45 "STEP_3(A3/D57)"))
    (pad 9 thru_hole circle (at -3.81 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(P1-Pad9)"))
    (pad 10 thru_hole circle (at -3.81 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 46 "DIR_3(A12/D66)"))
    (pad 11 thru_hole circle (at -1.27 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(P1-Pad11)"))
    (pad 12 thru_hole circle (at -1.27 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 39 "EN_2(D42)"))
    (pad 13 thru_hole circle (at 1.27 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(P1-Pad13)"))
    (pad 14 thru_hole circle (at 1.27 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 43 "STEP_2(D48)"))
    (pad 15 thru_hole circle (at 3.81 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(P1-Pad15)"))
    (pad 16 thru_hole circle (at 3.81 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 44 "DIR_2(A9/D63)"))
    (pad 17 thru_hole circle (at 6.35 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 9 D4))
    (pad 18 thru_hole circle (at 6.35 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 38 "EN_1(D44)"))
    (pad 19 thru_hole circle (at 8.89 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 8 D5))
    (pad 20 thru_hole circle (at 8.89 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 41 "STEP_1(A10/D64)"))
    (pad 21 thru_hole circle (at 11.43 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 37 "FAN2(D6)"))
    (pad 22 thru_hole circle (at 11.43 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 42 "DIR_1(A5/D59)"))
    (pad 23 thru_hole circle (at 13.97 1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 36 "FAN1(D11)"))
    (pad 24 thru_hole circle (at 13.97 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Z_PROBE(A11/D65)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/PIN_HEADER_TOP_2X12.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_4mm (layer F.Cu) (tedit 5A49422D)
    (at 134.65 98.45)
    (descr "Mounting Hole 4mm, no annular")
    (tags "mounting hole 4mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -5) (layer F.SilkS) hide)
    (fp_text value MountingHole_4mm (at 0 5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers *.Cu *.Mask)
      (clearance 1.5))
  )
  (module Mounting_Holes:MountingHole_4mm (layer F.Cu) (tedit 5A494244)
    (at 206.4 98.45)
    (descr "Mounting Hole 4mm, no annular")
    (tags "mounting hole 4mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -5) (layer F.SilkS) hide)
    (fp_text value MountingHole_4mm (at 0 5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers *.Cu *.Mask)
      (clearance 1.5))
  )
  (module VORON_V2.0:R_0603 (layer F.Cu) (tedit 59B295B8)
    (at 165.11306 122.37038)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 10.0k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 53 "Z_PROBE(A11/D65)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:PIN_HEADER_TOP_1X2 (layer F.Cu) (tedit 5A493BE8)
    (at 199.85 121.95 270)
    (fp_text reference FAN1 (at 0 2.54 270) (layer F.SilkS) hide)
    (fp_text value FAN1 (at 0 -2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VMOT))
    (pad 2 thru_hole circle (at 0 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(FAN1-Pad2)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/PIN_HEADER_TOP_1X2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:PIN_HEADER_TOP_1X2 (layer F.Cu) (tedit 5A493BD7)
    (at 205.55 121.95 270)
    (fp_text reference FAN2 (at 0 2.54 270) (layer F.SilkS) hide)
    (fp_text value FAN2 (at 0 -2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VMOT))
    (pad 2 thru_hole circle (at 0 0 270) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(FAN2-Pad2)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/PIN_HEADER_TOP_1X2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:PIN_HEADER_TOP_1X4 (layer F.Cu) (tedit 5A493C50)
    (at 182.0066 122.632)
    (fp_text reference P2 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 0 -2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at -3.81 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 D4))
    (pad 2 thru_hole circle (at -1.27 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 D5))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 "FAN2(D6)"))
    (pad 4 thru_hole circle (at 3.81 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 "FAN1(D11)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/PIN_HEADER_TOP_1X4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:SMA_Diode (layer F.Cu) (tedit 5A493C26)
    (at 169.078 125.1212 90)
    (fp_text reference D3 (at -0.0788 -2.178 90) (layer F.SilkS))
    (fp_text value D_Small (at 0 -3.81 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 53 "Z_PROBE(A11/D65)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/SMA_Diode.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:PIN_HEADER_TOP_2x4 (layer F.Cu) (tedit 5A493C55)
    (at 182.0066 126.45)
    (fp_text reference P4 (at 1.27 3.81) (layer F.SilkS) hide)
    (fp_text value CONN_02X04 (at 0 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at -3.81 1.27) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 2 thru_hole circle (at -3.81 -1.27) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole circle (at -1.27 1.27) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 4 thru_hole circle (at -1.27 -1.27) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole circle (at 1.27 1.27) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 6 thru_hole circle (at 1.27 -1.27) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 7 thru_hole circle (at 3.81 1.27) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 8 thru_hole circle (at 3.81 -1.27) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/VORON_V2.0_Expander_option2/VORON_V2.0.pretty/3D_Models/PIN_HEADER_TOP_2x4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VORON_V2.0:LOGO (layer F.Cu) (tedit 0)
    (at 146.25 120.15)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text SERVOS (at 182.15 120.3) (layer F.SilkS))
  (gr_text "Z PROBE\n" (at 172.5 120.2) (layer F.SilkS))
  (gr_text "-  S  +" (at 174.75 125.15 90) (layer F.SilkS))
  (gr_text "FAN2\n\n" (at 209.35 120.75 90) (layer F.SilkS))
  (gr_text "FAN1\n" (at 202.45 120.7 90) (layer F.SilkS))
  (gr_text BOT (at 154.85 120.25) (layer F.SilkS))
  (gr_text MZ (at 150.3 120.25) (layer F.SilkS))
  (gr_line (start 207.85 129.25) (end 194.55 129.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 210.55 126.55) (end 210.55 120.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 207.85 126.55) (end 210.55 126.55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 210.55 98.75) (end 210.55 120.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.55 98.25) (end 130.55 127.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 207.05 94.25) (end 134.55 94.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 206.55 98.25) (end 207.05 94.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 134.55 98.25) (end 130.55 98.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 194.55 129.25) (end 132.55 129.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 132.55 127.25) (end 132.55 129.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text + (at 203.05 106.5 90) (layer F.SilkS))
  (gr_text + (at 200.05 106.5 90) (layer F.SilkS))
  (gr_text "_\n" (at 199.35 111.75 90) (layer F.SilkS))
  (gr_text "Rev 2.0\n\n" (at 136.6 111.05 90) (layer F.SilkS))
  (gr_text "VORON 2\nEXPANDER" (at 133.2 111.1 90) (layer F.SilkS))
  (gr_text + (at 202.94 106.39 90) (layer B.SilkS))
  (gr_text _ (at 202.178 111.724 90) (layer B.SilkS))
  (gr_text _ (at 202.3 111.75 90) (layer F.SilkS))
  (gr_text MS3 (at 194.558 108.93 270) (layer F.SilkS))
  (gr_text MS2 (at 192.018 108.93 270) (layer F.SilkS))
  (gr_text MS1 (at 189.478 108.93 270) (layer F.SilkS))
  (gr_text MS3 (at 173.476 108.93 270) (layer F.SilkS))
  (gr_text MS2 (at 170.936 108.93 270) (layer F.SilkS))
  (gr_text MS1 (at 168.396 108.93 270) (layer F.SilkS))
  (gr_text MS3 (at 152.394 108.93 270) (layer F.SilkS))
  (gr_text MS2 (at 149.854 108.93 270) (layer F.SilkS))
  (gr_text MS1 (at 147.314 108.93 270) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.762))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 211.65 129.95) (xy 129.65 129.95) (xy 129.65 93.95) (xy 211.65 93.95) (xy 211.65 129.95)
      )
    )
  )
  (zone (net 3) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.762))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 210.65 129.95) (xy 129.65 129.95) (xy 129.65 93.95) (xy 211.65 93.95) (xy 210.65 129.95)
      )
    )
  )
)
