(kicad_pcb (version 20171130) (host pcbnew 5.1.5-52549c5~86~ubuntu19.10.1)
  (general
    (thickness 1.6)
    (drawings 26)
    (tracks 168)
    (zones 0)
    (modules 20)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.3048)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 GND)
  (net 3 "Net-(J1-Pad1)")
  (net 4 VSS)
  (net 5 "Net-(D1-Pad3)")
  (net 6 "Net-(C5-Pad2)")
  (net 7 "Net-(J4-Pad2)")
  (net 8 /Guard)
  (net 9 "Net-(U1-Pad1)")
  (net 10 "Net-(U1-Pad8)")
  (net 11 "Net-(J3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /Guard)
    (add_net GND)
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad8)")
    (add_net VDD)
    (add_net VSS)
  )
  (module op-amp-test:SOT-23_Handsoldering (layer B.Cu) (tedit 5E889FCF)
    (at 145.93 115.79 180)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D1 (at -0.0762 -2.794) (layer B.SilkS))
    (fp_text value D_Schottky (at 0 -2.5) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 3 smd rect (at 1.5 0 180) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D1-Pad3)"))
    (pad 2 smd rect (at -1.5 -0.95 180) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 1 smd rect (at -1.5 0.95 180) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
  )
  (module op-amp-test:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5E888671)
    (at 131.0132 115.7986)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 1.5 -2.5) (layer F.SilkS) hide)
    (fp_text value SHORT (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module op-amp-test:R_0805_HandSoldering (layer F.Cu) (tedit 5E888653)
    (at 139.7 115.7986 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -2.54 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad3)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module op-amp-test:R_0805_HandSoldering (layer F.Cu) (tedit 5E88863B)
    (at 135.2804 117.1448 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -3.5 0) (layer F.SilkS))
    (fp_text value 10M (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module op-amp-test:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 156.1719 111.3155 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0.1651 1.6891 90) (layer F.SilkS))
    (fp_text value 10M (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /Guard))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module op-amp-test:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 156.1846 118.5672 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value OPEN (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J4-Pad2)"))
  )
  (module op-amp-test:SA404_plug (layer F.Cu) (tedit 5E0CBC0B)
    (at 136.16 105.45)
    (fp_text reference U2 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA_Binding_Posts (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.5) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad3)"))
  )
  (module op-amp-test:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 135.2804 122.7328)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J3 (at 1.25 -4) (layer F.SilkS) hide)
    (fp_text value OPEN (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module op-amp-test:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 147.05 108.275 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 3.51 -0.075) (layer F.SilkS))
    (fp_text value 1K (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /Guard))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 147.15 105.475 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference C5 (at 3.04 -0.125) (layer F.SilkS))
    (fp_text value 1u (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 "Net-(C5-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 /Guard))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 144.5768 120.8 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference C4 (at -2.5678 0 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 152.4 116.8 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference C3 (at -2.85 -0.125 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 VDD))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 147.525 120.8 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0.2056 -2.1064 180) (layer F.SilkS))
    (fp_text value 1u (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 152.4 112.4 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference C1 (at 2.525 -0.2 180) (layer F.SilkS))
    (fp_text value 1u (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 VDD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module op-amp-test:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 144.272 125.7 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at -2.25 -2.725 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x03_Male (at 0 7.41 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 VSS))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module op-amp-test:SA404_plug (layer F.Cu) (tedit 5E0CBC0B)
    (at 155.21 124.65 270)
    (fp_text reference U5 (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value VIA_Binding_Posts (at 0 -3.81 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 5 5) (drill 3.5) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module op-amp-test:SA404_plug (layer F.Cu) (tedit 5E0CBC0B)
    (at 155.21 105.45 270)
    (fp_text reference U4 (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value VIA_Binding_Posts (at 0 -3.81 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 5 5) (drill 3.5) (layers *.Cu *.Mask)
      (net 8 /Guard))
  )
  (module op-amp-test:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA)
    (at 147.275 115.15)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at -3.13 -3.505) (layer F.SilkS))
    (fp_text value op-amp (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U1-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad2)"))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad3)"))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /Guard))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U1-Pad8)"))
  )
  (module op-amp-test:SOT-23_Handsoldering (layer F.Cu) (tedit 5A0AB76C)
    (at 140.081 120.7516 180)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 1.9812 -3.048) (layer F.SilkS) hide)
    (fp_text value 2N4117A (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95 180) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad3)"))
    (pad 2 smd rect (at -1.5 0.95 180) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad3)"))
    (pad 3 smd rect (at 1.5 0 180) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module op-amp-test:SOT-23_Handsoldering (layer F.Cu) (tedit 5A0AB76C)
    (at 140.075 110.7)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0.25 -2.975) (layer F.SilkS) hide)
    (fp_text value 2N4117A (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 -270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -1.5 0.95) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 3 smd rect (at 1.5 0) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GND (at 130.67 121.02) (layer F.SilkS))
  (gr_text "on/off RLoad " (at 153.9748 114.173 90) (layer F.SilkS))
  (gr_text "Pin 3" (at 131.4196 103.1494) (layer F.SilkS))
  (gr_text OVP (at 140.4112 107.9627) (layer F.SilkS))
  (gr_text Vin (at 131.0513 113.1062) (layer F.SilkS))
  (gr_text V- (at 141.7066 125.6792) (layer F.SilkS))
  (gr_text OVP (at 139.8016 124.1044) (layer F.SilkS))
  (gr_text OVP (at 146.1516 113.0046) (layer B.SilkS))
  (gr_text RIb (at 135.2169 113.1062) (layer F.SilkS))
  (gr_text "R OVP" (at 139.7 113.1062) (layer F.SilkS))
  (gr_text V+ (at 147.2184 123.3932) (layer F.SilkS))
  (gr_text "on/off Rin" (at 133.34 126.89 90) (layer F.SilkS))
  (gr_text GND (at 156.1084 121.5644) (layer F.SilkS))
  (gr_text GND (at 150.368 123.19) (layer F.SilkS))
  (gr_text Vout (at 151.257 103.0478) (layer F.SilkS))
  (gr_text "Opamp \nTests: \nIb,Noise,OVP, \nVos,Linearity" (at 129.4638 109.1438) (layer F.SilkS))
  (gr_line (start 129 102) (end 158.55 102) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 129 128) (end 129 102) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 158.55 128) (end 129 128) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 158.55 102) (end 158.55 128) (layer Edge.Cuts) (width 0.05))
  (zone (net 8) (net_name /Guard) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2286))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.22 114.9) (xy 146.224625 116.63) (xy 145.405 116.63) (xy 145.415 117.4) (xy 137.709275 117.3988)
        (xy 129.19075 117.3988) (xy 129.16535 114.1603) (xy 137.690225 114.1603) (xy 145.381148 114.16015) (xy 145.378853 114.89985)
      )
    )
  )
  (zone (net 8) (net_name /Guard) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.2659 114.1603) (xy 129.1717 114.1603) (xy 129.1463 117.3988) (xy 146.2405 117.3988)
      )
    )
  )
  (zone (net 8) (net_name /Guard) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.9606 114.3254) (xy 143.5608 114.3254) (xy 143.5481 112.8776) (xy 141.9479 112.8776)
      )
    )
  )
  (zone (net 8) (net_name /Guard) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.5608 117.2845) (xy 141.9606 117.2845) (xy 141.9733 118.7323) (xy 143.5735 118.7323)
      )
    )
  )
)
