(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "USLetter")
  (title_block
    (date "2024-01-30")
    (rev "B")
  )
  (layers
    (0 "F.Cu" signal "Top")
    (1 "In1.Cu" signal)
    (2 "In2.Cu" signal)
    (31 "B.Cu" signal "Bottom")
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 0.48) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 2" (type "prepreg") (thickness 0.48) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 3" (type "core") (thickness 0.48) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 106.35 103.5)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "VDD")
  (net 3 "/LED1B")
  (net 4 "Net-(D1-BA)")
  (net 5 "/LED1R")
  (net 6 "/PWM_G")
  (net 7 "/LED2B")
  (net 8 "Net-(D1-GA)")
  (net 9 "/LED2R")
  (net 10 "/LED3B")
  (net 11 "Net-(D1-RA)")
  (net 12 "/LED3R")
  (net 13 "/SCL")
  (net 14 "/SDA")
  (net 15 "/UPDI")
  (net 16 "/Int2")
  (net 17 "/Int1")
  (net 18 "/LSens")
  (net 19 "/LS_Pwr")
  (net 20 "/LED1G")
  (net 21 "/LED2G")
  (net 22 "/LED3G")
  (net 23 "/PWM_B")
  (net 24 "/PWM_R")
  (net 25 "/TxD")
  (net 26 "Net-(D2-BA)")
  (net 27 "/RxD")
  (net 28 "Net-(D2-GA)")
  (net 29 "Net-(D2-RA)")
  (net 30 "Net-(D3-BA)")
  (net 31 "Net-(D3-GA)")
  (net 32 "Net-(D3-RA)")
  (net 33 "unconnected-(U1-PB2-Pad14)")
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 114.125 103.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Digital HUD display.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C1" (at -0.88 0.94) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ADP_CustomFootprints:LED_RGB_PLCC-6" (layer "F.Cu")
    (at 110.6 103.5 -90)
    (descr "RGB LED PLCC-6")
    (tags "RGB LED PLCC-6")
    (property "Sheetfile" "Digital HUD display.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB symbol with red & blue reversed, e.g. Cree CLX6F-FKC")
    (attr smd)
    (fp_text reference "D1" (at 0.05 -1 180) (layer "F.SilkS"))
    (fp_text value "LED_RGB_reversed" (at 0 2.8 -90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 -1) (size 0.65 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/PWM_B") (pinfunction "RK") (pintype "passive"))
    (pad "2" smd rect (at -1.5 0) (size 0.65 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/PWM_G") (pinfunction "GK") (pintype "passive"))
    (pad "3" smd rect (at -1.5 1) (size 0.65 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "/PWM_R") (pinfunction "BK") (pintype "passive"))
    (pad "4" smd rect (at 1.5 1) (size 0.65 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(D1-BA)") (pinfunction "BA") (pintype "passive"))
    (pad "5" smd rect (at 1.5 0) (size 0.65 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(D1-GA)") (pinfunction "GA") (pintype "passive"))
    (pad "6" smd rect (at 1.5 -1) (size 0.65 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(D1-RA)") (pinfunction "RA") (pintype "passive"))
    (model "${KISYS3DMOD}/ADP_Custom.3dshapes/PLCC6_LED_3_5X3_4X2_8_CRW.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.5mm" (layer "F.Cu")
    (at 114.4 101.4)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "Digital HUD display.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "J1" (at 0 -1.648) (layer "F.SilkS") hide)
    (fp_text value "4" (at -1.25 -0.76) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
      (net 2 "VDD") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_D1.5mm" (layer "F.Cu")
    (at 114.4 105.6)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "Digital HUD display.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "J3" (at 0 -1.648) (layer "F.SilkS") hide)
    (fp_text value "1" (at -1.19 0.87) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 99.29 100.65 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Digital HUD display.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R11" (at -1.61 0.15 180) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/LSens") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ADP_CustomFootprints:LED_RGB_PLCC-6" (layer "F.Cu")
    (at 102.6 103.5 -90)
    (descr "RGB LED PLCC-6")
    (tags "RGB LED PLCC-6")
    (property "Sheetfile" "Digital HUD display.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB symbol with red & blue reversed, e.g. Cree CLX6F-FKC")
    (attr smd)
    (fp_text reference "D3" (at 0.05 -1.1 -180) (layer "F.SilkS"))
    (fp_text value "LED_RGB_reversed" (at 0 2.8 -90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 -1) (size 0.65 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/PWM_B") (pinfunction "RK") (pintype "passive"))
    (pad "2" smd rect (at -1.5 0) (size 0.65 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/PWM_G") (pinfunction "GK") (pintype "passive"))
    (pad "3" smd rect (at -1.5 1) (size 0.65 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "/PWM_R") (pinfunction "BK") (pintype "passive"))
    (pad "4" smd rect (at 1.5 1) (size 0.65 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "Net-(D3-BA)") (pinfunction "BA") (pintype "passive"))
    (pad "5" smd rect (at 1.5 0) (size 0.65 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "Net-(D3-GA)") (pinfunction "GA") (pintype "passive"))
    (pad "6" smd rect (at 1.5 -1) (size 0.65 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "Net-(D3-RA)") (pinfunction "RA") (pintype "passive"))
    (model "${KISYS3DMOD}/ADP_Custom.3dshapes/PLCC6_LED_3_5X3_4X2_8_CRW.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ADP_CustomFootprints:LED_RGB_PLCC-6" (layer "F.Cu")
    (at 106.6 103.5 -90)
    (descr "RGB LED PLCC-6")
    (tags "RGB LED PLCC-6")
    (property "Sheetfile" "Digital HUD display.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB symbol with red & blue reversed, e.g. Cree CLX6F-FKC")
    (attr smd)
    (fp_text reference "D2" (at 0.05 -1.05 180) (layer "F.SilkS"))
    (fp_text value "LED_RGB_reversed" (at 0 2.8 -90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 -1) (size 0.65 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/PWM_B") (pinfunction "RK") (pintype "passive"))
    (pad "2" smd rect (at -1.5 0) (size 0.65 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/PWM_G") (pinfunction "GK") (pintype "passive"))
    (pad "3" smd rect (at -1.5 1) (size 0.65 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "/PWM_R") (pinfunction "BK") (pintype "passive"))
    (pad "4" smd rect (at 1.5 1) (size 0.65 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(D2-BA)") (pinfunction "BA") (pintype "passive"))
    (pad "5" smd rect (at 1.5 0) (size 0.65 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "Net-(D2-GA)") (pinfunction "GA") (pintype "passive"))
    (pad "6" smd rect (at 1.5 -1) (size 0.65 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "Net-(D2-RA)") (pinfunction "RA") (pintype "passive"))
    (model "${KISYS3DMOD}/ADP_Custom.3dshapes/PLCC6_LED_3_5X3_4X2_8_CRW.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_0805_2012Metric" (layer "F.Cu")
    (at 99.3 103.4 90)
    (descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "Digital HUD display.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at 0 0 180) (layer "F.SilkS"))
    (fp_text value "SFH3716-Optoelectronics" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/LS_Pwr") (pinfunction "C") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/LSens") (pinfunction "E") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_LGA:LGA-12_2x2mm_P0.5mm" (layer "F.Cu")
    (at 96.4 103.4875 -90)
    (descr "LGA12")
    (tags "lga land grid array")
    (property "Sheetfile" "Digital HUD display.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "3-Axis Accelerometer, 2/4/8g range, I2C/SPI interface")
    (property "ki_keywords" "3-axis accelerometer spi mems")
    (clearance 0.15)
    (attr smd)
    (fp_text reference "U2" (at 1.7125 0.05) (layer "F.SilkS"))
    (fp_text value "LIS2HH12" (at 0 1.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.7625 -0.75 270) (size 0.375 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/SCL") (pinfunction "SCL/SPC") (pintype "input"))
    (pad "2" smd rect (at -0.7625 -0.25 270) (size 0.375 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VDD") (pinfunction "~{CS}") (pintype "input"))
    (pad "3" smd rect (at -0.7625 0.25 270) (size 0.375 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VDD") (pinfunction "SA0/SDO") (pintype "bidirectional"))
    (pad "4" smd rect (at -0.7625 0.75 270) (size 0.375 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/SDA") (pinfunction "SDA/SDI") (pintype "bidirectional"))
    (pad "5" smd rect (at -0.25 0.7625) (size 0.375 0.35) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "6" smd rect (at 0.25 0.7625) (size 0.375 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "7" smd rect (at 0.7625 0.75 270) (size 0.375 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "8" smd rect (at 0.7625 0.25 270) (size 0.375 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "9" smd rect (at 0.7625 -0.25 270) (size 0.375 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VDD") (pinfunction "Vdd") (pintype "power_in"))
    (pad "10" smd rect (at 0.7625 -0.75 270) (size 0.375 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VDD") (pinfunction "Vdd_IO") (pintype "power_in"))
    (pad "11" smd rect (at 0.25 -0.7625) (size 0.375 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/Int2") (pinfunction "INT2") (pintype "output"))
    (pad "12" smd rect (at -0.25 -0.7625) (size 0.375 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/Int1") (pinfunction "INT1") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_LGA.3dshapes/LGA-12_2x2mm_P0.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.5mm" (layer "B.Cu")
    (at 113.8 105.9)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "Digital HUD display.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "J2" (at 0 1.648) (layer "B.SilkS") hide)
    (fp_text value "2" (at 1.35 0.61) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 1.65) (layer "B.Fab"))
    (pad "1" smd circle (at 0 0) (size 1.5 1.5) (layers "B.Cu" "B.Mask")
      (net 13 "/SCL") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_D1.5mm" (layer "B.Cu")
    (at 113.9 101.1)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "Digital HUD display.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "J4" (at 0 1.648) (layer "B.SilkS") hide)
    (fp_text value "3" (at 1.31 -0.55) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 1.65) (layer "B.Fab"))
    (pad "1" smd circle (at 0 0) (size 1.5 1.5) (layers "B.Cu" "B.Mask")
      (net 14 "/SDA") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (at 110.65 102.35 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Digital HUD display.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R8" (at -1.25 -0.05 180) (layer "B.SilkS"))
    (fp_text value "680" (at 0 -1.17 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 20 "/LED1G") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(D1-GA)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (at 111.7 102.35 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Digital HUD display.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R7" (at -1.25 -0.2 180) (layer "B.SilkS"))
    (fp_text value "100" (at 0 -1.17 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/LED1B") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(D1-RA)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (at 109.6 102.35 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Digital HUD display.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R9" (at -1.25 0.2 180) (layer "B.SilkS"))
    (fp_text value "330" (at 0 -1.17 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "/LED1R") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(D1-BA)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DFN_QFN:VQFN-24-1EP_4x4mm_P0.5mm_EP2.45x2.45mm" (layer "B.Cu")
    (at 105.510742 103.5 45)
    (descr "VQFN, 24 Pin (http://www.ti.com/lit/ds/symlink/msp430f1101a.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "VQFN NoLead")
    (property "Sheetfile" "Digital HUD display.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at -0.007596 3.103674 45) (layer "B.SilkS"))
    (fp_text value "ATTiny3227-M" (at 0 -3.320001 45) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "B.Fab"))
    (pad "" smd roundrect (at -0.82 -0.82 45) (size 0.66 0.66) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.82 0 45) (size 0.66 0.66) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.82 0.82 45) (size 0.66 0.66) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 -0.82 45) (size 0.66 0.66) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 0 45) (size 0.66 0.66) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 0.82 45) (size 0.66 0.66) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.82 -0.82 45) (size 0.66 0.66) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.82 0 45) (size 0.66 0.66) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.82 0.82 45) (size 0.66 0.66) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -1.9875 1.25 45) (size 0.775 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "/RxD") (pinfunction "PA2") (pintype "bidirectional+no_connect"))
    (pad "2" smd roundrect (at -1.9875 0.75 45) (size 0.775 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "/LSens") (pinfunction "PA3") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -1.9875 0.25 45) (size 0.775 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd roundrect (at -1.9875 -0.25 45) (size 0.775 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "VDD") (pinfunction "VDD") (pintype "power_in"))
    (pad "5" smd roundrect (at -1.9875 -0.75 45) (size 0.775 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 19 "/LS_Pwr") (pinfunction "PA4") (pintype "bidirectional"))
    (pad "6" smd roundrect (at -1.9875 -1.25 45) (size 0.775 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 16 "/Int2") (pinfunction "PA5") (pintype "bidirectional"))
    (pad "7" smd roundrect (at -1.25 -1.9875 45) (size 0.25 0.775) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 17 "/Int1") (pinfunction "PA6") (pintype "bidirectional"))
    (pad "8" smd roundrect (at -0.75 -1.9875 45) (size 0.25 0.775) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "/LED3R") (pinfunction "PA7") (pintype "bidirectional"))
    (pad "9" smd roundrect (at -0.25 -1.9875 45) (size 0.25 0.775) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "/LED3G") (pinfunction "PB7") (pintype "bidirectional"))
    (pad "10" smd roundrect (at 0.25 -1.9875 45) (size 0.25 0.775) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "/LED3B") (pinfunction "PB6") (pintype "bidirectional"))
    (pad "11" smd roundrect (at 0.75 -1.9875 45) (size 0.25 0.775) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 23 "/PWM_B") (pinfunction "PB5") (pintype "bidirectional"))
    (pad "12" smd roundrect (at 1.25 -1.9875 45) (size 0.25 0.775) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "/PWM_G") (pinfunction "PB4") (pintype "bidirectional"))
    (pad "13" smd roundrect (at 1.9875 -1.25 45) (size 0.775 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 24 "/PWM_R") (pinfunction "PB3") (pintype "bidirectional"))
    (pad "14" smd roundrect (at 1.9875 -0.75 45) (size 0.775 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 33 "unconnected-(U1-PB2-Pad14)") (pinfunction "PB2") (pintype "bidirectional+no_connect"))
    (pad "15" smd roundrect (at 1.9875 -0.25 45) (size 0.775 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 14 "/SDA") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "16" smd roundrect (at 1.9875 0.25 45) (size 0.775 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 13 "/SCL") (pinfunction "PB0") (pintype "bidirectional"))
    (pad "17" smd roundrect (at 1.9875 0.75 45) (size 0.775 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/LED1B") (pinfunction "PC0") (pintype "bidirectional"))
    (pad "18" smd roundrect (at 1.9875 1.25 45) (size 0.775 0.25) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 20 "/LED1G") (pinfunction "PC1") (pintype "bidirectional"))
    (pad "19" smd roundrect (at 1.25 1.9875 45) (size 0.25 0.775) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "/LED1R") (pinfunction "PC2") (pintype "bidirectional"))
    (pad "20" smd roundrect (at 0.75 1.9875 45) (size 0.25 0.775) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "/LED2B") (pinfunction "PC3") (pintype "bidirectional"))
    (pad "21" smd roundrect (at 0.25 1.9875 45) (size 0.25 0.775) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 21 "/LED2G") (pinfunction "PC4") (pintype "bidirectional"))
    (pad "22" smd roundrect (at -0.25 1.9875 45) (size 0.25 0.775) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "/LED2R") (pinfunction "PC5") (pintype "bidirectional"))
    (pad "23" smd roundrect (at -0.75 1.9875 45) (size 0.25 0.775) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 15 "/UPDI") (pinfunction "PA0/UPDI") (pintype "bidirectional"))
    (pad "24" smd roundrect (at -1.25 1.9875 45) (size 0.25 0.775) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "/TxD") (pinfunction "PA1") (pintype "bidirectional+no_connect"))
    (pad "25" smd rect (at 0 0 45) (size 2.45 2.45) (property pad_prop_heatsink) (layers "B.Cu" "B.Mask")
      (net 1 "GND") (pinfunction "EP") (pintype "unspecified") (zone_connect 2))
    (model "${KICAD7_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/VQFN-24-1EP_4x4mm_P0.5mm_EP2.45x2.45mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (at 101.15 101.61 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Digital HUD display.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R1" (at 1.5 -0.04) (layer "B.SilkS"))
    (fp_text value "100" (at 0 -1.17) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "/LED3B") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(D3-RA)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (at 101.15 102.64 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Digital HUD display.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R2" (at 1.5 -0.01) (layer "B.SilkS"))
    (fp_text value "680" (at 0 -1.17) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "/LED3G") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(D3-GA)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (at 101.15 103.65 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Digital HUD display.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R3" (at 1.5 0) (layer "B.SilkS"))
    (fp_text value "330" (at 0 -1.17) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "/LED3R") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(D3-BA)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (at 111.7 105.35 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Digital HUD display.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R4" (at -1.25 -0.2 180) (layer "B.SilkS"))
    (fp_text value "100" (at 0 -1.17 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "/LED2B") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(D2-RA)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (at 110.65 105.35 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Digital HUD display.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R5" (at -1.25 -0.05 180) (layer "B.SilkS"))
    (fp_text value "680" (at 0 -1.17 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 21 "/LED2G") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(D2-GA)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (at 109.6 105.35 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Digital HUD display.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R6" (at -1.25 0.2 180) (layer "B.SilkS"))
    (fp_text value "330" (at 0 -1.17 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "/LED2R") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(D2-BA)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.5mm" (layer "B.Cu")
    (at 114.6 103.5)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "Digital HUD display.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "J6" (at 0 1.648) (layer "B.SilkS") hide)
    (fp_text value "Prg" (at -1.44 0 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 1.65) (layer "B.Fab"))
    (pad "1" smd circle (at 0 0) (size 1.5 1.5) (layers "B.Cu" "B.Mask")
      (net 15 "/UPDI") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (at 96.575 103.3 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Digital HUD display.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C3" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "4.7u" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (at 96.575 104.8 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Digital HUD display.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C2" (at -1.475 -0.8) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 115.7 106.652513) (end 115.7 100.35)
    (layer "Edge.Cuts"))
  (gr_line (start 115.35 100) (end 98.475 100)
    (layer "Edge.Cuts"))
  (gr_line (start 98.472487 107.002513) (end 115.35 107.002513)
    (layer "Edge.Cuts"))
  (gr_line (start 98.125 100.35) (end 98.125 100.652513)
    (layer "Edge.Cuts"))
  (gr_line (start 95.15 105.95) (end 97.775 105.95)
    (layer "Edge.Cuts"))
  (gr_line (start 94.8 101.352513) (end 94.8 105.6)
    (layer "Edge.Cuts"))
  (gr_arc (start 98.125 100.35) (mid 98.227513 100.102513) (end 98.475 100)
    (layer "Edge.Cuts"))
  (gr_arc (start 95.15 105.95) (mid 94.902513 105.847487) (end 94.8 105.6)
    (layer "Edge.Cuts"))
  (gr_arc (start 115.35 100) (mid 115.597487 100.102513) (end 115.7 100.35)
    (layer "Edge.Cuts"))
  (gr_arc (start 98.125 100.652513) (mid 98.022487 100.9) (end 97.775 101.002513)
    (layer "Edge.Cuts"))
  (gr_line (start 98.122487 106.652513) (end 98.125 106.3)
    (layer "Edge.Cuts"))
  (gr_arc (start 94.8 101.352513) (mid 94.902513 101.105026) (end 95.15 101.002513)
    (layer "Edge.Cuts"))
  (gr_line (start 97.775 101.002513) (end 95.15 101.002513)
    (layer "Edge.Cuts"))
  (gr_arc (start 115.7 106.652513) (mid 115.597487 106.9) (end 115.35 107.002513)
    (layer "Edge.Cuts"))
  (gr_arc (start 97.775 105.95) (mid 98.022487 106.052513) (end 98.125 106.3)
    (layer "Edge.Cuts"))
  (gr_arc (start 98.472487 107.002513) (mid 98.225 106.9) (end 98.122487 106.652513)
    (layer "Edge.Cuts"))
  (gr_text "6.29.25" (at 102.5 105.15) (layer "B.SilkS"))
  (zone (net 1) (net_name "GND") (layer "In2.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.7 107)
        (xy 94.8 107)
        (xy 94.8 100)
        (xy 115.7 100)
      )
    )
  )
)
