(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "+12V")
	(net 3 "+5V")
	(net 4 "unconnected-(J6-Pin_4-Pad4)")
	(net 5 "unconnected-(J6-Pin_5-Pad5)")
	(net 6 "Net-(J1-Pad3)")
	(net 7 "Net-(J1-Pad4)")
	(net 8 "+3.3V")
	(net 9 "unconnected-(J10-Pin_1-Pad1)")
	(net 10 "unconnected-(J10-Pin_2-Pad2)")
	(net 11 "unconnected-(J10-Pin_3-Pad3)")
	(net 12 "unconnected-(J10-Pin_4-Pad4)")
	(net 13 "/SDA")
	(net 14 "/SCL")
	(net 15 "/Tx")
	(net 16 "Net-(J11-Pin_1)")
	(net 17 "Net-(J17-SHIELD-PadS1)")
	(net 18 "/+Batt")
	(net 19 "Net-(J22-Pin_1)")
	(net 20 "unconnected-(J22-Pin_4-Pad4)")
	(net 21 "unconnected-(J22-Pin_5-Pad5)")
	(net 22 "unconnected-(J22-Pin_6-Pad6)")
	(net 23 "/Rx")
	(net 24 "Net-(J23-SHIELD-PadS1)")
	(net 25 "Net-(U1-VIN-)")
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x07_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 121.0818 113.2332 180)
		(descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x07 2.54mm single row")
		(property "Reference" "J22"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x07"
			(at 0 17.57 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x07_P2.54mm_Vertical"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 7.62 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(J22-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "+3.3V")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "unconnected-(J22-Pin_4-Pad4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "unconnected-(J22-Pin_5-Pad5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "unconnected-(J22-Pin_6-Pad6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/Rx")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:B4B-EH-ALFSN"
		(layer "F.Cu")
		(at 160.822 111.506)
		(property "Reference" "J13"
			(at 3.75 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "B4B-EH-ALFSN"
			(at 3.75 1.27 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "footprints:B4B-EH-ALFSN"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN_B4B-EH-A_JST")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr through_hole)
		(fp_text user "*"
			(at 0 1.27 0)
			(layer "F.SilkS")
		)
		(fp_text user "Copyright 2021 Accelerated Designs. All rights reserved."
			(at 0 1.27 0)
			(layer "Cmts.User")
		)
		(fp_text user "*"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+12V")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(pad "3" thru_hole circle
			(at 5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(J1-Pad3)")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(pad "4" thru_hole circle
			(at 7.5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J1-Pad4)")
			(pinfunction "4")
			(pintype "unspecified")
		)
	)
	(footprint "footprints:B4B-EH-ALFSN"
		(layer "F.Cu")
		(at 160.782 92.202)
		(property "Reference" "J16"
			(at 3.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "B4B-EH-ALFSN"
			(at 3.75 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "footprints:B4B-EH-ALFSN"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN_B4B-EH-A_JST")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr through_hole)
		(fp_text user "*"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "Copyright 2021 Accelerated Designs. All rights reserved."
			(at 0 0 0)
			(layer "Cmts.User")
		)
		(fp_text user "*"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+12V")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(pad "3" thru_hole circle
			(at 5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(J1-Pad3)")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(pad "4" thru_hole circle
			(at 7.5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J1-Pad4)")
			(pinfunction "4")
			(pintype "unspecified")
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 176.1755 95.758)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small"
			(at 0 2.7 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+12V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x07_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 136.4488 113.3348 180)
		(descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x07 2.54mm single row")
		(property "Reference" "J10"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x07"
			(at 0 17.57 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x07_P2.54mm_Vertical"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 7.62 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "unconnected-(J10-Pin_1-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "unconnected-(J10-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "unconnected-(J10-Pin_3-Pad3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "unconnected-(J10-Pin_4-Pad4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/SDA")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/SCL")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/Tx")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:B4B-EH-ALFSN"
		(layer "F.Cu")
		(at 174.498 111.506)
		(property "Reference" "J4"
			(at 3.75 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "B4B-EH-ALFSN"
			(at 3.75 1.27 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "footprints:B4B-EH-ALFSN"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN_B4B-EH-A_JST")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr through_hole)
		(fp_text user "*"
			(at 0 1.27 0)
			(layer "F.SilkS")
		)
		(fp_text user "Copyright 2021 Accelerated Designs. All rights reserved."
			(at 0 1.27 0)
			(layer "Cmts.User")
		)
		(fp_text user "*"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+12V")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(pad "3" thru_hole circle
			(at 5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(J1-Pad3)")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(pad "4" thru_hole circle
			(at 7.5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J1-Pad4)")
			(pinfunction "4")
			(pintype "unspecified")
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 141.1224 87.6554)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x01 2.54mm single row")
		(property "Reference" "J21"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x01"
			(at 0 2.33 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/+Batt")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:CONN_BM04B-SRSS-TB_SPK"
		(layer "F.Cu")
		(at 135.7892 89.6352 90)
		(tags "PRT-16766 ")
		(property "Reference" "J24"
			(at 0 1.4216 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "PRT-16766"
			(at 0 1.4216 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "footprints:CONN_BM04B-SRSS-TB_SPK"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "PRT-16766"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN_BM04B-SRSS-TB_SPK")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.4216 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 1.4216 90)
			(size 0.6096 1.5494)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at -0.499999 1.4216 90)
			(size 0.6096 1.5494)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "+3.3V")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at 0.499999 1.4216 90)
			(size 0.6096 1.5494)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "/SDA")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 1.5 1.4216 90)
			(size 0.6096 1.5494)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "/SCL")
			(pinfunction "4")
			(pintype "unspecified")
		)
		(pad "5" smd rect
			(at -2.799999 -1.103399 90)
			(size 1.1938 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "6" smd rect
			(at 2.799999 -1.103399 90)
			(size 1.1938 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 154.7622 90.8812 -90)
		(descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x02 2.54mm single row")
		(property "Reference" "J9"
			(at 0 -2.77 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 0 5.31 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+12V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 162.4595 102.108)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C6"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+12V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 140.8684 110.4646 180)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "J6"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x05"
			(at 0 12.49 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 5.08 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+12V")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "unconnected-(J6-Pin_4-Pad4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J6-Pin_5-Pad5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 176.1755 115.062)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C8"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+12V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 176.276 108.712)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at 0 -0.668 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+12V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 129.5804 106.045 180)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP1"
			(at 0 -1.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "SolderJumper_2_Open"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd custom
			(at -0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 3 "+5V")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 19 "Net-(J22-Pin_1)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 147.5486 89.408)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C12"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+12V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 162.4595 95.758)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small"
			(at 0 2.7 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+12V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:B4B-EH-ALFSN"
		(layer "F.Cu")
		(at 174.498 92.202)
		(property "Reference" "J1"
			(at 1.4616 -1.481 0)
			(layer "F.SilkS")
		)
		(property "Value" "B4B-EH-ALFSN"
			(at 1.4616 -1.481 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "footprints:B4B-EH-ALFSN"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN_B4B-EH-A_JST")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr through_hole)
		(fp_text user "*"
			(at -2.2884 -1.481 0)
			(layer "F.SilkS")
		)
		(fp_text user "Copyright 2021 Accelerated Designs. All rights reserved."
			(at -2.2884 -1.481 0)
			(layer "Cmts.User")
		)
		(fp_text user "*"
			(at -2.2884 -1.481 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+12V")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(pad "3" thru_hole circle
			(at 5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(J1-Pad3)")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(pad "4" thru_hole circle
			(at 7.5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J1-Pad4)")
			(pinfunction "4")
			(pintype "unspecified")
		)
	)
	(footprint "footprints:B4B-EH-ALFSN"
		(layer "F.Cu")
		(at 160.782 105.156)
		(property "Reference" "J5"
			(at 3.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "B4B-EH-ALFSN"
			(at 3.75 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "footprints:B4B-EH-ALFSN"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN_B4B-EH-A_JST")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr through_hole)
		(fp_text user "*"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "Copyright 2021 Accelerated Designs. All rights reserved."
			(at 0 0 0)
			(layer "Cmts.User")
		)
		(fp_text user "*"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+12V")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(pad "3" thru_hole circle
			(at 5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(J1-Pad3)")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(pad "4" thru_hole circle
			(at 7.5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J1-Pad4)")
			(pinfunction "4")
			(pintype "unspecified")
		)
	)
	(footprint "BM04B-GHS-TBT_LF__SN__N_:JST_BM04B-GHS-TBT(LF)(SN)(N)"
		(layer "F.Cu")
		(at 121.6688 89.7482 -90)
		(property "Reference" "J23"
			(at -1.96 -5.608 90)
			(layer "F.SilkS")
		)
		(property "Value" "BM04B-GHS-TBT(LF)(SN)(N)"
			(at 9.624 2.192 90)
			(layer "F.Fab")
		)
		(property "Footprint" "BM04B-GHS-TBT_LF__SN__N_:JST_BM04B-GHS-TBT(LF)(SN)(N)"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "JST"
			(at 31.9206 211.417 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "4.05mm"
			(at 31.9206 211.417 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "N/A"
			(at 31.9206 211.417 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 31.9206 211.417 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at 1.875 -3.35)
			(size 1.7 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "+5V")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.625 -3.35)
			(size 1.7 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "/Tx")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.625 -3.35)
			(size 1.7 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/Rx")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.875 -3.35)
			(size 1.7 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "S1" smd rect
			(at -3.725 0 180)
			(size 2.8 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "Net-(J23-SHIELD-PadS1)")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S2" smd rect
			(at 3.725 0 180)
			(size 2.8 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "Net-(J23-SHIELD-PadS1)")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 162.4595 115.062)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at 0 -0.668 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+12V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:B4B-EH-ALFSN"
		(layer "F.Cu")
		(at 174.498 98.552)
		(property "Reference" "J15"
			(at 3.75 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "B4B-EH-ALFSN"
			(at 3.75 1.27 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "footprints:B4B-EH-ALFSN"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN_B4B-EH-A_JST")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr through_hole)
		(fp_text user "*"
			(at 0 1.27 0)
			(layer "F.SilkS")
		)
		(fp_text user "Copyright 2021 Accelerated Designs. All rights reserved."
			(at 0 1.27 0)
			(layer "Cmts.User")
		)
		(fp_text user "*"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+12V")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(pad "3" thru_hole circle
			(at 5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(J1-Pad3)")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(pad "4" thru_hole circle
			(at 7.5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J1-Pad4)")
			(pinfunction "4")
			(pintype "unspecified")
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 120.7516 82.5246)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x01 2.54mm single row")
		(property "Reference" "J11"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x01"
			(at 0 2.33 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(J11-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "50THV100M10X10-5:50THV100M10X10.5"
		(layer "F.Cu")
		(at 149.352 98.806 180)
		(property "Reference" "C1"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "50THV100M10X10-5:50THV100M10X10.5"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr through_hole)
		(fp_text user "*"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "Copyright 2021 Accelerated Designs. All rights reserved."
			(at 0 0 0)
			(layer "Cmts.User")
		)
		(fp_text user "*"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4.1529 0 180)
			(size 3.6068 1.4986)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 4.1529 0 180)
			(size 3.6068 1.4986)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+12V")
			(pintype "passive")
		)
	)
	(footprint "footprints:B4B-EH-ALFSN"
		(layer "F.Cu")
		(at 160.782 98.552)
		(property "Reference" "J8"
			(at 3.75 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "B4B-EH-ALFSN"
			(at 3.75 1.27 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "footprints:B4B-EH-ALFSN"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN_B4B-EH-A_JST")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr through_hole)
		(fp_text user "*"
			(at 0 1.27 0)
			(layer "F.SilkS")
		)
		(fp_text user "Copyright 2021 Accelerated Designs. All rights reserved."
			(at 0 1.27 0)
			(layer "Cmts.User")
		)
		(fp_text user "*"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+12V")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(pad "3" thru_hole circle
			(at 5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(J1-Pad3)")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(pad "4" thru_hole circle
			(at 7.5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J1-Pad4)")
			(pinfunction "4")
			(pintype "unspecified")
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 176.1755 89.154)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C10"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+12V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Wire:SolderWire-2.5sqmm_1x02_P7.2mm_D2.4mm_OD3.6mm"
		(layer "F.Cu")
		(at 153.6192 111.9632 180)
		(descr "Soldered wire connection, for 2 times 2.5 mm² wires, basic insulation, conductor diameter 2.4mm, outer diameter 3.6mm, size source Multi-Contact FLEXI-E 2.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
		(tags "connector wire 2.5sqmm")
		(property "Reference" "J7"
			(at 3.6 -3.2 180)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 3.6 3.2 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Wire:SolderWire-2.5sqmm_1x02_P7.2mm_D2.4mm_OD3.6mm"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 3.6 0 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 4 4)
			(drill 3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.0625)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.2 0 180)
			(size 4 4)
			(drill 3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+12V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-2.5sqmm_1x02_P7.2mm_D2.4mm_OD3.6mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:B4B-EH-ALFSN"
		(layer "F.Cu")
		(at 174.498 105.156)
		(property "Reference" "J14"
			(at 3.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "B4B-EH-ALFSN"
			(at 3.75 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "footprints:B4B-EH-ALFSN"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN_B4B-EH-A_JST")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr through_hole)
		(fp_text user "*"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "Copyright 2021 Accelerated Designs. All rights reserved."
			(at 0 0 0)
			(layer "Cmts.User")
		)
		(fp_text user "*"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+12V")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(pad "3" thru_hole circle
			(at 5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(J1-Pad3)")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(pad "4" thru_hole circle
			(at 7.5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J1-Pad4)")
			(pinfunction "4")
			(pintype "unspecified")
		)
	)
	(footprint "B4B-EH-A-LF-SN-:B4B-EH-ALFSN"
		(layer "F.Cu")
		(at 146.431 85.4456)
		(property "Reference" "J18"
			(at 3.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "B4B-EH-ALFSN"
			(at 3.75 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "B4B-EH-A-LF-SN-:B4B-EH-ALFSN"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN_B4B-EH-A_JST")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr through_hole)
		(fp_text user "*"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "Copyright 2021 Accelerated Designs. All rights reserved."
			(at 0 0 0)
			(layer "Cmts.User")
		)
		(fp_text user "*"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+12V")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(pad "3" thru_hole circle
			(at 5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(J1-Pad3)")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(pad "4" thru_hole circle
			(at 7.5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J1-Pad4)")
			(pinfunction "4")
			(pintype "unspecified")
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 162.4595 108.712)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C7"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+12V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 141.0208 96.0374 180)
		(descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x02 2.54mm single row")
		(property "Reference" "J12"
			(at 0 -2.77 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at -2.032 4.802 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:B4B-EH-ALFSN"
		(layer "F.Cu")
		(at 174.498 85.598)
		(property "Reference" "J3"
			(at 3.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "B4B-EH-ALFSN"
			(at 3.75 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "footprints:B4B-EH-ALFSN"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN_B4B-EH-A_JST")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr through_hole)
		(fp_text user "*"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "Copyright 2021 Accelerated Designs. All rights reserved."
			(at 0 0 0)
			(layer "Cmts.User")
		)
		(fp_text user "*"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+12V")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(pad "3" thru_hole circle
			(at 5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(J1-Pad3)")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(pad "4" thru_hole circle
			(at 7.5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J1-Pad4)")
			(pinfunction "4")
			(pintype "unspecified")
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 176.1755 102.108)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C9"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+12V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PMC-1424THX:SW_PMC-1424THX"
		(layer "F.Cu")
		(at 132.8114 82.4992)
		(property "Reference" "S1"
			(at -8.168 -2.6064 0)
			(layer "F.SilkS")
		)
		(property "Value" "PMC-1424THX"
			(at -4.5104 2.6064 0)
			(layer "F.Fab")
		)
		(property "Footprint" "PMC-1424THX:SW_PMC-1424THX"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "PIC GmbH"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "4.1 mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "1.4"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -9.2 0)
			(size 1.5 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "Net-(J11-Pin_1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 9.2 0)
			(size 1.5 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 162.2055 89.154)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C11"
			(at 0 -0.668 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+12V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:B4B-EH-ALFSN"
		(layer "F.Cu")
		(at 160.8825 85.598)
		(property "Reference" "J2"
			(at 3.75 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "B4B-EH-ALFSN"
			(at 3.75 1.27 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "footprints:B4B-EH-ALFSN"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN_B4B-EH-A_JST")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr through_hole)
		(fp_text user "*"
			(at 0 1.27 0)
			(layer "F.SilkS")
		)
		(fp_text user "Copyright 2021 Accelerated Designs. All rights reserved."
			(at 0 1.27 0)
			(layer "Cmts.User")
		)
		(fp_text user "*"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+12V")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(pad "3" thru_hole circle
			(at 5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(J1-Pad3)")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(pad "4" thru_hole circle
			(at 7.5 0)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J1-Pad4)")
			(pinfunction "4")
			(pintype "unspecified")
		)
	)
	(footprint "BM04B-GHS-TBT_LF__SN__N_:JST_BM04B-GHS-TBT(LF)(SN)(N)"
		(layer "F.Cu")
		(at 128.4506 89.7536 -90)
		(property "Reference" "J17"
			(at -1.96 -5.608 90)
			(layer "F.SilkS")
		)
		(property "Value" "BM04B-GHS-TBT(LF)(SN)(N)"
			(at 9.624 2.192 90)
			(layer "F.Fab")
		)
		(property "Footprint" "BM04B-GHS-TBT_LF__SN__N_:JST_BM04B-GHS-TBT(LF)(SN)(N)"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "JST"
			(at 38.697 218.2042 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "4.05mm"
			(at 38.697 218.2042 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "N/A"
			(at 38.697 218.2042 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 38.697 218.2042 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at 1.875 -3.35)
			(size 1.7 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "+3.3V")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.625 -3.35)
			(size 1.7 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "/SCL")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.625 -3.35)
			(size 1.7 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "/SDA")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.875 -3.35)
			(size 1.7 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "S1" smd rect
			(at -3.725 0 180)
			(size 2.8 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(J17-SHIELD-PadS1)")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S2" smd rect
			(at 3.725 0 180)
			(size 2.8 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(J17-SHIELD-PadS1)")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
	)
	(footprint "INA219BID:SOIC127P599X175-8N"
		(layer "B.Cu")
		(at 152.0942 100.4824 180)
		(property "Reference" "U1"
			(at -0.385 3.537 0)
			(layer "B.SilkS")
		)
		(property "Value" "INA219BID"
			(at 7.87 -3.537 0)
			(layer "B.Fab")
		)
		(property "Footprint" "INA219BID:SOIC127P599X175-8N"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -2.47 1.905 180)
			(size 1.97 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.07)
			(net 1 "GND")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.47 0.635 180)
			(size 1.97 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.07)
			(net 1 "GND")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.47 -0.635 180)
			(size 1.97 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.07)
			(net 13 "/SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -2.47 -1.905 180)
			(size 1.97 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.07)
			(net 14 "/SCL")
			(pinfunction "SCL")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 2.47 -1.905 180)
			(size 1.97 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.07)
			(net 8 "+3.3V")
			(pinfunction "VS")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at 2.47 -0.635 180)
			(size 1.97 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.07)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "7" smd roundrect
			(at 2.47 0.635 180)
			(size 1.97 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.07)
			(net 25 "Net-(U1-VIN-)")
			(pinfunction "VIN-")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at 2.47 1.905 180)
			(size 1.97 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.07)
			(net 18 "/+Batt")
			(pinfunction "VIN+")
			(pintype "input")
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "B.Cu")
		(at 146.7612 101.6265 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C13"
			(at 0 1.43 90)
			(layer "B.SilkS")
		)
		(property "Value" "C_Small"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 90)
			(size 1.075 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 8 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 90)
			(size 1.075 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "B.Cu")
		(at 132.08 99.7364 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 1.65 90)
			(layer "B.SilkS")
		)
		(property "Value" "R_Small_US"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.208333)
			(net 8 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.208333)
			(net 13 "/SDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder"
		(layer "B.Cu")
		(at 150.9288 95.0468)
		(descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 0 2.62 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1/1% (PT2512FK-070R1L)"
			(at 0 -2.62 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -3.05 0)
			(size 1.4 3.35)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.178571)
			(net 25 "Net-(U1-VIN-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 3.05 0)
			(size 1.4 3.35)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.178571)
			(net 18 "/+Batt")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "B.Cu")
		(at 128.5748 99.7552 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 1.65 90)
			(layer "B.SilkS")
		)
		(property "Value" "R_Small_US"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "turtle_board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.208333)
			(net 8 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.208333)
			(net 14 "/SCL")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_circle
		(center 131.064 112.522)
		(end 132.564 112.522)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 187.7 112.522)
		(end 189.2 112.522)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 187.7 89.662)
		(end 189.2 89.662)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_poly
		(pts
			(xy 189.865 116.84) (xy 118.999 116.84) (xy 118.999 79.5782) (xy 189.865 79.5782)
		)
		(fill none)
		(layer "Edge.Cuts")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 1.27)
		)
		(polygon
			(pts
				(xy 187.505053 116.58371) (xy 119.151436 116.332) (xy 119.15134 79.704761) (xy 187.250957 79.702471)
			)
		)
	)
)
