<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="60.0202" y2="0" width="0" layer="20"/>
<wire x1="60.0202" y1="0" x2="59.9948" y2="39.0144" width="0" layer="20"/>
<wire x1="59.9948" y1="39.0144" x2="0" y2="39.0144" width="0" layer="20"/>
<wire x1="0" y1="39.0144" x2="0" y2="0" width="0" layer="20"/>
<text>DualLickCmp
J006330REVB</text>
<text>S</text>
<text>S</text>
<text>LICK PORTS</text>
<text>TTL OUT</text>
<text>USB POWER</text>
<text>20180816</text>
<text>IN1</text>
<text>IN2</text>
<text>THR1</text>
<text>THR2</text>
<text>GND</text>
</plain>
<libraries>
<library name="STEVES_BU">
<packages>
<package name="0805S">
</package>
<package name="0603S">
</package>
<package name="SO-16-7.5MM">
</package>
<package name="UMAX10">
</package>
<package name="LOGO_BMP_OP">
</package>
<package name="LOGO_JANELIA_2014_ENCLOSURE">
</package>
<package name="3310P">
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="10118194">
</package>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
<package name="1X05_LOCK">
</package>
</packages>
</library>
<library name="con-coax">
<description>&lt;b&gt;Coax Connectors&lt;/b&gt;&lt;p&gt;
Radiall  and M/A COM.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="AMP_227161">
<description>&lt;b&gt;JACK,  RIGHT ANGLE, 50 OHM, PCB, BNC&lt;/b&gt;&lt;p&gt;
Source: amp_227161.pdf</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R7" library="STEVES_BU" package="0805S" value="10K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="STEVES_BU" package="0805S" value="4M99">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="STEVES_BU" package="0805S" value="10K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="STEVES_BU" package="0805S" value="4M99">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="STEVES_BU" package="0805S" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="STEVES_BU" package="0805S" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="STEVES_BU" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="STEVES_BU" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="STEVES_BU" package="SO-16-7.5MM" value="ADUM5202">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="STEVES_BU" package="0805S" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="STEVES_BU" package="0805S" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="STEVES_BU" package="UMAX10" value="MAX9043">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="STEVES_BU" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="STEVES_BU" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="STEVES_BU" package="0805S" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="STEVES_BU" package="0805S" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="con-coax" package="AMP_227161" value="1-227161-0">
<attribute name="OC_NEWARK" value="33B3200"/>
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="1-227161"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="con-coax" package="AMP_227161" value="1-227161-0">
<attribute name="OC_NEWARK" value="33B3200"/>
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="1-227161"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J100" library="SparkFun" package="10118194" value="USB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="STEVES_BU" package="0805S" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="con-coax" package="AMP_227161" value="1-227161-0">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="1-227161"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="33B3200"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="con-coax" package="AMP_227161" value="1-227161-0">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="1-227161"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="33B3200"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="STEVES_BU" package="LOGO_BMP_OP" value="JFRC-LOGOLOGO_OP"/>
<element name="U$2" library="STEVES_BU" package="LOGO_JANELIA_2014_ENCLOSURE" value="JFRC-LOGOLOGO_JANELIA_2014_ECLOSURE"/>
<element name="R3" library="STEVES_BU" package="3310P" value="POT3310P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="STEVES_BU" package="0805S" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="STEVES_BU" package="3310P" value="POT3310P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="STEVES_BU" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ4" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ2" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ3" library="SparkFun" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun" package="1X05_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C4" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="C3" pad="2"/>
<contactref element="U2" pad="15"/>
<contactref element="C6" pad="2"/>
<contactref element="J3" pad="2"/>
<contactref element="U2" pad="9"/>
<contactref element="J1" pad="2"/>
<contactref element="LED1" pad="K"/>
<contactref element="LED2" pad="K"/>
<contactref element="R3" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="SJ1" pad="1"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="IN1">
<contactref element="U1" pad="4"/>
<contactref element="R2" pad="2"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="DET1">
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="U2" pad="13"/>
<contactref element="SJ2" pad="1"/>
</signal>
<signal name="DET2">
<contactref element="R8" pad="1"/>
<contactref element="U1" pad="8"/>
<contactref element="U2" pad="14"/>
<contactref element="SJ3" pad="1"/>
</signal>
<signal name="GISO">
<contactref element="U2" pad="8"/>
<contactref element="U2" pad="5"/>
<contactref element="C5" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="J4" pad="2"/>
<contactref element="J100" pad="GND"/>
<contactref element="U2" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="U1" pad="10"/>
<contactref element="C3" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="IN2">
<contactref element="R7" pad="2"/>
<contactref element="U1" pad="6"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="LP2">
<contactref element="R7" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="OUT2">
<contactref element="J4" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="SJ3" pad="2"/>
</signal>
<signal name="VDD">
<contactref element="C4" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="L1" pad="2"/>
<contactref element="U2" pad="16"/>
<contactref element="U2" pad="11"/>
<contactref element="SJ4" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="C5" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="U2" pad="7"/>
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="6"/>
<contactref element="L2" pad="1"/>
<contactref element="SJ4" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="R3" pad="2"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="R8" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="LP1">
<contactref element="R2" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U2" pad="4"/>
<contactref element="J2" pad="1"/>
<contactref element="SJ2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R5" pad="2"/>
<contactref element="R3" pad="3"/>
<contactref element="R6" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="J100" pad="VBUS"/>
<contactref element="L2" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="R6" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="7"/>
<contactref element="JP1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
