(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 0)
    (no_connects 0)
    (area 99.035238 83.494999 118.47619 97.320002)
    (thickness 1.6)
    (drawings 4)
    (tracks 46)
    (zones 0)
    (modules 2)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.006)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.027)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 5834D5CF)
    (at 114.3 90.17)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U1 (at 0 -1.27) (layer F.SilkS))
    (fp_text value SOIC-8-N (at 0 1.27) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Testlib:MOLEX-87264-1052 (layer F.Cu) (tedit 5834D933)
    (at 104.14 90.17)
    (fp_text reference JSP1 (at 0 0 90) (layer F.SilkS))
    (fp_text value 87264 (at 0 5.5) (layer F.Fab))
    (pad 5 thru_hole circle (at -2.25 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -2.25 -2) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at -2.25 2) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at -2.25 4) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at -2.25 -3.75) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 2.25 4) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 2.25 2) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 2.25 0) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 2.25 -2) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.25 -3.75) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask))
  )
  (gr_line (start 119.38 82.55) (end 99.695 82.55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.38 97.79) (end 119.38 82.55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.695 97.79) (end 119.38 97.79) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.695 82.55) (end 99.695 97.79) (angle 90) (layer Edge.Cuts) (width 0.15))
)
