(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 112)
    (no_connects 0)
    (area 29.114287 35.4 171.600001 131.650001)
    (thickness 1.6)
    (drawings 20)
    (tracks 482)
    (zones 0)
    (modules 48)
    (nets 38)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFEF77F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 +3V3)
  (net 5 "Net-(C4-Pad2)")
  (net 6 +24V)
  (net 7 "Net-(D1-Pad1)")
  (net 8 "Net-(D1-Pad3)")
  (net 9 /ETH0_TX+)
  (net 10 /ETH0_TX-)
  (net 11 /ETH0_RX+)
  (net 12 /ETH0_RX-)
  (net 13 /ETH_PWR+)
  (net 14 /ETH_PWR-)
  (net 15 /Omega_RX)
  (net 16 /Omega_TX)
  (net 17 "Net-(C8-Pad1)")
  (net 18 /PPoE+)
  (net 19 /USBPWR)
  (net 20 /MOTOR1)
  (net 21 "Net-(C3-Pad1)")
  (net 22 /MOTOR2)
  (net 23 "Net-(C7-Pad1)")
  (net 24 "Net-(C14-Pad1)")
  (net 25 /SENS0_N)
  (net 26 /PIR)
  (net 27 /SENS2_N)
  (net 28 /SENS1_N)
  (net 29 /LED_GN)
  (net 30 /LED_RD)
  (net 31 /BUTTON)
  (net 32 /PWM_MOTOR)
  (net 33 /EN2_MOTOR)
  (net 34 /EN1_MOTOR)
  (net 35 /I2C_C)
  (net 36 /I2C_D)
  (net 37 /SENSE)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /BUTTON)
    (add_net /EN1_MOTOR)
    (add_net /EN2_MOTOR)
    (add_net /ETH0_RX+)
    (add_net /ETH0_RX-)
    (add_net /ETH0_TX+)
    (add_net /ETH0_TX-)
    (add_net /I2C_C)
    (add_net /I2C_D)
    (add_net /LED_GN)
    (add_net /LED_RD)
    (add_net /Omega_RX)
    (add_net /Omega_TX)
    (add_net /PIR)
    (add_net /PWM_MOTOR)
    (add_net /SENS0_N)
    (add_net /SENS1_N)
    (add_net /SENS2_N)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad3)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 1)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +24V)
    (add_net +3V3)
    (add_net /ETH_PWR+)
    (add_net /ETH_PWR-)
    (add_net /MOTOR1)
    (add_net /MOTOR2)
    (add_net /PPoE+)
    (add_net /SENSE)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad2)")
  )
  (net_class PowerSmall ""
    (clearance 0.15)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /USBPWR)
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 59479217)
    (at 136.398 106.172 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 4.064 0 180) (layer F.SilkS))
    (fp_text value 220nF (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 591A2C54)
    (at 106.934 109.474 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at -4.17 0.024 270) (layer F.SilkS))
    (fp_text value 15nF (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 20 /MOTOR1))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 594792E2)
    (at 124.206 109.474 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at -4.318 0 270) (layer F.SilkS))
    (fp_text value 15nF (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /MOTOR2))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 594791AF)
    (at 108.458 92.456 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at -2.54 -1.778 360) (layer F.SilkS))
    (fp_text value 22nF (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /MOTOR2))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 59479373)
    (at 102.616 100.838 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C5 (at 4.064 0 360) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 +24V))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 591A2BF1)
    (at 143.764 86.868)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C6 (at -4.254 0.106 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 594793C2)
    (at 106.934 87.376 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C7 (at -2.286 -1.778 450) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58AA84D1)
    (at 102.616 90.424 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C8 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 59479225)
    (at 151.384 92.456 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C9 (at -4.064 0 360) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5947929A)
    (at 84.836 109.728 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C10 (at 0 2.032 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 +24V))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 59479177)
    (at 86.36 86.614)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C12 (at 0.254 -1.778) (layer F.SilkS))
    (fp_text value 100nF (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.778) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D7.5mm_P2.50mm (layer F.Cu) (tedit 59479382)
    (at 96.266 102.87 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=7.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 7.5mm Electrolytic Capacitor")
    (fp_text reference C13 (at 4.826 -3.81 180) (layer F.SilkS))
    (fp_text value "22uF 25V" (at 1.25 4.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/CP_Radial_D7.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58AA84D1)
    (at 105.918 73.406 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C14 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm-3 (layer B.Cu) (tedit 59479328)
    (at 96.774 96.012 90)
    (descr "LED, diameter 5.0mm, 2 pins, diameter 5.0mm, 3 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-59EGC(Ver.17A).pdf")
    (tags "LED diameter 5.0mm 2 pins diameter 5.0mm 3 pins")
    (fp_text reference D1 (at 7.62 0 180) (layer B.SilkS))
    (fp_text value "Everlight 339-1SURSYGW/S530-A3" (at 2.54 -3.96 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad3)"))
    (model LEDs.3dshapes/LED_D5.0mm-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad locked (layer F.Cu) (tedit 591A2AD3)
    (at 78.5 73.75)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference MH1 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad locked (layer F.Cu) (tedit 591A2AB0)
    (at 156 73.75)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference MH2 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad locked (layer F.Cu) (tedit 591A2AC4)
    (at 78.75 110.25)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference MH3 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad locked (layer F.Cu) (tedit 591A2ABA)
    (at 156 110.25)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference MH4 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 591A2B96)
    (at 159.512 94.742 180)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference P1 (at -0.148 -2.62 180) (layer F.SilkS))
    (fp_text value FDI_Cable (at 0 15.03 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /Omega_RX))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /Omega_TX))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 591A2BCD)
    (at 118.872 84.582 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 4.082 0.116 180) (layer F.SilkS))
    (fp_text value 470 (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 29 /LED_GN))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D1-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 591A2BC6)
    (at 122.682 84.582 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 4.082 -0.09 180) (layer F.SilkS))
    (fp_text value 1k2 (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 30 /LED_RD))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 594791EA)
    (at 144.272 98.044 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 2k2 (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 25 /SENS0_N))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 594791F6)
    (at 140.462 106.172 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R8 (at 4.064 0 180) (layer F.SilkS))
    (fp_text value 2k2 (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 28 /SENS1_N))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 594791F0)
    (at 144.272 106.172 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at 4.064 0 180) (layer F.SilkS))
    (fp_text value 2k2 (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 27 /SENS2_N))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 594793D2)
    (at 105.156 81.788 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at -3.302 -0.254 270) (layer F.SilkS))
    (fp_text value 49.9_1% (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /ETH0_TX-))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 594793AE)
    (at 101.854 85.344)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at -1.016 -1.778) (layer F.SilkS))
    (fp_text value 49.9_1% (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 /ETH0_RX+))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 594793AA)
    (at 96.266 85.344 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 1.016 1.778 180) (layer F.SilkS))
    (fp_text value 49.9_1% (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 /ETH0_RX-))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_6mm_h4.3mm (layer B.Cu) (tedit 59479320)
    (at 89.408 91.186 180)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=4.3mm")
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 3.302 2.286 360) (layer B.SilkS))
    (fp_text value "Omron PB" (at 3.75 -6.7 180) (layer B.Fab))
    (pad 2 thru_hole circle (at 0 -4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 31 /BUTTON))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole circle (at 6.5 -4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 31 /BUTTON))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (model Buttons_Switches_THT.3dshapes/SW_PUSH_6mm_h4.3mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D7.5mm_P2.50mm (layer F.Cu) (tedit 59479391)
    (at 86.614 102.87 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=7.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 7.5mm Electrolytic Capacitor")
    (fp_text reference C11 (at -2.286 3.81 180) (layer F.SilkS))
    (fp_text value "10uF 50VDC" (at 1.25 4.81 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +24V))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D7.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA_Handsoldering (layer F.Cu) (tedit 594792CF)
    (at 74.168 114.554 270)
    (descr "Diode SMA Handsoldering")
    (tags "Diode SMA Handsoldering")
    (attr smd)
    (fp_text reference D2 (at -5.334 0 360) (layer F.SilkS))
    (fp_text value STPS1L30A (at 0 2.6 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 270) (layer F.Fab))
    (pad 1 smd rect (at -2.5 0 270) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 6 +24V))
    (pad 2 smd rect (at 2.5 0 270) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 19 /USBPWR))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA_Handsoldering (layer F.Cu) (tedit 59479191)
    (at 75.184 89.154 90)
    (descr "Diode SMA Handsoldering")
    (tags "Diode SMA Handsoldering")
    (attr smd)
    (fp_text reference D3 (at 0.254 2.794 90) (layer F.SilkS))
    (fp_text value STPS1L30A (at 0 2.6 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 90) (layer F.Fab))
    (pad 1 smd rect (at -2.5 0 90) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 6 +24V))
    (pad 2 smd rect (at 2.5 0 90) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 18 /PPoE+))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module plan44:USB_Micro-B-SMD (layer F.Cu) (tedit 5947928F)
    (at 81.534 117.094)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (clearance 0.18)
    (attr smd)
    (fp_text reference J5 (at 0 -3.556) (layer F.SilkS))
    (fp_text value USB_Micro_AB (at 0 5.3) (layer F.Fab))
    (pad 6 thru_hole circle (at -2.25 -1.65) (size 1.1 1.1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.3 -1.35 90) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 19 /USBPWR))
    (pad 2 smd rect (at -0.65 -1.35 90) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0 -1.35 90) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.65 -1.35 90) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.3 -1.35 90) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at -4.15 1.4 90) (size 1.55 1.55) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at 4.25 1.4 90) (size 1.55 1.55) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at 2.25 -1.65) (size 1.1 1.1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_2x02_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC5)
    (at 77.47 79.502)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference P2 (at 1.27 -2.33) (layer F.SilkS))
    (fp_text value CONN_02X02 (at 1.27 4.87) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /PPoE+))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /ETH_PWR+))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /ETH_PWR-))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x02_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 594791CE)
    (at 132.842 84.582 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at -4.064 0 360) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 31 /BUTTON))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 594791D5)
    (at 132.842 74.93 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 4.064 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 32 /PWM_MOTOR))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 594791A4)
    (at 104.902 95.504 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at -4.064 0 270) (layer F.SilkS))
    (fp_text value 10R (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 20 /MOTOR1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 594791C2)
    (at 105.156 78.994 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 1.016 1.524 180) (layer F.SilkS))
    (fp_text value 49.9_1% (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /ETH0_TX+))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module plan44:STELVIO-2P-508 (layer F.Cu) (tedit 59479263)
    (at 110.49 113.792 180)
    (attr virtual)
    (fp_text reference J1 (at 12.7 3.302 360) (layer F.SilkS))
    (fp_text value STELVIO-2P-508 (at 12.7 -11.43 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 15.24 0 180) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 6 +24V))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
  )
  (module plan44:STELVIO-4P-508 (layer F.Cu) (tedit 59479274)
    (at 124.46 113.792 180)
    (attr virtual)
    (fp_text reference J2 (at 7.62 3.048 360) (layer F.SilkS))
    (fp_text value STELVIO-4P-508 (at 7.62 -11.43 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 15.24 0 180) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 20 /MOTOR1))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 22 /MOTOR2))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 25 /SENS0_N))
    (pad 4 thru_hole circle (at 0 0 180) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59479230)
    (at 155.702 94.742 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0 -2.54 180) (layer F.SilkS))
    (fp_text value PIR (at 0 7.41 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /PIR))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module plan44:HLJ-6115ANL (layer F.Cu) (tedit 5947930C)
    (at 93.98 71.628)
    (descr "ETHERNET CONNECTOR (MAGJACK) FOR POE")
    (tags "ETHERNET CONNECTOR (MAGJACK) FOR POE")
    (attr virtual)
    (fp_text reference J6 (at -11.684 -6.096 180) (layer F.SilkS))
    (fp_text value HLJ-6115ANL (at -1.4 -8.75) (layer F.Fab))
    (pad "" np_thru_hole circle (at 4.45 -0.5) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 3.15468 5.8801) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 9 /ETH0_TX+))
    (pad 2 thru_hole circle (at 1.88468 8.4201) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 10 /ETH0_TX-))
    (pad 3 thru_hole circle (at 0.61468 5.8801) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 11 /ETH0_RX+))
    (pad 4 thru_hole circle (at -0.65278 8.4201) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 24 "Net-(C14-Pad1)"))
    (pad 5 thru_hole circle (at -1.92278 5.8801) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 24 "Net-(C14-Pad1)"))
    (pad 6 thru_hole circle (at -3.19278 8.4201) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 12 /ETH0_RX-))
    (pad 7 thru_hole circle (at -4.46278 5.8801) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 13 /ETH_PWR+))
    (pad 8 thru_hole circle (at -5.73278 8.4201) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 14 /ETH_PWR-))
    (pad 9 thru_hole circle (at 5.36956 -5.36956) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad 10 thru_hole circle (at 2.82956 -5.36956) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad 11 thru_hole circle (at -5.32892 -5.36956) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad 12 thru_hole circle (at -7.86892 -5.36956) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad S1 thru_hole circle (at 6.477 2.54) (size 3.048 3.048) (drill 1.59766) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
    (pad S2 thru_hole circle (at -9.017 2.54) (size 3.048 3.048) (drill 1.59766) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
    (pad "" np_thru_hole circle (at -6.95 -0.5) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
  )
  (module plan44:ONION-OMEGA (layer F.Cu) (tedit 59479302)
    (at 130.81 79.248 270)
    (descr "FOOTPRINT FOR ONION OMEGA")
    (tags "FOOTPRINT FOR ONION OMEGA")
    (attr virtual)
    (fp_text reference U1 (at -12.192 -22.352 360) (layer F.SilkS))
    (fp_text value ONION-OMEGA2 (at 0.20828 18.96364 270) (layer F.SilkS))
    (pad B1 thru_hole rect (at 12.39774 -13.99794 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
    (pad B2 thru_hole circle (at 12.39774 -11.99896 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 4 +3V3))
    (pad B3 thru_hole circle (at 12.39774 -9.99998 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad B4 thru_hole circle (at 12.39774 -7.99846 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad B5 thru_hole circle (at 12.39774 -5.99948 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 15 /Omega_RX))
    (pad B6 thru_hole circle (at 12.39774 -3.99796 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 16 /Omega_TX))
    (pad B7 thru_hole circle (at 12.39774 -1.99898 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 31 /BUTTON))
    (pad B8 thru_hole circle (at 12.39774 0 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad B9 thru_hole circle (at 12.39774 1.99898 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 10 /ETH0_TX-))
    (pad B10 thru_hole circle (at 12.39774 3.99796 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 9 /ETH0_TX+))
    (pad B11 thru_hole circle (at 12.39774 5.99948 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 12 /ETH0_RX-))
    (pad B12 thru_hole circle (at 12.39774 7.99846 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 11 /ETH0_RX+))
    (pad B13 thru_hole circle (at 12.39774 9.99998 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 30 /LED_RD))
    (pad B14 thru_hole circle (at 12.39774 11.99896 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 29 /LED_GN))
    (pad B15 thru_hole circle (at 12.39774 13.99794 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 35 /I2C_C))
    (pad B16 thru_hole circle (at 12.39774 15.99946 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 36 /I2C_D))
    (pad A1 thru_hole rect (at -11.99896 -13.99794 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
    (pad A2 thru_hole circle (at -11.99896 -11.99896 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 26 /PIR))
    (pad A3 thru_hole circle (at -11.99896 -9.99998 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 34 /EN1_MOTOR))
    (pad A4 thru_hole circle (at -11.99896 -7.99846 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 33 /EN2_MOTOR))
    (pad A5 thru_hole circle (at -11.99896 -5.99948 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 27 /SENS2_N))
    (pad A6 thru_hole circle (at -11.99896 -3.99796 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 28 /SENS1_N))
    (pad A7 thru_hole circle (at -11.99896 -1.99898 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad A8 thru_hole circle (at -11.99896 0 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 32 /PWM_MOTOR))
    (pad A9 thru_hole circle (at -11.99896 1.99898 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad A10 thru_hole circle (at -11.99896 3.99796 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad A11 thru_hole circle (at -11.99896 5.99948 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad A12 thru_hole circle (at -11.99896 7.99846 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad A13 thru_hole circle (at -11.99896 9.99998 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad A14 thru_hole circle (at -11.99896 11.99896 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad A15 thru_hole circle (at -11.99896 13.99794 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 25 /SENS0_N))
    (pad A16 thru_hole circle (at -11.99896 15.99946 270) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
  )
  (module Housings_DIP:DIP-18_W7.62mm_LongPads (layer F.Cu) (tedit 5947920C)
    (at 126.492 98.806 270)
    (descr "18-lead dip package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference U2 (at -2.54 -0.762 360) (layer F.SilkS))
    (fp_text value L6202 (at 3.81 22.71 270) (layer F.Fab))
    (fp_text user %R (at 3.81 10.16 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /SENSE))
    (pad 10 thru_hole oval (at 7.62 20.32 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /MOTOR1))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /PWM_MOTOR))
    (pad 11 thru_hole oval (at 7.62 17.78 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 7.62 15.24 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /EN1_MOTOR))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 13 thru_hole oval (at 7.62 12.7 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 14 thru_hole oval (at 7.62 10.16 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 15 thru_hole oval (at 7.62 7.62 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 7.62 5.08 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /EN2_MOTOR))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /MOTOR2))
    (pad 17 thru_hole oval (at 7.62 2.54 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(C3-Pad1)"))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +24V))
    (pad 18 thru_hole oval (at 7.62 0 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-18_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6_Handsoldering (layer F.Cu) (tedit 5947921E)
    (at 138.938 98.552 90)
    (descr "6-pin SOT-23 package, Handsoldering")
    (tags "SOT-23-6 Handsoldering")
    (attr smd)
    (fp_text reference U3 (at 3.302 -1.016 180) (layer F.SilkS))
    (fp_text value MCP3421A0T-E/CH (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 -0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 37 /SENSE))
    (pad 2 smd rect (at -1.35 0 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.35 0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 35 /I2C_C))
    (pad 4 smd rect (at 1.35 0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 36 /I2C_D))
    (pad 6 smd rect (at 1.35 -0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1.35 0 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module plan44:STELVIO-4P-508 (layer F.Cu) (tedit 59479284)
    (at 148.59 113.792 180)
    (attr virtual)
    (fp_text reference J4 (at 7.366 3.048 360) (layer F.SilkS))
    (fp_text value STELVIO-4P-508 (at 7.62 -11.43 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 15.24 0 180) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 28 /SENS1_N))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 27 /SENS2_N))
    (pad 4 thru_hole circle (at 0 0 180) (size 2.54 2.54) (drill 1.19888) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
  )
  (module plan44:Recom-R78Cxx (layer F.Cu) (tedit 594792C4)
    (at 79.756 98.044 270)
    (descr "Recom R-78HBxx.0.5")
    (tags "Recom DCDC R-78")
    (fp_text reference U4 (at 9.398 5.588 360) (layer F.SilkS))
    (fp_text value Recom_R78Cxx (at 2.4 -3.2 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole oval (at 5.08 0 270) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 6 +24V))
    (pad 3 thru_hole oval (at 0 0 270) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 4 +3V3))
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 594792A1)
    (at 92.202 108.204)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C15 (at 0 2.032) (layer F.SilkS))
    (fp_text value 100nF (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module plan44:CRM2512_current_sense_R (layer F.Cu) (tedit 594791FF)
    (at 127.254 100.838 90)
    (fp_text reference R5 (at 3.048 4.318 180) (layer F.SilkS))
    (fp_text value 1R/2W (at -1.7 1 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7 4.2 90) (size 2.54 3.7) (layers F.Cu F.Paste F.Mask)
      (net 37 /SENSE))
    (pad 1 smd rect (at -4.4 4.2 90) (size 2.54 3.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (gr_text "DCMotor\nController\n© plan44.ch" (at 160.782 102.362) (layer F.SilkS))
  (dimension 2.9 (width 0.3) (layer Dwgs.User)
    (gr_text "2.900 mm" (at 39 130.3 270) (layer Dwgs.User))
    (feature1 (pts (xy 67.8 123.6) (xy 36.4 123.6)))
    (feature2 (pts (xy 67.8 120.7) (xy 36.4 120.7)))
    (crossbar (pts (xy 39.1 120.7) (xy 39.1 123.6)))
    (arrow1a (pts (xy 39.1 123.6) (xy 38.513579 122.473496)))
    (arrow1b (pts (xy 39.1 123.6) (xy 39.686421 122.473496)))
    (arrow2a (pts (xy 39.1 120.7) (xy 38.513579 121.826504)))
    (arrow2b (pts (xy 39.1 120.7) (xy 39.686421 121.826504)))
  )
  (dimension 2.9 (width 0.3) (layer Dwgs.User)
    (gr_text "2.900 mm" (at 34.9 53.7 90) (layer Dwgs.User))
    (feature1 (pts (xy 67.8 60.3) (xy 32 60.3)))
    (feature2 (pts (xy 67.8 63.2) (xy 32 63.2)))
    (crossbar (pts (xy 34.7 63.2) (xy 34.7 60.3)))
    (arrow1a (pts (xy 34.7 60.3) (xy 35.286421 61.426504)))
    (arrow1b (pts (xy 34.7 60.3) (xy 34.113579 61.426504)))
    (arrow2a (pts (xy 34.7 63.2) (xy 35.286421 62.073496)))
    (arrow2b (pts (xy 34.7 63.2) (xy 34.113579 62.073496)))
  )
  (gr_line (start 72 120) (end 72 64) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.5 120) (end 72 120) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.5 64) (end 162.5 120) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72 64) (end 162.5 64) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 108 (width 0.3) (layer Dwgs.User)
    (gr_text "108.000 mm" (at 117.25 36.75) (layer Dwgs.User))
    (feature1 (pts (xy 171.25 73.8) (xy 171.25 35.4)))
    (feature2 (pts (xy 63.25 73.8) (xy 63.25 35.4)))
    (crossbar (pts (xy 63.25 38.1) (xy 171.25 38.1)))
    (arrow1a (pts (xy 171.25 38.1) (xy 170.123496 38.686421)))
    (arrow1b (pts (xy 171.25 38.1) (xy 170.123496 37.513579)))
    (arrow2a (pts (xy 63.25 38.1) (xy 64.376504 38.686421)))
    (arrow2b (pts (xy 63.25 38.1) (xy 64.376504 37.513579)))
  )
  (dimension 8 (width 0.3) (layer Dwgs.User)
    (gr_text "8.000 mm" (at 57 47.5) (layer Dwgs.User))
    (feature1 (pts (xy 63.25 73.8) (xy 63.25 45.05)))
    (feature2 (pts (xy 71.25 73.8) (xy 71.25 45.05)))
    (crossbar (pts (xy 71.25 47.75) (xy 63.25 47.75)))
    (arrow1a (pts (xy 63.25 47.75) (xy 64.376504 47.163579)))
    (arrow1b (pts (xy 63.25 47.75) (xy 64.376504 48.336421)))
    (arrow2a (pts (xy 71.25 47.75) (xy 70.123496 47.163579)))
    (arrow2b (pts (xy 71.25 47.75) (xy 70.123496 48.336421)))
  )
  (dimension 8 (width 0.3) (layer Dwgs.User)
    (gr_text "8.000 mm" (at 34.9 69.8 90) (layer Dwgs.User))
    (feature1 (pts (xy 67.8 63.3) (xy 36.3 63.3)))
    (feature2 (pts (xy 67.8 71.3) (xy 36.3 71.3)))
    (crossbar (pts (xy 39 71.3) (xy 39 63.3)))
    (arrow1a (pts (xy 39 63.3) (xy 39.586421 64.426504)))
    (arrow1b (pts (xy 39 63.3) (xy 38.413579 64.426504)))
    (arrow2a (pts (xy 39 71.3) (xy 39.586421 70.173496)))
    (arrow2b (pts (xy 39 71.3) (xy 38.413579 70.173496)))
  )
  (dimension 49.5 (width 0.3) (layer Dwgs.User)
    (gr_text "49.500 mm" (at 37.7 96.05 270) (layer Dwgs.User))
    (feature1 (pts (xy 67.8 120.8) (xy 36.35 120.8)))
    (feature2 (pts (xy 67.8 71.3) (xy 36.35 71.3)))
    (crossbar (pts (xy 39.05 71.3) (xy 39.05 120.8)))
    (arrow1a (pts (xy 39.05 120.8) (xy 38.463579 119.673496)))
    (arrow1b (pts (xy 39.05 120.8) (xy 39.636421 119.673496)))
    (arrow2a (pts (xy 39.05 71.3) (xy 38.463579 72.426504)))
    (arrow2b (pts (xy 39.05 71.3) (xy 39.636421 72.426504)))
  )
  (dimension 41.5 (width 0.3) (layer Dwgs.User)
    (gr_text "41.500 mm" (at 43.35 92.05 270) (layer Dwgs.User))
    (feature1 (pts (xy 67.8 112.8) (xy 42 112.8)))
    (feature2 (pts (xy 67.8 71.3) (xy 42 71.3)))
    (crossbar (pts (xy 44.7 71.3) (xy 44.7 112.8)))
    (arrow1a (pts (xy 44.7 112.8) (xy 44.113579 111.673496)))
    (arrow1b (pts (xy 44.7 112.8) (xy 45.286421 111.673496)))
    (arrow2a (pts (xy 44.7 71.3) (xy 44.113579 72.426504)))
    (arrow2b (pts (xy 44.7 71.3) (xy 45.286421 72.426504)))
  )
  (dimension 2.5 (width 0.3) (layer Dwgs.User)
    (gr_text "2.500 mm" (at 58.4 80 90) (layer Dwgs.User))
    (feature1 (pts (xy 67.8 71.3) (xy 55.8 71.3)))
    (feature2 (pts (xy 67.8 73.8) (xy 55.8 73.8)))
    (crossbar (pts (xy 58.5 73.8) (xy 58.5 71.3)))
    (arrow1a (pts (xy 58.5 71.3) (xy 59.086421 72.426504)))
    (arrow1b (pts (xy 58.5 71.3) (xy 57.913579 72.426504)))
    (arrow2a (pts (xy 58.5 73.8) (xy 59.086421 72.673496)))
    (arrow2b (pts (xy 58.5 73.8) (xy 57.913579 72.673496)))
  )
  (dimension 92 (width 0.3) (layer Dwgs.User)
    (gr_text "92.000 mm" (at 117.25 46.4) (layer Dwgs.User))
    (feature1 (pts (xy 163.25 70.5) (xy 163.25 45.05)))
    (feature2 (pts (xy 71.25 70.5) (xy 71.25 45.05)))
    (crossbar (pts (xy 71.25 47.75) (xy 163.25 47.75)))
    (arrow1a (pts (xy 163.25 47.75) (xy 162.123496 48.336421)))
    (arrow1b (pts (xy 163.25 47.75) (xy 162.123496 47.163579)))
    (arrow2a (pts (xy 71.25 47.75) (xy 72.376504 48.336421)))
    (arrow2b (pts (xy 71.25 47.75) (xy 72.376504 47.163579)))
  )
  (dimension 7.25 (width 0.3) (layer Dwgs.User)
    (gr_text "7.250 mm" (at 84.8 43.5) (layer Dwgs.User))
    (feature1 (pts (xy 71.25 73.8) (xy 71.25 40.9)))
    (feature2 (pts (xy 78.5 73.8) (xy 78.5 40.9)))
    (crossbar (pts (xy 78.5 43.6) (xy 71.25 43.6)))
    (arrow1a (pts (xy 71.25 43.6) (xy 72.376504 43.013579)))
    (arrow1b (pts (xy 71.25 43.6) (xy 72.376504 44.186421)))
    (arrow2a (pts (xy 78.5 43.6) (xy 77.373496 43.013579)))
    (arrow2b (pts (xy 78.5 43.6) (xy 77.373496 44.186421)))
  )
  (dimension 77.5 (width 0.3) (layer Dwgs.User)
    (gr_text "77.500 mm" (at 117.25 51.75) (layer Dwgs.User))
    (feature1 (pts (xy 156 77) (xy 156 50.4)))
    (feature2 (pts (xy 78.5 77) (xy 78.5 50.4)))
    (crossbar (pts (xy 78.5 53.1) (xy 156 53.1)))
    (arrow1a (pts (xy 156 53.1) (xy 154.873496 53.686421)))
    (arrow1b (pts (xy 156 53.1) (xy 154.873496 52.513579)))
    (arrow2a (pts (xy 78.5 53.1) (xy 79.626504 53.686421)))
    (arrow2b (pts (xy 78.5 53.1) (xy 79.626504 52.513579)))
  )
  (dimension 36.5 (width 0.3) (layer Dwgs.User)
    (gr_text "36.500 mm" (at 61.45 92.05 270) (layer Dwgs.User))
    (feature1 (pts (xy 85.6 110.3) (xy 60.1 110.3)))
    (feature2 (pts (xy 85.6 73.8) (xy 60.1 73.8)))
    (crossbar (pts (xy 62.8 73.8) (xy 62.8 110.3)))
    (arrow1a (pts (xy 62.8 110.3) (xy 62.213579 109.173496)))
    (arrow1b (pts (xy 62.8 110.3) (xy 63.386421 109.173496)))
    (arrow2a (pts (xy 62.8 73.8) (xy 62.213579 74.926504)))
    (arrow2b (pts (xy 62.8 73.8) (xy 63.386421 74.926504)))
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 72.644 64.516) (xy 162.052 64.516) (xy 162.052 119.38) (xy 72.644 118.872)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 72.644 64.516) (xy 162.052 64.516) (xy 162.052 119.38) (xy 72.644 118.872)
      )
    )
  )
)
