(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6002)
    (drawings 8)
    (tracks 55)
    (zones 0)
    (modules 5)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (1 In1.Cu power hide)
    (2 In2.Cu power hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.2032)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 101.69 148.73)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-PadB8)")
  (net 3 "Net-(J1-PadA8)")
  (net 4 D+)
  (net 5 VBUS)
  (net 6 D-)
  (net 7 Shield)
  (net 8 CC2)
  (net 9 CC1)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net CC1)
    (add_net CC2)
    (add_net D+)
    (add_net D-)
    (add_net GND)
    (add_net "Net-(J1-PadA8)")
    (add_net "Net-(J1-PadB8)")
    (add_net Shield)
    (add_net VBUS)
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 96.35092 151.08712 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0.1524 1.53924 90) (layer F.SilkS))
    (fp_text value 56k (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 CC1))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 VBUS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 96.2036 142.5324)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.2) (layer Cmts.User))
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 91.74336 147.55144 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at -0.01524 1.48336 270) (layer F.SilkS))
    (fp_text value 56k (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 CC2))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 VBUS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_C_Receptacle_GCT_USB4085 (layer B.Cu) (tedit 5D743833)
    (at 94.94 151.7 90)
    (descr "USB 2.0 Type C Receptacle, https://gct.co/Files/Drawings/USB4085.pdf")
    (tags "USB Type-C Receptacle Through-hole Right angle")
    (fp_text reference J1 (at 2.7033 1.8859 90) (layer B.SilkS))
    (fp_text value USB_C_Receptacle_USB2.0 (at 2.975 -9.925 90) (layer B.Fab))
    (fp_text user %R (at 2.975 -4.025 90) (layer B.Fab))
    (fp_text user "PCB Edge" (at 2.975 -6.1 90) (layer Dwgs.User))
    (pad S1 thru_hole oval (at 7.3 -4.36 90) (size 0.9 1.7) (drill oval 0.6 1.4) (layers *.Cu *.Mask)
      (net 7 Shield))
    (pad S1 thru_hole oval (at -1.35 -4.36 90) (size 0.9 1.7) (drill oval 0.6 1.4) (layers *.Cu *.Mask)
      (net 7 Shield))
    (pad S1 thru_hole oval (at 7.3 -0.98 90) (size 0.9 2.4) (drill oval 0.6 2.1) (layers *.Cu *.Mask)
      (net 7 Shield))
    (pad S1 thru_hole oval (at -1.35 -0.98 90) (size 0.9 2.4) (drill oval 0.6 2.1) (layers *.Cu *.Mask)
      (net 7 Shield))
    (pad B6 thru_hole circle (at 3.4 -1.35 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 4 D+))
    (pad B1 thru_hole circle (at 5.95 -1.35 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B4 thru_hole circle (at 5.1 -1.35 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 5 VBUS))
    (pad B5 thru_hole circle (at 4.25 -1.35 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 8 CC2))
    (pad B12 thru_hole circle (at 0 -1.35 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B8 thru_hole circle (at 1.7 -1.35 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-PadB8)"))
    (pad B7 thru_hole circle (at 2.55 -1.35 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 6 D-))
    (pad B9 thru_hole circle (at 0.85 -1.35 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 5 VBUS))
    (pad A12 thru_hole circle (at 5.95 0 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad A9 thru_hole circle (at 5.1 0 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 5 VBUS))
    (pad A8 thru_hole circle (at 4.25 0 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-PadA8)"))
    (pad A7 thru_hole circle (at 3.4 0 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 6 D-))
    (pad A6 thru_hole circle (at 2.55 0 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 4 D+))
    (pad A5 thru_hole circle (at 1.7 0 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 9 CC1))
    (pad A4 thru_hole circle (at 0.85 0 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 5 VBUS))
    (pad A1 thru_hole circle (at 0 0 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_C_Receptacle_GCT_USB4085.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:usb-PCB (layer F.Cu) (tedit 542BB0AF)
    (at 110.33 148.73 90)
    (attr virtual)
    (fp_text reference J2 (at 0.13 -7.85 90) (layer F.Fab) hide)
    (fp_text value USB_A_PLUG (at 0.29 -10.13 90) (layer F.Fab) hide)
    (pad 2 connect rect (at 1.3 -5.15 90) (size 2 7.5) (layers F.Cu F.Mask)
      (net 6 D-))
    (pad 3 connect rect (at -1.3 -5.15 90) (size 2 7.5) (layers F.Cu F.Mask)
      (net 4 D+))
    (pad 4 connect rect (at -3.81 -4.9 90) (size 1.9 8) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 connect rect (at 3.81 -4.9 90) (size 1.9 8) (layers F.Cu F.Mask)
      (net 5 VBUS))
  )
  (gr_line (start 98.25 140.729) (end 98.25 140.729) (layer Edge.Cuts) (width 0.05))
  (gr_text "finny made this" (at 87.39488 148.87224 270) (layer F.SilkS))
  (gr_line (start 85.14952 140.72392) (end 98.25084 140.729) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 85.13936 154.75488) (end 85.14952 140.72392) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 98.25 142.75) (end 98.25 140.729) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 110.25 154.75) (end 85.13936 154.75488) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 110.25 142.75) (end 110.25 154.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 98.25 142.75) (end 110.25 142.75) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.2032) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 83.04 139.07) (xy 111.41 138.81) (xy 111.48 161.44) (xy 81.76 160.03)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.25 142.72) (xy 110.24 142.72) (xy 110.24 154.74) (xy 98.25 154.74)
      )
    )
  )
  (zone (net 7) (net_name Shield) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.2032) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 82.97 139.72) (xy 111.57 139.84) (xy 111.47 158.96) (xy 82.7 158.49)
      )
    )
  )
  (zone (net 7) (net_name Shield) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.2032) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 100.8518 158.8773) (xy 100.8137 139.3447) (xy 79.1856 137.681) (xy 79.6682 160.8458)
      )
    )
  )
  (zone (net 5) (net_name VBUS) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.2032) (thermal_bridge_width 0.2032))
    (polygon
      (pts
        (xy 79.80028 137.69116) (xy 113.40956 137.04092) (xy 112.46468 161.23188) (xy 77.4838 158.4074)
      )
    )
  )
)
