<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<text>  UV
Timer</text>
<wire x1="0" y1="0" x2="54.45125" y2="0" width="0" layer="20"/>
<wire x1="54.45125" y1="0" x2="54.45125" y2="30.7975" width="0" layer="20"/>
<wire x1="54.45125" y1="30.7975" x2="0" y2="30.7975" width="0" layer="20"/>
<wire x1="0" y1="30.7975" x2="0" y2="0" width="0" layer="20"/>
<text>Circuit by: Bogdan Raducanu</text>
<text>PCB by: Nicky</text>
</plain>
<libraries>
<library name="rcl">
<packages>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
<package name="SMC_A">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
</packages>
</library>
<library name="atmel">
<packages>
<package name="SO20L">
<description>&lt;B&gt;Small Outline Package&lt;/B&gt; SOIC 0.300"</description>
</package>
</packages>
</library>
<library name="luckylight">
<packages>
<package name="KW4">
</package>
</packages>
</library>
<library name="crystal">
<packages>
<package name="HC49/S">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="switch-omron">
<packages>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-amp-quick">
<packages>
<package name="02PA">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
<package name="03PA">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="testpad">
<packages>
<package name="TP10R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-252">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DPAK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl" package="C0805K" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="rcl" package="SMC_A" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rcl" package="C0805K" value="18p"/>
<element name="C6" library="rcl" package="C0805K" value="18p"/>
<element name="IC2" library="atmel" package="SO20L" value="ATTiny2313">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="luckylight" package="KW4" value="KW4-361ASB"/>
<element name="Q1" library="crystal" package="HC49/S" value="4MHz"/>
<element name="R1" library="rcl" package="M0805" value="680">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl" package="M0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl" package="M0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="rcl" package="M0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="rcl" package="M0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="rcl" package="M0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="rcl" package="M0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="M0805" value="680">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="M0805" value="680">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="M0805" value="680">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="M0805" value="680">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="rcl" package="M0805" value="680">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="rcl" package="M0805" value="680">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rcl" package="M0805" value="680">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="M0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="switch-omron" package="B3F-10XX" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S2" library="switch-omron" package="B3F-10XX" value=""/>
<element name="S3" library="switch-omron" package="B3F-10XX" value=""/>
<element name="S4" library="switch-omron" package="B3F-10XX" value=""/>
<element name="SL1" library="con-amp-quick" package="02PA" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SL2" library="con-amp-quick" package="03PA" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SL3" library="con-amp-quick" package="03PA" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP1" library="testpad" package="TP10R" value="PTR1TP10R">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="U1" library="SparkFun-PowerIC" package="TO-252" value="+5V">
<attribute name="PROD_ID" value="VREG-12370"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="SparkFun-DiscreteSemi" package="DPAK" value="IRLR2905">
<attribute name="PROD_ID" value="TRANS-09984"/>
</element>
</elements>
<signals>
<signal name="12V">
<contactref element="C2" pad="1"/>
<contactref element="SL1" pad="1"/>
<contactref element="SL3" pad="3"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="S2" pad="3"/>
<contactref element="S2" pad="4"/>
<contactref element="S3" pad="3"/>
<contactref element="S3" pad="4"/>
<contactref element="S4" pad="3"/>
<contactref element="S4" pad="4"/>
<contactref element="IC2" pad="10"/>
<contactref element="C4" pad="-"/>
<contactref element="C3" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="SL2" pad="1"/>
<contactref element="SL1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="3"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="R1" pad="2"/>
<contactref element="IC3" pad="11"/>
</signal>
<signal name="N$13">
<contactref element="IC3" pad="7"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="IC3" pad="10"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="IC3" pad="5"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="C1">
<contactref element="IC3" pad="12"/>
<contactref element="IC2" pad="19"/>
</signal>
<signal name="C2">
<contactref element="IC3" pad="9"/>
<contactref element="IC2" pad="16"/>
</signal>
<signal name="C3">
<contactref element="IC3" pad="8"/>
<contactref element="IC2" pad="15"/>
</signal>
<signal name="C4">
<contactref element="IC3" pad="6"/>
<contactref element="IC2" pad="12"/>
</signal>
<signal name="A">
<contactref element="R1" pad="1"/>
<contactref element="IC2" pad="18"/>
</signal>
<signal name="B">
<contactref element="R2" pad="1"/>
<contactref element="IC2" pad="14"/>
</signal>
<signal name="C">
<contactref element="R3" pad="1"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="D">
<contactref element="R4" pad="1"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="E">
<contactref element="R5" pad="1"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="F">
<contactref element="R6" pad="1"/>
<contactref element="IC2" pad="17"/>
</signal>
<signal name="G">
<contactref element="R7" pad="1"/>
<contactref element="IC2" pad="11"/>
</signal>
<signal name="H">
<contactref element="R8" pad="1"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="N$32">
<contactref element="IC2" pad="1"/>
<contactref element="TP1" pad="TP"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="IC2" pad="20"/>
<contactref element="C4" pad="+"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="ON">
<contactref element="IC2" pad="8"/>
<contactref element="Q3" pad="1"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="PAUSE">
<contactref element="R11" pad="2"/>
<contactref element="IC2" pad="9"/>
</signal>
<signal name="RED_LED">
<contactref element="R11" pad="1"/>
<contactref element="SL2" pad="2"/>
<contactref element="SL3" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="S1" pad="1"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="S2" pad="1"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="S1">
<contactref element="R12" pad="2"/>
<contactref element="IC3" pad="4"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="S2">
<contactref element="R13" pad="2"/>
<contactref element="IC3" pad="3"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="S3">
<contactref element="R14" pad="2"/>
<contactref element="IC3" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="S4">
<contactref element="R15" pad="2"/>
<contactref element="IC3" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R14" pad="1"/>
<contactref element="S3" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R15" pad="1"/>
<contactref element="S4" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="IC2" pad="4"/>
<contactref element="C6" pad="2"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="IC2" pad="5"/>
<contactref element="C5" pad="2"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="UV_LED">
<contactref element="SL3" pad="1"/>
<contactref element="Q3" pad="4"/>
</signal>
<signal name="UV_GND">
<contactref element="R10" pad="1"/>
<contactref element="SL2" pad="3"/>
<contactref element="Q3" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
