(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~86~ubuntu16.04.1)
  (general
    (thickness 1.6)
    (drawings 65)
    (tracks 570)
    (zones 0)
    (modules 83)
    (nets 46)
  )
  (page USLetter)
  (title_block
    (title "Active Balun - Version 1")
    (date 2020-06-03)
    (rev -)
    (company "Amateur Radio")
    (comment 2 creativecommons.org/licenses/by/4.0/)
    (comment 3 "License: CC BY 4.0")
    (comment 4 "Author: Zach Leffke, KJ4QLP")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1.27)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 0.889)
    (user_trace_width 1.016)
    (user_trace_width 1.27)
    (user_trace_width 1.524)
    (user_trace_width 1.778)
    (user_trace_width 2.032)
    (trace_clearance 0.254)
    (zone_clearance 0.762)
    (zone_45_only no)
    (trace_min 0.254)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (user_via 0.762 0.381)
    (user_via 1.016 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 12.065 12.065)
    (pad_drill 12.065)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFDFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(A1-Pad1)")
  (net 2 "Net-(B1-Pad1)")
  (net 3 "Net-(C1-Pad1)")
  (net 4 GND)
  (net 5 "Net-(C2-Pad2)")
  (net 6 "Net-(C3-Pad1)")
  (net 7 "Net-(C4-Pad1)")
  (net 8 "Net-(C4-Pad2)")
  (net 9 "Net-(C5-Pad1)")
  (net 10 "Net-(C5-Pad2)")
  (net 11 "Net-(C6-Pad2)")
  (net 12 "Net-(C7-Pad1)")
  (net 13 "Net-(C7-Pad2)")
  (net 14 "Net-(C8-Pad1)")
  (net 15 "Net-(C9-Pad2)")
  (net 16 "Net-(C10-Pad2)")
  (net 17 "Net-(C12-Pad2)")
  (net 18 "Net-(FB1-Pad1)")
  (net 19 "Net-(FB2-Pad1)")
  (net 20 "Net-(FB3-Pad2)")
  (net 21 +8V)
  (net 22 "Net-(R3-Pad1)")
  (net 23 "Net-(D7-Pad2)")
  (net 24 "Net-(A2-Pad1)")
  (net 25 "Net-(B2-Pad1)")
  (net 26 "Net-(JP1-Pad2)")
  (net 27 "Net-(JP1-Pad1)")
  (net 28 "Net-(JP2-Pad1)")
  (net 29 "Net-(C16-Pad1)")
  (net 30 "Net-(C11-Pad1)")
  (net 31 VCC)
  (net 32 "Net-(C14-Pad2)")
  (net 33 "Net-(C16-Pad2)")
  (net 34 "Net-(JP4-Pad2)")
  (net 35 "Net-(JP5-Pad2)")
  (net 36 "Net-(JP6-Pad2)")
  (net 37 "Net-(C17-Pad1)")
  (net 38 "Net-(C18-Pad1)")
  (net 39 "Net-(C19-Pad1)")
  (net 40 "Net-(C19-Pad2)")
  (net 41 "Net-(C20-Pad2)")
  (net 42 "Net-(C21-Pad2)")
  (net 43 "Net-(JP2-Pad3)")
  (net 44 "Net-(C13-Pad2)")
  (net 45 "Net-(C22-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.254)
    (diff_pair_gap 0.254)
    (add_net +8V)
    (add_net GND)
    (add_net "Net-(A1-Pad1)")
    (add_net "Net-(A2-Pad1)")
    (add_net "Net-(B1-Pad1)")
    (add_net "Net-(B2-Pad1)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(C14-Pad2)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C16-Pad2)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C19-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C20-Pad2)")
    (add_net "Net-(C21-Pad2)")
    (add_net "Net-(C22-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(FB1-Pad1)")
    (add_net "Net-(FB2-Pad1)")
    (add_net "Net-(FB3-Pad2)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(JP2-Pad1)")
    (add_net "Net-(JP2-Pad3)")
    (add_net "Net-(JP4-Pad2)")
    (add_net "Net-(JP5-Pad2)")
    (add_net "Net-(JP6-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net VCC)
  )
  (module TestPoint:TestPoint_Pad_2.5x2.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 117.475 136.525)
    (descr "SMD rectangular pad as test Point, square 2.5mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP6 (at 0 9.525) (layer F.SilkS))
    (fp_text value GND (at 0 2.25) (layer F.Fab))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2.5 2.5) (layers F.Cu F.Mask)
      (net 4 GND))
  )
  (module TestPoint:TestPoint_Pad_2.5x2.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 136.525 117.475)
    (descr "SMD rectangular pad as test Point, square 2.5mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP5 (at 9.525 0) (layer F.SilkS))
    (fp_text value GND (at 0 2.25) (layer F.Fab))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2.5 2.5) (layers F.Cu F.Mask)
      (net 4 GND))
  )
  (module TestPoint:TestPoint_Pad_2.5x2.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 98.425 79.375)
    (descr "SMD rectangular pad as test Point, square 2.5mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP4 (at 0 -8.255) (layer F.SilkS))
    (fp_text value GND (at 0 2.25) (layer F.Fab))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2.5 2.5) (layers F.Cu F.Mask)
      (net 4 GND))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 5EE6FAF0)
    (at 132.645704 83.254296)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference G4 (at 3.81 -5.715) (layer F.SilkS))
    (fp_text value GND (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 0 0.069296) (size 6.4 6.4) (drill 3.200001) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 56DDBCCA)
    (at 83.254296 132.645704)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference G3 (at -7.054296 3.879296) (layer F.SilkS))
    (fp_text value GND (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 128.27 102.235 180)
    (attr smd)
    (fp_text reference C15 (at 0 -1.27) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 1.05 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 21 +8V))
  )
  (module NetTie:NetTie-2_SMD_Pad0.5mm (layer F.Cu) (tedit 5A1CF6D3)
    (at 107.95 120.015 270)
    (descr "Net tie, 2 pin, 0.5mm square SMD pads")
    (tags "net tie")
    (attr virtual)
    (fp_text reference JP7 (at 0 -2.54 180) (layer F.SilkS))
    (fp_text value " " (at 0 1.2 90) (layer F.Fab))
    (pad 2 smd circle (at 0.5 0 270) (size 0.5 0.5) (layers F.Cu)
      (net 13 "Net-(C7-Pad2)"))
    (pad 1 smd circle (at -0.5 0 270) (size 0.5 0.5) (layers F.Cu)
      (net 26 "Net-(JP1-Pad2)"))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5EE6FC27)
    (at 125.73 90.17)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H3 (at 12.7 -10.795) (layer F.SilkS))
    (fp_text value conn_pass (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 12.065 12.065) (drill 12.065) (layers *.Cu *.Mask))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 115.316 122.174 90)
    (attr smd)
    (fp_text reference C21 (at -2.921 -1.651 90) (layer F.SilkS))
    (fp_text value 4700pF (at 0 1.95 90) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 1.05 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(C21-Pad2)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 117.348 117.856 270)
    (attr smd)
    (fp_text reference C20 (at 0 -1.524 90) (layer F.SilkS))
    (fp_text value 1500pF (at 0 1.95 90) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 1.05 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C20-Pad2)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 112.268 118.872)
    (attr smd)
    (fp_text reference C19 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 4700pF (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C19-Pad1)"))
    (pad 2 smd rect (at 1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C19-Pad2)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 116.332 125.222 180)
    (attr smd)
    (fp_text reference C18 (at 0 -1.84) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 1.05 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 115.316 114.046 90)
    (attr smd)
    (fp_text reference C17 (at 0 -1.524 90) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.95 90) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 1.05 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 98.425 130.175 180)
    (attr smd)
    (fp_text reference C16 (at 3.175 0) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C16-Pad1)"))
    (pad 2 smd rect (at 1.05 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C16-Pad2)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 128.27 113.665 180)
    (attr smd)
    (fp_text reference C14 (at 0 1.27) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 1.05 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C14-Pad2)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 87.63 102.235)
    (attr smd)
    (fp_text reference C13 (at 0 1.27) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C13-Pad2)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 87.63 113.665)
    (attr smd)
    (fp_text reference C12 (at 0 -1.27) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C12-Pad2)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 120.015 130.175)
    (attr smd)
    (fp_text reference C11 (at 0 1.397) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 100.965 123.19 180)
    (attr smd)
    (fp_text reference C10 (at 2.413 0 90) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 1.05 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C10-Pad2)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 100.965 116.84 180)
    (attr smd)
    (fp_text reference C9 (at 2.413 0 90) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 1.05 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C9-Pad2)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 102.455 130.175 180)
    (attr smd)
    (fp_text reference C8 (at 0 -1.524) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1.05 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C16-Pad1)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 106.9 123.825)
    (attr smd)
    (fp_text reference C7 (at -2.506 0.127) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C7-Pad2)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 87.63 107.95)
    (attr smd)
    (fp_text reference C6 (at -2.54 0) (layer F.SilkS))
    (fp_text value 1000pF (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(B1-Pad1)"))
    (pad 2 smd rect (at 1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C6-Pad2)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 101.6 107.95)
    (attr smd)
    (fp_text reference C5 (at 0 -1.27) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C5-Pad2)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 114.3 107.95)
    (attr smd)
    (fp_text reference C4 (at 0 -1.27) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C4-Pad2)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 128.27 107.95)
    (attr smd)
    (fp_text reference C3 (at 2.54 0) (layer F.SilkS))
    (fp_text value 1000pF (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(A1-Pad1)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 103.505 101.6)
    (attr smd)
    (fp_text reference C2 (at 0 -1.27) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C2-Pad2)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 112.395 101.6)
    (attr smd)
    (fp_text reference C1 (at 0 -1.27) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 122.555 119.38 225)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.82 45) (layer F.SilkS))
    (fp_text value 33 (at 0 1.82 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 225) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 30 "Net-(C11-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 225) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 32 "Net-(C14-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 106.68 100.2 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -1.14 1.905 90) (layer F.SilkS))
    (fp_text value 30 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 5 "Net-(C2-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 21 +8V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 109.22 100.2 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -1.14 -1.82 90) (layer F.SilkS))
    (fp_text value 30 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 "Net-(C1-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 21 +8V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 112.268 121.158 180)
    (attr smd)
    (fp_text reference L12 (at 2.54 -2.286 270) (layer F.SilkS))
    (fp_text value 100nH (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(C21-Pad2)"))
    (pad 2 smd rect (at 1.05 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(JP2-Pad3)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 117.348 122.174 270)
    (attr smd)
    (fp_text reference L11 (at 0 -1.524 90) (layer F.SilkS))
    (fp_text value 330nH (at 0 1.95 90) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C20-Pad2)"))
    (pad 2 smd rect (at 1.05 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C18-Pad1)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 115.316 117.856 90)
    (attr smd)
    (fp_text reference L10 (at 1.016 -1.524 90) (layer F.SilkS))
    (fp_text value 100nH (at 0 1.95 90) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C19-Pad2)"))
    (pad 2 smd rect (at 1.05 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C17-Pad1)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 112.268 123.19 180)
    (attr smd)
    (fp_text reference L9 (at 0 -1.524) (layer F.SilkS))
    (fp_text value 4.7uH (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 1.05 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 117.348 114.046 90)
    (attr smd)
    (fp_text reference L8 (at 0 1.524 90) (layer F.SilkS))
    (fp_text value 4.7uH (at 0 1.95 90) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 1.05 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391EB7)
    (at 105.41 116.205 180)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP5 (at 1.905 1.905 270) (layer F.SilkS))
    (fp_text value " " (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0 0 180) (size 1 1.5) (layers F.Cu F.Mask)
      (net 35 "Net-(JP5-Pad2)"))
    (pad 3 smd custom (at 1.3 0 180) (size 1 0.5) (layers F.Cu F.Mask)
      (net 4 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy -0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy -0.55 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -1.3 0 180) (size 1 0.5) (layers F.Cu F.Mask)
      (net 26 "Net-(JP1-Pad2)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391EB7)
    (at 110.49 116.205)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP4 (at 1.905 -1.905 90) (layer F.SilkS))
    (fp_text value " " (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0 0) (size 1 1.5) (layers F.Cu F.Mask)
      (net 34 "Net-(JP4-Pad2)"))
    (pad 3 smd custom (at 1.3 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 4 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy -0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy -0.55 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -1.3 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 26 "Net-(JP1-Pad2)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391EB7)
    (at 107.95 121.285)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value " " (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0 0) (size 1 1.5) (layers F.Cu F.Mask)
      (net 13 "Net-(C7-Pad2)"))
    (pad 3 smd custom (at 1.3 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 43 "Net-(JP2-Pad3)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy -0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy -0.55 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -1.3 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 28 "Net-(JP2-Pad1)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391EB7)
    (at 107.95 118.745)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value " " (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0 0) (size 1 1.5) (layers F.Cu F.Mask)
      (net 26 "Net-(JP1-Pad2)"))
    (pad 3 smd custom (at 1.3 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 39 "Net-(C19-Pad1)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy -0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy -0.55 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -1.3 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 27 "Net-(JP1-Pad1)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)) (width 0))
      ))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 127.635 118.745 315)
    (attr smd)
    (fp_text reference R5 (at 0 -1.796051 135) (layer F.SilkS))
    (fp_text value 470 (at 0 1.95 135) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 315) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C14-Pad2)"))
    (pad 2 smd rect (at 1.05 0 315) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D7-Pad2)"))
  )
  (module Package_TO_SOT_SMD:SOT-89-3 (layer F.Cu) (tedit 5C33D6E8)
    (at 107.315 127.635)
    (descr "SOT-89-3, http://ww1.microchip.com/downloads/en/DeviceDoc/3L_SOT-89_MB_C04-029C.pdf")
    (tags SOT-89-3)
    (attr smd)
    (fp_text reference U3 (at 0 3.175) (layer F.SilkS))
    (fp_text value GALI-6 (at 0.3 3.5) (layer F.Fab))
    (fp_text user %R (at 0.5 0 90) (layer F.Fab))
    (pad 2 smd custom (at -1.5625 0) (size 1.475 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.7375 -0.8665) (xy 3.8625 -0.8665) (xy 3.8625 0.8665) (xy 0.7375 0.8665)) (width 0))
      ))
    (pad 3 smd rect (at -1.65 1.5) (size 1.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C8-Pad1)"))
    (pad 1 smd rect (at -1.65 -1.5) (size 1.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-263-2 (layer F.Cu) (tedit 5A70FB7B)
    (at 109.22 90.805)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404")
    (attr smd)
    (fp_text reference U4 (at 6.985 -6.35) (layer F.SilkS))
    (fp_text value L7808 (at 0 6.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd rect (at 0.95 2.775) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 5.8 -2.775) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 0.95 -2.775) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 5.8 2.775) (size 4.55 5.25) (layers F.Paste))
    (pad 2 smd rect (at 3.375 0) (size 9.4 10.8) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 3 smd rect (at -5.775 2.54) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 21 +8V))
    (pad 1 smd rect (at -5.775 -2.54) (size 4.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(C22-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-263-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_1812_4532Metric (layer F.Cu) (tedit 5B301BBE)
    (at 97.79 133.35)
    (descr "Inductor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference GDT1 (at -3.81 0 90) (layer F.SilkS))
    (fp_text value " " (at 0 2.65) (layer F.Fab))
    (fp_text user %R (at 0 0.635) (layer F.Fab))
    (pad 2 smd roundrect (at 2.1375 0) (size 1.125 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 4 GND))
    (pad 1 smd roundrect (at -2.1375 0) (size 1.125 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 33 "Net-(C16-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1812_4532Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_1008_2520Metric (layer F.Cu) (tedit 5D4AF589)
    (at 91.44 117.035 90)
    (descr "Inductor SMD 1008 (2520 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://ecsxtal.com/store/pdf/ECS-MPI2520-SMD-POWER-INDUCTOR.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L6 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 4.7uH (at 0 2.05 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.075 0 90) (size 1.25 2.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 17 "Net-(C12-Pad2)"))
    (pad 1 smd roundrect (at -1.075 0 90) (size 1.25 2.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 31 VCC))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1008_2520Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMB_Handsoldering (layer F.Cu) (tedit 590B3D55)
    (at 97.79 91.44 270)
    (descr "Diode SMB (DO-214AA) Handsoldering")
    (tags "Diode SMB (DO-214AA) Handsoldering")
    (attr smd)
    (fp_text reference D8 (at 0 2.694077 90) (layer F.SilkS))
    (fp_text value MBRS2040LT3G (at 0 3 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.796051 90) (layer F.Fab))
    (pad 2 smd rect (at 2.7 0 270) (size 3.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C13-Pad2)"))
    (pad 1 smd rect (at -2.7 0 270) (size 3.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(C22-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 94.615 121.285 225)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP3 (at 0 1.796051 45) (layer F.SilkS))
    (fp_text value " " (at 0 1.9 45) (layer F.Fab))
    (pad 2 smd custom (at 0.65 0 225) (size 1 0.5) (layers F.Cu F.Mask)
      (net 33 "Net-(C16-Pad2)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 225) (size 1 0.5) (layers F.Cu F.Mask)
      (net 31 VCC) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 107.95 106.045 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP6 (at -2.54 0 270) (layer F.SilkS))
    (fp_text value " " (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 36 "Net-(JP6-Pad2)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 4 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 112.395 130.175)
    (attr smd)
    (fp_text reference FB3 (at 0 1.397) (layer F.SilkS))
    (fp_text value FBval (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(FB3-Pad2)"))
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 97.79 127.635 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D6 (at -1.905 0 180) (layer F.SilkS))
    (fp_text value 1N4148WS (at 0.1 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 270) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C16-Pad1)"))
    (pad 1 smd rect (at -1.05 0 270) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 99.695 127.635 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D5 (at 1.905 0 180) (layer F.SilkS))
    (fp_text value 1N4148WS (at 0.1 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 90) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1.05 0 90) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C16-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 87.63 109.855 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D4 (at 2.54 0) (layer F.SilkS))
    (fp_text value 1N4148WS (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(B1-Pad1)"))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 87.63 106.045)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D3 (at -2.54 0) (layer F.SilkS))
    (fp_text value 1N4148WS (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(B1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 128.27 106.045)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D2 (at 2.54 0) (layer F.SilkS))
    (fp_text value 1N4148WS (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(A1-Pad1)"))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 128.27 109.855 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1 (at -2.54 0) (layer F.SilkS))
    (fp_text value 1N4148WS (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(A1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_2.5x2.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 79.375 98.425 90)
    (descr "SMD rectangular pad as test Point, square 2.5mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP3 (at 0 -8.255 90) (layer F.SilkS))
    (fp_text value GND (at 0 2.25 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.15 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 2.5 2.5) (layers F.Cu F.Mask)
      (net 4 GND))
  )
  (module TestPoint:TestPoint_Pad_2.5x2.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 85.725 98.425 90)
    (descr "SMD rectangular pad as test Point, square 2.5mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP2 (at 0 -14.605 90) (layer F.SilkS))
    (fp_text value +V (at 0 2.25 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.15 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 2.5 2.5) (layers F.Cu F.Mask)
      (net 44 "Net-(C13-Pad2)"))
  )
  (module digikey-footprints:Jumper_Tin_P10.9mm (layer F.Cu) (tedit 5D28919E)
    (at 124.46 107.95 270)
    (attr smd)
    (fp_text reference J2 (at 7.62 0 180) (layer F.SilkS))
    (fp_text value S1621-46R (at 0 2.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 5.45 0 270) (size 2.4 2.8) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C14-Pad2)"))
    (pad 1 smd rect (at -5.45 0 270) (size 2.4 2.8) (layers F.Cu F.Paste F.Mask)
      (net 21 +8V))
  )
  (module digikey-footprints:Jumper_Tin_P10.9mm (layer F.Cu) (tedit 5D28919E)
    (at 91.44 107.95 270)
    (attr smd)
    (fp_text reference J3 (at -7.62 0 180) (layer F.SilkS))
    (fp_text value S1621-46R (at 0 2.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 5.45 0 270) (size 2.4 2.8) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C12-Pad2)"))
    (pad 1 smd rect (at -5.45 0 270) (size 2.4 2.8) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C13-Pad2)"))
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-3528-15_AVX-H (layer F.Cu) (tedit 5B342532)
    (at 101.6 85.09)
    (descr "Tantalum Capacitor SMD AVX-H (3528-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C22 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.35) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.5375 0) (size 1.325 2.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 45 "Net-(C22-Pad2)"))
    (pad 1 smd roundrect (at -1.5375 0) (size 1.325 2.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3528-15_AVX-H.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 56DDBCCA)
    (at 90.17 90.17)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference G2 (at -11.43 -11.43 45) (layer F.SilkS))
    (fp_text value GND (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 56DDBCCA)
    (at 125.73 125.73)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference G1 (at 11.43 11.43 45) (layer F.SilkS))
    (fp_text value GND (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 132.645704 132.645704)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H2 (at 5.149296 5.149296) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 83.254296 83.254296)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H1 (at -5.149296 -5.149296) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.7mm_Pad_Via (layer F.Cu) (tedit 56DDBE44)
    (at 107.95 79.375)
    (descr "Mounting Hole 3.7mm")
    (tags "mounting hole 3.7mm")
    (attr virtual)
    (fp_text reference B2 (at 5.715 0 90) (layer F.SilkS))
    (fp_text value RIGHT (at 0 4.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.962221 -1.962221) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 25 "Net-(B2-Pad1)"))
    (pad 1 thru_hole circle (at 0 -2.775) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 25 "Net-(B2-Pad1)"))
    (pad 1 thru_hole circle (at -1.962221 -1.962221) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 25 "Net-(B2-Pad1)"))
    (pad 1 thru_hole circle (at -2.775 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 25 "Net-(B2-Pad1)"))
    (pad 1 thru_hole circle (at -1.962221 1.962221) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 25 "Net-(B2-Pad1)"))
    (pad 1 thru_hole circle (at 0 2.775) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 25 "Net-(B2-Pad1)"))
    (pad 1 thru_hole circle (at 1.962221 1.962221) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 25 "Net-(B2-Pad1)"))
    (pad 1 thru_hole circle (at 2.775 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 25 "Net-(B2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 7.4 7.4) (drill 3.7) (layers *.Cu *.Mask)
      (net 25 "Net-(B2-Pad1)"))
  )
  (module MountingHole:MountingHole_3.7mm_Pad_Via (layer F.Cu) (tedit 56DDBE44)
    (at 107.95 136.525)
    (descr "Mounting Hole 3.7mm")
    (tags "mounting hole 3.7mm")
    (attr virtual)
    (fp_text reference A2 (at 5.715 0 90 unlocked) (layer F.SilkS))
    (fp_text value LEFT (at 0 4.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.962221 -1.962221) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 24 "Net-(A2-Pad1)"))
    (pad 1 thru_hole circle (at 0 -2.775) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 24 "Net-(A2-Pad1)"))
    (pad 1 thru_hole circle (at -1.962221 -1.962221) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 24 "Net-(A2-Pad1)"))
    (pad 1 thru_hole circle (at -2.775 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 24 "Net-(A2-Pad1)"))
    (pad 1 thru_hole circle (at -1.962221 1.962221) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 24 "Net-(A2-Pad1)"))
    (pad 1 thru_hole circle (at 0 2.775) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 24 "Net-(A2-Pad1)"))
    (pad 1 thru_hole circle (at 1.962221 1.962221) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 24 "Net-(A2-Pad1)"))
    (pad 1 thru_hole circle (at 2.775 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 24 "Net-(A2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 7.4 7.4) (drill 3.7) (layers *.Cu *.Mask)
      (net 24 "Net-(A2-Pad1)"))
  )
  (module TestPoint:TestPoint_Pad_D2.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 83.82 118.11)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP1 (at -12.7 0 90) (layer F.SilkS))
    (fp_text value "+V TestPoint" (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -1.905) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 2 2) (layers F.Cu F.Mask)
      (net 22 "Net-(R3-Pad1)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 101.6 103.505 180)
    (attr smd)
    (fp_text reference FB2 (at 0.635 -1.524 180) (layer F.SilkS))
    (fp_text value HZ0805C202R-10 (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(FB2-Pad1)"))
    (pad 2 smd rect (at 1.05 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C5-Pad1)"))
  )
  (module Connector_Coaxial:SMA_Amphenol_132134_Vertical locked (layer F.Cu) (tedit 5B2F4DB6)
    (at 90.17 125.73 135)
    (descr https://www.amphenolrf.com/downloads/dl/file/id/2187/product/2843/132134_customer_drawing.pdf)
    (tags "SMA THT Female Jack Vertical ExtendedLegs")
    (fp_text reference J1 (at 0 -4.75 135) (layer F.SilkS))
    (fp_text value OUT (at 0 5 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54 135) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54 135) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54 135) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at 2.54 2.54 135) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 0 0 135) (size 2.05 2.05) (drill 1.5) (layers *.Cu *.Mask)
      (net 33 "Net-(C16-Pad2)"))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Amphenol_132134_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-89-3 (layer F.Cu) (tedit 5C33D6E8)
    (at 96.52 106.045 90)
    (descr "SOT-89-3, http://ww1.microchip.com/downloads/en/DeviceDoc/3L_SOT-89_MB_C04-029C.pdf")
    (tags SOT-89-3)
    (attr smd)
    (fp_text reference U2 (at 2.54 -1.905) (layer F.SilkS))
    (fp_text value GALI-74 (at 0.3 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0.5 0) (layer F.Fab))
    (pad 2 smd custom (at -1.5625 0 90) (size 1.475 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.7375 -0.8665) (xy 3.8625 -0.8665) (xy 3.8625 0.8665) (xy 0.7375 0.8665)) (width 0))
      ))
    (pad 3 smd rect (at -1.65 1.5 90) (size 1.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C5-Pad1)"))
    (pad 1 smd rect (at -1.65 -1.5 90) (size 1.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C6-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-89-3 (layer F.Cu) (tedit 5C33D6E8)
    (at 119.38 109.855 270)
    (descr "SOT-89-3, http://ww1.microchip.com/downloads/en/DeviceDoc/3L_SOT-89_MB_C04-029C.pdf")
    (tags SOT-89-3)
    (attr smd)
    (fp_text reference U1 (at 2.54 -1.905) (layer F.SilkS))
    (fp_text value GALI-74 (at 0.3 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0.5 0) (layer F.Fab))
    (pad 2 smd custom (at -1.5625 0 270) (size 1.475 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.7375 -0.8665) (xy 3.8625 -0.8665) (xy 3.8625 0.8665) (xy 0.7375 0.8665)) (width 0))
      ))
    (pad 3 smd rect (at -1.65 1.5 270) (size 1.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C4-Pad2)"))
    (pad 1 smd rect (at -1.65 -1.5 270) (size 1.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module minicircuits_footprints:Mini-Circuits_CD542_H2.84mm (layer F.Cu) (tedit 5A365E23)
    (at 107.95 110.49 90)
    (descr https://ww2.minicircuits.com/case_style/CD542.pdf)
    (tags "RF Transformer")
    (attr smd)
    (fp_text reference TR1 (at -0.635 -4.826 90) (layer F.SilkS))
    (fp_text value ADT2-1T (at 0 5.08 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 6 smd rect (at 2.54 -2.54 90) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C5-Pad2)"))
    (pad 5 smd rect (at 2.54 0 90) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(JP6-Pad2)"))
    (pad 4 smd rect (at 2.54 2.54 90) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 3 smd rect (at -2.54 2.54 90) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(JP4-Pad2)"))
    (pad 2 smd rect (at -2.54 0 90) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -2.54 -2.54 90) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(JP5-Pad2)"))
    (model ${KISYS3DMOD}/RF_Mini-Circuits.3dshapes/Mini-Circuits_CD542_H2.84mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 87.63 118.11)
    (attr smd)
    (fp_text reference R3 (at 0 1.27) (layer F.SilkS))
    (fp_text value 4.72k (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 31 VCC))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 116.205 130.175)
    (attr smd)
    (fp_text reference L7 (at 0 1.397) (layer F.SilkS))
    (fp_text value 4.7uH (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(FB3-Pad2)"))
    (pad 2 smd rect (at 1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C11-Pad1)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 102.87 121.285)
    (attr smd)
    (fp_text reference L5 (at 1.27 1.27) (layer F.SilkS))
    (fp_text value 100nH (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C10-Pad2)"))
    (pad 2 smd rect (at 1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(JP2-Pad1)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 99.822 120.015 270)
    (attr smd)
    (fp_text reference L4 (at 0 1.397 90) (layer F.SilkS))
    (fp_text value 330nH (at 0 1.95 90) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C9-Pad2)"))
    (pad 2 smd rect (at 1.05 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C10-Pad2)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 102.87 118.745 180)
    (attr smd)
    (fp_text reference L3 (at -1.27 -1.27) (layer F.SilkS))
    (fp_text value 100nH (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(JP1-Pad1)"))
    (pad 2 smd rect (at 1.05 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C9-Pad2)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 105.63 103.505 180)
    (attr smd)
    (fp_text reference L2 (at 0.22 -1.27) (layer F.SilkS))
    (fp_text value 4.7uH (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at 1.05 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(FB2-Pad1)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 110.27 103.505)
    (attr smd)
    (fp_text reference L1 (at 0.22 1.27) (layer F.SilkS))
    (fp_text value 4.7uH (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(FB1-Pad1)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 114.3 103.505)
    (attr smd)
    (fp_text reference FB1 (at 0.889 1.524) (layer F.SilkS))
    (fp_text value HZ0805C202R-10 (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(FB1-Pad1)"))
    (pad 2 smd rect (at 1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C4-Pad2)"))
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5B36C52C)
    (at 130.175 121.285 135)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D7 (at 0 1.796051 135) (layer F.SilkS))
    (fp_text value LED (at 0 1.65 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 135) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(D7-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 135) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.7mm_Pad_Via (layer F.Cu) (tedit 56DDBE44)
    (at 79.375 107.95)
    (descr "Mounting Hole 3.7mm")
    (tags "mounting hole 3.7mm")
    (attr virtual)
    (fp_text reference B1 (at 0 5.715 180) (layer F.SilkS))
    (fp_text value RIGHT (at 0 4.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.962221 -1.962221) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(B1-Pad1)"))
    (pad 1 thru_hole circle (at 0 -2.775) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(B1-Pad1)"))
    (pad 1 thru_hole circle (at -1.962221 -1.962221) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(B1-Pad1)"))
    (pad 1 thru_hole circle (at -2.775 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(B1-Pad1)"))
    (pad 1 thru_hole circle (at -1.962221 1.962221) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(B1-Pad1)"))
    (pad 1 thru_hole circle (at 0 2.775) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(B1-Pad1)"))
    (pad 1 thru_hole circle (at 1.962221 1.962221) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(B1-Pad1)"))
    (pad 1 thru_hole circle (at 2.775 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(B1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 7.4 7.4) (drill 3.7) (layers *.Cu *.Mask)
      (net 2 "Net-(B1-Pad1)"))
  )
  (module MountingHole:MountingHole_3.7mm_Pad_Via (layer F.Cu) (tedit 56DDBE44)
    (at 136.525 107.95)
    (descr "Mounting Hole 3.7mm")
    (tags "mounting hole 3.7mm")
    (attr virtual)
    (fp_text reference A1 (at 0 5.715 unlocked) (layer F.SilkS))
    (fp_text value LEFT (at 0 4.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.962221 -1.962221) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(A1-Pad1)"))
    (pad 1 thru_hole circle (at 0 -2.775) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(A1-Pad1)"))
    (pad 1 thru_hole circle (at -1.962221 -1.962221) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(A1-Pad1)"))
    (pad 1 thru_hole circle (at -2.775 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(A1-Pad1)"))
    (pad 1 thru_hole circle (at -1.962221 1.962221) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(A1-Pad1)"))
    (pad 1 thru_hole circle (at 0 2.775) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(A1-Pad1)"))
    (pad 1 thru_hole circle (at 1.962221 1.962221) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(A1-Pad1)"))
    (pad 1 thru_hole circle (at 2.775 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(A1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 7.4 7.4) (drill 3.7) (layers *.Cu *.Mask)
      (net 1 "Net-(A1-Pad1)"))
  )
  (gr_text "v1\nrev-\n" (at 137.795 98.425) (layer F.SilkS))
  (gr_text "KJ4QLP, 20200615" (at 135.255 135.255 45) (layer F.SilkS))
  (gr_text GND (at 117.475 133.985) (layer F.SilkS))
  (gr_text GND (at 133.985 117.475 90) (layer F.SilkS))
  (gr_text GND (at 98.425 81.915 180) (layer F.SilkS))
  (gr_text N/S (at 139.065 92.075) (layer F.SilkS))
  (gr_text E/W (at 77.47 125.73) (layer F.SilkS))
  (gr_text E/S (at 136.525 102.235) (layer F.SilkS))
  (gr_text S/E (at 102.235 136.525 90) (layer F.SilkS))
  (gr_text N/W (at 102.235 79.375 90) (layer F.SilkS))
  (gr_text W/N (at 79.375 102.235) (layer F.SilkS))
  (gr_text N (at 92.075 75.565) (layer F.SilkS))
  (gr_text GND (at 86.995 86.995 45) (layer F.SilkS))
  (gr_text GND (at 128.905 128.905 45) (layer F.SilkS))
  (gr_text "+V\nTEST" (at 80.01 118.11 90) (layer F.SilkS))
  (gr_text 12V (at 85.725 95.885) (layer F.SilkS))
  (gr_text GND (at 79.375 95.885) (layer F.SilkS))
  (gr_text "Do Not \nService\nWhen \nLED Is On" (at 135.89 123.825 90) (layer F.SilkS))
  (gr_text "Based on LWA FEE v1.7" (at 86.995 141.605) (layer F.SilkS))
  (gr_text SN: (at 117.475 79.375) (layer F.SilkS))
  (gr_text "Active Dipole Balun\n" (at 113.665 98.425) (layer F.SilkS))
  (gr_line (start 73.025 120.65) (end 73.025 129.54) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 73.025 129.54) (end 76.2 132.715) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 142.875 95.25) (end 142.875 86.36) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 129.54 142.875) (end 142.875 129.54) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 129.54 73.025) (end 142.875 86.36) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 73.025 86.36) (end 86.36 73.025) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 76.2 132.715) (end 86.36 142.875) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 142.875 129.54) (end 142.875 95.25) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 86.36 142.875) (end 129.54 142.875) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 73.025 86.36) (end 73.025 120.65) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 86.36 73.025) (end 129.54 73.025) (layer Edge.Cuts) (width 0.05))
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.762))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.875 86.36) (xy 142.875 129.54) (xy 129.54 142.875) (xy 86.36 142.875) (xy 73.025 129.54)
        (xy 73.025 86.36) (xy 86.36 73.025) (xy 129.54 73.025)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.762))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.875 86.36) (xy 142.875 129.54) (xy 129.54 142.875) (xy 86.36 142.875) (xy 73.025 129.54)
        (xy 73.025 86.36) (xy 86.36 73.025) (xy 129.54 73.025)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.762))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.875 86.36) (xy 142.875 129.54) (xy 129.54 142.875) (xy 86.36 142.875) (xy 73.025 129.54)
        (xy 73.025 86.36) (xy 86.36 73.025) (xy 129.54 73.025)
      )
    )
  )
)
