(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 128)
    (tracks 344)
    (zones 0)
    (modules 38)
    (nets 39)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.381)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (trace_clearance 0.2)
    (zone_clearance 0.762)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1.5)
    (via_drill 1)
    (via_min_size 0)
    (via_min_drill 0)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "GABE_project/"))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 VCC)
  (net 4 DTR)
  (net 5 "Net-(D1-Pad2)")
  (net 6 "Net-(D2-Pad2)")
  (net 7 "Net-(D3-Pad2)")
  (net 8 "Net-(J2-Pad1)")
  (net 9 "Net-(J2-Pad2)")
  (net 10 RXD)
  (net 11 TXD)
  (net 12 "Net-(J5-Pad5)")
  (net 13 "Net-(J6-Pad1)")
  (net 14 "Net-(J6-Pad2)")
  (net 15 "Net-(R3-Pad1)")
  (net 16 "Net-(C6-Pad1)")
  (net 17 "Net-(C7-Pad2)")
  (net 18 "Net-(C8-Pad1)")
  (net 19 SDA)
  (net 20 SCL)
  (net 21 "Net-(J6-Pad4)")
  (net 22 "Net-(J6-Pad3)")
  (net 23 D0_MQ3)
  (net 24 A0_MQ3)
  (net 25 A0_MQ5)
  (net 26 D0_MQ5)
  (net 27 D0_MQ7)
  (net 28 D0_MQ135)
  (net 29 DHT_sig)
  (net 30 g_rx)
  (net 31 g_tx)
  (net 32 "Net-(J12-Pad1)")
  (net 33 bt_tx)
  (net 34 bt_rx)
  (net 35 "Net-(J12-Pad6)")
  (net 36 A0_MQ135)
  (net 37 A0_MQ7)
  (net 38 "Net-(R5-Pad1)")
  (net_class Default "Questo è il gruppo di collegamenti predefinito"
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 1.5)
    (via_drill 1)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net A0_MQ135)
    (add_net A0_MQ3)
    (add_net A0_MQ5)
    (add_net A0_MQ7)
    (add_net D0_MQ135)
    (add_net D0_MQ3)
    (add_net D0_MQ5)
    (add_net D0_MQ7)
    (add_net DHT_sig)
    (add_net DTR)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(J12-Pad1)")
    (add_net "Net-(J12-Pad6)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J5-Pad5)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(J6-Pad4)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net RXD)
    (add_net SCL)
    (add_net SDA)
    (add_net TXD)
    (add_net VCC)
    (add_net bt_rx)
    (add_net bt_tx)
    (add_net g_rx)
    (add_net g_tx)
  )
  (module Housings_DIP:DIP-28_W7.62mm_LongPads (layer F.Cu) (tedit 5BB50333)
    (at 106.68 77.724)
    (descr "28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference U1 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value ATMEGA328P-PU (at 3.81 35.35) (layer F.Fab))
    (fp_text user %R (at 3.81 16.51) (layer F.Fab))
    (pad 28 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 SCL))
    (pad 14 thru_hole oval (at 0 33.02) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 bt_tx))
    (pad 27 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 SDA))
    (pad 13 thru_hole oval (at 0 30.48) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 DHT_sig))
    (pad 26 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 A0_MQ7))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad2)"))
    (pad 25 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 A0_MQ135))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad1)"))
    (pad 24 thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 A0_MQ5))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C6-Pad1)"))
    (pad 23 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 A0_MQ3))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C8-Pad1)"))
    (pad 22 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 21 thru_hole oval (at 7.62 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 20 thru_hole oval (at 7.62 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 g_rx))
    (pad 19 thru_hole oval (at 7.62 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(J6-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 g_tx))
    (pad 18 thru_hole oval (at 7.62 25.4) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(J6-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(R5-Pad1)"))
    (pad 17 thru_hole oval (at 7.62 27.94) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J6-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 RXD))
    (pad 16 thru_hole oval (at 7.62 30.48) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J6-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 TXD))
    (pad 15 thru_hole oval (at 7.62 33.02) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 bt_rx))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 DTR))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-28_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 104.902 133.35 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 5.08 0) (layer F.SilkS))
    (fp_text value 10u (at 1.25 3.81 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D7.5mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 101.092 85.344 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*2.5mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 2.5mm Capacitor")
    (fp_text reference C2 (at -0.508 2.794 270) (layer F.SilkS))
    (fp_text value 22p (at 2.5 2.56 270) (layer F.Fab))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole circle (at 5 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D7.5mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D7.5mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 110.998 133.604 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*2.5mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 2.5mm Capacitor")
    (fp_text reference C3 (at 2.5 -2.56 270) (layer F.SilkS))
    (fp_text value 0.1u (at 2.5 2.56 270) (layer F.Fab))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D7.5mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D7.5mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 80.518 133.096 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*2.5mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 2.5mm Capacitor")
    (fp_text reference C4 (at 2.54 2.54 90) (layer F.SilkS))
    (fp_text value 0.1u (at 2.5 2.56 270) (layer F.Fab))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole circle (at 5 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D7.5mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 86.36 133.136 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C5 (at 5.04 0) (layer F.SilkS))
    (fp_text value 10u (at 1.25 3.81 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D7.5mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 96.012 101.092 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*2.5mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 2.5mm Capacitor")
    (fp_text reference C6 (at 3.048 2.286 270) (layer F.SilkS))
    (fp_text value 22p (at 2.5 2.56 270) (layer F.Fab))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D7.5mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D7.5mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 87.884 75.184 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*2.5mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 2.5mm Capacitor")
    (fp_text reference C7 (at 2.5 -2.56 180) (layer F.SilkS))
    (fp_text value 100n (at 2.5 2.56 180) (layer F.Fab))
    (fp_text user %R (at 2.5 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(C7-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 DTR))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D7.5mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D7.5mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 96.012 96.012 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*2.5mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 2.5mm Capacitor")
    (fp_text reference C8 (at 4.064 -2.286 90) (layer F.SilkS))
    (fp_text value 22p (at 2.5 2.56 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(C8-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D7.5mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5BB510A3)
    (at 92.71 142.24)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D1 (at 3.81 -2.06) (layer F.SilkS))
    (fp_text value 1N4001 (at 3.81 2.06) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D4.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 68.326 133.096 270)
    (descr "LED, diameter 4.0mm, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-43GD(Ver.12B).pdf")
    (tags "LED diameter 4.0mm 2 pins")
    (fp_text reference D2 (at 5.334 0) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.46 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D4.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D4.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 78.74 83.82)
    (descr "LED, diameter 4.0mm, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-43GD(Ver.12B).pdf")
    (tags "LED diameter 4.0mm 2 pins")
    (fp_text reference D3 (at 1.27 -3.46) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.46) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D4.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_gmkds:gmkds_3-2-7,62 (layer F.Cu) (tedit 5BB510C3)
    (at 122.682 137.668)
    (descr "2-way 7,62mm pitch terminal block, Phoenix GMKDS series")
    (fp_text reference Batt. (at 0 -6.858) (layer F.SilkS))
    (fp_text value "" (at 0 6.6) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 3.81 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(D1-Pad2)"))
    (model walter/conn_gmkds/gmkds_3-2-7,62.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 98.06 111.93 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (offset (xyz 0 -1.269999980926514 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 131.572 85.852 180)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (fp_text reference J3 (at 2.54 -0.508 270) (layer F.SilkS))
    (fp_text value Misure (at 0 15.03 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x06_Pitch2.54mm.wrl
      (offset (xyz 0 -6.349999904632568 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 123.19 74.93 270)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J4 (at 0 -2.794 270) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 SDA))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 SCL))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (offset (xyz 0 -1.269999980926514 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 66.63 85.63 180)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (fp_text reference J5 (at -0.172 16.288 180) (layer F.SilkS))
    (fp_text value CH340G (at 0 15.03 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J5-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 TXD))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 RXD))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(C7-Pad2)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x06_Pitch2.54mm.wrl
      (offset (xyz 0 -6.349999904632568 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 131.572 99.06 180)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference J6 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value dig2 (at 0 9.95 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J6-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J6-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J6-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J6-Pad1)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x04_Pitch2.54mm.wrl
      (offset (xyz 0 -3.809999942779541 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Angled_1x04_Pitch2.54mm (layer F.Cu) (tedit 5BB5105E)
    (at 136.398 143.764 90)
    (descr "Through hole angled socket strip, 1x04, 2.54mm pitch, 8.51mm socket length, single row")
    (tags "Through hole angled socket strip THT 1x04 2.54mm single row")
    (fp_text reference J7 (at -4.826 -2.794 90) (layer F.SilkS))
    (fp_text value MQ3 (at -5.08 4.826 90) (layer F.SilkS))
    (fp_text user %R (at -4.38 -2.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 D0_MQ3))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 A0_MQ3))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Angled_1x04_Pitch2.54mm.wrl
      (offset (xyz 0 -3.809999942779541 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Angled_1x04_Pitch2.54mm (layer F.Cu) (tedit 5BB50FB8)
    (at 61.468 58.42 270)
    (descr "Through hole angled socket strip, 1x04, 2.54mm pitch, 8.51mm socket length, single row")
    (tags "Through hole angled socket strip THT 1x04 2.54mm single row")
    (fp_text reference J8 (at -2.032 -2.794 270) (layer F.SilkS))
    (fp_text value MQ5 (at -4.572 5.08 270) (layer F.SilkS))
    (fp_text user %R (at -4.38 -2.27 270) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 A0_MQ5))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 D0_MQ5))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Angled_1x04_Pitch2.54mm.wrl
      (offset (xyz 0 -3.809999942779541 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 116.84 60.96 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J9 (at 0.254 -2.794 90) (layer F.SilkS))
    (fp_text value sens_dig (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81 180) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 D0_MQ7))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 D0_MQ135))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 D0_MQ5))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 D0_MQ3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 100.076 117.348 90)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (fp_text reference J10 (at 0 -3.048 90) (layer F.SilkS))
    (fp_text value DHT11 (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 DHT_sig))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x03_Pitch2.54mm.wrl
      (offset (xyz 0 -2.539999961853027 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 74.168 90.932 90)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference J11 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value GPS_NEO6M (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 g_rx))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 g_tx))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x04_Pitch2.54mm.wrl
      (offset (xyz 0 -3.809999942779541 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 131.572 117.856 180)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (fp_text reference J12 (at 0.254 -3.302 180) (layer F.SilkS))
    (fp_text value Conn_01x06_Female (at 0 15.03 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J12-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 bt_tx))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 bt_rx))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J12-Pad6)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x06_Pitch2.54mm.wrl
      (offset (xyz 0 -6.349999904632568 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Angled_1x04_Pitch2.54mm (layer F.Cu) (tedit 5BB50FA1)
    (at 143.764 58.42 270)
    (descr "Through hole angled socket strip, 1x04, 2.54mm pitch, 8.51mm socket length, single row")
    (tags "Through hole angled socket strip THT 1x04 2.54mm single row")
    (fp_text reference J13 (at -3.556 -2.794 270) (layer F.SilkS))
    (fp_text value MQ135 (at -4.826 5.08 270) (layer F.SilkS))
    (fp_text user %R (at -4.38 -2.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 D0_MQ135))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 A0_MQ135))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Angled_1x04_Pitch2.54mm.wrl
      (offset (xyz 0 -3.809999942779541 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Angled_1x04_Pitch2.54mm (layer F.Cu) (tedit 5BB5101A)
    (at 53.848 143.764 90)
    (descr "Through hole angled socket strip, 1x04, 2.54mm pitch, 8.51mm socket length, single row")
    (tags "Through hole angled socket strip THT 1x04 2.54mm single row")
    (fp_text reference J14 (at -4.826 10.414 90) (layer F.SilkS))
    (fp_text value MQ7 (at -5.588 5.08 90) (layer F.SilkS))
    (fp_text user %R (at -4.38 -2.27 90) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 A0_MQ7))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 D0_MQ7))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Angled_1x04_Pitch2.54mm.wrl
      (offset (xyz 0 -3.809999942779541 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 89.916 64.008 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 4.064 2.794 180) (layer F.SilkS))
    (fp_text value 10k_supp2 (at 3.81 2.31 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 DTR))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 111.83 63.31 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 3.81 -2.724 270) (layer F.SilkS))
    (fp_text value 10k (at 3.81 2.31 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 DTR))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 89.916 69.088 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 4.064 -2.794 180) (layer F.SilkS))
    (fp_text value 10k (at 3.81 2.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(R3-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 74.422 132.588 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 9.652 0) (layer F.SilkS))
    (fp_text value 220 (at 3.81 2.31 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 93.98 83.82 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 3.81 -2.54 180) (layer F.SilkS))
    (fp_text value 220 (at 3.81 2.31 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(R5-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH-12mm_Wuerth-430476085716 (layer F.Cu) (tedit 59BC4CF4)
    (at 107.188 69.088 180)
    (descr "SW PUSH 12mm http://katalog.we-online.de/em/datasheet/430476085716.pdf")
    (tags "tact sw push 12mm")
    (fp_text reference SW1 (at 6.35 -4.66 180) (layer F.SilkS))
    (fp_text value SW_Push (at 6.35 9.93 180) (layer F.Fab))
    (fp_text user %R (at 6.35 2.54 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 5 180) (size 3 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 DTR))
    (pad 1 thru_hole oval (at 0 0 180) (size 3 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 "Net-(R3-Pad1)"))
    (pad 2 thru_hole oval (at 12.5 5 180) (size 3 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 DTR))
    (pad 1 thru_hole oval (at 12.5 0 180) (size 3 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH-12mm_Wuerth-430476085716.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 58CE52AD)
    (at 98.298 134.112 180)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference U2 (at 2.54 -3.62 180) (layer F.SilkS))
    (fp_text value LM7805_TO220 (at 2.54 3.92 180) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 180) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-4H_Vertical (layer F.Cu) (tedit 58CD2E9C)
    (at 101.092 101.092 90)
    (descr "Crystal THT HC-49-4H http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49-4H")
    (fp_text reference Y1 (at -4.826 -0.254 90) (layer F.SilkS))
    (fp_text value 16MHz (at 2.44 3.525 90) (layer F.Fab))
    (fp_text user %R (at 2.44 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 4.88 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C8-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_HC49-4H_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.5mm (layer F.Cu) (tedit 5BB51454)
    (at 121.92 122.428)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference "" (at 0 -3.5) (layer F.SilkS))
    (fp_text value "" (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.5mm (layer F.Cu) (tedit 5BB5145A)
    (at 73.66 121.92)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference "" (at 0 -3.5) (layer F.SilkS))
    (fp_text value "" (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.5mm (layer F.Cu) (tedit 5BB51450)
    (at 121.92 68.58)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference "" (at 0 -3.5) (layer F.SilkS))
    (fp_text value "" (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.5mm (layer F.Cu) (tedit 5BB5144B)
    (at 73.66 68.58)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference "" (at 0 -3.5) (layer F.SilkS))
    (fp_text value "" (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (gr_text "Mezzina\nCito" (at 148.844 136.144) (layer F.SilkS))
  (gr_text "GABE Project" (at 144.018 133.858) (layer F.SilkS))
  (gr_text "GM@DEISLab\n03102018" (at 149.098 66.802) (layer B.SilkS))
  (gr_text M4 (at 70.612 65.278) (layer F.SilkS))
  (gr_text M3 (at 126.492 66.802) (layer F.SilkS))
  (gr_text M2 (at 70.104 124.968) (layer F.SilkS))
  (gr_text M1 (at 125.984 125.222) (layer F.SilkS))
  (gr_text Pwr (at 128.27 79.502 90) (layer F.SilkS))
  (gr_text Comparators (at 120.904 63.754) (layer F.SilkS))
  (gr_text dBL (at 125.476 58.42) (layer F.SilkS))
  (gr_text dTR (at 122.682 58.42) (layer F.SilkS))
  (gr_text dTL (at 120.396 58.42) (layer F.SilkS))
  (gr_text dBR (at 117.856 58.42) (layer F.SilkS))
  (gr_text Digital (at 128.27 95.25 90) (layer F.SilkS))
  (gr_text BT (at 128.27 111.76 90) (layer F.SilkS))
  (gr_text Vcc (at 136.144 115.316) (layer F.SilkS))
  (gr_text gnd (at 136.144 113.03) (layer F.SilkS))
  (gr_text TX (at 135.382 110.236) (layer F.SilkS))
  (gr_text RX (at 135.382 107.95) (layer F.SilkS))
  (gr_text 10# (at 136.144 99.06) (layer F.SilkS))
  (gr_text 11# (at 136.144 96.774) (layer F.SilkS))
  (gr_text 12 (at 135.382 93.98) (layer F.SilkS))
  (gr_text 13 (at 135.382 91.44) (layer F.SilkS))
  (gr_text "Vcc\n" (at 135.128 83.82 90) (layer F.SilkS))
  (gr_text --- (at 133.858 83.312 90) (layer F.SilkS))
  (gr_text gnd (at 134.874 76.454 90) (layer F.SilkS))
  (gr_text ---------- (at 133.858 72.136 90) (layer F.SilkS))
  (gr_text SDA/A4 (at 123.19 77.216 90) (layer F.SilkS))
  (gr_text SCL/A5 (at 120.65 77.216 90) (layer F.SilkS))
  (gr_text 10k (at 112.776 67.31) (layer F.SilkS))
  (gr_text DTR (at 105.918 61.722) (layer F.SilkS))
  (gr_text gnd (at 98.044 71.12) (layer F.SilkS))
  (gr_text gnd (at 99.06 65.024) (layer F.SilkS))
  (gr_text 10k (at 87.122 64.008) (layer F.SilkS))
  (gr_text 10k (at 87.122 69.088) (layer F.SilkS))
  (gr_text 0.1u (at 90.17 76.708 270) (layer F.SilkS))
  (gr_text 6 (at 101.346 109.474) (layer F.SilkS))
  (gr_text 5* (at 98.806 109.474) (layer F.SilkS))
  (gr_text 16M (at 102.108 98.806) (layer F.SilkS))
  (gr_text 22p (at 97.282 103.632) (layer F.SilkS))
  (gr_text 22p (at 97.028 93.726) (layer F.SilkS))
  (gr_text 22p (at 102.108 87.884) (layer F.SilkS))
  (gr_text 220 (at 91.186 83.82) (layer F.SilkS))
  (gr_text "Calibrations\nLed" (at 76.708 82.55) (layer F.SilkS))
  (gr_text CH340G (at 60.96 78.486 90) (layer F.SilkS))
  (gr_text DTR (at 63.5 85.598) (layer F.SilkS))
  (gr_text RXD (at 63.5 83.058) (layer F.SilkS))
  (gr_text TXD (at 63.5 80.518) (layer F.SilkS))
  (gr_text Vcc (at 63.5 77.978) (layer F.SilkS))
  (gr_text NC (at 63.5 75.438) (layer F.SilkS))
  (gr_text gnd (at 63.5 72.898) (layer F.SilkS))
  (gr_text "Status\nLed" (at 65.024 133.604) (layer F.SilkS))
  (gr_text TXD (at 79.248 93.472) (layer F.SilkS))
  (gr_text RXD (at 76.708 93.472) (layer F.SilkS))
  (gr_text gnd (at 81.788 93.472) (layer F.SilkS))
  (gr_text Vcc (at 74.168 93.472) (layer F.SilkS))
  (gr_text gnd (at 105.156 119.888) (layer F.SilkS))
  (gr_text Vcc (at 102.616 119.888) (layer F.SilkS))
  (gr_text S (at 100.076 119.888) (layer F.SilkS))
  (gr_text 220 (at 74.422 136.398 90) (layer F.SilkS))
  (gr_text 0.1u (at 80.518 135.89) (layer F.SilkS))
  (gr_text 0.1u (at 110.998 136.144) (layer F.SilkS))
  (gr_text 10u (at 89.154 131.572) (layer F.SilkS))
  (gr_text 10u (at 107.95 131.826) (layer F.SilkS))
  (gr_text - (at 118.618 144.526) (layer F.SilkS))
  (gr_text + (at 127.254 144.526) (layer F.SilkS))
  (gr_text A0 (at 144.272 141.224) (layer F.SilkS))
  (gr_text gnd (at 139.192 141.224) (layer F.SilkS))
  (gr_text Vcc (at 136.652 141.224) (layer F.SilkS))
  (gr_text D0 (at 141.732 141.224) (layer F.SilkS))
  (gr_text D0 (at 58.928 140.716) (layer F.SilkS))
  (gr_text A0 (at 61.468 140.716) (layer F.SilkS))
  (gr_text Vcc (at 53.848 140.716) (layer F.SilkS))
  (gr_text gnd (at 56.388 140.716) (layer F.SilkS))
  (gr_text D0 (at 56.388 60.96) (layer F.SilkS))
  (gr_text A0 (at 53.848 60.96) (layer F.SilkS))
  (gr_text gnd (at 58.928 60.96) (layer F.SilkS))
  (gr_text Vcc (at 61.468 60.96) (layer F.SilkS))
  (gr_text A0 (at 136.144 60.96) (layer F.SilkS))
  (gr_text D0 (at 138.684 60.96) (layer F.SilkS))
  (gr_text gnd (at 141.224 60.96) (layer F.SilkS))
  (gr_text Vcc (at 143.764 60.96) (layer F.SilkS))
  (gr_text DHT (at 102.108 123.19) (layer F.SilkS))
  (gr_text "GPS 6M NEO" (at 77.47 101.6) (layer F.SilkS))
  (gr_line (start 48.26 68.58) (end 58.42 68.58) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 48.26 45.72) (end 48.26 68.58) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 68.58 45.72) (end 48.26 45.72) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 68.58 55.88) (end 68.58 45.72) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.54 55.88) (end 68.58 55.88) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.54 45.72) (end 129.54 55.88) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.86 45.72) (end 129.54 45.72) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.86 68.58) (end 149.86 45.72) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.7 68.58) (end 149.86 68.58) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.7 132.08) (end 139.7 68.58) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.86 132.08) (end 139.7 132.08) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.86 157.48) (end 149.86 132.08) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.54 157.48) (end 149.86 157.48) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.54 147.32) (end 129.54 157.48) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 68.58 147.32) (end 129.54 147.32) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 68.58 157.48) (end 68.58 147.32) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 48.26 157.48) (end 68.58 157.48) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 48.26 132.08) (end 48.26 157.48) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 58.42 132.08) (end 48.26 132.08) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 58.42 68.58) (end 58.42 132.08) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.762))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.895 46.355) (xy 67.945 46.355) (xy 67.945 67.945) (xy 48.895 67.945)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.762))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.175 46.355) (xy 149.225 46.355) (xy 149.225 67.945) (xy 130.175 67.945)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.762))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.895 132.715) (xy 48.895 156.845) (xy 67.945 156.845) (xy 67.945 132.715)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.762))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.175 156.845) (xy 130.175 132.715) (xy 149.225 132.715) (xy 149.225 156.845)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.762))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 59.055 146.685) (xy 138.43 146.685) (xy 139.065 146.685) (xy 139.065 56.515) (xy 59.69 56.515)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.762))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.895 132.715) (xy 48.895 156.845) (xy 67.945 156.845) (xy 67.945 132.715)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.762))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.175 156.845) (xy 149.225 156.845) (xy 149.225 132.715) (xy 130.81 132.715) (xy 130.175 132.715)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.762))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 59.055 146.05) (xy 139.065 146.05) (xy 139.065 56.515) (xy 59.69 56.515)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.762))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.175 46.355) (xy 149.225 46.355) (xy 149.225 67.945) (xy 130.175 67.945)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.762))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.895 46.355) (xy 67.945 46.355) (xy 67.945 67.945) (xy 48.895 67.945)
      )
    )
  )
)
