(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "ENIG")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+3V3")
  (net 2 "/SCL")
  (net 3 "/SDA")
  (net 4 "/WakeAlarm")
  (net 5 "GND")
  (net 6 "Net-(BT1-Pad1)")
  (net 7 "+12V")
  (net 8 "Net-(C6-Pad2)")
  (net 9 "Net-(C7-Pad1)")
  (net 10 "unconnected-(U1-Pad1)")
  (net 11 "/HeaterCTL")
  (net 12 "unconnected-(U1-Pad9)")
  (net 13 "Net-(R1-Pad1)")
  (net 14 "/MOSI")
  (net 15 "/MISO")
  (net 16 "/CLK")
  (net 17 "unconnected-(U2-Pad12)")
  (net 18 "unconnected-(U2-Pad13)")
  (net 19 "unconnected-(U2-Pad14)")
  (net 20 "unconnected-(U2-Pad15)")
  (net 21 "unconnected-(U2-Pad19)")
  (net 22 "unconnected-(U2-Pad20)")
  (net 23 "unconnected-(U2-Pad22)")
  (net 24 "unconnected-(U2-Pad23)")
  (net 25 "unconnected-(U2-Pad24)")
  (net 26 "unconnected-(U2-Pad25)")
  (net 27 "unconnected-(U2-Pad26)")
  (net 28 "unconnected-(U2-Pad27)")
  (net 29 "unconnected-(U2-Pad28)")
  (net 30 "/TEMPSense")
  (net 31 "/Heater")
  (net 32 "/Reset")
  (net 33 "/TX")
  (net 34 "/RX")
  (net 35 "unconnected-(1111-Pad4)")
  (net 36 "Net-(R7-Pad1)")
  (net 37 "unconnected-(1111-Pad9)")
  (net 38 "Net-(R8-Pad2)")
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 107.95 116.205 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at 2.54 -0.635 90) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.4 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 121.92 123.19)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at 3.720463 -2.791317) (layer "F.SilkS"))
    (fp_text value "AMS1117-3.3" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -3.15 -2.3) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd rect (at -3.15 0) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+3V3") (pinfunction "VO") (pintype "power_out"))
    (pad "2" smd rect (at 3.15 0) (size 2 3.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+3V3") (pinfunction "VO") (pintype "power_out"))
    (pad "3" smd rect (at -3.15 2.3) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "+12V") (pinfunction "VI") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 103.505 104.775 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x04" (at 0 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "/Reset") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "/MOSI") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "/MISO") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/CLK") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 106.045 121.285)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C11" (at -1.27 -1.43) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(BT1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:10mm Crewmate" (layer "F.Cu")
    (tedit 0)
    (at 138.43 136.525)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "Susmogus" (at 0 5.715) (layer "F.Mask"))
    (fp_text value "LOGO" (at 0.75 0) (layer "F.Cu") hide)
  )
  (footprint "Package_QFP:TQFP-32_7x7mm_P0.8mm" (layer "F.Cu")
    (tedit 5A02F146)
    (at 134.645 111.995)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at -7.01 -0.235 90) (layer "F.SilkS"))
    (fp_text value "ATmega328P-A" (at 0 6.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -4.25 -2.8) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/HeaterCTL") (pinfunction "PD3") (pintype "bidirectional"))
    (pad "2" smd rect (at -4.25 -2) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/WakeAlarm") (pinfunction "PD4") (pintype "bidirectional"))
    (pad "3" smd rect (at -4.25 -1.2) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd rect (at -4.25 -0.4) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (pad "5" smd rect (at -4.25 0.4) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "6" smd rect (at -4.25 1.2) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+3V3") (pinfunction "VCC") (pintype "passive"))
    (pad "7" smd rect (at -4.25 2) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(C6-Pad2)") (pinfunction "XTAL1/PB6") (pintype "bidirectional"))
    (pad "8" smd rect (at -4.25 2.8) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(C7-Pad1)") (pinfunction "XTAL2/PB7") (pintype "bidirectional"))
    (pad "9" smd rect (at -2.8 4.25 90) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/MOSI") (pinfunction "PD5") (pintype "bidirectional"))
    (pad "10" smd rect (at -2 4.25 90) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/MISO") (pinfunction "PD6") (pintype "bidirectional"))
    (pad "11" smd rect (at -1.2 4.25 90) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/CLK") (pinfunction "PD7") (pintype "bidirectional"))
    (pad "12" smd rect (at -0.4 4.25 90) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "unconnected-(U2-Pad12)") (pinfunction "PB0") (pintype "bidirectional"))
    (pad "13" smd rect (at 0.4 4.25 90) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "unconnected-(U2-Pad13)") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "14" smd rect (at 1.2 4.25 90) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "unconnected-(U2-Pad14)") (pinfunction "PB2") (pintype "bidirectional"))
    (pad "15" smd rect (at 2 4.25 90) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "unconnected-(U2-Pad15)") (pinfunction "PB3") (pintype "bidirectional"))
    (pad "16" smd rect (at 2.8 4.25 90) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/SCL") (pinfunction "PB4") (pintype "bidirectional"))
    (pad "17" smd rect (at 4.25 2.8) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/SDA") (pinfunction "PB5") (pintype "bidirectional"))
    (pad "18" smd rect (at 4.25 2) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+3V3") (pinfunction "AVCC") (pintype "power_in"))
    (pad "19" smd rect (at 4.25 1.2) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "unconnected-(U2-Pad19)") (pinfunction "ADC6") (pintype "input"))
    (pad "20" smd rect (at 4.25 0.4) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "unconnected-(U2-Pad20)") (pinfunction "AREF") (pintype "passive"))
    (pad "21" smd rect (at 4.25 -0.4) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "22" smd rect (at 4.25 -1.2) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "unconnected-(U2-Pad22)") (pinfunction "ADC7") (pintype "input"))
    (pad "23" smd rect (at 4.25 -2) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "unconnected-(U2-Pad23)") (pinfunction "PC0") (pintype "bidirectional"))
    (pad "24" smd rect (at 4.25 -2.8) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "unconnected-(U2-Pad24)") (pinfunction "PC1") (pintype "bidirectional"))
    (pad "25" smd rect (at 2.8 -4.25 90) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "unconnected-(U2-Pad25)") (pinfunction "PC2") (pintype "bidirectional"))
    (pad "26" smd rect (at 2 -4.25 90) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "unconnected-(U2-Pad26)") (pinfunction "PC3") (pintype "bidirectional"))
    (pad "27" smd rect (at 1.2 -4.25 90) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "unconnected-(U2-Pad27)") (pinfunction "PC4") (pintype "bidirectional"))
    (pad "28" smd rect (at 0.4 -4.25 90) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "unconnected-(U2-Pad28)") (pinfunction "PC5") (pintype "bidirectional"))
    (pad "29" smd rect (at -0.4 -4.25 90) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/Reset") (pinfunction "~{RESET}/PC6") (pintype "bidirectional"))
    (pad "30" smd rect (at -1.2 -4.25 90) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/TX") (pinfunction "PD0") (pintype "bidirectional"))
    (pad "31" smd rect (at -2 -4.25 90) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/RX") (pinfunction "PD1") (pintype "bidirectional"))
    (pad "32" smd rect (at -2.8 -4.25 90) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/TEMPSense") (pinfunction "PD2") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/TQFP-32_7x7mm_P0.8mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Generic:RX8130CE" (layer "F.Cu")
    (tedit 0)
    (at 111.125 116.205 90)
    (descr "RX8130CE-2")
    (tags "Integrated Circuit")
    (property "Arrow Part Number" "RX8130CE")
    (property "Arrow Price/Stock" "https://www.arrow.com/en/products/rx8130ce/epson-electronics-america")
    (property "Datasheet_1" "https://www.mouser.in/Search/DownloadDatasheet?url=https%3A%2F%2Fwww.mouser.in%2Fdatasheet%2F2%2F137%2FRX8130CE_en-1825324.pdf")
    (property "Footprint_1" "RX8130CE")
    (property "Height" "1")
    (property "Manufacturer_Name" "Epson Timing")
    (property "Manufacturer_Part_Number" "RX8130CE")
    (property "Mouser Part Number" "")
    (property "Mouser Price/Stock" "")
    (property "Reference_1" "U5")
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (property "Value_1" "RX8130CE")
    (attr smd)
    (fp_text reference "1111" (at 1.905 4.445 90) (layer "F.SilkS") hide)
    (fp_text value "RX8130CE" (at 0 0.275 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0.275 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at -1.55 1 90) (size 0.7 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+3V3") (pinfunction "VIO") (pintype "passive"))
    (pad "2" smd rect locked (at -0.7 1 90) (size 0.4 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/SCL") (pinfunction "SCL") (pintype "passive"))
    (pad "3" smd rect locked (at 0 1 90) (size 0.4 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/SDA") (pinfunction "SDA") (pintype "passive"))
    (pad "4" smd rect locked (at 0.7 1 90) (size 0.4 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "unconnected-(1111-Pad4)") (pinfunction "FOUT") (pintype "passive"))
    (pad "5" smd rect locked (at 1.55 1 90) (size 0.7 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "Net-(R7-Pad1)") (pinfunction "~{RST}") (pintype "passive"))
    (pad "6" smd rect locked (at 1.55 -1 90) (size 0.7 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/WakeAlarm") (pinfunction "~{IRQ}") (pintype "passive"))
    (pad "7" smd rect locked (at 0.7 -1 90) (size 0.4 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "8" smd rect locked (at 0 -1 90) (size 0.4 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+3V3") (pinfunction "VDD") (pintype "passive"))
    (pad "9" smd rect locked (at -0.7 -1 90) (size 0.4 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "unconnected-(1111-Pad9)") (pinfunction "VOUT") (pintype "passive"))
    (pad "10" smd rect locked (at -1.55 -1 90) (size 0.7 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(R8-Pad2)") (pinfunction "VBAT") (pintype "passive"))
    (model "RX8130CE.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 109.842482 141.598741 90)
    (fp_text reference "" (at 0 0 90) (layer "F.SilkS"))
    (fp_text value "" (at 0 0 90) (layer "F.SilkS"))
    (pad "1" smd rect (at 0 0 90) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND") (pinfunction "GND") (pintype "power_in"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 127.455 127.5 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at -3.04 -0.18 90) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 115.57 120.015 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 4.445 0 90) (layer "F.SilkS"))
    (fp_text value "4.2K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/SCL") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 114.3 122.555 135)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.43 135) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.43 135) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 135) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(BT1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 135) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(R8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 142.968648 114.59781 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 2.251745 -0.182683) (layer "F.SilkS"))
    (fp_text value "2.2K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.8 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/TEMPSense") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 124.425 116.27 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at -0.14058 1.486015 90) (layer "F.SilkS"))
    (fp_text value "10pF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 141.26 112.74 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0.049562 1.65718 90) (layer "F.SilkS"))
    (fp_text value "C" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 124.425 113.095 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at -0.14058 1.486015 90) (layer "F.SilkS"))
    (fp_text value "10pF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Generic:TO-252-3_Cable" (layer "F.Cu")
    (tedit 5A70F30B)
    (at 149.86 113.665)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Ud" (at 1.905 0 90) (layer "F.SilkS") hide)
    (fp_text value "DS18B20" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (fp_circle (center -1 5) (end 0 5) (layer "Edge.Cuts") (width 0.12) (fill none))
    (fp_circle (center -1 -5) (end 0 -5) (layer "Edge.Cuts") (width 0.12) (fill none))
    (pad "1" smd rect (at -4.2 -2.28) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd rect (at -4.2 0) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/TEMPSense") (pinfunction "DQ") (pintype "bidirectional"))
    (pad "3" smd rect (at -4.2 2.28) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+3V3") (pinfunction "VDD") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TO-252-3_TabPin2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 116.84 120.015 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 2.54 0 90) (layer "F.SilkS"))
    (fp_text value "4.2K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/SDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 144.145 104.775 90)
    (fp_text reference "" (at 0 0 90) (layer "F.SilkS"))
    (fp_text value "" (at 0 0 90) (layer "F.SilkS"))
    (pad "1" smd rect (at 0 0 90) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/RX") (pinfunction "GND") (pintype "power_in"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 124.392443 118.89983 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at -2.899441 0.038789) (layer "F.SilkS"))
    (fp_text value ".1uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 141.605 109.386483 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0.743913 -1.443091 90) (layer "F.SilkS"))
    (fp_text value "4.2K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/Reset") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:PHOENIX_1803277" (layer "F.Cu")
    (tedit 64359783)
    (at 109.42 127.34525 -90)
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -5.55025 7.185 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 4.83471 9.04384 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at -1.905 0 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "+12V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 1.905 0 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "GND") (pinfunction "Pin_2") (pintype "passive"))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 103.505 141.605 90)
    (fp_text reference "" (at 0 0 90) (layer "F.SilkS"))
    (fp_text value "" (at 0 0 90) (layer "F.SilkS"))
    (pad "1" smd rect (at 0 0 90) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/SDA") (pinfunction "GND") (pintype "power_in"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113.665 128.905 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 0.14058 2.54 90) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "+12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 107.95 141.605 90)
    (fp_text reference "" (at 0 0 90) (layer "F.SilkS"))
    (fp_text value "" (at 0 0 90) (layer "F.SilkS"))
    (pad "1" smd rect (at 0 0 90) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+3V3") (pinfunction "GND") (pintype "power_in"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 132.715 123.825 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "4.2K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Crystal_HC18-U_Vertical" (layer "F.Cu")
    (tedit 5A1AD3B7)
    (at 120.305 116.115 90)
    (descr "Crystal THT HC-18/U, http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-18/U")
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Y1" (at 8.804856 0.071059) (layer "F.SilkS"))
    (fp_text value "Crystal" (at 2.45 3.525 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.45 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C7-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 4.9 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C6-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_HC18-U_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 146.685 104.775 90)
    (fp_text reference "" (at 0 0 90) (layer "F.SilkS"))
    (fp_text value "" (at 0 0 90) (layer "F.SilkS"))
    (pad "2" smd rect (at 0 0 90) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/TX") (pinfunction "DQ") (pintype "bidirectional"))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 105.389311 141.589753 90)
    (fp_text reference "" (at 0 0 90) (layer "F.SilkS"))
    (fp_text value "" (at 0 0 90) (layer "F.SilkS"))
    (pad "1" smd rect (at 0 0 90) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/SCL") (pinfunction "GND") (pintype "power_in"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 128.725 127.5 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at -3.018182 -0.437297 90) (layer "F.SilkS"))
    (fp_text value ".1uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 136.345 127.5 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at -3.040001 -0.017414 90) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/Heater") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DFN_QFN:DFN-10-1EP_3x3mm_P0.5mm_EP1.75x2.7mm" (layer "F.Cu")
    (tedit 5EA4BEDC)
    (at 132.535 126.23)
    (descr "10-Lead Plastic Dual Flat No-Lead Package, 3x3mm Body (see Atmel Appnote 8826)")
    (tags "DFN 0.5")
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -2.475) (layer "F.SilkS"))
    (fp_text value "LS12052BD33" (at 0.13 3.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd rect (at -0.3875 0.62) (size 0.6 1.05) (layers "F.Paste"))
    (pad "" smd rect (at -0.3875 -0.62) (size 0.6 1.05) (layers "F.Paste"))
    (pad "" smd rect (at 0.3875 -0.62) (size 0.6 1.05) (layers "F.Paste"))
    (pad "" smd rect (at 0.3875 0.62) (size 0.6 1.05) (layers "F.Paste"))
    (pad "1" smd rect (at -1.45 -1) (size 0.85 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "unconnected-(U1-Pad1)") (pinfunction "SS") (pintype "input"))
    (pad "2" smd rect (at -1.45 -0.5) (size 0.85 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/HeaterCTL") (pinfunction "EN") (pintype "input"))
    (pad "3" smd rect (at -1.45 0) (size 0.85 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "+12V") (pinfunction "IN") (pintype "power_in"))
    (pad "4" smd rect (at -1.45 0.5) (size 0.85 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "+12V") (pinfunction "IN") (pintype "power_in"))
    (pad "5" smd rect (at -1.45 1) (size 0.85 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "+12V") (pinfunction "IN") (pintype "power_in"))
    (pad "6" smd rect (at 1.45 1) (size 0.85 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/Heater") (pinfunction "OUT") (pintype "power_out"))
    (pad "7" smd rect (at 1.45 0.5) (size 0.85 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/Heater") (pinfunction "OUT") (pintype "power_out"))
    (pad "8" smd rect (at 1.45 0) (size 0.85 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/Heater") (pinfunction "OUT") (pintype "power_out"))
    (pad "9" smd rect (at 1.45 -0.5) (size 0.85 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "unconnected-(U1-Pad9)") (pinfunction "BFET") (pintype "output"))
    (pad "10" smd rect (at 1.45 -1) (size 0.85 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(R1-Pad1)") (pinfunction "ILIM") (pintype "input"))
    (pad "11" smd rect (at 0 0) (size 1.75 2.7) (layers "F.Cu" "F.Mask")
      (net 5 "GND") (pinfunction "GND") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/DFN-10-1EP_3x3mm_P0.5mm_EP1.75x2.7mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 137.615 127.5 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at -3.04 -0.18 90) (layer "F.SilkS"))
    (fp_text value ".1uf" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/Heater") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 116.205 111.76 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 2.54 0 180) (layer "F.SilkS"))
    (fp_text value "4.2K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.8 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(R7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:PHOENIX_1803277" (layer "B.Cu")
    (tedit 64359783)
    (at 145.215 127.98025 -90)
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R2" (at -1.520835 2.196195 90) (layer "B.SilkS"))
    (fp_text value "Heater" (at -6.69525 -2.105 -180) (layer "F.SilkS"))
    (pad "1" thru_hole rect locked (at -1.905 0 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 31 "/Heater") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 1.905 0 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "GND") (pintype "passive"))
  )
  (footprint "Generic:BAT_BAT-HLD-003-SMT" (layer "B.Cu")
    (tedit 6442D358)
    (at 125.095 133.985 180)
    (property "Sheetfile" "WetSensorHeater.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "BT1" (at -10.055 12.389) (layer "B.SilkS"))
    (fp_text value "Battery_Cell" (at 2.391 -11.389) (layer "B.Fab"))
    (pad "1" smd circle locked (at 0 0 180) (size 17.9 17.9) (layers "B.Cu" "B.Mask")
      (net 6 "Net-(BT1-Pad1)") (pinfunction "+") (pintype "passive"))
    (pad "2" smd rect locked (at -12.9 0 180) (size 5.7 6.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "GND") (pinfunction "-") (pintype "passive"))
    (pad "2" smd rect locked (at 12.9 0 180) (size 5.7 6.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "GND") (pinfunction "-") (pintype "passive"))
  )
  (gr_rect (start 101.6 102.87) (end 152.4 144.145) (layer "Edge.Cuts") (width 0.2) (fill none))
  (gr_text "DSG By Arsenio Menendez\nNASA GSFC 4/28/23\nRev 1.0" (at 126.365 109.22) (layer "B.SilkS"))
  (gr_text "SENSE WIRE\n" (at 151.520956 113.672272 90) (layer "F.SilkS"))
  (gr_text " ^     ^\nBrain here?" (at 133.985 120.015) (layer "F.SilkS"))
  (gr_text "The part that is \nlike a light switch" (at 125.095 137.16) (layer "F.SilkS"))
  (gr_text "Heater dew Deleter\n" (at 125.73 104.775) (layer "F.SilkS"))
  (gr_text "Remgulator\n" (at 121.285 131.445) (layer "F.SilkS"))
  (gr_text "Yeater" (at 147.32 134.62) (layer "F.SilkS"))
  (gr_text "GND\n" (at 148.600668 111.444681) (layer "F.SilkS"))
  (gr_text "CLK\n" (at 111.125 107.315 90) (layer "F.SilkS"))
  (gr_text "RX\nTX" (at 145.415 107.315 90) (layer "F.SilkS"))
  (gr_text "3V3" (at 148.697639 116.012028) (layer "F.SilkS"))
  (gr_text "MOS\n" (at 106.045 107.315 90) (layer "F.SilkS"))
  (gr_text "Power\nIN" (at 105.41 133.985) (layer "F.SilkS"))
  (gr_text "MIS\n" (at 108.585 107.315 90) (layer "F.SilkS"))
  (gr_text "3V3\nGND\n\n" (at 109.855 138.43 90) (layer "F.SilkS"))
  (gr_text "BUS\n" (at 148.59 113.665) (layer "F.SilkS"))
  (gr_text "SDA\nSCL\n" (at 104.487575 138.43 90) (layer "F.SilkS"))
  (gr_text "RST" (at 103.505 107.315 90) (layer "F.SilkS"))
  (gr_text "+\n-" (at 111.997741 127.339561) (layer "F.SilkS"))
  (gr_text "Flava Flav\nRegion" (at 103.505 115.57 90) (layer "F.SilkS"))
  (zone (net 5) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.67 144.78)
        (xy 100.965 144.78)
        (xy 100.965 102.235)
        (xy 153.67 102.235)
      )
    )
  )
  (zone (net 5) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.67 144.78)
        (xy 100.965 144.78)
        (xy 100.965 102.235)
        (xy 153.67 102.235)
      )
    )
  )
)
