<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<wire x1="13" y1="73.29119375" x2="13" y2="32.430053125" width="0" layer="20"/>
<wire x1="13" y1="32.430053125" x2="16.452553125" y2="28.9775" width="0" layer="20" curve="90"/>
<wire x1="16.452553125" y1="28.9775" x2="61.7473625" y2="28.9775" width="0" layer="20"/>
<wire x1="61.7473625" y1="28.9775" x2="64.74" y2="31.9701375" width="0" layer="20" curve="90"/>
<wire x1="64.74" y1="31.9701375" x2="64.74" y2="73.790053125" width="0" layer="20"/>
<wire x1="64.74" y1="73.790053125" x2="61.070053125" y2="77.46" width="0" layer="20" curve="90"/>
<wire x1="61.070053125" y1="77.46" x2="17.16880625" y2="77.46" width="0" layer="20"/>
<wire x1="17.16880625" y1="77.46" x2="13" y2="73.29119375" width="0" layer="20" curve="90"/>
<text>MC34063 Buck+Boost V1.1</text>
<text>MC34063 Buck + Boost V1.1</text>
<text>SEGASONICFAN DESIGNS</text>
<text>+5V OUT</text>
<text>+12V
OUT</text>
<text>+5V IN</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="SO08">
</package>
<package name="R1210">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="153CLV-0605">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
</packages>
</library>
<library name="eagle-ltspice">
<description>Default symbols for import LTspice schematics&lt;p&gt;
2012-10-29 alf@cadsoft.de&lt;br&gt;</description>
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="nxp_60">
<description>&lt;H1&gt;NXP Library&lt;/H1&gt;
&lt;author&gt;marco.kuystermans@nxp.com&lt;/author&gt;&lt;p&gt;

&lt;H2&gt;Disclaimer:&lt;/H2&gt;
&lt;i&gt;The information contained in this library is made available for general information and public access only. By using our 
library, you accept this disclaimer in full. If you disagree with any part of this disclaimer, you must not use our library.
Use of this library is permitted on the basis that NXP will not be liable for any loss or damage including without limitation, indirect or consequential loss or 
damage, arising out of or in connection with the use of this library.&lt;/i&gt;

&lt;H2&gt;Information:&lt;/H2&gt;
&lt;ul&gt;&lt;li&gt;Footprints are according to NXP footprint information, see &lt;a href=http://www.nxp.com&gt;NXP website&lt;/a&gt;
&lt;li&gt;SMD Footprints in this library are for reflow soldering only.
&lt;li&gt;&lt;b&gt;Library is generated as a courtesy: Information is NOT guaranteed, use at your own risk&lt;/b&gt;
&lt;li&gt;NXP package numbers (SOT/SOD) numbers used
&lt;/ul&gt;
Please send your comments to the mail address above.</description>
<packages>
<package name="SOD128">
<description>&lt;li&gt;&lt;b&gt;SOD128&lt;/b&gt;&lt;hr&gt; &lt;ul&gt;&lt;li&gt;Plastic surface-mounted package; 2 leads&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: -- &lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: --&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="SSFD - transistor- TO-252 DPAK">
<packages>
<package name="DPAK">
<description>&lt;b&gt;DPAK&lt;/b&gt; CASE 369-07&lt;br&gt;
Source MOTOROLA / ON Semiconductor mjd32-d.pdf</description>
</package>
</packages>
</library>
<library name="inductors">
<description>&lt;b&gt;Inductors and Filters&lt;/b&gt;&lt;p&gt;
Based on the previous library ind-a.lbr&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DR73">
<description>&lt;b&gt;High Power Density, High Efficiency, Shielded Inductors&lt;/b&gt;&lt;p&gt;
Source: coiltronics_dr_series.pdf</description>
</package>
<package name="DR125">
<description>&lt;b&gt;High Power Density, High Efficiency, Shielded Inductors&lt;/b&gt;&lt;p&gt;
Source: coiltronics_dr_series.pdf</description>
</package>
</packages>
</library>
<library name="JST XH 2.54 for for GG PBP">
<packages>
<package name="JST-XH-02-PACKAGE-LONG-PAD">
<description>&lt;b&gt;JST XH Connector Long Pads (Package)&lt;/b&gt;&lt;p&gt;

Wire to board connector.

Pitch: 2,54 mm, (0.100")&lt;p&gt;
Number of pins: &lt;b&gt;2&lt;/b&gt;&lt;b&gt;&lt;P&gt;

&lt;b&gt;Created by Rembrandt Electronics&lt;/b&gt;&lt;p&gt;
&lt;b&gt;www.rembrandtelectronics.com&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="SSFD_LED_0603">
<packages>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP20R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Cap no frame for 240P">
<packages>
<package name="140CLH-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, High temperature 140 CLH&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D3" library="diode" package="SOT23" value="BAT54">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="adafruit" package="SO08" value="MC33063/MC34063D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="nxp_60" package="SOD128" value="RB055LAM-30CT-ND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="R1210" value="0.08ohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="eagle-ltspice" package="C0603" value="150pF">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="adafruit" package="153CLV-0605" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="eagle-ltspice" package="C0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="adafruit" package="R0603" value="180ohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SSFD - transistor- TO-252 DPAK" package="DPAK" value="4A Ipk min">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="adafruit" package="R0603" value="13K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="adafruit" package="R0603" value="1K5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="inductors" package="DR125" value="DR125">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="JST XH 2.54 for for GG PBP" package="JST-XH-02-PACKAGE-LONG-PAD" value="+VBATT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X2" library="JST XH 2.54 for for GG PBP" package="JST-XH-02-PACKAGE-LONG-PAD" value="+12V OUT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="adafruit" package="SO08" value="MC33063/MC34063D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="nxp_60" package="SOD128" value="RB055LAM-30CT-ND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="eagle-ltspice" package="C0603" value="470pF">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="adafruit" package="153CLV-0605" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="eagle-ltspice" package="C0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="adafruit" package="R0603" value="3K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="adafruit" package="R0603" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3" library="inductors" package="DR73" value="DR73">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="adafruit" package="153CLV-0605" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="adafruit" package="R1210" value="0.08ohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X3" library="JST XH 2.54 for for GG PBP" package="JST-XH-02-PACKAGE-LONG-PAD" value="+5V OUT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="R0603" value="2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="R0603" value="2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="R0603" value="2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="SSFD_LED_0603" package="CHIP-LED0603" value="SSF_LED_0603">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="SSFD_LED_0603" package="CHIP-LED0603" value="SSF_LED_0603">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="SSFD_LED_0603" package="CHIP-LED0603" value="SSF_LED_0603">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+VIN" library="testpad" package="TP20R" value="TPSQTP20R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="+12V" library="testpad" package="TP20R" value="TPSQTP20R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="+5V" library="testpad" package="TP20R" value="TPSQTP20R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="eagle-ltspice" package="C0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="eagle-ltspice" package="C0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="Cap no frame for 240P" package="140CLH-0810" value="470uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="Cap no frame for 240P" package="140CLH-0810" value="470uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="Cap no frame for 240P" package="140CLH-0810" value="470uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="Cap no frame for 240P" package="140CLH-0810" value="470uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="adafruit" package="R0603" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="DGND">
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="-"/>
<contactref element="Q1" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="D3" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="IC1" pad="4"/>
<contactref element="X1" pad="2"/>
<contactref element="X2" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C14" pad="-"/>
<contactref element="R15" pad="2"/>
<contactref element="C16" pad="-"/>
<contactref element="D6" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="IC2" pad="4"/>
<contactref element="X3" pad="2"/>
<contactref element="LED3" pad="C"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="C3" pad="-"/>
<contactref element="C7" pad="-"/>
<contactref element="C8" pad="-"/>
<contactref element="C9" pad="-"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="3"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R5" pad="2"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="N$9">
<contactref element="Q1" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="+12V">
<contactref element="D4" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="D3" pad="3"/>
<contactref element="X2" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="+12V" pad="TP"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="+"/>
<contactref element="C7" pad="+"/>
<contactref element="C8" pad="+"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="5"/>
<contactref element="R6" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="1"/>
<contactref element="Q1" pad="3"/>
<contactref element="D4" pad="2"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="+VBATT">
<contactref element="X1" pad="1"/>
<contactref element="IC2" pad="6"/>
<contactref element="C15" pad="1"/>
<contactref element="C14" pad="+"/>
<contactref element="R12" pad="1"/>
<contactref element="IC1" pad="6"/>
<contactref element="C6" pad="1"/>
<contactref element="C5" pad="+"/>
<contactref element="R4" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="+VIN" pad="TP"/>
</signal>
<signal name="N$7">
<contactref element="IC2" pad="7"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC2" pad="1"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="IC2" pad="3"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="C16" pad="+"/>
<contactref element="L3" pad="2"/>
<contactref element="R14" pad="1"/>
<contactref element="X3" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="+5V" pad="TP"/>
<contactref element="C1" pad="2"/>
<contactref element="C9" pad="+"/>
</signal>
<signal name="SWITCH">
<contactref element="IC2" pad="2"/>
<contactref element="D6" pad="1"/>
<contactref element="L3" pad="1"/>
</signal>
<signal name="IPK">
<contactref element="R5" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$1">
<contactref element="LED2" pad="A"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="5V">
<contactref element="R3" pad="2"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="C1" pad="1"/>
<contactref element="IC2" pad="5"/>
<contactref element="R14" pad="2"/>
<contactref element="R15" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
