(kicad_pcb (version 4) (host pcbnew 4.0.3-stable)
  (general
    (links 71)
    (no_connects 6)
    (area 71.2852 42.266399 127.456401 84.2898)
    (thickness 1.6)
    (drawings 14)
    (tracks 266)
    (zones 0)
    (modules 56)
    (nets 28)
  )
  (page A3)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.36)
    (user_trace_width 0.508)
    (user_trace_width 0.8636)
    (user_trace_width 1.016)
    (user_trace_width 1.27)
    (user_trace_width 1.524)
    (user_trace_width 1.778)
    (user_trace_width 2.032)
    (trace_clearance 0.254)
    (zone_clearance 0.708)
    (zone_45_only yes)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.397 1.397)
    (pad_drill 0.8128)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 71.4502 84.1248)
    (visible_elements 7FFFF7FF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory C:/Users/JaneCharlie/Desktop/Chuck/PW3B_LPF/PW3B_LPF))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 VDD)
  (net 4 "Net-(B1-Pad1)")
  (net 5 "Net-(B2-Pad1)")
  (net 6 "Net-(B3-Pad1)")
  (net 7 "Net-(C1-Pad1)")
  (net 8 "Net-(C1-Pad2)")
  (net 9 "Net-(C3-Pad2)")
  (net 10 "Net-(C4-Pad1)")
  (net 11 "Net-(C4-Pad2)")
  (net 12 "Net-(C9-Pad1)")
  (net 13 "Net-(C14-Pad1)")
  (net 14 "Net-(C10-Pad1)")
  (net 15 "Net-(C10-Pad2)")
  (net 16 "Net-(C14-Pad2)")
  (net 17 "Net-(C15-Pad1)")
  (net 18 "Net-(C15-Pad2)")
  (net 19 "Net-(M1-Pad1)")
  (net 20 "Net-(M3-Pad1)")
  (net 21 "Net-(R3-Pad1)")
  (net 22 "Net-(R18-Pad1)")
  (net 23 "Net-(R8-Pad1)")
  (net 24 "Net-(C2-Pad2)")
  (net 25 "Net-(C3-Pad1)")
  (net 26 "Net-(C8-Pad2)")
  (net 27 "Net-(R14-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net GND)
    (add_net "Net-(B1-Pad1)")
    (add_net "Net-(B2-Pad1)")
    (add_net "Net-(B3-Pad1)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C14-Pad2)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C15-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(M1-Pad1)")
    (add_net "Net-(M3-Pad1)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(R18-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net VCC)
    (add_net VDD)
  )
  (module 22Ga_pad_ell_med (layer F.Cu) (tedit 586D2E14)
    (at 92 43.8 180)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference M1 (at -1.875 -1.75 180) (layer F.SilkS))
    (fp_text value CONN_1 (at 0.08 -1.35 180) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 2.0828 1.8796) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(M1-Pad1)"))
  )
  (module 22Ga_pad_ell_med (layer F.Cu) (tedit 586D2E0E)
    (at 95.9 43.8 180)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference B1 (at -2.2 0.02 180) (layer F.SilkS))
    (fp_text value CONN_1 (at 0.23 -1.52 180) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 2.0828 1.8796) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(B1-Pad1)"))
  )
  (module 22Ga_pad_ell_med (layer F.Cu) (tedit 586D2E31)
    (at 76.8 43.8 180)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference M2 (at 2.325 0.025 180) (layer F.SilkS))
    (fp_text value CONN_1 (at -1.54 -1.13 180) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 2.0828 1.8796) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C4-Pad2)"))
  )
  (module 22Ga_pad_ell_med (layer F.Cu) (tedit 586D2E29)
    (at 80.6 43.8 180)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference B2 (at 0 -1.8 180) (layer F.SilkS))
    (fp_text value CONN_1 (at -1.77 -1.07 180) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 2.0828 1.8796) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(B2-Pad1)"))
  )
  (module 22Ga_pad_ell_med (layer F.Cu) (tedit 586D2E23)
    (at 84.4 43.8 180)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference M3 (at -0.1 -1.8 180) (layer F.SilkS))
    (fp_text value CONN_1 (at -1.71 -1.02 180) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 2.0828 1.8796) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(M3-Pad1)"))
  )
  (module 22Ga_pad_ell_med (layer F.Cu) (tedit 586D2E1D)
    (at 88.2 43.8 180)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference B3 (at 0.125 -1.8 180) (layer F.SilkS))
    (fp_text value CONN_1 (at -1.43 -1.07 180) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 2.0828 1.8796) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(B3-Pad1)"))
  )
  (module 22Ga_pad_ell_med (layer F.Cu) (tedit 5823CA70)
    (at 100.5 43.8)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference T2 (at 2.1 -0.06) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 2.794) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0) (size 2.0828 1.8796) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(R14-Pad2)"))
  )
  (module 22Ga_pad_ell_med (layer F.Cu) (tedit 586D2E01)
    (at 109.19 43.8 180)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference T1 (at -2.14 0.06 180) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 -1.41 180) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 2.0828 1.8796) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(R18-Pad1)"))
  )
  (module 22Ga_pad_ell_med (layer F.Cu) (tedit 5823C2E2)
    (at 123.3 75.6)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference OGnd (at -0.11 1.54 180) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 2.794) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0) (size 2.0828 1.8796) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module 22Ga_pad_ell_med (layer F.Cu) (tedit 5823C89C)
    (at 73.3 70.4 180)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference IGnd (at -2.11 -0.06 360) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 2.794 180) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 2.0828 1.8796) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module 22Ga_pad_ell_med (layer F.Cu) (tedit 5823C2CC)
    (at 73.4 74.3)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference IN (at 1.78 0.09) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 2.794) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0) (size 2.0828 1.8796) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C1-Pad2)"))
  )
  (module 22Ga_pad_ell_med (layer F.Cu) (tedit 5823C2DA)
    (at 120.6754 78.0034 180)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference OUT (at 0.0454 -1.6766 180) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 2.794 180) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 2.0828 1.8796) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(C15-Pad1)"))
  )
  (module 22Ga_pad_ell_med (layer F.Cu) (tedit 58225D79)
    (at 114.02 45.96 45)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference Res3 (at -0.035355 -1.661701 45) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 2.794 45) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0 45) (size 2.0828 1.8796) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(R14-Pad2)"))
  )
  (module 22Ga_pad_ell_med (layer F.Cu) (tedit 58225D51)
    (at 117.57 47.39 45)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference Res4 (at -0.035355 -1.661701 45) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 2.794 45) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0 45) (size 2.0828 1.8796) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(R14-Pad2)"))
  )
  (module 22Ga_pad_ell_med (layer F.Cu) (tedit 58225DB4)
    (at 116.86 52.17 45)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference Res1 (at -0.025 -1.575 45) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 2.794 45) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0 45) (size 2.0828 1.8796) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(R14-Pad2)"))
  )
  (module 22Ga_pad_ell_med (layer F.Cu) (tedit 58225541)
    (at 113.25 50.71 45)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference Res2 (at -0.075 -1.6 45) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 2.794 45) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0 45) (size 2.0828 1.8796) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(R14-Pad2)"))
  )
  (module Res_.25watt_ovalpad1 (layer F.Cu) (tedit 58202160)
    (at 106.62 46.88)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R12 (at -0.1 0.075) (layer F.SilkS))
    (fp_text value 4K7 (at -1 0.1) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -5.08 0) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(C10-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(R18-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Nichi_22uF_25V (layer F.Cu) (tedit 582240F8)
    (at 116.09 62.37 270)
    (descr "Condensateur e = 1 pas")
    (tags C)
    (fp_text reference C17 (at -0.01 -1.53 360) (layer F.SilkS))
    (fp_text value 22u (at 0.02 1.58 270) (layer F.SilkS) hide)
    (fp_text user + (at -1.21 1.38 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.25 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 VDD))
    (pad 2 thru_hole oval (at 1.125 0 270) (size 1.397 1.6) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/c_vert_c1v5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_.25watt_ovalpad1 (layer F.Cu) (tedit 582020BF)
    (at 80.62 53.11 90)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R7 (at 0.01 0.08 90) (layer F.SilkS))
    (fp_text value 20K (at 0 0.127 90) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -5.08 0 90) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(R8-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C4-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_.25watt_ovalpad1 (layer F.Cu) (tedit 58202091)
    (at 109.8 72.05)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R15 (at 0 0.075) (layer F.SilkS))
    (fp_text value 4K7 (at 0 0.127) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -5.08 0) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C14-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(C14-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_.25watt_ovalpad1 (layer F.Cu) (tedit 58202008)
    (at 106.7054 79.629)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R16 (at 0 0.127) (layer F.SilkS))
    (fp_text value 332 (at 0 0.127) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -5.08 0) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C14-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(C15-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_.25watt_ovalpad1 (layer F.Cu) (tedit 5823C316)
    (at 78.4 76.89 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R1 (at 0 -0.03 270) (layer F.SilkS))
    (fp_text value 261K (at 0 0.127 270) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -5.08 0 270) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 3 VDD))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C1-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_.25watt_ovalpad1 (layer F.Cu) (tedit 58202107)
    (at 86.3 52.3 90)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R9 (at 0 0.05 90) (layer F.SilkS))
    (fp_text value 8K2 (at 0 0.127 90) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -5.08 0 90) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C10-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(M3-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_.25watt_ovalpad1 (layer F.Cu) (tedit 582021FB)
    (at 97.4 54 90)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R13 (at 0 0.05 90) (layer F.SilkS))
    (fp_text value 2K (at 0 0.127 90) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -5.08 0 90) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(C8-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(R14-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_.25watt_ovalpad1 (layer F.Cu) (tedit 557E3F4E)
    (at 91.9 51.4 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R5 (at -0.00444 -0.1366 270) (layer F.SilkS))
    (fp_text value 8K2 (at 0 0.127 270) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -5.08 0 270) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(M1-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(C3-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_.25watt_ovalpad1 (layer F.Cu) (tedit 58203369)
    (at 94.7 52.6 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R6 (at 0 -0.1 270) (layer F.SilkS))
    (fp_text value 17K4 (at 0 0.127 270) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -5.08 0 270) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(B1-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(C3-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_.25watt_ovalpad1 (layer F.Cu) (tedit 582020D5)
    (at 83.42 53.11 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R8 (at -0.01 -0.055 270) (layer F.SilkS))
    (fp_text value 127K (at 0 0.127 270) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -5.08 0 270) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(B2-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(R8-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_.25watt_ovalpad1 (layer F.Cu) (tedit 5823C310)
    (at 80.899 76.89 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R3 (at 0.008 -0.071 270) (layer F.SilkS))
    (fp_text value 2K2 (at 0 0.127 270) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -5.08 0 270) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(R3-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C1-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_.25watt_ovalpad1 (layer F.Cu) (tedit 5823C308)
    (at 88.6206 77.3684 180)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R2 (at 0.0806 -0.0216 180) (layer F.SilkS))
    (fp_text value 8K2 (at 0 0.127 180) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -5.08 0 180) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(C2-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C3-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_.25watt_ovalpad1 (layer F.Cu) (tedit 582023CC)
    (at 89.15 53.11 90)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R10 (at 0.01 0.05 90) (layer F.SilkS))
    (fp_text value 17K4 (at 0 0.127 90) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -5.08 0 90) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C10-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(B3-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_.25watt_ovalpad1 (layer F.Cu) (tedit 5823C2FF)
    (at 88.6206 74.9554 180)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R4 (at -0.0294 -0.0646 180) (layer F.SilkS))
    (fp_text value 3K6 (at 0 0.127 180) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -5.08 0 180) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(C3-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C3-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_.25watt_ovalpad1 (layer F.Cu) (tedit 5823C39A)
    (at 122.51 56.13 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R17 (at 0 -0.075 270) (layer F.SilkS))
    (fp_text value 261K (at 0 0.127 450) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -5.08 0 270) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 3 VDD))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_.25watt_ovalpad1 (layer F.Cu) (tedit 582022A1)
    (at 120 66.25 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R18 (at -0.0106 -0.0616 270) (layer F.SilkS))
    (fp_text value 261K (at 0 0.127 270) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -5.08 0 270) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 3 VDD))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module 22Ga_pad_ell (layer F.Cu) (tedit 586D2DF8)
    (at 125.56 58.79 90)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference GND (at 1.9 0 180) (layer F.SilkS))
    (fp_text value CONN_1 (at 0.23 -1.51 90) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0 90) (size 2.286 1.9812) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module Nichi_22uF_25V (layer F.Cu) (tedit 586D3297)
    (at 123.975 66.25)
    (descr "Condensateur e = 1 pas")
    (tags C)
    (fp_text reference C16 (at 0.1816 -1.484 180) (layer F.SilkS))
    (fp_text value 47u (at 0.02 1.58) (layer F.SilkS) hide)
    (fp_text user + (at -1.21 1.38) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.25 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole oval (at 1.125 0) (size 1.397 1.6) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/c_vert_c1v5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DIP-8__300_ELL (layer F.Cu) (tedit 558A4038)
    (at 106 65.105 180)
    (descr "8 pins DIL package, elliptical pads")
    (tags DIL)
    (fp_text reference U2 (at 3.27 0.04 270) (layer F.SilkS) hide)
    (fp_text value LT1351 (at 0 0 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -3.81 3.81 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at -1.27 3.81 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(C14-Pad2)"))
    (pad 3 thru_hole oval (at 1.27 3.81 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C9-Pad1)"))
    (pad 4 thru_hole oval (at 3.81 3.81 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole oval (at 3.81 -3.81 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 1.27 -3.81 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C14-Pad1)"))
    (pad 7 thru_hole oval (at -1.27 -3.81 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 8 thru_hole oval (at -3.81 -3.81 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (model dil/dil_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DIP-8__300_ELL (layer F.Cu) (tedit 586920C0)
    (at 84.305 65.105 180)
    (descr "8 pins DIL package, elliptical pads")
    (tags DIL)
    (fp_text reference U1 (at 3.445 0.005 180) (layer F.SilkS) hide)
    (fp_text value LT1352 (at 0 0 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -3.81 3.81 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C10-Pad1)"))
    (pad 2 thru_hole oval (at -1.27 3.81 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(R8-Pad1)"))
    (pad 3 thru_hole oval (at 1.27 3.81 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 VDD))
    (pad 4 thru_hole oval (at 3.81 3.81 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole oval (at 3.81 -3.81 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(R3-Pad1)"))
    (pad 6 thru_hole oval (at 1.27 -3.81 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C3-Pad2)"))
    (pad 7 thru_hole oval (at -1.27 -3.81 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(C3-Pad1)"))
    (pad 8 thru_hole oval (at -3.81 -3.81 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model dil/dil_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 68pF_silvermica (layer F.Cu) (tedit 57FDFF5E)
    (at 85.471 72.1868 180)
    (descr "Condensateur = 2 pas")
    (tags C)
    (fp_text reference C3 (at 0 0 180) (layer F.SilkS))
    (fp_text value 100p (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -2 0 180) (size 1.63 1.5) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(C3-Pad1)"))
    (pad 2 thru_hole oval (at 2 0 180) (size 1.63 1.5) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C3-Pad2)"))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module connect:22Ga_pad_ell_med (layer F.Cu) (tedit 586D2E08)
    (at 104.8 43.8 180)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference T3 (at -2.15 0.05 360) (layer F.SilkS))
    (fp_text value CONN_1 (at -0.03 -1.46 180) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 2.0828 1.8796) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C9-Pad1)"))
  )
  (module connect:22Ga_pad_ell_med (layer F.Cu) (tedit 582257C1)
    (at 123.875 70.25 270)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference V+ (at -0.825 -2.075 360) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 2.794 270) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0 270) (size 2.0828 1.8796) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
  )
  (module connect:PWE_scriptlogo20F_mirrored (layer F.Cu) (tedit 0)
    (at 102.9208 82.423)
    (fp_text reference VAL (at 0 0) (layer F.SilkS) hide)
    (fp_text value REF (at 0 0) (layer F.SilkS) hide)
  )
  (module PWE_scriptlogo20B:PWE_scriptlogo20B (layer F.Cu) (tedit 0)
    (at 102.7 82.4)
    (fp_text reference VAL (at 0 0) (layer F.SilkS) hide)
    (fp_text value REF (at 0 0) (layer F.SilkS) hide)
  )
  (module discret:Res_.25watt_ovalpad1 (layer F.Cu) (tedit 586C55A3)
    (at 120 53.64 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R11 (at 0.055 -0.07 270) (layer F.SilkS))
    (fp_text value 4K2 (at 0 0.127 270) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -5.08 0 270) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(R18-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 3 VDD))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module discret:Res_.25watt_ovalpad1 (layer F.Cu) (tedit 586C55B4)
    (at 111.94 58.1)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R14 (at 0 0) (layer F.SilkS))
    (fp_text value 4K2 (at 0 0.127) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -5.08 0) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(C14-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 3 VDD))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:Wima470p_FKP2_ell (layer F.Cu) (tedit 586D3250)
    (at 76.66736 48.95088 90)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference C4 (at 0 0.127 180) (layer F.SilkS))
    (fp_text value 2n7 (at 0 0.127 90) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -2.5 0 90) (size 1.8 1.651) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C4-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.8 1.651) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C4-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:Wima470p_FKP2_ell (layer F.Cu) (tedit 586D322F)
    (at 101.4 52.3 90)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference C5 (at 0 0.127 180) (layer F.SilkS))
    (fp_text value 1u5 (at 0 0.127 90) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -2.5 0 90) (size 1.8 1.651) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C10-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.8 1.651) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(C10-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:Wima470p_FKP2_ell (layer F.Cu) (tedit 586D327E)
    (at 109.0422 75.819)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference C8 (at 0 0.127) (layer F.SilkS))
    (fp_text value 220p (at 0 0.127) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -2.5 0) (size 1.8 1.651) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C14-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0) (size 1.8 1.651) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(C14-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:Wima1uF_ovalpads (layer F.Cu) (tedit 586D3240)
    (at 116.1288 78.3844 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference C9 (at 0 0.127 360) (layer F.SilkS))
    (fp_text value 1u5 (at 0 0.127 270) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -2.5 0 270) (size 1.8 1.651) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(C15-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.8 1.651) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(C15-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:Wima1uF_ovalpads (layer F.Cu) (tedit 586D3239)
    (at 88.6714 81.28)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference C2 (at 0 0.127) (layer F.SilkS))
    (fp_text value 1u (at 0 0.127) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -2.5 0) (size 1.8 1.651) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.5 0) (size 1.8 1.651) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(C2-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:Wima1uF_ovalpads (layer F.Cu) (tedit 586D2D59)
    (at 74.48804 79.51724 90)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference C1 (at 0 0.127 180) (layer F.SilkS))
    (fp_text value 100n (at 0 0.127 90) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -2.5 0 90) (size 1.8 1.651) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.8 1.651) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C1-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:Siemens_.1uF_X7R50v (layer F.Cu) (tedit 586D2C42)
    (at 92.9 69 180)
    (descr "Condensateur e = 1 pas")
    (tags C)
    (fp_text reference C23 (at 0 -0.075 180) (layer F.SilkS))
    (fp_text value .1u (at -0.1 -0.1 180) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -2.5 0 180) (size 1.6 1.5) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.6 1.5) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:Siemens_.1uF_X7R50v (layer F.Cu) (tedit 586D2C42)
    (at 114.93 68.93)
    (descr "Condensateur e = 1 pas")
    (tags C)
    (fp_text reference C24 (at 0 -0.075) (layer F.SilkS))
    (fp_text value .1u (at -0.1 -0.1) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -2.5 0) (size 1.6 1.5) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole oval (at 2.5 0) (size 1.6 1.5) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:Siemens_.1uF_X7R50v (layer F.Cu) (tedit 586D2C42)
    (at 77.8002 61.50864 90)
    (descr "Condensateur e = 1 pas")
    (tags C)
    (fp_text reference C21 (at 0 -0.075 90) (layer F.SilkS))
    (fp_text value .1u (at -0.1 -0.1 90) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -2.5 0 90) (size 1.6 1.5) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 3 VDD))
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.6 1.5) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:Siemens_.1uF_X7R50v (layer F.Cu) (tedit 586D2C42)
    (at 97.2 62.1 180)
    (descr "Condensateur e = 1 pas")
    (tags C)
    (fp_text reference C22 (at 0 -0.075 180) (layer F.SilkS))
    (fp_text value .1u (at -0.1 -0.1 180) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -2.5 0 180) (size 1.6 1.5) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 3 VDD))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.6 1.5) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:Wima.68uF_ell (layer F.Cu) (tedit 586D3843)
    (at 99.5 73.9 180)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference C6 (at 0 0 180) (layer F.SilkS))
    (fp_text value 8n2 (at 0 0.127 180) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -2.5 0 180) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C14-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.8 1.651) (drill 0.812799) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(C8-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:Wima470p_FKP2_ell (layer F.Cu) (tedit 586D36B4)
    (at 107.88 54.1)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference C7 (at 0 0.127) (layer F.SilkS))
    (fp_text value 6n8 (at 0 0.127) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -2.5 0) (size 1.8 1.651) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C9-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0) (size 1.8 1.651) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 3 VDD))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 72.125 42.325) (end 71.55 42.9) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 127.4064 51.3842) (end 118.3386 42.3164) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 127.4064 53.8988) (end 127.4064 51.3588) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.7986 42.3164) (end 118.3386 42.3164) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 127.4064 74.5998) (end 127.4064 74.5744) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.9322 84.074) (end 127.4064 74.5998) (angle 90) (layer Edge.Cuts) (width 0.1))
  (target plus (at 71.4502 84.1248) (size 0.33) (width 0.01) (layer Edge.Cuts))
  (gr_line (start 127.4064 53.848) (end 127.4064 74.5744) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 71.52132 83.48472) (end 72.10806 84.07146) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 71.52132 81.43494) (end 71.52132 83.48472) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 71.5276 81.45828) (end 71.5276 42.93) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.9322 84.074) (end 72.1 84.074) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.125 42.3184) (end 115.819 42.3184) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text "PW3B Bass Preamp v1.0 by Charlie Escher 2017\nCreative Commons CC BY-NC-SA 4.0\nNoncommercial ShareAlike License" (at 73.46 56.16 90) (layer B.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.708))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.381) (thermal_bridge_width 0.8382))
    (polygon
      (pts
        (xy 127.1524 42.6974) (xy 127.1778 83.9216) (xy 71.7296 83.947) (xy 71.8058 42.5704)
      )
    )
    (polygon
      (pts        (xy 85.2424 73.3806) (xy 86.614 73.3806) (xy 87.8 70.75) (xy 87.9 70.04) (xy 87.9 69.96)
        (xy 85.2424 69.9516)
      )
    )
    (polygon
      (pts        (xy 78.64 69.95) (xy 78.64 73.38) (xy 85.23 73.38) (xy 85.23 69.95)
      )
    )
    (polygon
      (pts        (xy 102.09 70.34) (xy 102.09 70.76) (xy 107.21 70.76) (xy 107.21 70.34)
      )
    )
    (polygon
      (pts        (xy 72.2 65.7) (xy 72.7 65.2) (xy 76.8 65.2) (xy 76.8 63.1) (xy 72.7 63.1)
        (xy 72.2 62.6)
      )
    )
    (polygon
      (pts        (xy 89.53 59.54) (xy 89.53 62.92) (xy 90.03 62.92) (xy 90.03 59.54)
      )
    )
    (polygon
      (pts        (xy 79.56 62.77) (xy 79.83 62.77) (xy 79.83 62.76) (xy 79.76 62.57)
      )
    )
    (polygon
      (pts        (xy 100.55 60.82) (xy 100.95 61.22) (xy 100.95 61.19) (xy 100.58 60.82)
      )
    )
    (polygon
      (pts        (xy 103.38 59.29) (xy 103.38 60.21) (xy 108.52 60.21) (xy 108.52 58.2) (xy 105.23 58.64)
        (xy 104.49 58.64) (xy 104.02 58.64) (xy 103.59 58.91)
      )
    )
    (polygon
      (pts        (xy 79.53 59.35) (xy 79.55 59.38) (xy 79.95 59.9) (xy 80.28 59.9) (xy 80.28 59.34)
      )
    )
  )
)
