(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")
  (general
    (thickness 1.6)
    (drawings 15)
    (tracks 111)
    (zones 0)
    (modules 34)
    (nets 18)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(BT1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C1-Pad1)")
  (net 4 "Net-(D1-Pad2)")
  (net 5 "Net-(J1-Pad1)")
  (net 6 "Net-(J3-Pad1)")
  (net 7 "Net-(J4-Pad1)")
  (net 8 "Net-(LED1-Pad2)")
  (net 9 "Net-(LED1-Pad1)")
  (net 10 "Net-(LED2-Pad2)")
  (net 11 "Net-(Q1-Pad3)")
  (net 12 "Net-(Q1-Pad2)")
  (net 13 "Net-(R5-Pad2)")
  (net 14 "Net-(R6-Pad2)")
  (net 15 "Net-(R7-Pad2)")
  (net 16 "Net-(SW2-Pad1)")
  (net 17 "Net-(L1-Pad1)")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.3)
    (diff_pair_gap 0.5)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(L1-Pad1)")
  )
  (net_class Standard ""
    (clearance 0.3)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(LED1-Pad1)")
    (add_net "Net-(LED1-Pad2)")
    (add_net "Net-(LED2-Pad2)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(SW2-Pad1)")
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 92.837 56.007)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R9 (at 5.163 -0.007) (layer F.SilkS))
    (fp_text value 510k (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J4-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(L1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 92.837 52)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R8 (at 5.163 0) (layer F.SilkS))
    (fp_text value 510k (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(R7-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(L1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Joe_footprint_Library:Kazoosh!_small_Logo_Bottom_Silkscreen (layer F.Cu) (tedit 606654F2)
    (at 66.8 64.9 270)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Joe_footprint_Library:OSHW-Logo2_7.3x6mm_Bottom_SilkScreen (layer F.Cu) (tedit 6066530D)
    (at 114.7 61.1)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_Bottom_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module Joe_footprint_Library:KiCad-Logo_5mm_Bottom_SilkScreen (layer F.Cu) (tedit 60664BF7)
    (at 114.7 70.1)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value KiCad-Logo_5mm_Bottom_SilkScreen (at 0 3.81) (layer F.Fab) hide)
  )
  (module Joe_footprint_Library:SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm_Relief (layer F.Cu) (tedit 60661A43)
    (at 76 56 270)
    (descr "Soldered wire connection with feed through strain relief, for a single 0.5 mm² wire, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm strain-relief")
    (attr virtual)
    (fp_text reference J4 (at 0 10 180) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 15.1 270) (layer F.Fab))
    (fp_text user %R (at 0 6.3) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 12.6 270) (size 2.6 2.6) (drill 2.6) (layers *.Cu *.Mask))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask) (roundrect_rratio 0.119048)
      (net 7 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm_Relief.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Joe_footprint_Library:SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm_Relief (layer F.Cu) (tedit 60661A43)
    (at 76 52 270)
    (descr "Soldered wire connection with feed through strain relief, for a single 0.5 mm² wire, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm strain-relief")
    (attr virtual)
    (fp_text reference J3 (at 0 10 180) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 15.1 270) (layer F.Fab))
    (fp_text user %R (at 0 6.3) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 12.6 270) (size 2.6 2.6) (drill 2.6) (layers *.Cu *.Mask))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask) (roundrect_rratio 0.119048)
      (net 6 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm_Relief.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Joe_footprint_Library:SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm_Relief (layer F.Cu) (tedit 60661A43)
    (at 76 74 270)
    (descr "Soldered wire connection with feed through strain relief, for a single 0.5 mm² wire, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm strain-relief")
    (attr virtual)
    (fp_text reference J2 (at 0 10 180) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 15.1 270) (layer F.Fab))
    (fp_text user %R (at 0 6.3) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 12.6 270) (size 2.6 2.6) (drill 2.6) (layers *.Cu *.Mask))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask) (roundrect_rratio 0.119048)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm_Relief.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Joe_footprint_Library:SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm_Relief (layer F.Cu) (tedit 60661A43)
    (at 76 78 270)
    (descr "Soldered wire connection with feed through strain relief, for a single 0.5 mm² wire, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm strain-relief")
    (attr virtual)
    (fp_text reference J1 (at 0 10 180) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 15.1 270) (layer F.Fab))
    (fp_text user %R (at 0 6.3) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 12.6 270) (size 2.6 2.6) (drill 2.6) (layers *.Cu *.Mask))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask) (roundrect_rratio 0.119048)
      (net 5 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm_Relief.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 70 76)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference M3 (at 0 0) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_Pad_TopBottom (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 connect circle (at 0 0) (size 6.4 6.4) (layers B.Cu B.Mask))
    (pad 1 connect circle (at 0 0) (size 6.4 6.4) (layers F.Cu F.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 70 54)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference M3 (at 0 0) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_Pad_TopBottom (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask))
    (pad 1 connect circle (at 0 0) (size 6.4 6.4) (layers F.Cu F.Mask))
    (pad 1 connect circle (at 0 0) (size 6.4 6.4) (layers B.Cu B.Mask))
  )
  (module Package_TO_SOT_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 5A02FF81)
    (at 79.883 73.533 270)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q3 (at 6.223 -2.032 180) (layer F.SilkS))
    (fp_text value 2N7000 (at 2.54 2.79 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 5A02FF81)
    (at 84.074 73.533 270)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at 6.096 -2.032 180) (layer F.SilkS))
    (fp_text value 2N7000 (at 2.54 2.79 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Joe_footprint_Library:PROTO26 (layer F.Cu) (tedit 6065C0AB)
    (at 102.235 61.2394)
    (fp_text reference PROTO (at 0 -2.2394) (layer F.SilkS) hide)
    (fp_text value PROTO26 (at 0 0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at -7.62 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -5.08 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -2.54 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 2.54 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 5.08 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 7.62 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at -2.54 2.54) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 0 2.54) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -7.62 2.54) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 2.54 2.54) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 7.62 2.54) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at -5.08 2.54) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 5.08 2.54) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at -2.54 5.08) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 18 thru_hole circle (at 0 5.08) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at -7.62 5.08) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at -5.08 5.08) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 21 thru_hole circle (at 7.62 5.08) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at 5.08 5.08) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at 2.54 5.08) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 24 thru_hole circle (at -2.54 7.62) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 26 thru_hole circle (at 2.54 7.62) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 25 thru_hole circle (at 0 7.62) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at -5.08 7.62) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 22 thru_hole circle (at -7.62 7.62) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
  )
  (module Joe_footprint_Library:PROTO28 (layer F.Cu) (tedit 6065C050)
    (at 81.915 61.2394)
    (fp_text reference PROTO (at 0.085 -2.2394) (layer F.SilkS) hide)
    (fp_text value PROTO28 (at 0 0.5) (layer F.Fab))
    (pad 27 thru_hole circle (at 5.08 7.62) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 28 thru_hole circle (at 7.62 7.62) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 22 thru_hole circle (at -7.62 7.62) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at -5.08 7.62) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 25 thru_hole circle (at 0 7.62) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 26 thru_hole circle (at 2.54 7.62) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 24 thru_hole circle (at -2.54 7.62) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at 2.54 5.08) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at 5.08 5.08) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 21 thru_hole circle (at 7.62 5.08) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at -5.08 5.08) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at -7.62 5.08) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 18 thru_hole circle (at 0 5.08) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at -2.54 5.08) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 5.08 2.54) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at -5.08 2.54) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 7.62 2.54) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 2.54 2.54) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -7.62 2.54) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 0 2.54) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at -2.54 2.54) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 7.62 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 5.08 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 2.54 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -2.54 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -5.08 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -7.62 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask))
  )
  (module Battery:BatteryHolder_Keystone_2466_1xAAA (layer F.Cu) (tedit 6065BF14)
    (at 70 65)
    (descr "1xAAA Battery Holder, Keystone, Plastic Case, http://www.keyelco.com/product-pdf.cfm?p=1031")
    (tags "AAA battery holder Keystone")
    (fp_text reference BT1 (at 0 -4 180) (layer F.SilkS))
    (fp_text value "NiMH 1,25V 600mAh" (at 22.86 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (fp_text user + (at -3.81 0) (layer F.SilkS))
    (fp_text user - (at 48.26 0) (layer F.SilkS))
    (fp_text user "NiMH 1,2V 600mAh" (at 22.098 5.842) (layer F.SilkS))
    (pad 2 thru_hole circle (at 44.7 0) (size 2 2) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad1)"))
    (model ${KISYS3DMOD}/Battery.3dshapes/BatteryHolder_Keystone_2466_1xAAA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Joe_footprint_Library:SW_PUSH_6mm_H5mm_4pin (layer F.Cu) (tedit 6062355E)
    (at 115 56 180)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (fp_text reference SW2 (at 3.25 2.25) (layer F.SilkS))
    (fp_text value SW_Push_standard_6x6_four_pins (at 3.75 6.7) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 3 thru_hole circle (at 6.5 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 6.5 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 "Net-(SW2-Pad1)"))
    (pad 2 thru_hole circle (at 0 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 "Net-(SW2-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 120 52)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 3.81 4) (layer F.SilkS))
    (fp_text value ATtiny85V-10PU (at 3.81 9.95) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(LED1-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J4-Pad1)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(R6-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(R7-Pad2)"))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(R5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(SW2-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Array_SIP4 (layer F.Cu) (tedit 5A14249F)
    (at 115 74 180)
    (descr "4-pin Resistor SIP pack")
    (tags R)
    (fp_text reference U1 (at 11 0) (layer F.SilkS))
    (fp_text value YX8051_JF (at 5.08 2.4) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(L1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Array_SIP4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_Slide_1P2T_CK_OS102011MS2Q (layer F.Cu) (tedit 5C5044D5)
    (at 63 63 270)
    (descr "CuK miniature slide switch, OS series, SPDT, https://www.ckswitches.com/media/1428/os.pdf")
    (tags "switch SPDT")
    (fp_text reference SW1 (at 8 0 180) (layer F.SilkS))
    (fp_text value SW_SPDT (at 2 3 90) (layer F.Fab))
    (fp_text user %R (at 3.99 -2.99 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.5 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad1)"))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.5 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(L1-Pad1)"))
    (pad 3 thru_hole oval (at 4 0 270) (size 1.5 2.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" thru_hole oval (at -2.1 0 270) (size 2.2 3.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 6.1 0 270) (size 2.2 3.5) (drill 1.5) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_Slide_1P2T_CK_OS102011MS2Q.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 79.883 52)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 5.08 0) (layer F.SilkS))
    (fp_text value 120 (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(R7-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 131 70.06 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 5.06 0 90) (layer F.SilkS))
    (fp_text value 120 (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(R6-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(LED2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 134.2 59.9 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 5.1 0.2 90) (layer F.SilkS))
    (fp_text value 120 (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(R5-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(LED1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 128 78 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 5.08 0) (layer F.SilkS))
    (fp_text value 220k (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 102 78 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.08 0) (layer F.SilkS))
    (fp_text value 510k (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(Q1-Pad3)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 90.043 56 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 0) (layer F.SilkS))
    (fp_text value 330k (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 102 74 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 0) (layer F.SilkS))
    (fp_text value 1M (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(Q1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 5A02FF81)
    (at 88.265 73.533 270)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 6.217 -2.0955 180) (layer F.SilkS))
    (fp_text value 2N7000 (at 2.54 2.79 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(Q1-Pad3)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 131 75)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference LED2 (at 1.27 4) (layer F.SilkS))
    (fp_text value LED_GN (at 1.27 3.96) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(LED2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(LED1-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 131 55)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference LED1 (at 1.27 -3.96) (layer F.SilkS))
    (fp_text value LED_GN (at 1.27 3.96) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(LED1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(LED1-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 115 78 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference L1 (at 5.08 0) (layer F.SilkS))
    (fp_text value 47uH (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(L1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 120 64 270)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D1 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value BAT48RL (at 5.08 2.12 90) (layer F.Fab))
    (fp_text user K (at 2 -1 90) (layer F.SilkS))
    (fp_text user K (at 0 -1.8 90) (layer F.Fab))
    (fp_text user %R (at 5.38 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 128 64 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (fp_text reference C2 (at 2.5 0) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.5) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 127 70 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C1 (at 1.25 -4.4) (layer F.SilkS))
    (fp_text value 220uF (at 1.25 4.4) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "CPU\nRESET" (at 112 53.8 270) (layer B.SilkS))
  (gr_text "8MHz CLOCK\n8kByte FLASH\n2kByte RAM" (at 123.8 55.7 -90) (layer B.SilkS))
  (gr_text "prototyping area: hack the solaranimals!" (at 92 58.6) (layer B.SilkS))
  (gr_text "open hardware: github.com/kazoosh" (at 92 71.5) (layer B.SilkS))
  (dimension 39 (width 0.15) (layer Dwgs.User)
    (gr_text "39.000 mm" (at 78.5 45.7) (layer Dwgs.User))
    (feature1 (pts (xy 98 49) (xy 98 46.413579)))
    (feature2 (pts (xy 59 49) (xy 59 46.413579)))
    (crossbar (pts (xy 59 47) (xy 98 47)))
    (arrow1a (pts (xy 98 47) (xy 96.873496 47.586421)))
    (arrow1b (pts (xy 98 47) (xy 96.873496 46.413579)))
    (arrow2a (pts (xy 59 47) (xy 60.126504 47.586421)))
    (arrow2b (pts (xy 59 47) (xy 60.126504 46.413579)))
  )
  (gr_text V1.3 (at 104.8 54 -90) (layer F.SilkS))
  (gr_text RESET (at 106.2 54 270) (layer F.SilkS))
  (gr_text "- SOLAR +" (at 60.5 76 270) (layer F.SilkS))
  (gr_text PIEZO (at 60.5 54 270) (layer F.SilkS))
  (dimension 32 (width 0.15) (layer Dwgs.User)
    (gr_text "32,000 mm" (at 143.3 65 270) (layer Dwgs.User))
    (feature1 (pts (xy 137 81) (xy 142.586421 81)))
    (feature2 (pts (xy 137 49) (xy 142.586421 49)))
    (crossbar (pts (xy 142 49) (xy 142 81)))
    (arrow1a (pts (xy 142 81) (xy 141.413579 79.873496)))
    (arrow1b (pts (xy 142 81) (xy 142.586421 79.873496)))
    (arrow2a (pts (xy 142 49) (xy 141.413579 50.126504)))
    (arrow2b (pts (xy 142 49) (xy 142.586421 50.126504)))
  )
  (dimension 78 (width 0.15) (layer Dwgs.User)
    (gr_text "78,000 mm" (at 98 42.7) (layer Dwgs.User))
    (feature1 (pts (xy 137 49) (xy 137 43.413579)))
    (feature2 (pts (xy 59 49) (xy 59 43.413579)))
    (crossbar (pts (xy 59 44) (xy 137 44)))
    (arrow1a (pts (xy 137 44) (xy 135.873496 44.586421)))
    (arrow1b (pts (xy 137 44) (xy 135.873496 43.413579)))
    (arrow2a (pts (xy 59 44) (xy 60.126504 44.586421)))
    (arrow2b (pts (xy 59 44) (xy 60.126504 43.413579)))
  )
  (gr_line (start 137 49) (end 137 81) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 59 49) (end 137 49) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 59 81) (end 59 49) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137 81) (end 59 81) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 32) (thermal_gap 1.16) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 137 81) (xy 59 81) (xy 59 49) (xy 137 49)
      )
    )
  )
  (zone (net 3) (net_name "Net-(C1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.25 81) (xy 118.5 81) (xy 118.5 49) (xy 129.25 49)
      )
    )
  )
)
