(kicad_pcb (version 4) (host pcbnew 4.0.4-2.fc26-product)
  (general
    (links 173)
    (no_connects 0)
    (area 82.4233 118.704762 104.9855 150.402)
    (thickness 1)
    (drawings 5)
    (tracks 261)
    (zones 0)
    (modules 29)
    (nets 45)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.152)
    (user_trace_width 0.152)
    (user_trace_width 0.152)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.36)
    (user_trace_width 0.5)
    (trace_clearance 0.152)
    (zone_clearance 0.25)
    (zone_45_only yes)
    (trace_min 0.075)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.69)
    (via_drill 0.33)
    (via_min_size 0.69)
    (via_min_drill 0.33)
    (user_via 0.69 0.33)
    (user_via 0.69 0.33)
    (user_via 0.8 0.5)
    (user_via 1.3 1)
    (user_via 2 1)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2)
    (pad_drill 2)
    (pad_to_mask_clearance 0.075)
    (solder_mask_min_width 0.1)
    (aux_axis_origin 0 0)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x012fc_80000007)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VBUS)
  (net 3 U10/vdd)
  (net 4 U10/d+)
  (net 5 J10/ID)
  (net 6 U10/d-)
  (net 7 3V3)
  (net 8 U10/vpp)
  (net 9 U10/RESET)
  (net 10 U10/P)
  (net 11 U7/BYP)
  (net 12 1V2)
  (net 13 U30/CDONE)
  (net 14 creset)
  (net 15 usck)
  (net 16 ucs)
  (net 17 usdo)
  (net 18 usdi)
  (net 19 U8/BYP)
  (net 20 CLK)
  (net 21 U10/O)
  (net 22 U10/I)
  (net 23 led0/rs)
  (net 24 led1/rs)
  (net 25 3V3/rs)
  (net 26 led4/rs)
  (net 27 led0)
  (net 28 led1)
  (net 29 led4)
  (net 30 U30/IOL_2B_3)
  (net 31 U30/IOL_2A_3)
  (net 32 U30/IOL_4A_3)
  (net 33 U30/IOL_4B_GBIN7_3)
  (net 34 U30/IOL_5B_3)
  (net 35 U30/IOL_5A_GBIN6_3)
  (net 36 U30/IOR_35_GBIN3)
  (net 37 U30/IOT_45)
  (net 38 U30/IOT_47)
  (net 39 1V8)
  (net 40 U6/BYP)
  (net 41 tp0)
  (net 42 tp1)
  (net 43 tp2)
  (net 44 tp3)
  (net_class Default "This is the default net class."
    (clearance 0.152)
    (trace_width 0.152)
    (via_dia 0.69)
    (via_drill 0.33)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net 1V2)
    (add_net 1V8)
    (add_net 3V3)
    (add_net 3V3/rs)
    (add_net CLK)
    (add_net GND)
    (add_net J10/ID)
    (add_net U10/I)
    (add_net U10/O)
    (add_net U10/P)
    (add_net U10/RESET)
    (add_net U10/d+)
    (add_net U10/d-)
    (add_net U10/vdd)
    (add_net U10/vpp)
    (add_net U30/CDONE)
    (add_net U30/IOL_2A_3)
    (add_net U30/IOL_2B_3)
    (add_net U30/IOL_4A_3)
    (add_net U30/IOL_4B_GBIN7_3)
    (add_net U30/IOL_5A_GBIN6_3)
    (add_net U30/IOL_5B_3)
    (add_net U30/IOR_35_GBIN3)
    (add_net U30/IOT_45)
    (add_net U30/IOT_47)
    (add_net U6/BYP)
    (add_net U7/BYP)
    (add_net U8/BYP)
    (add_net VBUS)
    (add_net creset)
    (add_net led0)
    (add_net led0/rs)
    (add_net led1)
    (add_net led1/rs)
    (add_net led4)
    (add_net led4/rs)
    (add_net tp0)
    (add_net tp1)
    (add_net tp2)
    (add_net tp3)
    (add_net ucs)
    (add_net usck)
    (add_net usdi)
    (add_net usdo)
  )
  (module QFN24_4x4 (layer F.Cu) (tedit 0)
    (at 95.5 141.05 90)
    (descr DocString)
    (tags Keywords)
    (attr smd)
    (fp_text reference U10 (at -0.75 -2.85 90) (layer F.SilkS))
    (fp_text value 6FDK2 (at 0 1.27 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.9 -1.25 90) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 usck) (zone_connect 2))
    (pad 2 smd rect (at -1.9 -0.75 90) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 3 smd rect (at -1.9 -0.25 90) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 U10/d+) (zone_connect 2))
    (pad 4 smd rect (at -1.9 0.25 90) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 U10/d-) (zone_connect 2))
    (pad 5 smd rect (at -1.9 0.75 90) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3) (zone_connect 2))
    (pad 6 smd rect (at -1.9 1.25 90) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 U10/vdd) (zone_connect 2))
    (pad 13 smd rect (at 1.9 1.25 90) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask)
      (zone_connect 2))
    (pad 14 smd rect (at 1.9 0.75 90) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask)
      (zone_connect 2))
    (pad 15 smd rect (at 1.9 0.25 90) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask)
      (zone_connect 2))
    (pad 16 smd rect (at 1.9 -0.25 90) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 U10/vpp) (zone_connect 2))
    (pad 17 smd rect (at 1.9 -0.75 90) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask)
      (zone_connect 2))
    (pad 18 smd rect (at 1.9 -1.25 90) (size 0.6 0.25) (layers F.Cu F.Paste F.Mask)
      (zone_connect 2))
    (pad 7 smd rect (at -1.25 1.9 90) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 VBUS) (zone_connect 2))
    (pad 8 smd rect (at -0.75 1.9 90) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 VBUS) (zone_connect 2))
    (pad 9 smd rect (at -0.25 1.9 90) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 U10/RESET) (zone_connect 2))
    (pad 10 smd rect (at 0.25 1.9 90) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (zone_connect 2))
    (pad 11 smd rect (at 0.75 1.9 90) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 creset) (zone_connect 2))
    (pad 12 smd rect (at 1.25 1.9 90) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 led4) (zone_connect 2))
    (pad 19 smd rect (at 1.25 -1.9 90) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 U10/O) (zone_connect 2))
    (pad 20 smd rect (at 0.75 -1.9 90) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 U10/I) (zone_connect 2))
    (pad 21 smd rect (at 0.25 -1.9 90) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 U10/P) (zone_connect 2))
    (pad 22 smd rect (at -0.25 -1.9 90) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 ucs) (zone_connect 2))
    (pad 23 smd rect (at -0.75 -1.9 90) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 usdo) (zone_connect 2))
    (pad 24 smd rect (at -1.25 -1.9 90) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 usdi) (zone_connect 2))
    (pad 25 smd rect (at 0 0 90) (size 2.6 2.6) (layers F.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 25 smd rect (at -0.65 -0.65 90) (size 0.919239 0.919239) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 25 smd rect (at -0.65 0.65 90) (size 0.919239 0.919239) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 25 smd rect (at 0.65 -0.65 90) (size 0.919239 0.919239) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 25 smd rect (at 0.65 0.65 90) (size 0.919239 0.919239) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 25 thru_hole circle (at -1 -1 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 25 thru_hole circle (at -1 0 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 25 thru_hole circle (at -1 1 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 25 thru_hole circle (at 0 -1 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 25 thru_hole circle (at 0 0 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 25 thru_hole circle (at 0 1 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 25 thru_hole circle (at 1 -1 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 25 thru_hole circle (at 1 0 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 25 thru_hole circle (at 1 1 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module 0805 (layer F.Cu) (tedit 54DCFFA6)
    (at 102.667546 137.999348 90)
    (attr smd)
    (fp_text reference C5 (at 0 -1.27 90) (layer F.SilkS) hide)
    (fp_text value "10 uF" (at 0 1.27 90) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.9 0 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3))
    (pad 2 smd rect (at 0.9 0 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module 0402 (layer F.Cu) (tedit 0)
    (at 98.2 143.55)
    (attr smd)
    (fp_text reference C11 (at 0 -1) (layer F.SilkS) hide)
    (fp_text value "1 uF" (at 0 1.27) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 U10/vdd))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module 0805 (layer F.Cu) (tedit 54DCFFA6)
    (at 95.75 137.2 90)
    (attr smd)
    (fp_text reference C12 (at 0 -1.27 90) (layer F.SilkS) hide)
    (fp_text value "10 uF" (at 0 1.27 90) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.9 0 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 U10/vpp))
    (pad 2 smd rect (at 0.9 0 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module SOT23-5 (layer F.Cu) (tedit 0)
    (at 101.825 141.1)
    (descr DocString)
    (tags Keywords)
    (attr smd)
    (fp_text reference U7 (at 0.525 0.05) (layer F.SilkS))
    (fp_text value CGK8Y (at 0 1.27) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.35 -0.95) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 VBUS))
    (pad 2 smd rect (at -1.35 0) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.35 0.95) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 VBUS))
    (pad 4 smd rect (at 1.35 0.95) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 U7/BYP))
    (pad 5 smd rect (at 1.35 -0.95) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3))
  )
  (module SC70-5 (layer F.Cu) (tedit 0)
    (at 96.45 128.8 180)
    (descr DocString)
    (tags Keywords)
    (attr smd)
    (fp_text reference U8 (at 0 0 270) (layer F.SilkS))
    (fp_text value 6DXQ7 (at 0 1.27 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.95 -0.65 180) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3))
    (pad 2 smd rect (at -0.95 0 180) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -0.95 0.65 180) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3))
    (pad 4 smd rect (at 0.95 0.65 180) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 19 U8/BYP))
    (pad 5 smd rect (at 0.95 -0.65 180) (size 0.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 1V2))
  )
  (module osc_2.5x2 (layer F.Cu) (tedit 0)
    (at 98.25 134.85 180)
    (descr DocString)
    (tags Keywords)
    (attr smd)
    (fp_text reference U9 (at -2.25 0.05 180) (layer F.SilkS))
    (fp_text value K7CM9 (at 0 1.27 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.75 -0.95 180) (size 1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3) (zone_connect 2))
    (pad 2 smd rect (at -0.75 0.95 180) (size 1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 3 smd rect (at 0.75 0.95 180) (size 1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 20 CLK) (zone_connect 2))
    (pad 4 smd rect (at 0.75 -0.95 180) (size 1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3) (zone_connect 2))
  )
  (module UFL (layer F.Cu) (tedit 56494A9A)
    (at 94.3 121.3 270)
    (descr DocString)
    (tags Keywords)
    (attr smd)
    (fp_text reference P1 (at -0.05 -3.15 450) (layer F.SilkS))
    (fp_text value 6BPPF (at 0 6 270) (layer Cmts.User) hide)
    (pad 2 smd rect (at -1.3 0 270) (size 1.5 4) (layers F.Cu)
      (net 1 GND))
    (pad 2 smd rect (at 0 1.6 270) (size 3.5 1.3) (layers F.Cu)
      (net 1 GND))
    (pad 2 smd rect (at 0 -1.6 270) (size 3.5 1.3) (layers F.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at -1.7 1.3 270) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.6 2.1 270) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.6 2.1 270) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 thru_hole circle (at 1.7 1.3 270) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.7 -1.3 270) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 thru_hole circle (at 1.7 -1.3 270) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.6 -2.1 270) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 smd rect (at 0 -1.3 270) (size 1.9 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 1.3 270) (size 1.9 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.3 0 270) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 41 tp0))
    (pad 2 smd rect (at -1.3 0 270) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -0.6 -2.1 270) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
  )
  (module 0402 (layer F.Cu) (tedit 0)
    (at 100.85 135.8)
    (attr smd)
    (fp_text reference C20 (at 0 -1) (layer F.SilkS) hide)
    (fp_text value "1 uF" (at 0 1.27) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module 0402 (layer F.Cu) (tedit 0)
    (at 88 135.75 180)
    (attr smd)
    (fp_text reference C21 (at 0 -1 180) (layer F.SilkS) hide)
    (fp_text value "1 uF" (at 0 1.27 180) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module 0402 (layer F.Cu) (tedit 0)
    (at 95.7 130.7)
    (attr smd)
    (fp_text reference C22 (at 0 -1) (layer F.SilkS) hide)
    (fp_text value "1 uF" (at 0 1.27) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module 0805 (layer F.Cu) (tedit 54DCFFA6)
    (at 99.5 127.65)
    (attr smd)
    (fp_text reference C2 (at 0 -1.27) (layer F.SilkS) hide)
    (fp_text value "10 uF" (at 0 1.27) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.9 0) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3))
    (pad 2 smd rect (at 0.9 0) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module 0603 (layer F.Cu) (tedit 54DB8A31)
    (at 98.65 132.45)
    (attr smd)
    (fp_text reference D40 (at 2.3 0) (layer F.SilkS))
    (fp_text value QF838 (at 0 1.27) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 led0/rs))
    (pad 2 smd rect (at 0.75 0) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module 0603 (layer F.Cu) (tedit 54DB8A31)
    (at 98.65 131.15)
    (attr smd)
    (fp_text reference D41 (at 2.35 0) (layer F.SilkS))
    (fp_text value QF838 (at 0 1.27) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 led1/rs))
    (pad 2 smd rect (at 0.75 0) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module 0603 (layer F.Cu) (tedit 54DB8A31)
    (at 102.9 146.9 270)
    (attr smd)
    (fp_text reference D43 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value QF838 (at 0 1.27 270) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 25 3V3/rs))
    (pad 2 smd rect (at 0.75 0 270) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module 0603 (layer F.Cu) (tedit 54DB8A31)
    (at 99.2 137.4)
    (attr smd)
    (fp_text reference D44 (at 0 1.3) (layer F.SilkS))
    (fp_text value QF838 (at 0 1.27) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 26 led4/rs))
    (pad 2 smd rect (at 0.75 0) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module 0402 (layer F.Cu) (tedit 0)
    (at 96.2 132.65)
    (attr smd)
    (fp_text reference R40 (at 0 -1) (layer F.SilkS) hide)
    (fp_text value "1 k" (at 0 1.27) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.5) (layers F.Cu F.Paste F.Mask)
      (net 27 led0))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.5) (layers F.Cu F.Paste F.Mask)
      (net 23 led0/rs))
  )
  (module 0402 (layer F.Cu) (tedit 0)
    (at 96.2 131.85)
    (attr smd)
    (fp_text reference R41 (at 0 -1) (layer F.SilkS) hide)
    (fp_text value "1 k" (at 0 1.27) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.5) (layers F.Cu F.Paste F.Mask)
      (net 28 led1))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.5) (layers F.Cu F.Paste F.Mask)
      (net 24 led1/rs))
  )
  (module 0402 (layer F.Cu) (tedit 0)
    (at 102.9 144.65 270)
    (attr smd)
    (fp_text reference R43 (at 0 -1 270) (layer F.SilkS) hide)
    (fp_text value "1 k" (at 0 1.27 270) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.5) (layers F.Cu F.Paste F.Mask)
      (net 25 3V3/rs))
  )
  (module 0402 (layer F.Cu) (tedit 0)
    (at 97.4 137.85 90)
    (attr smd)
    (fp_text reference R44 (at 0 -1 90) (layer F.SilkS) hide)
    (fp_text value "1 k" (at 0 1.27 90) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.5) (layers F.Cu F.Paste F.Mask)
      (net 29 led4))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.5) (layers F.Cu F.Paste F.Mask)
      (net 26 led4/rs))
  )
  (module QFN32_5x5 (layer F.Cu) (tedit 0)
    (at 91.9 133.3)
    (attr smd)
    (fp_text reference U30 (at -2.75 -3.8) (layer F.SilkS))
    (fp_text value B4CF9 (at 0 1.27) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.425 -1.75) (size 0.7 0.254) (layers F.Cu F.Paste F.Mask)
      (net 30 U30/IOL_2B_3))
    (pad 2 smd rect (at -2.425 -1.25) (size 0.7 0.254) (layers F.Cu F.Paste F.Mask)
      (net 31 U30/IOL_2A_3))
    (pad 3 smd rect (at -2.425 -0.75) (size 0.7 0.254) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -2.425 -0.25) (size 0.7 0.254) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3))
    (pad 5 smd rect (at -2.425 0.25) (size 0.7 0.254) (layers F.Cu F.Paste F.Mask)
      (net 32 U30/IOL_4A_3))
    (pad 6 smd rect (at -2.425 0.75) (size 0.7 0.254) (layers F.Cu F.Paste F.Mask)
      (net 33 U30/IOL_4B_GBIN7_3))
    (pad 7 smd rect (at -2.425 1.25) (size 0.7 0.254) (layers F.Cu F.Paste F.Mask)
      (net 34 U30/IOL_5B_3))
    (pad 8 smd rect (at -2.425 1.75) (size 0.7 0.254) (layers F.Cu F.Paste F.Mask)
      (net 35 U30/IOL_5A_GBIN6_3))
    (pad 17 smd rect (at 2.425 1.75) (size 0.7 0.254) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3))
    (pad 18 smd rect (at 2.425 1.25) (size 0.7 0.254) (layers F.Cu F.Paste F.Mask)
      (net 16 ucs))
    (pad 19 smd rect (at 2.425 0.75) (size 0.7 0.254) (layers F.Cu F.Paste F.Mask)
      (net 36 U30/IOR_35_GBIN3))
    (pad 20 smd rect (at 2.425 0.25) (size 0.7 0.254) (layers F.Cu F.Paste F.Mask)
      (net 20 CLK))
    (pad 21 smd rect (at 2.425 -0.25) (size 0.7 0.254) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 22 smd rect (at 2.425 -0.75) (size 0.7 0.254) (layers F.Cu F.Paste F.Mask)
      (net 27 led0))
    (pad 23 smd rect (at 2.425 -1.25) (size 0.7 0.254) (layers F.Cu F.Paste F.Mask)
      (net 28 led1))
    (pad 24 smd rect (at 2.425 -1.75) (size 0.7 0.254) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3))
    (pad 9 smd rect (at -1.75 2.425) (size 0.254 0.7) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3))
    (pad 10 smd rect (at -1.25 2.425) (size 0.254 0.7) (layers F.Cu F.Paste F.Mask)
      (net 14 creset))
    (pad 11 smd rect (at -0.75 2.425) (size 0.254 0.7) (layers F.Cu F.Paste F.Mask)
      (net 13 U30/CDONE))
    (pad 12 smd rect (at -0.25 2.425) (size 0.254 0.7) (layers F.Cu F.Paste F.Mask)
      (net 18 usdi))
    (pad 13 smd rect (at 0.25 2.425) (size 0.254 0.7) (layers F.Cu F.Paste F.Mask)
      (net 17 usdo))
    (pad 14 smd rect (at 0.75 2.425) (size 0.254 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 1.25 2.425) (size 0.254 0.7) (layers F.Cu F.Paste F.Mask)
      (net 15 usck))
    (pad 16 smd rect (at 1.75 2.425) (size 0.254 0.7) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3))
    (pad 25 smd rect (at 1.75 -2.425) (size 0.254 0.7) (layers F.Cu F.Paste F.Mask)
      (net 12 1V2))
    (pad 26 smd rect (at 1.25 -2.425) (size 0.254 0.7) (layers F.Cu F.Paste F.Mask)
      (net 37 U30/IOT_45))
    (pad 27 smd rect (at 0.75 -2.425) (size 0.254 0.7) (layers F.Cu F.Paste F.Mask)
      (net 38 U30/IOT_47))
    (pad 28 smd rect (at 0.25 -2.425) (size 0.254 0.7) (layers F.Cu F.Paste F.Mask)
      (net 39 1V8))
    (pad 29 smd rect (at -0.25 -2.425) (size 0.254 0.7) (layers F.Cu F.Paste F.Mask)
      (net 41 tp0))
    (pad 30 smd rect (at -0.75 -2.425) (size 0.254 0.7) (layers F.Cu F.Paste F.Mask)
      (net 42 tp1))
    (pad 31 smd rect (at -1.25 -2.425) (size 0.254 0.7) (layers F.Cu F.Paste F.Mask)
      (net 44 tp3))
    (pad 32 smd rect (at -1.75 -2.425) (size 0.254 0.7) (layers F.Cu F.Paste F.Mask)
      (net 43 tp2))
    (pad 33 smd rect (at 0 0) (size 3.75 3.75) (layers F.Cu F.Mask)
      (net 1 GND) (solder_mask_margin -0.3))
    (pad 33 smd rect (at -0.7875 -0.7875) (size 1.113693 1.113693) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 33 smd rect (at -0.7875 0.7875) (size 1.113693 1.113693) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 33 smd rect (at 0.7875 -0.7875) (size 1.113693 1.113693) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 33 smd rect (at 0.7875 0.7875) (size 1.113693 1.113693) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 33 thru_hole circle (at 0 0) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
  )
  (module USB_micro_B (layer F.Cu) (tedit 5817B1D7)
    (at 95.8 150)
    (descr DocString)
    (tags Keywords)
    (zone_connect 2)
    (attr smd)
    (fp_text reference J10 (at -5.6 -3.4 90) (layer F.SilkS))
    (fp_text value JVWW9 (at -0.25 -2.55) (layer Cmts.User) hide)
    (pad 5 smd rect (at -1.2 -1.45) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 3 smd rect (at 0 -4.325) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 4 U10/d+) (zone_connect 2))
    (pad 4 smd rect (at 0.65 -4.325) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 5 J10/ID) (zone_connect 2))
    (pad 1 smd rect (at -1.3 -4.325) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 2 VBUS) (zone_connect 2))
    (pad 2 smd rect (at -0.65 -4.325) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 6 U10/d-) (zone_connect 2))
    (pad 5 smd rect (at 1.3 -4.325) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 5 smd rect (at 1.2 -1.45) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 5 thru_hole circle (at 0 -2) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 5 thru_hole circle (at 0 -0.8) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 5 smd rect (at 3.8 -1.45) (size 1.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 5 smd rect (at -3.8 -1.45) (size 1.8 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 5 thru_hole circle (at 0 -1.4) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 5 thru_hole circle (at -2.5 -1.4) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 5 thru_hole circle (at -2.5 -2.1) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 5 thru_hole circle (at -2.5 -0.7) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 5 thru_hole circle (at 2.5 -2.1) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 5 thru_hole circle (at 2.5 -0.7) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 5 thru_hole circle (at 2.5 -1.4) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 5 smd rect (at -3.1 -4.2) (size 2.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 5 smd rect (at 3.1 -4.2) (size 2.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 5 thru_hole circle (at -5 -2.1) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 5 thru_hole circle (at -5 -1.4) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 5 thru_hole circle (at -5 -0.7) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 5 thru_hole circle (at 5 -2.1) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 5 thru_hole circle (at 5 -1.4) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 5 thru_hole circle (at 5 -0.7) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 5 thru_hole circle (at 4.7 -4) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 5 thru_hole circle (at 4.7 -3.3) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 5 thru_hole circle (at 4.7 -4.7) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 5 thru_hole circle (at -4.7 -4.7) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 5 thru_hole circle (at -4.7 -3.3) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 5 thru_hole circle (at -4.7 -4) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
  )
  (module 0805 (layer F.Cu) (tedit 54DCFFA6)
    (at 94.15 128.8 90)
    (attr smd)
    (fp_text reference C25 (at 0 -1.27 90) (layer F.SilkS) hide)
    (fp_text value "10 uF" (at 0 1.27 90) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.9 0 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 1V2))
    (pad 2 smd rect (at 0.9 0 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module 0805 (layer F.Cu) (tedit 54DCFFA6)
    (at 98.85 141.15 90)
    (attr smd)
    (fp_text reference C10 (at 0 -1.27 90) (layer F.SilkS) hide)
    (fp_text value "10 uF" (at 0 1.27 90) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.9 0 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 VBUS))
    (pad 2 smd rect (at 0.9 0 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module 0805 (layer F.Cu) (tedit 54DCFFA6)
    (at 92.55 128.8 90)
    (attr smd)
    (fp_text reference C26 (at 0 -1.27 90) (layer F.SilkS) hide)
    (fp_text value "10 uF" (at 0 1.27 90) (layer Cmts.User) hide)
    (pad 1 smd rect (at -0.9 0 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 39 1V8))
    (pad 2 smd rect (at 0.9 0 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module SOT23-5 (layer F.Cu) (tedit 0)
    (at 97.25 125.2 180)
    (descr DocString)
    (tags Keywords)
    (attr smd)
    (fp_text reference U6 (at 0 0 270) (layer F.SilkS))
    (fp_text value VQ8V4 (at 0 1.27 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.35 -0.95 180) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3))
    (pad 2 smd rect (at -1.35 0 180) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.35 0.95 180) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 3V3))
    (pad 4 smd rect (at 1.35 0.95 180) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (net 40 U6/BYP))
    (pad 5 smd rect (at 1.35 -0.95 180) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (net 39 1V8))
  )
  (module UFL (layer F.Cu) (tedit 56494A9A)
    (at 89.35 121.3 270)
    (descr DocString)
    (tags Keywords)
    (attr smd)
    (fp_text reference P2 (at -1 3 450) (layer F.SilkS))
    (fp_text value 6BPPF (at 0 6 270) (layer Cmts.User) hide)
    (pad 2 smd rect (at -1.3 0 270) (size 1.5 4) (layers F.Cu)
      (net 1 GND))
    (pad 2 smd rect (at 0 1.6 270) (size 3.5 1.3) (layers F.Cu)
      (net 1 GND))
    (pad 2 smd rect (at 0 -1.6 270) (size 3.5 1.3) (layers F.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at -1.7 1.3 270) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.6 2.1 270) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.6 2.1 270) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 thru_hole circle (at 1.7 1.3 270) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.7 -1.3 270) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 thru_hole circle (at 1.7 -1.3 270) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.6 -2.1 270) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 smd rect (at 0 -1.3 270) (size 1.9 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 1.3 270) (size 1.9 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.3 0 270) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 42 tp1))
    (pad 2 smd rect (at -1.3 0 270) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -0.6 -2.1 270) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
  )
  (module UFL (layer F.Cu) (tedit 56494A9A)
    (at 85.7 130.45)
    (descr DocString)
    (tags Keywords)
    (attr smd)
    (fp_text reference P3 (at -0.45 3.2) (layer F.SilkS))
    (fp_text value 6BPPF (at 0 6) (layer Cmts.User) hide)
    (pad 2 smd rect (at -1.3 0) (size 1.5 4) (layers F.Cu)
      (net 1 GND))
    (pad 2 smd rect (at 0 1.6) (size 3.5 1.3) (layers F.Cu)
      (net 1 GND))
    (pad 2 smd rect (at 0 -1.6) (size 3.5 1.3) (layers F.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at -1.7 1.3) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.6 2.1) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.6 2.1) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 thru_hole circle (at 1.7 1.3) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.7 -1.3) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 thru_hole circle (at 1.7 -1.3) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.6 -2.1) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 smd rect (at 0 -1.3) (size 1.9 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 1.3) (size 1.9 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.3 0) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 43 tp2))
    (pad 2 smd rect (at -1.3 0) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -0.6 -2.1) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
  )
  (module UFL (layer F.Cu) (tedit 56494A9A)
    (at 85.7 125.4)
    (descr DocString)
    (tags Keywords)
    (attr smd)
    (fp_text reference P4 (at -0.9 -3.1) (layer F.SilkS))
    (fp_text value 6BPPF (at 0 6) (layer Cmts.User) hide)
    (pad 2 smd rect (at -1.3 0) (size 1.5 4) (layers F.Cu)
      (net 1 GND))
    (pad 2 smd rect (at 0 1.6) (size 3.5 1.3) (layers F.Cu)
      (net 1 GND))
    (pad 2 smd rect (at 0 -1.6) (size 3.5 1.3) (layers F.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at -1.7 1.3) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 thru_hole circle (at -0.6 2.1) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.6 2.1) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 thru_hole circle (at 1.7 1.3) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 thru_hole circle (at -1.7 -1.3) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 thru_hole circle (at 1.7 -1.3) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 thru_hole circle (at 0.6 -2.1) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
    (pad 2 smd rect (at 0 -1.3) (size 1.9 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 1.3) (size 1.9 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.3 0) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 44 tp3))
    (pad 2 smd rect (at -1.3 0) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -0.6 -2.1) (size 0.7 0.7) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin -0.1) (zone_connect 2))
  )
  (gr_text "ICE40LP384 test\nRev 1" (at 85.8 142.85 90) (layer F.Mask))
  (gr_line (start 104.5 150) (end 104.5 119) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 83.5 119) (end 104.5 119) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 83.5 150) (end 83.5 119) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.5 150) (end 83.5 150) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 84 119.5) (xy 104 119.5) (xy 104 149.5) (xy 84 149.5)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.3)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 84 119.5) (xy 104 119.5) (xy 104 149.5) (xy 84 149.5)
      )
    )
  )
)
