(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 27)
    (no_connects 0)
    (area 122.656512 65.251301 173.329601 116.019581)
    (thickness 1.6002)
    (drawings 40)
    (tracks 208)
    (zones 0)
    (modules 6)
    (nets 10)
  )
  (page A4)
  (title_block
    (date "17 feb 2011")
  )
  (layers
    (0 Front signal)
    (31 Back signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.4064)
    (trace_clearance 0.2032)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2032)
    (segment_width 0.381)
    (edge_width 0.2032)
    (via_size 0.8128)
    (via_drill 0.508)
    (via_min_size 0.8128)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3048)
    (pcb_text_size 1.524 2.032)
    (mod_edge_width 0.381)
    (mod_text_size 1.524 1.524)
    (mod_text_width 0.3048)
    (pad_size 2.2352 2.2352)
    (pad_drill 1.5748)
    (pad_to_mask_clearance 0.254)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /SIG1)
  (net 2 /SIG2)
  (net 3 /SIG3)
  (net 4 /SIG4)
  (net 5 /SIG5)
  (net 6 /SIG6)
  (net 7 /SIG7)
  (net 8 /SIG8)
  (net 9 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.4064)
    (via_dia 0.8128)
    (via_drill 0.508)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /SIG1)
    (add_net /SIG2)
    (add_net /SIG3)
    (add_net /SIG4)
    (add_net /SIG5)
    (add_net /SIG6)
    (add_net /SIG7)
    (add_net /SIG8)
    (add_net GND)
  )
  (module C1 (layer Front) (tedit 4CE6B46D)
    (at 139.1031 81.79308 225)
    (descr "Condensateur e = 1 pas")
    (tags C)
    (fp_text reference C1 (at 4.318 1.016 225) (layer F.SilkS))
    (fp_text value 220pF (at -5.08 1.016 225) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.27 0 225) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 /SIG4))
    (pad 2 thru_hole circle (at 1.27 0 225) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SIG5))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module C1 (layer Front) (tedit 4CE6B455)
    (at 157.06344 99.75342 45)
    (descr "Condensateur e = 1 pas")
    (tags C)
    (fp_text reference C2 (at -4.318 1.016 45) (layer F.SilkS))
    (fp_text value 220pF (at 5.08 1.016 45) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.27 0 45) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 /SIG7))
    (pad 2 thru_hole circle (at 1.27 0 45) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 /SIG8))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RJ45-RJHSE-5380 (layer Front) (tedit 4D1D5420)
    (at 130.12166 72.81164 225)
    (fp_text reference J3 (at 0.2921 6.99516 225) (layer F.SilkS))
    (fp_text value RJ45 (at 0.254 2.54 225) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 6.35 0 225) (size 3.2512 3.2512) (drill 3.2512) (layers *.Cu *.Mask F.SilkS)
      (solder_mask_margin 0.1016) (clearance 0.1016))
    (pad "" thru_hole circle (at -6.35 0 225) (size 3.2512 3.2512) (drill 3.2512) (layers *.Cu *.Mask F.SilkS)
      (solder_mask_margin 0.1016) (clearance 0.1016))
    (pad 1 thru_hole circle (at 3.556 -2.54 225) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 2.54 -4.318 225) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at 1.524 -2.54 225) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 /SIG1))
    (pad 4 thru_hole circle (at 0.508 -4.318 225) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole circle (at -0.508 -2.54 225) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole circle (at -1.524 -4.318 225) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 /SIG2))
    (pad 7 thru_hole circle (at -2.54 -2.54 225) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /SIG4))
    (pad 8 thru_hole circle (at -3.556 -4.318 225) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SIG5))
    (pad "" thru_hole circle (at 6.858 -9.144 225) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 4.572 -9.144 225) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -4.572 -9.144 225) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -6.858 -9.144 225) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole circle (at 8.128 -3.429 225) (size 2.2352 2.2352) (drill 1.5748) (layers *.Cu *.Mask F.SilkS)
      (net 9 GND))
    (pad 9 thru_hole circle (at -8.128 -3.429 225) (size 2.2352 2.2352) (drill 1.5748) (layers *.Cu *.Mask F.SilkS)
      (net 9 GND))
  )
  (module RJ45-RJHSE-5380 (layer Front) (tedit 4D1D54E9)
    (at 166.04488 72.81164 135)
    (fp_text reference J2 (at 0.06858 7.3533 405) (layer F.SilkS))
    (fp_text value RJ45 (at 0.06858 1.60528 405) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 6.35 0 135) (size 3.2512 3.2512) (drill 3.2512) (layers *.Cu *.Mask F.SilkS)
      (solder_mask_margin 0.1016) (clearance 0.1016))
    (pad "" thru_hole circle (at -6.35 0 135) (size 3.2512 3.2512) (drill 3.2512) (layers *.Cu *.Mask F.SilkS)
      (solder_mask_margin 0.1016) (clearance 0.1016))
    (pad 1 thru_hole circle (at 3.556 -2.54 135) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 /SIG1))
    (pad 2 thru_hole circle (at 2.54 -4.318 135) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 /SIG2))
    (pad 3 thru_hole circle (at 1.524 -2.54 135) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /SIG3))
    (pad 4 thru_hole circle (at 0.508 -4.318 135) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /SIG4))
    (pad 5 thru_hole circle (at -0.508 -2.54 135) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SIG5))
    (pad 6 thru_hole circle (at -1.524 -4.318 135) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /SIG6))
    (pad 7 thru_hole circle (at -2.54 -2.54 135) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /SIG7))
    (pad 8 thru_hole circle (at -3.556 -4.318 135) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 /SIG8))
    (pad "" thru_hole circle (at 6.858 -9.144 135) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 4.572 -9.144 135) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -4.572 -9.144 135) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -6.858 -9.144 135) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole circle (at 8.128 -3.429 135) (size 2.2352 2.2352) (drill 1.5748) (layers *.Cu *.Mask F.SilkS)
      (net 9 GND))
    (pad 9 thru_hole circle (at -8.128 -3.429 135) (size 2.2352 2.2352) (drill 1.5748) (layers *.Cu *.Mask F.SilkS)
      (net 9 GND))
  )
  (module RJ45-RJHSE-5380 (layer Front) (tedit 4D1D5403)
    (at 166.04488 108.73232 45)
    (fp_text reference J4 (at 0.0635 7.22122 45) (layer F.SilkS))
    (fp_text value RJ45 (at 0.254 2.54 45) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 6.35 0 45) (size 3.2512 3.2512) (drill 3.2512) (layers *.Cu *.Mask F.SilkS)
      (solder_mask_margin 0.1016) (clearance 0.1016))
    (pad "" thru_hole circle (at -6.35 0 45) (size 3.2512 3.2512) (drill 3.2512) (layers *.Cu *.Mask F.SilkS)
      (solder_mask_margin 0.1016) (clearance 0.1016))
    (pad 1 thru_hole circle (at 3.556 -2.54 45) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 2.54 -4.318 45) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at 1.524 -2.54 45) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /SIG3))
    (pad 4 thru_hole circle (at 0.508 -4.318 45) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole circle (at -0.508 -2.54 45) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole circle (at -1.524 -4.318 45) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /SIG6))
    (pad 7 thru_hole circle (at -2.54 -2.54 45) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /SIG7))
    (pad 8 thru_hole circle (at -3.556 -4.318 45) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 /SIG8))
    (pad "" thru_hole circle (at 6.858 -9.144 45) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 4.572 -9.144 45) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -4.572 -9.144 45) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -6.858 -9.144 45) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole circle (at 8.128 -3.429 45) (size 2.2352 2.2352) (drill 1.5748) (layers *.Cu *.Mask F.SilkS)
      (net 9 GND))
    (pad 9 thru_hole circle (at -8.128 -3.429 45) (size 2.2352 2.2352) (drill 1.5748) (layers *.Cu *.Mask F.SilkS)
      (net 9 GND))
  )
  (module RJ45-RJHSE-5380 (layer Front) (tedit 4D1D54F0)
    (at 130.12166 108.73232 315)
    (fp_text reference J1 (at -0.06604 7.22122 405) (layer F.SilkS))
    (fp_text value RJ45 (at 0.2921 1.83388 405) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 6.35 0 315) (size 3.2512 3.2512) (drill 3.2512) (layers *.Cu *.Mask F.SilkS)
      (solder_mask_margin 0.1016) (clearance 0.1016))
    (pad "" thru_hole circle (at -6.35 0 315) (size 3.2512 3.2512) (drill 3.2512) (layers *.Cu *.Mask F.SilkS)
      (solder_mask_margin 0.1016) (clearance 0.1016))
    (pad 1 thru_hole circle (at 3.556 -2.54 315) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 /SIG1))
    (pad 2 thru_hole circle (at 2.54 -4.318 315) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 /SIG2))
    (pad 3 thru_hole circle (at 1.524 -2.54 315) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /SIG3))
    (pad 4 thru_hole circle (at 0.508 -4.318 315) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /SIG4))
    (pad 5 thru_hole circle (at -0.508 -2.54 315) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SIG5))
    (pad 6 thru_hole circle (at -1.524 -4.318 315) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /SIG6))
    (pad 7 thru_hole circle (at -2.54 -2.54 315) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /SIG7))
    (pad 8 thru_hole circle (at -3.556 -4.318 315) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 /SIG8))
    (pad "" thru_hole circle (at 6.858 -9.144 315) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 4.572 -9.144 315) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -4.572 -9.144 315) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -6.858 -9.144 315) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole circle (at 8.128 -3.429 315) (size 2.2352 2.2352) (drill 1.5748) (layers *.Cu *.Mask F.SilkS)
      (net 9 GND))
    (pad 9 thru_hole circle (at -8.128 -3.429 315) (size 2.2352 2.2352) (drill 1.5748) (layers *.Cu *.Mask F.SilkS)
      (net 9 GND))
  )
  (gr_text "Michael Ossmann <mike@ossmann.com>" (at 148.08454 90.77198 225) (layer B.SilkS))
  (gr_text "Throwing Star LAN Tap" (at 148.08454 90.77198 45) (layer F.SilkS))
  (gr_text http://greatscottgadgets.com/ (at 145.92808 88.61806 225) (layer B.SilkS))
  (gr_text "Great Scott Gadgets" (at 150.23846 92.92844 225) (layer B.SilkS))
  (gr_arc (start 148.08454 103.34498) (end 144.67078 104.96042) (angle 232) (layer Edge.Cuts) (width 0.2032))
  (gr_arc (start 135.51154 90.77198) (end 133.89356 87.36076) (angle 232) (layer Edge.Cuts) (width 0.2032))
  (gr_arc (start 148.08454 78.19898) (end 151.49576 76.58354) (angle 232) (layer Edge.Cuts) (width 0.2032))
  (gr_arc (start 160.655 90.77198) (end 162.27298 94.18574) (angle 232) (layer Edge.Cuts) (width 0.2032))
  (gr_line (start 173.228 99.75342) (end 162.27298 94.18574) (angle 90) (layer Edge.Cuts) (width 0.2032))
  (gr_line (start 157.06344 115.91798) (end 151.49576 104.96042) (angle 90) (layer Edge.Cuts) (width 0.2032))
  (gr_line (start 139.1031 115.91798) (end 144.67078 104.96042) (angle 90) (layer Edge.Cuts) (width 0.2032))
  (gr_line (start 122.93854 99.75342) (end 133.89356 94.18574) (angle 90) (layer Edge.Cuts) (width 0.2032))
  (gr_line (start 122.93854 81.79308) (end 133.89356 87.36076) (angle 90) (layer Edge.Cuts) (width 0.2032))
  (gr_line (start 139.1031 65.62852) (end 144.67078 76.58354) (angle 90) (layer Edge.Cuts) (width 0.2032))
  (gr_line (start 173.228 115.91798) (end 157.06344 115.91798) (angle 90) (layer Edge.Cuts) (width 0.2032))
  (gr_line (start 173.228 115.91798) (end 173.228 99.75342) (angle 90) (layer Edge.Cuts) (width 0.2032))
  (gr_line (start 122.93854 115.91798) (end 139.1031 115.91798) (angle 90) (layer Edge.Cuts) (width 0.2032))
  (gr_line (start 122.93854 115.91798) (end 122.93854 99.75342) (angle 90) (layer Edge.Cuts) (width 0.2032))
  (gr_line (start 122.93854 65.62852) (end 122.93854 81.79308) (angle 90) (layer Edge.Cuts) (width 0.2032))
  (gr_line (start 122.93854 65.62852) (end 139.1031 65.62852) (angle 90) (layer Edge.Cuts) (width 0.2032))
  (gr_line (start 157.06344 65.62852) (end 151.49576 76.58354) (angle 90) (layer Edge.Cuts) (width 0.2032))
  (gr_line (start 173.228 65.62852) (end 157.06344 65.62852) (angle 90) (layer Edge.Cuts) (width 0.2032))
  (gr_line (start 173.228 81.79308) (end 162.27298 87.36076) (angle 90) (layer Edge.Cuts) (width 0.2032))
  (gr_line (start 173.228 65.62852) (end 173.228 81.79308) (angle 90) (layer Edge.Cuts) (width 0.2032))
  (zone (net 9) (net_name GND) (layer Front) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.2032)
    (fill (mode segment) (arc_segments 16) (thermal_gap 0.2032) (thermal_bridge_width 0.4064))
    (polygon
      (pts
        (xy 172.50918 115.19916) (xy 172.42028 100.3808) (xy 162.45078 95.2627) (xy 158.85922 95.2627) (xy 156.16428 92.56776)
        (xy 156.16428 88.9762) (xy 158.85922 86.28126) (xy 162.45078 86.28126) (xy 172.42028 81.16316) (xy 172.50918 66.3448)
        (xy 157.69336 66.43624) (xy 152.57272 76.4032) (xy 152.57272 79.99476) (xy 149.88032 82.6897) (xy 146.28622 82.6897)
        (xy 143.59382 79.99476) (xy 143.59382 76.4032) (xy 138.47318 66.43624) (xy 123.65736 66.3448) (xy 123.74626 81.16316)
        (xy 133.71576 86.28126) (xy 137.30732 86.28126) (xy 140.00226 88.9762) (xy 140.00226 92.56776) (xy 137.21842 95.3516)
        (xy 133.44652 95.3516) (xy 123.74626 100.3808) (xy 123.65736 115.19916) (xy 138.47318 115.10772) (xy 143.59382 105.14076)
        (xy 143.59382 101.5492) (xy 146.28622 98.85426) (xy 149.88032 98.85426) (xy 152.57272 101.5492) (xy 152.57272 105.14076)
        (xy 157.69336 115.10772)
      )
    )
  )
  (zone (net 9) (net_name GND) (layer Back) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.2032)
    (fill (mode segment) (arc_segments 16) (thermal_gap 0.2032) (thermal_bridge_width 0.4064))
    (polygon
      (pts
        (xy 172.50918 115.19916) (xy 172.42028 100.3808) (xy 162.45078 95.2627) (xy 158.85922 95.2627) (xy 156.16428 92.56776)
        (xy 156.16428 88.9762) (xy 158.85922 86.28126) (xy 162.45078 86.28126) (xy 172.42028 81.16316) (xy 172.50918 66.3448)
        (xy 157.69336 66.43624) (xy 152.57272 76.4032) (xy 152.57272 79.99476) (xy 149.88032 82.6897) (xy 146.28622 82.6897)
        (xy 143.59382 79.99476) (xy 143.59382 76.4032) (xy 138.47318 66.43624) (xy 123.65736 66.3448) (xy 123.74626 81.16316)
        (xy 133.71576 86.28126) (xy 137.30732 86.28126) (xy 140.00226 88.9762) (xy 140.00226 92.56776) (xy 137.21842 95.3516)
        (xy 133.44652 95.3516) (xy 123.74626 100.3808) (xy 123.65736 115.19916) (xy 138.47318 115.10772) (xy 143.59382 105.14076)
        (xy 143.59382 101.5492) (xy 146.28622 98.85426) (xy 149.88032 98.85426) (xy 152.57272 101.5492) (xy 152.57272 105.14076)
        (xy 157.69336 115.10772)
      )
    )
  )
)
