<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="31.74" x2="0" y2="1.27" width="0" layer="20"/>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="0" x2="61.9" y2="0" width="0" layer="20"/>
<wire x1="61.9" y1="0" x2="63.17" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="63.17" y1="1.27" x2="63.17" y2="31.74" width="0" layer="20"/>
<wire x1="63.17" y1="31.74" x2="61.9" y2="33.01" width="0" layer="20" curve="90"/>
<wire x1="61.9" y1="33.01" x2="1.27" y2="33.01" width="0" layer="20"/>
<wire x1="1.27" y1="33.01" x2="0" y2="31.74" width="0" layer="20" curve="90"/>
<text>VIN</text>
<text>GND</text>
<text>VOUT</text>
<text>ATMakers</text>
<text>FreedomWing</text>
<text>#____________</text>
<text>RST</text>
<text>3V</text>
<text>AREF</text>
<text>GND</text>
<text>A0</text>
<text>A1</text>
<text>A2</text>
<text>A3</text>
<text>A4</text>
<text>A5</text>
<text>BAT</text>
<text>EN</text>
<text>USB</text>
<text>VERT</text>
<text>HOR</text>
<text>REF</text>
<text>5747844-4</text>
<text>ATMakers</text>
<text>FreedomWing</text>
<text>Rev D</text>
<text>w/AbleGamers &amp; GRA-V</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="FEATHERWING_DIM">
</package>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="DO41-7">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X16">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X12">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DB9_MALE">
<description>&lt;h3&gt;9 Pin Serial Connector - Male PCB Mount Right Angle&lt;/h3&gt;
0.318" style. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:11&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/15944.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;DB9&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJW">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ATMakers">
<packages>
<package name="SWDIP2_256X170P100">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J2" library="SparkFun-Connectors" package="DB9_MALE" value="">
<attribute name="PROD_ID" value="CONN-09904"/>
</element>
<element name="MS1" library="adafruit" package="FEATHERWING_DIM" value="FEATHERWING_NODIM"/>
<element name="R1" library="adafruit" package="0207/10" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="0207/10" value="47K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="0207/10" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="0207/10" value="47K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="adafruit" package="0207/10" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="adafruit" package="0207/10" value="47K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinhead" package="1X16" value="">
<attribute name="POPULARITY" value="17"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinhead" package="1X12" value="">
<attribute name="POPULARITY" value="28"/>
<attribute name="VALUE"/>
</element>
<element name="POLOLU" library="pinhead" package="1X03" value="U3V12F12">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="92"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="adafruit" package="DO41-7" value="">
<attribute name="VALUE"/>
</element>
<element name="D2" library="adafruit" package="DO41-7" value="">
<attribute name="VALUE"/>
</element>
<element name="VBAT" library="jumper" package="SJW" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="3"/>
<attribute name="VALUE"/>
</element>
<element name="USB" library="jumper" package="SJW" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="3"/>
<attribute name="VALUE"/>
</element>
<element name="RESET" library="ATMakers" package="SWDIP2_256X170P100" value="1825966-1">
<attribute name="BUILT_BY" value="EMA_UL_Team"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2016 Accelerated Designs. All rights reserved"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="1825966-1"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="TE Connectivity"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="R4" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="POLOLU" pad="2"/>
<contactref element="MS1" pad="4"/>
<contactref element="JP1" pad="4"/>
<contactref element="J2" pad="8"/>
<contactref element="RESET" pad="2"/>
</signal>
<signal name="USB">
<contactref element="MS1" pad="26"/>
<contactref element="JP2" pad="10"/>
<contactref element="USB" pad="2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="MS1" pad="7"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="N$6">
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="JP1" pad="8"/>
<contactref element="MS1" pad="8"/>
</signal>
<signal name="N$9">
<contactref element="R3" pad="2"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="R5" pad="2"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="JP2" pad="1"/>
<contactref element="MS1" pad="17"/>
</signal>
<signal name="N$3">
<contactref element="JP2" pad="2"/>
<contactref element="MS1" pad="18"/>
</signal>
<signal name="N$4">
<contactref element="JP2" pad="3"/>
<contactref element="MS1" pad="19"/>
</signal>
<signal name="N$11">
<contactref element="JP2" pad="4"/>
<contactref element="MS1" pad="20"/>
</signal>
<signal name="N$12">
<contactref element="JP2" pad="5"/>
<contactref element="MS1" pad="21"/>
</signal>
<signal name="N$13">
<contactref element="JP2" pad="6"/>
<contactref element="MS1" pad="22"/>
</signal>
<signal name="N$14">
<contactref element="MS1" pad="23"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="N$15">
<contactref element="JP2" pad="8"/>
<contactref element="MS1" pad="24"/>
</signal>
<signal name="N$16">
<contactref element="MS1" pad="25"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="VBAT">
<contactref element="MS1" pad="28"/>
<contactref element="JP2" pad="12"/>
<contactref element="VBAT" pad="2"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$18">
<contactref element="JP1" pad="16"/>
<contactref element="MS1" pad="16"/>
</signal>
<signal name="N$19">
<contactref element="MS1" pad="15"/>
<contactref element="JP1" pad="15"/>
</signal>
<signal name="N$20">
<contactref element="JP1" pad="14"/>
<contactref element="MS1" pad="14"/>
</signal>
<signal name="N$21">
<contactref element="MS1" pad="13"/>
<contactref element="JP1" pad="13"/>
</signal>
<signal name="N$22">
<contactref element="JP1" pad="12"/>
<contactref element="MS1" pad="12"/>
</signal>
<signal name="N$23">
<contactref element="MS1" pad="11"/>
<contactref element="JP1" pad="11"/>
</signal>
<signal name="N$27">
<contactref element="MS1" pad="3"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="3V">
<contactref element="JP1" pad="2"/>
<contactref element="MS1" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="MS1" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="RESET" pad="1"/>
</signal>
<signal name="V12">
<contactref element="POLOLU" pad="3"/>
<contactref element="J2" pad="7"/>
<contactref element="J2" pad="9"/>
</signal>
<signal name="N$17">
<contactref element="JP1" pad="10"/>
<contactref element="MS1" pad="10"/>
</signal>
<signal name="N$24">
<contactref element="JP2" pad="11"/>
<contactref element="MS1" pad="27"/>
</signal>
<signal name="N$29">
<contactref element="MS1" pad="6"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$30">
<contactref element="MS1" pad="5"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$7">
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="MS1" pad="9"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="VMAX">
<contactref element="POLOLU" pad="1"/>
<contactref element="USB" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="VBAT" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
