(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Vtune")
  (net 2 "RF_Out")
  (net 3 "+5V")
  (net 4 "GND")
  (footprint "VCO:SolderWirePad_single_1mmDrill" (layer "F.Cu")
    (tedit 0)
    (at 109.8804 84.836)
    (property "Sheetfile" "KiCADtutorial.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "TP4" (at 2.34134 0.37284 unlocked) (layer "F.SilkS"))
    (fp_text value "GND" (at 2.34134 1.89684 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 2.159 4.318) (size 2.49936 2.49936) (drill 1.00076) (layers *.Mask "F.Cu" "In1.Cu" "B.Cu" "F.SilkS")
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
  )
  (footprint "VCO:SolderWirePad_single_1mmDrill" (layer "F.Cu")
    (tedit 0)
    (at 110.1344 98.8822)
    (property "Sheetfile" "KiCADtutorial.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "TP5" (at 2.159 6.858 unlocked) (layer "F.SilkS"))
    (fp_text value "GND" (at 2.159 8.636 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 2.159 4.318) (size 2.49936 2.49936) (drill 1.00076) (layers *.Mask "F.Cu" "In1.Cu" "B.Cu" "F.SilkS")
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
  )
  (footprint "VCO:SolderWirePad_single_1mmDrill" (layer "F.Cu")
    (tedit 0)
    (at 120.1166 103.2002)
    (property "Sheetfile" "KiCADtutorial.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "TP1" (at 2.1082 6.6802 unlocked) (layer "F.SilkS"))
    (fp_text value "Vtune" (at 2.159 8.2296 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 2.159 4.318) (size 2.49936 2.49936) (drill 1.00076) (layers *.Mask "F.Cu" "In1.Cu" "B.Cu" "F.SilkS")
      (net 1 "Vtune") (pinfunction "1") (pintype "passive"))
  )
  (footprint "VCO:SolderWirePad_single_1mmDrill" (layer "F.Cu")
    (tedit 0)
    (at 109.982 91.2876)
    (property "Sheetfile" "KiCADtutorial.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "TP3" (at 2.0828 6.731 unlocked) (layer "F.SilkS"))
    (fp_text value "+5V" (at 2.0066 8.1026 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 2.159 4.318) (size 2.49936 2.49936) (drill 1.00076) (layers *.Mask "F.Cu" "In1.Cu" "B.Cu" "F.SilkS")
      (net 3 "+5V") (pinfunction "1") (pintype "passive"))
  )
  (footprint "VCO:MINI-16-SM" (layer "F.Cu")
    (tedit 0)
    (at 116.84 90.932)
    (property "Sheetfile" "KiCADtutorial.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 15.0622 -0.4064 unlocked) (layer "F.SilkS"))
    (fp_text value "VCO" (at -0.1524 -2.1336 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 14.986 unlocked) (layer "F.Fab") hide)
    (pad "1" smd circle (at 5.461 12.7) (size 1.524 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Vtune") (pinfunction "Vtune") (pintype "input"))
    (pad "2" smd circle (at 7.239 0) (size 1.524 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "RF_Out") (pinfunction "RF_Out") (pintype "input"))
    (pad "3" smd circle (at 0 4.699) (size 1.524 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+5V") (pinfunction "VCC") (pintype "input"))
    (pad "GND" smd circle (at 12.7 2.413) (size 1.524 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "GND" smd circle (at 2.159 0) (size 1.524 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "GND" smd circle (at 0 2.159) (size 1.524 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "GND" smd custom (at 1.524 1.524) (size 1.524 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy -0.7112 -0.7112)
            (xy 3.7592 -0.7112)
            (xy 3.7592 1.2192)
            (xy 7.6708 1.2192)
            (xy 7.6708 -0.7112)
            (xy 10.3632 -0.7112)
            (xy 10.3632 10.414)
            (xy 5.8928 10.414)
            (xy 5.8928 8.382)
            (xy 1.9812 8.382)
            (xy 1.9812 10.414)
            (xy -0.7112 10.414)
            (xy -0.7112 5.1308)
            (xy 1.27 5.1308)
            (xy 1.27 1.2192)
            (xy -0.7112 1.2192)
            (xy -0.7112 0.254)
          ) (width 0.2) (fill yes))
      ))
    (pad "GND" smd circle (at 9.779 0) (size 1.524 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "GND" smd circle (at 12.7 7.493) (size 1.524 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "GND" smd circle (at 0 9.779) (size 1.524 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "GND" smd circle (at 12.7 4.953) (size 1.524 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "GND" smd circle (at 10.541 12.7) (size 1.524 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "GND" smd circle (at 8.001 12.7) (size 1.524 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "GND" smd circle (at 4.699 0) (size 1.524 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "GND" smd circle (at 12.7 10.033) (size 1.524 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "GND" smd circle (at 0 7.239) (size 1.524 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "GND" smd circle (at 2.921 12.7) (size 1.524 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
  )
  (footprint "VCO:SMA Molex 0732512120" (layer "F.Cu")
    (tedit 0)
    (at 118.9482 83.8962)
    (attr smd)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "SMA Molex 0732512120" (at 4.191 -2.413 unlocked) (layer "F.Fab") hide)
    (pad "1" smd rect (at 5.08 2.286) (size 1.778 4.191) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "RF_Out"))
    (pad "2" smd rect (at 1.524 2.286) (size 2.667 4.191) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "3" smd rect (at 8.636 2.286) (size 2.667 4.191) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND"))
    (pad "4" smd rect (at 8.636 2.286) (size 2.667 4.191) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND"))
    (pad "5" smd rect (at 1.524 2.286) (size 2.667 4.191) (layers "B.Cu" "F.Paste" "B.Mask")
      (net 4 "GND"))
  )
  (footprint "VCO:SolderWirePad_single_1mmDrill" (layer "F.Cu")
    (tedit 0)
    (at 128.4732 102.8446)
    (property "Sheetfile" "KiCADtutorial.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "TP4" (at 2.413 6.858 unlocked) (layer "F.SilkS"))
    (fp_text value "GND" (at 2.413 8.636 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 2.159 4.318) (size 2.49936 2.49936) (drill 1.00076) (layers *.Mask "F.Cu" "In1.Cu" "B.Cu" "F.SilkS")
      (net 4 "GND") (pinfunction "1") (pintype "passive"))
  )
  (gr_rect (start 134.62 83.8454) (end 109.1438 112.7252) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "VCO\nBreadboard" (at 113.6396 110.3376) (layer "F.SilkS"))
  (zone (net 4) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.1778))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.8326 111.9378)
        (xy 110.0582 111.9378)
        (xy 110.0582 84.4296)
        (xy 133.8326 84.4296)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.1778))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.858 111.9124)
        (xy 110.0836 111.9124)
        (xy 110.0836 84.4042)
        (xy 133.858 84.4042)
      )
    )
  )
)
