(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 0)
    (no_connects 0)
    (area 106.924999 49.924999 125.075001 134.075001)
    (thickness 1.6)
    (drawings 42)
    (tracks 199)
    (zones 0)
    (modules 29)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.1)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.7 1.3)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "Ceci est la Netclass par défaut"
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer B.Cu) (tedit 58D0379B)
    (at 110.25 66.75)
    (fp_text reference bat+ (at -0.25 -2) (layer B.SilkS))
    (fp_text value "" (at 0 -2.54) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer B.Cu) (tedit 58D0378A)
    (at 121.35 67)
    (fp_text reference 510- (at 0.65 -3.5) (layer B.SilkS))
    (fp_text value "" (at 0 -2.54) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.3 2.3) (drill 1.5) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D037D0)
    (at 113.5 73)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.25 0.25) (drill 0.25) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D03781)
    (at 113.75 80.75)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.25 0.25) (drill 0.25) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D03772)
    (at 118 83.75)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.25 0.25) (drill 0.25) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D0377A)
    (at 118 82.25)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.25 0.25) (drill 0.25) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D03763)
    (at 115.5 90.5)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.25 0.25) (drill 0.25) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D036F4)
    (at 113 118)
    (fp_text reference 0 (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D036EC)
    (at 119 118)
    (fp_text reference 100 (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D03721)
    (at 122.25 78)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D0371C)
    (at 122.25 80.5)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D03717)
    (at 122.25 83)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D03711)
    (at 122.25 85.5)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D03708)
    (at 122.25 88)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D03703)
    (at 122.25 90.5)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D0374A)
    (at 109.75 90.5)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D03742)
    (at 109.75 88)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D0373B)
    (at 109.75 85.5)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D03733)
    (at 109.75 83)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D0372E)
    (at 109.75 80.5)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D03728)
    (at 109.75 78)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58D037DF)
    (at 120 82.75 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "" (at 0 1.65 270) (layer B.SilkS))
    (fp_text value "" (at 0 -1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin -0.1))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin -0.1))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-669_LFPAK (layer B.Cu) (tedit 58D01FAD)
    (at 116 68 90)
    (descr "LFPAK www.nxp.com/documents/leaflet/939775016838_LR.pdf")
    (tags "LFPAK SOT-669 Power-SO8")
    (solder_mask_margin 0.07)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference "" (at -0.27 3.48 90) (layer B.SilkS))
    (fp_text value "" (at -0.27 -3.52 90) (layer B.Fab))
    (fp_text user %R (at -0.04 0 90) (layer B.Fab))
    (pad 5 smd rect (at 0.16 1.15 90) (size 0.6 0.9) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at -0.69 1.15 90) (size 0.6 0.9) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 1.01 1.15 90) (size 0.6 0.9) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 0.16 -1.15 90) (size 0.6 0.9) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at -0.69 -1.15 90) (size 0.6 0.9) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 1.01 -1.15 90) (size 0.6 0.9) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 1.01 0 90) (size 0.6 0.9) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at -0.69 0 90) (size 0.6 0.9) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 2.86 1.88 180) (size 0.6 0.9) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 2.86 -1.88 180) (size 0.6 0.9) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 2.86 0.6 180) (size 0.6 0.9) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -2.86 0.64 180) (size 0.7 1.15) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -2.86 1.91 180) (size 0.7 1.15) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 3 smd rect (at -2.86 -0.64 180) (size 0.7 1.15) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 5 smd rect (at 2.61 0 180) (size 4.7 1.55) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.07))
    (pad 5 smd rect (at 0.41 0 180) (size 4.2 3.3) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.07))
    (pad 4 smd rect (at -2.86 -1.91 180) (size 0.7 1.15) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.07) (solder_paste_margin -0.05))
    (pad 5 smd rect (at 2.86 -0.6 180) (size 0.6 0.9) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 0.16 0 90) (size 0.6 0.9) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-669_LFPAK.wrl
      (at (xyz -0.01 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 90))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH_6mm_h5mm (layer F.Cu) (tedit 58D037B4)
    (at 112.75 57.5)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (fp_text reference "" (at 3.25 -2) (layer F.SilkS))
    (fp_text value "" (at 3.75 6.7) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
    (model Buttons_Switches_THT.3dshapes/SW_PUSH_6mm_h5mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D036FA)
    (at 116 121)
    (fp_text reference 50 (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer B.Cu) (tedit 58D03795)
    (at 116.6 73)
    (fp_text reference Bat- (at -3.8 0.2) (layer B.SilkS))
    (fp_text value "" (at 0 -2.54) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.3 2.3) (drill 1.5) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D03769)
    (at 116.75 90.5)
    (fp_text reference "" (at 0 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.25 0.25) (drill 0.25) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
  )
  (module LEDs:LED_D3.0mm_FlatTop (layer F.Cu) (tedit 58D036E1)
    (at 114.75 102.5)
    (descr "LED, Round, FlatTop, diameter 3.0mm, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-47XEC(Ver.9A).pdf")
    (tags "LED Round FlatTop diameter 3.0mm 2 pins")
    (fp_text reference Led (at 1.27 -2.96) (layer F.SilkS))
    (fp_text value "" (at 1.27 2.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (solder_mask_margin -0.1))
    (model LEDs.3dshapes/LED_D3.0mm_FlatTop.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58D038FB)
    (at 121 102.75)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference "" (at 0 -1.65) (layer F.SilkS))
    (fp_text value "" (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin -0.1))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin -0.1))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Adaptateur\nSmartPWM\nv2.0" (at 116.25 128.75) (layer F.Cu))
  (gr_text "Adaptateur\nSmartPWM\nv2.0" (at 116.25 128.75) (layer B.Cu))
  (gr_line (start 107 134) (end 107 133) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125 134) (end 107 134) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125 50) (end 125 134) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107 50) (end 125 50) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107 92) (end 107 50) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107 134) (end 107 92) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.1) (thermal_bridge_width 0.15))
    (polygon
      (pts
        (xy 125 134) (xy 107 134) (xy 107 50) (xy 125 50)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.1) (thermal_bridge_width 0.15))
    (polygon
      (pts
        (xy 125 134) (xy 107 134) (xy 107 50) (xy 125 50)
      )
    )
  )
)
