<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<text>Reyax RYN25AI GPS Breakout v1</text>
<text>KD0GLS 2016</text>
<text>GND</text>
<text>+5V</text>
<text>PPS</text>
<text>RXD</text>
<text>TXD</text>
<text>NC</text>
<wire x1="3.175" y1="0" x2="23.495" y2="0" width="0.254" layer="20"/>
<wire x1="26.67" y1="3.175" x2="26.67" y2="41.275" width="0.254" layer="20"/>
<wire x1="23.495" y1="44.45" x2="3.175" y2="44.45" width="0.254" layer="20"/>
<wire x1="0" y1="41.275" x2="0" y2="3.175" width="0.254" layer="20"/>
<wire x1="0" y1="3.175" x2="3.175" y2="0" width="0.254" layer="20" curve="90"/>
<wire x1="23.495" y1="0" x2="26.67" y2="3.175" width="0.254" layer="20" curve="90"/>
<wire x1="26.67" y1="41.275" x2="23.495" y2="44.45" width="0.254" layer="20" curve="90"/>
<wire x1="3.175" y1="44.45" x2="0" y2="41.275" width="0.254" layer="20" curve="90"/>
</plain>
<libraries>
<library name="kd0gls">
<description>KD0GLS Amateur Radio Design Library</description>
<packages>
<package name="0805">
</package>
<package name="SOT23-6">
<description>Revised pad sizes and positions per SN74LVC1T45DBVR data sheet.</description>
</package>
<package name="SOT23-3">
<description>Revised pad sizes and spacing per LM3480 data sheet.</description>
</package>
<package name="GPS_REYAX_RNA25AI">
</package>
<package name="CONN_BREAKAWAY_1X6_100">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="kd0gls" package="0805" value="0.1uF"/>
<element name="C2" library="kd0gls" package="0805" value="0.1uF"/>
<element name="JP1" library="kd0gls" package="CONN_BREAKAWAY_1X6_100" value="CONN_BREAKAWAY_1X6_100"/>
<element name="U4" library="kd0gls" package="SOT23-6" value="74LVC1T45DBV"/>
<element name="U3" library="kd0gls" package="SOT23-6" value="74LVC1T45DBV"/>
<element name="U2" library="kd0gls" package="SOT23-6" value="74LVC1T45DBV"/>
<element name="U1" library="kd0gls" package="SOT23-3" value="LM3480"/>
<element name="U5" library="kd0gls" package="GPS_REYAX_RNA25AI" value="GPS_REYAX_RYN25AI"/>
<element name="R1" library="kd0gls" package="0805" value="10K"/>
</elements>
<signals>
<signal name="GND">
<contactref element="JP1" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="U3" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="U4" pad="2"/>
<contactref element="U5" pad="9"/>
<contactref element="U5" pad="5"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U3" pad="5"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="5V">
<contactref element="U2" pad="1"/>
<contactref element="U3" pad="1"/>
<contactref element="U4" pad="1"/>
<contactref element="JP1" pad="3"/>
<contactref element="U1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="U5" pad="2"/>
<contactref element="U4" pad="5"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="TXDB">
<contactref element="U3" pad="4"/>
<contactref element="U5" pad="3"/>
</signal>
<signal name="RXDB">
<contactref element="U4" pad="4"/>
<contactref element="U5" pad="4"/>
</signal>
<signal name="PPSB">
<contactref element="U2" pad="4"/>
<contactref element="U5" pad="12"/>
</signal>
<signal name="3V3">
<contactref element="U2" pad="6"/>
<contactref element="U3" pad="6"/>
<contactref element="U4" pad="6"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="TXDA">
<contactref element="U3" pad="3"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="RXDA">
<contactref element="U4" pad="3"/>
<contactref element="JP1" pad="4"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="PPSA">
<contactref element="U2" pad="3"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$7">
</signal>
<signal name="N$8">
</signal>
</signals>
</board>
</drawing>
</eagle>
