(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.5313)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(1 "In1.Cu" signal)
		(2 "In2.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.04318)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(color "FR4 natural")
				(thickness 0.199898)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.017272)
			)
			(layer "dielectric 2"
				(type "core")
				(color "FR4 natural")
				(thickness 0.9906)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.017272)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(color "FR4 natural")
				(thickness 0.199898)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.04318)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(property "ADDRESS1" "22605 Gateway Center Drive")
	(property "ADDRESS2" "Clarksburg")
	(property "ADDRESS3" "MD")
	(property "ADDRESS4" "USA 20871")
	(property "DOCUMENTNUMBER" "")
	(property "ORGANIZATION" "Thales DSI")
	(property "SHEETTOTAL" "5")
	(net 0 "")
	(net 1 "GND")
	(net 2 "Net-(U1-SCLK)")
	(net 3 "Net-(U1-SDO)")
	(net 4 "Net-(U1-VDD)")
	(net 5 "Net-(U1-~{CS})")
	(net 6 "Net-(U1-RF1)")
	(net 7 "Net-(U1-SDI)")
	(net 8 "Net-(U1-RF2)")
	(net 9 "Net-(U1-SFL)")
	(net 10 "Net-(U1-VSS)")
	(net 11 "Net-(U1-BYP)")
	(net 12 "Net-(U1-~{RST})")
	(footprint "t_BGA:CC-40-12_ADI_X"
		(layer "F.Cu")
		(at 103.7082 43.942)
		(tags "ADMV8513ACCZ ")
		(property "Reference" "U2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "368388-502"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_BGA:CC-40-12_ADI_X"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Digitally Tunable Band-Pass Filter, 90 MHz-225 MHz, 10mmx10mm 90~225MHz Tunable BPF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CASE/PACKAGE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAX OPERATING TEMPERATURE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAX SUPPLY VOLTAGE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFG_ID" "Analog Devices"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFG_ITM_ID" "ADMV8502ACCZ-R7"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MIN OPERATING TEMPERATURE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MIN SUPPLY VOLTAGE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MOUNTING TECHNOLOGY" "SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PINS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS COMPLIANT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*ADMV85xx_10x10mm*")
		(sheetname "Root")
		(sheetfile "ADMV.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -5.6388 -4.5 0)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -5.6388 -4.5 0)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -3.4544 -4.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -3.4544 -4.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -4.5466 -4.499999 90)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -4.5466 -3.6 90)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "Net-(U1-VSS)")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -4.5466 -2.7 90)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -4.5466 -1.799999 90)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "Net-(U1-RF2)")
			(pinfunction "RF1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -4.5466 -0.900001 90)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -4.5466 0 90)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -4.5466 0.900001 90)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -4.5466 1.799999 90)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -4.5466 2.7 90)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at -4.5466 3.6 90)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at -4.5466 4.500001 90)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at -3.6 4.5466)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at -2.7 4.5466)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at -1.799999 4.5466)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at -0.900001 4.5466)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at 0 4.5466)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at 0.900001 4.5466)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "18" smd rect
			(at 1.799999 4.5466)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "19" smd rect
			(at 2.7 4.5466)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "20" smd rect
			(at 3.6 4.5466)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "21" smd rect
			(at 4.5466 4.499999 90)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "22" smd rect
			(at 4.5466 3.6 90)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "23" smd rect
			(at 4.5466 2.7 90)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "24" smd rect
			(at 4.5466 1.799999 90)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "25" smd rect
			(at 4.5466 0.900001 90)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "26" smd rect
			(at 4.5466 0 90)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "27" smd rect
			(at 4.5466 -0.900001 90)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "28" smd rect
			(at 4.5466 -1.800001 90)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "Net-(U1-RF1)")
			(pinfunction "RF2")
			(pintype "passive")
		)
		(pad "29" smd rect
			(at 4.5466 -2.7 90)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "30" smd rect
			(at 4.5466 -3.6 90)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "Net-(U1-VDD)")
			(pinfunction "VDD")
			(pintype "passive")
		)
		(pad "31" smd rect
			(at 4.5466 -4.500001 90)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "32" smd rect
			(at 3.6 -4.5466)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "Net-(U1-BYP)")
			(pinfunction "BYP")
			(pintype "passive")
		)
		(pad "33" smd rect
			(at 2.7 -4.5466)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "Net-(U1-SFL)")
			(pinfunction "SFL")
			(pintype "passive")
		)
		(pad "34" smd rect
			(at 1.799999 -4.5466)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "Net-(U1-SCLK)")
			(pinfunction "SCLK")
			(pintype "passive")
		)
		(pad "35" smd rect
			(at 0.900001 -4.5466)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(U1-SDO)")
			(pinfunction "SDO")
			(pintype "passive")
		)
		(pad "36" smd rect
			(at 0 -4.5466)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "Net-(U1-SDI)")
			(pinfunction "SDI")
			(pintype "passive")
		)
		(pad "37" smd rect
			(at -0.900001 -4.5466)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "38" smd rect
			(at -1.799999 -4.5466)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "Net-(U1-~{CS})")
			(pinfunction "~{CS}")
			(pintype "passive")
		)
		(pad "39" smd rect
			(at -2.7 -4.5466)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "40" smd rect
			(at -3.6 -4.5466)
			(size 0.5588 0.6096)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "Net-(U1-~{RST})")
			(pinfunction "~{RST}")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at -3.075 -1.025)
			(size 1.8542 1.8542)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at -3.075 1.025)
			(size 1.8542 1.8542)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at -3.075 3.075)
			(size 1.8542 1.8542)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at -2.6686 -2.6686)
			(size 1.016 1.016)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at -1.02511 -2.6686)
			(size 1.8542 1.016)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at -1.025 -1.025)
			(size 1.8542 1.8542)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at -1.025 1.025)
			(size 1.8542 1.8542)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at -1.025 3.075)
			(size 1.8542 1.8542)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at 1.02489 -2.6686)
			(size 1.8542 1.016)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at 1.02489 -1.025)
			(size 1.8542 1.8542)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at 1.02489 1.025)
			(size 1.8542 1.8542)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at 1.02489 3.075)
			(size 1.8542 1.8542)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at 2.66849 -2.6686)
			(size 1.016 1.016)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at 3.07489 -1.025)
			(size 1.8542 1.8542)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at 3.07489 1.025)
			(size 1.8542 1.8542)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at 3.07489 3.075)
			(size 1.8542 1.8542)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
	)
	(footprint "t_BGA:CC-40-12_ADI_X"
		(layer "B.Cu")
		(at 103.7082 43.942 180)
		(tags "ADMV8513ACCZ ")
		(property "Reference" "U1"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "368388-502"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "t_BGA:CC-40-12_ADI_X"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Digitally Tunable Band-Pass Filter, 90 MHz-225 MHz, 10mmx10mm 90~225MHz Tunable BPF"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CASE/PACKAGE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MAX OPERATING TEMPERATURE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MAX SUPPLY VOLTAGE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFG_ID" "Analog Devices"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFG_ITM_ID" "ADMV8502ACCZ-R7"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MIN OPERATING TEMPERATURE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MIN SUPPLY VOLTAGE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MOUNTING TECHNOLOGY" "SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PINS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ROHS COMPLIANT" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*ADMV85xx_10x10mm*")
		(sheetname "Root")
		(sheetfile "ADMV.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -5.6388 4.5 0)
			(layer "B.SilkS")
		)
		(fp_text user "*"
			(at -5.6388 4.5 0)
			(layer "B.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(fp_text user "*"
			(at -3.4544 4.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(fp_text user "*"
			(at -3.4544 4.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -4.5466 4.499999 90)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -4.5466 3.6 90)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 10 "Net-(U1-VSS)")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -4.5466 2.7 90)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -4.5466 1.799999 90)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 6 "Net-(U1-RF1)")
			(pinfunction "RF1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -4.5466 0.900001 90)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -4.5466 0 90)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -4.5466 -0.900001 90)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -4.5466 -1.799999 90)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -4.5466 -2.7 90)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at -4.5466 -3.6 90)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at -4.5466 -4.500001 90)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at -3.6 -4.5466 180)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at -2.7 -4.5466 180)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at -1.799999 -4.5466 180)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at -0.900001 -4.5466 180)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at 0 -4.5466 180)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at 0.900001 -4.5466 180)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "18" smd rect
			(at 1.799999 -4.5466 180)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "19" smd rect
			(at 2.7 -4.5466 180)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "20" smd rect
			(at 3.6 -4.5466 180)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "21" smd rect
			(at 4.5466 -4.499999 90)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "22" smd rect
			(at 4.5466 -3.6 90)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "23" smd rect
			(at 4.5466 -2.7 90)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "24" smd rect
			(at 4.5466 -1.799999 90)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "25" smd rect
			(at 4.5466 -0.900001 90)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "26" smd rect
			(at 4.5466 0 90)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "27" smd rect
			(at 4.5466 0.900001 90)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "28" smd rect
			(at 4.5466 1.800001 90)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 8 "Net-(U1-RF2)")
			(pinfunction "RF2")
			(pintype "passive")
		)
		(pad "29" smd rect
			(at 4.5466 2.7 90)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "30" smd rect
			(at 4.5466 3.6 90)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 4 "Net-(U1-VDD)")
			(pinfunction "VDD")
			(pintype "passive")
		)
		(pad "31" smd rect
			(at 4.5466 4.500001 90)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "32" smd rect
			(at 3.6 4.5466 180)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 11 "Net-(U1-BYP)")
			(pinfunction "BYP")
			(pintype "passive")
		)
		(pad "33" smd rect
			(at 2.7 4.5466 180)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 9 "Net-(U1-SFL)")
			(pinfunction "SFL")
			(pintype "passive")
		)
		(pad "34" smd rect
			(at 1.799999 4.5466 180)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "Net-(U1-SCLK)")
			(pinfunction "SCLK")
			(pintype "passive")
		)
		(pad "35" smd rect
			(at 0.900001 4.5466 180)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 3 "Net-(U1-SDO)")
			(pinfunction "SDO")
			(pintype "passive")
		)
		(pad "36" smd rect
			(at 0 4.5466 180)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 7 "Net-(U1-SDI)")
			(pinfunction "SDI")
			(pintype "passive")
		)
		(pad "37" smd rect
			(at -0.900001 4.5466 180)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "38" smd rect
			(at -1.799999 4.5466 180)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 5 "Net-(U1-~{CS})")
			(pinfunction "~{CS}")
			(pintype "passive")
		)
		(pad "39" smd rect
			(at -2.7 4.5466 180)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "40" smd rect
			(at -3.6 4.5466 180)
			(size 0.5588 0.6096)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 12 "Net-(U1-~{RST})")
			(pinfunction "~{RST}")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at -3.075 -3.075 180)
			(size 1.8542 1.8542)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at -3.075 -1.025 180)
			(size 1.8542 1.8542)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at -3.075 1.025 180)
			(size 1.8542 1.8542)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at -2.6686 2.6686 180)
			(size 1.016 1.016)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at -1.02511 2.6686 180)
			(size 1.8542 1.016)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at -1.025 -3.075 180)
			(size 1.8542 1.8542)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at -1.025 -1.025 180)
			(size 1.8542 1.8542)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at -1.025 1.025 180)
			(size 1.8542 1.8542)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at 1.02489 -3.075 180)
			(size 1.8542 1.8542)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at 1.02489 -1.025 180)
			(size 1.8542 1.8542)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at 1.02489 1.025 180)
			(size 1.8542 1.8542)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at 1.02489 2.6686 180)
			(size 1.8542 1.016)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at 2.66849 2.6686 180)
			(size 1.016 1.016)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at 3.07489 -3.075 180)
			(size 1.8542 1.8542)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at 3.07489 -1.025 180)
			(size 1.8542 1.8542)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "EP" smd rect
			(at 3.07489 1.025 180)
			(size 1.8542 1.8542)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
	)
	(gr_line
		(start 98.679 38.354)
		(end 98.171 38.862)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.171 38.862)
		(end 98.171 49.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.171 49.53)
		(end 109.347 49.53)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 109.347 49.53)
		(end 109.347 38.354)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 109.347 38.354)
		(end 98.679 38.354)
		(layer "Edge.Cuts")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "In1.Cu" "In2.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.254)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 98.3488 38.5318) (xy 109.093 38.5318) (xy 109.093 49.3014) (xy 98.3234 49.3014)
			)
		)
	)
)
