<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0.254" x2="9.0351" y2="0.254" width="0" layer="20"/>
<wire x1="9.0351" y1="0.254" x2="9.0351" y2="17.069" width="0" layer="20"/>
<wire x1="9.0351" y1="17.069" x2="0" y2="17.069" width="0" layer="20"/>
<wire x1="0" y1="17.069" x2="0" y2="0.254" width="0" layer="20"/>
<text>1</text>
<text>Tool</text>
<text>Target</text>
</plain>
<libraries>
<library name="tag-connect">
<description>&lt;h3&gt;TAG-CONNECT ICSP Connector&lt;/h3&gt;&lt;BR&gt;&lt;I&gt;Manufacturer:&lt;/I&gt; &lt;a href="http://www.tag-connect.com"&gt;Tag-Connect&lt;/a&gt;&lt;BR&gt;
&lt;BR&gt;Cable for easy In-Circuit Serial Programming. Designed for Microchip ICD2, suitable for many others.&lt;BR&gt;
Two variants - one "with legs" (for hands-free fit on PCB) and another "without legs" for quick programming.

&lt;p&gt;
&lt;TABLE cellspacing=0 cellpadding=0 border=0&gt;
&lt;TR&gt;&lt;TD width=20&gt;&lt;/TD&gt;&lt;TD&gt;
&lt;TABLE cellspacing=0 cellpadding=1 border=1&gt;
&lt;TR bgcolor=silver&gt;&lt;TD align=center&gt;PAD&lt;/TD&gt;&lt;TD align=center&gt;Description&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;1&lt;/TD&gt;&lt;TD&gt;MCLR/Vpp&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;2&lt;/TD&gt;&lt;TD&gt;Vdd&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;3&lt;/TD&gt;&lt;TD&gt;GND&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;4&lt;/TD&gt;&lt;TD&gt;PGD (ISPDAT)&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;5&lt;/TD&gt;&lt;TD&gt;PGC (ISPCLK)&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;6&lt;/TD&gt;&lt;TD&gt;nc (used for LVP)&lt;/TD&gt;&lt;/TR&gt;
&lt;/TABLE&gt;
&lt;/TD&gt;&lt;/TR&gt;&lt;/TABLE&gt;&lt;BR&gt;&lt;BR&gt;

©2009 ROFA.cz - modified and updated by Robert Darlington &amp;#8249;rdarlington@gmail.com&amp;#8250;</description>
<packages>
<package name="TC2030-MCP">
<description>&lt;b&gt;TAG-CONNECT ICSP Connector&lt;/b&gt; - Legged version&lt;BR&gt;&lt;I&gt;Manufacturer:&lt;/I&gt; &lt;a href="http://www.tag-connect.com"&gt;Tag-Connect&lt;/a&gt;
&lt;p&gt;
Cable for easy In-Circuit Serial Programming. Designed for Microchip ICD2, suitable for many others.
&lt;p&gt;
&lt;b&gt;NOTE:&lt;/b&gt; Eagle's default spacing for drill holes does not leave sufficent room for routing traces for this footprint and should be adjusted. &lt;br&gt;
This setting can be found in the board layout editor under the Edit menu.  Select "Design Rules" and then the Distance tab.  8 mils for Drill/Hole works well.
&lt;br&gt;
&lt;TABLE cellspacing=0 cellpadding=0 border=0&gt;
&lt;TR&gt;&lt;TD width=20&gt;&lt;/TD&gt;&lt;TD&gt;
&lt;TABLE cellspacing=0 cellpadding=1 border=1&gt;
&lt;TR bgcolor=silver&gt;&lt;TD align=center&gt;PAD&lt;/TD&gt;&lt;TD align=center&gt;Description&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;1&lt;/TD&gt;&lt;TD&gt;MCLR/Vpp&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;2&lt;/TD&gt;&lt;TD&gt;Vdd&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;3&lt;/TD&gt;&lt;TD&gt;GND&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;4&lt;/TD&gt;&lt;TD&gt;PGD (ISPDAT)&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;5&lt;/TD&gt;&lt;TD&gt;PGC (ISPCLK)&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;6&lt;/TD&gt;&lt;TD&gt;nc (used for LVP)&lt;/TD&gt;&lt;/TR&gt;
&lt;/TABLE&gt;
&lt;/TD&gt;&lt;/TR&gt;&lt;/TABLE&gt;&lt;BR&gt;&lt;BR&gt;
©2009 ROFA.cz - modified and updated by Robert Darlington &amp;#8249;rdarlington@gmail.com&amp;#8250;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="aerodynes">
<description>My own parts list for Aerodynes projects.</description>
<packages>
<package name="1X4-1.27MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="--" library="tag-connect" package="TC2030-MCP" value=""/>
<element name="-" library="pinhead" package="1X03" value=""/>
<element name="U$1" library="aerodynes" package="1X4-1.27MM" value="1X04-CONN1.27"/>
</elements>
<signals>
<signal name="SBWTDIO">
<contactref element="--" pad="1"/>
<contactref element="U$1" pad="P$3"/>
</signal>
<signal name="TCK">
<contactref element="--" pad="3"/>
</signal>
<signal name="VCC_TARGET">
<contactref element="--" pad="4"/>
<contactref element="-" pad="1"/>
</signal>
<signal name="GND">
<contactref element="--" pad="5"/>
<contactref element="U$1" pad="P$4"/>
</signal>
<signal name="SBWTCK">
<contactref element="--" pad="6"/>
<contactref element="U$1" pad="P$2"/>
</signal>
<signal name="VCC_TOOL">
<contactref element="--" pad="2"/>
<contactref element="-" pad="3"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="P$1"/>
<contactref element="-" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
