<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.1">
<drawing>
<board>
<plain>
<wire x1="-32" y1="18.6257" x2="-32" y2="10.6257" width="0.1524" layer="20" locked="yes"/>
<wire x1="-32" y1="10.6257" x2="-21.3743" y2="10.6257" width="0.1524" layer="20" locked="yes"/>
<wire x1="-21.3743" y1="10.6257" x2="-14" y2="18" width="0.1524" layer="20" curve="90" locked="yes"/>
<wire x1="-14" y1="18" x2="-14" y2="24.3287" width="0.1524" layer="20" locked="yes"/>
<wire x1="-8.4086" y1="29.9201" x2="-14" y2="24.3287" width="0.1524" layer="20" curve="90" locked="yes"/>
<wire x1="-8.4086" y1="29.9201" x2="10.0822" y2="29.9201" width="0.1524" layer="20" locked="yes"/>
<wire x1="15.6736" y1="24.3287" x2="10.0822" y2="29.9201" width="0.1524" layer="20" curve="90" locked="yes"/>
<wire x1="15.6736" y1="24.3287" x2="15.6736" y2="18" width="0.1524" layer="20" locked="yes"/>
<wire x1="15.6736" y1="18" x2="23.0479" y2="10.6257" width="0.1524" layer="20" curve="90" locked="yes"/>
<wire x1="23.0479" y1="10.6257" x2="34" y2="10.6257" width="0.1524" layer="20" locked="yes"/>
<wire x1="34" y1="18.6257" x2="34" y2="10.6257" width="0.1524" layer="20" locked="yes"/>
<wire x1="25.6736" y1="18.6257" x2="34" y2="18.6257" width="0.1524" layer="20" locked="yes"/>
<wire x1="23.6736" y1="20.6257" x2="25.6736" y2="18.6257" width="0.1524" layer="20" curve="90" locked="yes"/>
<wire x1="23.6736" y1="24.3287" x2="23.6736" y2="20.6257" width="0.1524" layer="20" locked="yes"/>
<wire x1="23.6736" y1="24.3287" x2="10.0822" y2="37.9201" width="0.1524" layer="20" curve="90" locked="yes"/>
<wire x1="-8.4086" y1="37.9201" x2="10.0822" y2="37.9201" width="0.1524" layer="20" locked="yes"/>
<wire x1="-8.4086" y1="37.9201" x2="-22" y2="24.3287" width="0.1524" layer="20" curve="90" locked="yes"/>
<wire x1="-22" y1="20.6257" x2="-22" y2="24.3287" width="0.1524" layer="20" locked="yes"/>
<wire x1="-24" y1="18.6257" x2="-22" y2="20.6257" width="0.1524" layer="20" curve="90" locked="yes"/>
<wire x1="-32" y1="18.6257" x2="-24" y2="18.6257" width="0.1524" layer="20" locked="yes"/>
</plain>
<libraries>
<library name="my liib">
<packages>
<package name="5050661422">
<description>&lt;b&gt;505066-1422-1&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="5050701422">
<description>&lt;b&gt;505070-1422-2&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="my liib" package="5050661422" value="505066-1422">
<attribute name="DESCRIPTION" value="SlimStack Board-to-Board Connector, 0.35mm Pitch, SSB RP Series, Receptacle, 0.60mm Mated Height, 2.00mm Mated Width,  Circuits, Armor Nail"/>
<attribute name="HEIGHT" value="0.63mm"/>
<attribute name="MANUFACTURER_NAME" value="Molex"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="505066-1422"/>
<attribute name="MOUSER_PART_NUMBER" value="538-505066-1422"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Molex/505066-1422?qs=byeeYqUIh0O5SJsk39MHXQ%3D%3D"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="my liib" package="5050701422" value="505070-1422">
<attribute name="DESCRIPTION" value="SlimStack Board-to-Board Connector, 0.35mm Pitch, SSB RP Series, Plug, 0.60 or 0.70mm Mated Height, 2.00mm Mated Width,  Circuits, Armor Nail, 0.15mm Fitting Nail Width"/>
<attribute name="HEIGHT" value="0.53mm"/>
<attribute name="MANUFACTURER_NAME" value="Molex"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="505070-1422"/>
<attribute name="MOUSER_PART_NUMBER" value="538-505070-1422"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Molex/505070-1422?qs=byeeYqUIh0MJdy30K67lng%3D%3D"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="P1">
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="P3">
<contactref element="J1" pad="3"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="P5">
<contactref element="J1" pad="5"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="P7">
<contactref element="J1" pad="7"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="P9">
<contactref element="J1" pad="9"/>
<contactref element="J2" pad="9"/>
</signal>
<signal name="P11">
<contactref element="J1" pad="11"/>
<contactref element="J2" pad="11"/>
</signal>
<signal name="P13">
<contactref element="J1" pad="13"/>
<contactref element="J2" pad="13"/>
</signal>
<signal name="P2">
<contactref element="J1" pad="2"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="P4">
<contactref element="J1" pad="4"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="P6">
<contactref element="J1" pad="6"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="P8">
<contactref element="J1" pad="8"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="P10">
<contactref element="J1" pad="10"/>
<contactref element="J2" pad="10"/>
</signal>
<signal name="P12">
<contactref element="J1" pad="12"/>
<contactref element="J2" pad="12"/>
</signal>
<signal name="P14">
<contactref element="J1" pad="14"/>
<contactref element="J2" pad="14"/>
</signal>
<signal name="N$2">
<contactref element="J1" pad="MP4"/>
<contactref element="J2" pad="MP4"/>
</signal>
<signal name="N$3">
<contactref element="J1" pad="MP3"/>
<contactref element="J2" pad="MP3"/>
</signal>
<signal name="N$4">
<contactref element="J2" pad="MP1"/>
<contactref element="J1" pad="MP1"/>
</signal>
<signal name="N$5">
<contactref element="J1" pad="MP2"/>
<contactref element="J2" pad="MP2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
