(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 10)
    (no_connects 0)
    (area 109.144999 87.046999 129.869001 105.993001)
    (thickness 1.6)
    (drawings 7)
    (tracks 18)
    (zones 0)
    (modules 5)
    (nets 13)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.006)
    (trace_clearance 0.006)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.006)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.027)
    (via_drill 0.013)
    (via_min_size 0.027)
    (via_min_drill 0.013)
    (uvia_size 0.03)
    (uvia_drill 0.02)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 "Net-(D1-Pad2)")
  (net 3 +3V3)
  (net 4 "Net-(J1-Pad3)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 GND)
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(J1-Pad10)")
  (net 10 "Net-(J1-Pad11)")
  (net 11 "Net-(J1-Pad12)")
  (net 12 "Net-(D1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.006)
    (trace_width 0.006)
    (via_dia 0.027)
    (via_drill 0.013)
    (uvia_dia 0.03)
    (uvia_drill 0.02)
  )
  (net_class pwr ""
    (clearance 0.06)
    (trace_width 0.5)
    (via_dia 0.027)
    (via_drill 0.013)
    (uvia_dia 0.03)
    (uvia_drill 0.02)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
  )
  (net_class sig ""
    (clearance 0.03)
    (trace_width 0.45)
    (via_dia 0.027)
    (via_drill 0.013)
    (uvia_dia 0.03)
    (uvia_drill 0.02)
    (add_net "Net-(D1-Pad2)")
  )
  (module TO_SOT_Packages_SMD:TSOT-23_HandSoldering (layer Top) (tedit 595EB9D0)
    (at 120.142 92.202 90)
    (descr "5-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_5_05-08-1635.pdf")
    (tags "TSOT-23 Hand-soldering")
    (attr smd)
    (fp_text reference D1 (at 3.81 0 360) (layer F.SilkS))
    (fp_text value Schottky (at 0.127 -1.016 90) (layer F.Fab))
    (pad 1 smd rect (at -1.71 -0.95 90) (size 2 0.65) (layers Top F.Paste F.Mask)
      (net 12 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at -1.71 0.95 90) (size 2 0.65) (layers Top F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 3 smd rect (at 1.71 0 90) (size 2 0.65) (layers Top F.Paste F.Mask)
      (net 1 +5V))
  )
  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer Top) (tedit 595EB8BB)
    (at 113.538 90.424 270)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference J2 (at 6.223 1.143 360) (layer F.SilkS))
    (fp_text value JST_XH_01X02 (at 2.413 4.445 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(D1-Pad1)"))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TSOT-23_HandSoldering (layer Top) (tedit 595EBC9F)
    (at 114.681 100.457 180)
    (descr "5-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_5_05-08-1635.pdf")
    (tags "TSOT-23 Hand-soldering")
    (attr smd)
    (fp_text reference Q1 (at 0 -2.54 360) (layer F.SilkS))
    (fp_text value MOSFET (at 0.127 0.889 180) (layer F.Fab))
    (pad 1 smd rect (at -1.71 -0.95 180) (size 2 0.65) (layers Top F.Paste F.Mask)
      (net 11 "Net-(J1-Pad12)"))
    (pad 2 smd rect (at -1.71 0.95 180) (size 2 0.65) (layers Top F.Paste F.Mask)
      (net 6 GND))
    (pad 3 smd rect (at 1.71 0 180) (size 2 0.65) (layers Top F.Paste F.Mask)
      (net 12 "Net-(D1-Pad1)"))
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer Top) (tedit 595EB8B1)
    (at 120.142 100.584 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 4.064 0 180) (layer F.SilkS))
    (fp_text value 100K (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers Top F.Paste F.Mask)
      (net 11 "Net-(J1-Pad12)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers Top F.Paste F.Mask)
      (net 6 GND))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x06_Pitch2.54mm (layer Bottom) (tedit 588DE958)
    (at 124.714 90.17 180)
    (descr "Through hole straight socket strip, 2x06, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x06 2.54mm double row")
    (fp_text reference J1 (at -1.27 2.33 180) (layer B.SilkS))
    (fp_text value CONN_02X06 (at -1.27 -15.03 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at -2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at -2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 5 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at -2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 7 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 thru_hole oval (at -2.54 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 9 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 10 thru_hole oval (at -2.54 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad10)"))
    (pad 11 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad11)"))
    (pad 12 thru_hole oval (at -2.54 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad12)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x06_Pitch2.54mm.wrl
      (at (xyz -0.05 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (gr_text "- +" (at 111.125 91.694 270) (layer B.SilkS))
  (gr_text v1 (at 111.76 103.505 270) (layer Bottom))
  (gr_text "RPi Fan PWM\nInterface" (at 119.126 96.52 270) (layer Bottom))
  (gr_line (start 109.22 87.122) (end 129.794 87.122) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.22 105.918) (end 109.22 87.122) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.794 105.918) (end 109.22 105.918) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.794 87.122) (end 129.794 105.918) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 6) (net_name GND) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.429 86.106) (xy 130.429 106.553) (xy 103.251 106.553) (xy 103.251 86.106) (xy 103.886 86.106)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.429 86.106) (xy 130.429 106.553) (xy 103.251 106.553) (xy 103.251 86.106) (xy 103.886 86.106)
      )
    )
  )
)
