(kicad_pcb (version 20171130) (host pcbnew "(5.0.2)-1")
  (general
    (thickness 1.6)
    (drawings 35)
    (tracks 208)
    (zones 0)
    (modules 3)
    (nets 23)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(IC1-Pad1)")
  (net 2 "Net-(IC1-Pad2)")
  (net 3 "Net-(IC1-Pad3)")
  (net 4 "Net-(IC1-Pad4)")
  (net 5 "Net-(IC1-Pad5)")
  (net 6 "Net-(IC1-Pad6)")
  (net 7 "Net-(IC1-Pad7)")
  (net 8 "Net-(IC1-Pad8)")
  (net 9 "Net-(IC1-Pad9)")
  (net 10 "Net-(IC1-Pad10)")
  (net 11 "Net-(IC1-Pad11)")
  (net 12 "Net-(IC1-Pad12)")
  (net 13 "Net-(IC1-Pad13)")
  (net 14 "Net-(IC1-Pad14)")
  (net 15 "Net-(IC1-Pad15)")
  (net 16 "Net-(IC1-Pad16)")
  (net 17 "Net-(IC1-Pad17)")
  (net 18 "Net-(IC1-Pad18)")
  (net 19 "Net-(IC1-Pad19)")
  (net 20 "Net-(IC1-Pad20)")
  (net 21 "Net-(IC1-Pad21)")
  (net 22 "Net-(J1-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad14)")
    (add_net "Net-(IC1-Pad15)")
    (add_net "Net-(IC1-Pad16)")
    (add_net "Net-(IC1-Pad17)")
    (add_net "Net-(IC1-Pad18)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad20)")
    (add_net "Net-(IC1-Pad21)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC1-Pad4)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC1-Pad6)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(IC1-Pad9)")
    (add_net "Net-(J1-Pad5)")
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 124.46 76.2)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x10 (at 0 25.19) (layer F.Fab))
    (fp_text user %R (at 0 11.43 90) (layer F.Fab))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(IC1-Pad9)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(IC1-Pad11)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(IC1-Pad13)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(IC1-Pad14)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(IC1-Pad15)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(IC1-Pad16)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(IC1-Pad18)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(IC1-Pad17)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(IC1-Pad19)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(IC1-Pad20)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer F.Cu) (tedit 5C62AF46)
    (at 142.24 76.2)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x10 (at 0 25.19) (layer F.Fab))
    (fp_text user %R (at 0 11.43 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(IC1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(IC1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(IC1-Pad4)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(IC1-Pad5)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(IC1-Pad12)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(IC1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(IC1-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(IC1-Pad6)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(IC1-Pad3)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:CPT007BA02GMR (layer F.Cu) (tedit 5C62A19F)
    (at 133.35 87.63)
    (descr QFN20)
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference IC1 (at 0 0) (layer F.SilkS))
    (fp_text value CP2102N-A01-GQFN20 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.103 -1.265) (size 0.29 0.29) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(IC1-Pad1)"))
    (pad 2 smd rect (at -1.188 -0.75 90) (size 0.25 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at -1.188 -0.25 90) (size 0.25 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(IC1-Pad3)"))
    (pad 4 smd rect (at -1.188 0.25 90) (size 0.25 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(IC1-Pad4)"))
    (pad 5 smd rect (at -1.188 0.75 90) (size 0.25 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad5)"))
    (pad 6 smd rect (at -1.103 1.265) (size 0.29 0.29) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(IC1-Pad6)"))
    (pad 7 smd rect (at -0.588 1.35) (size 0.25 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad7)"))
    (pad 8 smd rect (at -0.088 1.35) (size 0.25 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad8)"))
    (pad 9 smd rect (at 0.412 1.35) (size 0.25 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad9)"))
    (pad 10 smd rect (at 0.912 1.35) (size 0.25 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(IC1-Pad10)"))
    (pad 11 smd rect (at 1.427 1.265) (size 0.29 0.29) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(IC1-Pad11)"))
    (pad 12 smd rect (at 1.513 0.75 90) (size 0.25 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(IC1-Pad12)"))
    (pad 13 smd rect (at 1.513 0.25 90) (size 0.25 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad13)"))
    (pad 14 smd rect (at 1.513 -0.25 90) (size 0.25 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad14)"))
    (pad 15 smd rect (at 1.513 -0.75 90) (size 0.25 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(IC1-Pad15)"))
    (pad 16 smd rect (at 1.427 -1.265) (size 0.29 0.29) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(IC1-Pad16)"))
    (pad 17 smd rect (at 0.912 -1.35) (size 0.25 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(IC1-Pad17)"))
    (pad 18 smd rect (at 0.412 -1.35) (size 0.25 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(IC1-Pad18)"))
    (pad 19 smd rect (at -0.088 -1.35) (size 0.25 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(IC1-Pad19)"))
    (pad 20 smd rect (at -0.588 -1.35) (size 0.25 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(IC1-Pad20)"))
    (pad 21 smd rect (at 0.162 0) (size 1.75 1.75) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(IC1-Pad21)"))
  )
  (gr_text 2019-2-12 (at 127.889 87.63 -90) (layer B.SilkS))
  (gr_text Gough (at 132.969 87.63 -90) (layer B.SilkS))
  (gr_text Tom (at 136.779 87.63 -90) (layer B.SilkS))
  (gr_line (start 122.936 100.584) (end 122.936 74.676) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.764 100.584) (end 122.936 100.584) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.764 74.676) (end 143.764 100.584) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122.936 74.676) (end 143.764 74.676) (layer Edge.Cuts) (width 0.15))
  (gr_text CP2102N (at 133.2992 80.3148 -90) (layer F.SilkS))
  (gr_text GPIO.1 (at 140.335 76.2) (layer F.SilkS))
  (gr_text GPIO.0 (at 140.335 78.74) (layer F.SilkS))
  (gr_text D+ (at 140.335 81.28) (layer F.SilkS))
  (gr_text D- (at 140.335 83.82) (layer F.SilkS))
  (gr_text GND (at 140.335 88.9) (layer F.SilkS))
  (gr_text VREGIN (at 140.335 91.44) (layer F.SilkS))
  (gr_text VBUS (at 140.335 93.98) (layer F.SilkS))
  (gr_text VDD (at 140.335 96.52) (layer F.SilkS))
  (gr_text GND (at 140.335 99.06) (layer F.SilkS))
  (gr_text GPIO.2 (at 126.365 76.2) (layer F.SilkS))
  (gr_text GPIO.3 (at 126.365 78.74) (layer F.SilkS))
  (gr_text RXD (at 126.365 81.28) (layer F.SilkS))
  (gr_text TXD (at 126.365 83.82) (layer F.SilkS))
  (gr_text RTS (at 126.365 86.36) (layer F.SilkS))
  (gr_text CTS (at 126.365 88.9) (layer F.SilkS))
  (gr_text SUSPEND (at 126.365 91.44) (layer F.SilkS))
  (gr_text WAKEUP (at 126.365 93.98) (layer F.SilkS))
  (gr_text SUSPENDB (at 126.365 96.52) (layer F.SilkS))
  (gr_text RSTB (at 126.365 99.06) (layer F.SilkS))
)
