(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-2")
  (general
    (thickness 1.6)
    (drawings 16)
    (tracks 74)
    (zones 0)
    (modules 16)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/solid/"))
  )
  (net 0 "")
  (net 1 "Net-(EXP1-Pad8)")
  (net 2 "Net-(EXP1-Pad6)")
  (net 3 "Net-(EXP1-Pad5)")
  (net 4 "Net-(EXP1-Pad4)")
  (net 5 "Net-(EXP1-Pad3)")
  (net 6 "Net-(EXP1-Pad2)")
  (net 7 "Net-(EXP1-Pad1)")
  (net 8 "Net-(EXP1-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(EXP1-Pad1)")
    (add_net "Net-(EXP1-Pad2)")
    (add_net "Net-(EXP1-Pad3)")
    (add_net "Net-(EXP1-Pad4)")
    (add_net "Net-(EXP1-Pad5)")
    (add_net "Net-(EXP1-Pad6)")
    (add_net "Net-(EXP1-Pad7)")
    (add_net "Net-(EXP1-Pad8)")
  )
  (module misc_footprints:OXY_EXP (layer F.Cu) (tedit 5DFE71A6)
    (at 232.275 119.75)
    (fp_text reference EXP1 (at -8.89 -7.62) (layer F.SilkS) hide)
    (fp_text value OXY_EXP (at 0 -6.35) (layer F.Fab))
    (pad 6 smd rect (at 5.5 0) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(EXP1-Pad6)"))
    (pad 6 smd rect (at -5.5 0) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(EXP1-Pad6)"))
    (pad 7 smd rect (at 2.8 2) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(EXP1-Pad7)"))
    (pad 1 smd rect (at 2 2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(EXP1-Pad1)"))
    (pad 2 smd rect (at 1.2 2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(EXP1-Pad2)"))
    (pad 3 smd rect (at 0.4 2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(EXP1-Pad3)"))
    (pad 4 smd rect (at -0.4 2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(EXP1-Pad4)"))
    (pad 5 smd rect (at -1.2 2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(EXP1-Pad5)"))
    (pad 6 smd rect (at -2 2) (size 0.5 2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(EXP1-Pad6)"))
    (pad 8 smd rect (at -2.8 2) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(EXP1-Pad8)"))
  )
  (module misc_footprints:AGB_EXP (layer F.Cu) (tedit 5DFE6AAF)
    (at 232.3 128.15)
    (fp_text reference EXP2 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value AGB_EXP (at 0 -1.27) (layer F.Fab))
    (pad 6 thru_hole oval (at 5 2.25) (size 1.75 2.75) (drill oval 1 2) (layers *.Cu *.Mask)
      (net 2 "Net-(EXP1-Pad6)"))
    (pad 6 thru_hole oval (at -5 2.25) (size 1.75 2.75) (drill oval 1 2) (layers *.Cu *.Mask)
      (net 2 "Net-(EXP1-Pad6)"))
    (pad 2 thru_hole circle (at 2.125 1.75) (size 0.75 0.75) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 "Net-(EXP1-Pad2)"))
    (pad 4 thru_hole circle (at 0 1.75) (size 0.75 0.75) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 "Net-(EXP1-Pad4)"))
    (pad 6 thru_hole circle (at -2.125 1.75) (size 0.75 0.75) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(EXP1-Pad6)"))
    (pad 1 thru_hole circle (at 2.125 0) (size 0.75 0.75) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 "Net-(EXP1-Pad1)"))
    (pad 3 thru_hole circle (at 0 0) (size 0.75 0.75) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 "Net-(EXP1-Pad3)"))
    (pad 5 thru_hole circle (at -2.125 0) (size 0.75 0.75) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 "Net-(EXP1-Pad5)"))
  )
  (module Connector_PinHeader_1.00mm:PinHeader_1x01_P1.00mm_Vertical (layer F.Cu) (tedit 59FED738)
    (at 236 124)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (fp_text reference J1 (at 0 -1.56) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Male (at 0 1.56) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 "Net-(EXP1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x01_P1.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.00mm:PinHeader_1x01_P1.00mm_Vertical (layer F.Cu) (tedit 59FED738)
    (at 233 124)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (fp_text reference J2 (at 0 -1.56) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Male (at 0 1.56) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 "Net-(EXP1-Pad3)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x01_P1.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.00mm:PinHeader_1x01_P1.00mm_Vertical (layer F.Cu) (tedit 59FED738)
    (at 230 124)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (fp_text reference J3 (at 0 -1.56) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Male (at 0 1.56) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 "Net-(EXP1-Pad5)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x01_P1.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.00mm:PinHeader_1x01_P1.00mm_Vertical (layer F.Cu) (tedit 59FED738)
    (at 236 126.5)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (fp_text reference J4 (at 0 -1.56) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Male (at 0 1.56) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 "Net-(EXP1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x01_P1.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.00mm:PinHeader_1x01_P1.00mm_Vertical (layer F.Cu) (tedit 59FED738)
    (at 234.5 124)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (fp_text reference J5 (at 0 -1.56) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Male (at 0 1.56) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 "Net-(EXP1-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x01_P1.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.00mm:PinHeader_1x01_P1.00mm_Vertical (layer F.Cu) (tedit 59FED738)
    (at 233 126.5)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (fp_text reference J6 (at 0 -1.56) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Male (at 0 1.56) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 "Net-(EXP1-Pad3)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x01_P1.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.00mm:PinHeader_1x01_P1.00mm_Vertical (layer F.Cu) (tedit 59FED738)
    (at 237.5 124)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (fp_text reference J7 (at 0 -1.56) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Male (at 0 1.56) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 "Net-(EXP1-Pad7)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x01_P1.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.00mm:PinHeader_1x01_P1.00mm_Vertical (layer F.Cu) (tedit 59FED738)
    (at 231.5 124)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (fp_text reference J8 (at 0 -1.56) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Male (at 0 1.56) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 "Net-(EXP1-Pad4)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x01_P1.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.00mm:PinHeader_1x01_P1.00mm_Vertical (layer F.Cu) (tedit 59FED738)
    (at 227 124)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (fp_text reference J9 (at 0 -1.56) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Male (at 0 1.56) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(EXP1-Pad8)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x01_P1.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.00mm:PinHeader_1x01_P1.00mm_Vertical (layer F.Cu) (tedit 59FED738)
    (at 230 126.5)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (fp_text reference J10 (at 0 -1.56) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Male (at 0 1.56) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 "Net-(EXP1-Pad5)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x01_P1.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.00mm:PinHeader_1x01_P1.00mm_Vertical (layer F.Cu) (tedit 59FED738)
    (at 228.5 124)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (fp_text reference J11 (at 0 -1.56) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Male (at 0 1.56) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(EXP1-Pad6)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x01_P1.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.00mm:PinHeader_1x01_P1.00mm_Vertical (layer F.Cu) (tedit 59FED738)
    (at 234.485001 126.5)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (fp_text reference J12 (at 0 -1.56) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Male (at 0 1.56) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 "Net-(EXP1-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x01_P1.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.00mm:PinHeader_1x01_P1.00mm_Vertical (layer F.Cu) (tedit 59FED738)
    (at 231.5 126.5)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (fp_text reference J13 (at 0 -1.56) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Male (at 0 1.56) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 "Net-(EXP1-Pad4)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x01_P1.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.00mm:PinHeader_1x01_P1.00mm_Vertical (layer F.Cu) (tedit 59FED738)
    (at 228.5 126.5)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (fp_text reference J14 (at 0 -1.56) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Male (at 0 1.56) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(EXP1-Pad6)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x01_P1.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text makho (at 232.3 131.3) (layer B.Cu))
  (gr_text "This side bottom of Micro" (at 232.3 121.9) (layer B.SilkS))
  (gr_text CHG+ (at 237.5 122.7) (layer F.SilkS))
  (gr_text CHG- (at 227.2 122.7) (layer F.SilkS))
  (gr_arc (start 238.2 119.5) (end 239 119.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 226.3 119.5) (end 226.3 118.7) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 226.3 131.2) (end 225.5 131.2) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 238.2 131.2) (end 238.2 132) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 238.2 132) (end 226.3 132) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 225.5 119.5) (end 225.5 131.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 227.75 118.7) (end 226.3 118.7) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 239 119.5) (end 239 131.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 236.8 118.7) (end 238.2 118.7) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 227.75 120.75) (end 227.75 118.7) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 236.8 120.75) (end 227.75 120.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 236.8 118.7) (end 236.8 120.75) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name "Net-(EXP1-Pad6)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 239 132) (xy 225.5 132) (xy 225.5 118.7) (xy 239 118.7)
      )
    )
  )
  (zone (net 2) (net_name "Net-(EXP1-Pad6)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 239 132) (xy 225.5 132) (xy 225.5 118.7) (xy 239 118.7)
      )
    )
  )
)
