(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A5")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(D1-K)")
  (net 2 "VCC")
  (net 3 "Net-(D2-K)")
  (net 4 "/RXI_{0}")
  (net 5 "/TXI_{0}")
  (net 6 "/D-")
  (net 7 "/D+")
  (net 8 "unconnected-(J2-ID-Pad4)")
  (net 9 "GND")
  (net 10 "/S_{0}")
  (net 11 "/S_{1}")
  (footprint "Connector_USB:USB_Micro-B_Molex-105017-0001" (layer "F.Cu")
    (at 86.654 77.1545)
    (descr "http://www.molex.com/pdm_docs/sd/1050170001_sd.pdf")
    (tags "Micro-USB SMD Typ-B")
    (property "Sheetfile" "vgaterm-io-faceboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "USB Micro Type B connector")
    (property "ki_keywords" "connector USB micro")
    (attr smd)
    (fp_text reference "J2" (at 1.23 -3.2405) (layer "F.SilkS"))
    (fp_text value "USB_B_Micro UART" (at 0.3 4.3375) (layer "F.Fab"))
    (fp_text user "PCB Edge" (at 0 2.6875) (layer "Dwgs.User"))
    (fp_text user "${REFERENCE}" (at 0 0.8875) (layer "F.Fab"))
    (pad "1" smd rect (at -1.3 -1.4625) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "VCC") (pinfunction "VBUS") (pintype "power_out"))
    (pad "2" smd rect (at -0.65 -1.4625) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/D-") (pinfunction "D-") (pintype "bidirectional"))
    (pad "3" smd rect (at 0 -1.4625) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/D+") (pinfunction "D+") (pintype "bidirectional"))
    (pad "4" smd rect (at 0.65 -1.4625) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "unconnected-(J2-ID-Pad4)") (pinfunction "ID") (pintype "passive+no_connect"))
    (pad "5" smd rect (at 1.3 -1.4625) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "6" thru_hole oval (at -3.5 1.2375 180) (size 1.2 1.9) (drill oval 0.6 1.3) (layers "*.Cu" "*.Mask")
      (net 9 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at -2.9 1.2375) (size 1.2 1.9) (layers "F.Cu" "F.Mask")
      (net 9 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" thru_hole circle (at -2.5 -1.4625) (size 1.45 1.45) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 9 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at -1 1.2375) (size 1.5 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at 1 1.2375) (size 1.5 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" thru_hole circle (at 2.5 -1.4625) (size 1.45 1.45) (drill 0.85) (layers "*.Cu" "*.Mask")
      (net 9 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at 2.9 1.2375) (size 1.2 1.9) (layers "F.Cu" "F.Mask")
      (net 9 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" thru_hole oval (at 3.5 1.2375) (size 1.2 1.9) (drill oval 0.6 1.3) (layers "*.Cu" "*.Mask")
      (net 9 "GND") (pinfunction "Shield") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_USB.3dshapes/USB_Micro-B_Molex-105017-0001.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D1.8mm_W1.8mm_H2.4mm_Horizontal_O1.27mm_Z1.6mm" (layer "F.Cu")
    (at 78.486 73.406)
    (descr "LED, ,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins")
    (tags "LED   diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins")
    (property "Sheetfile" "vgaterm-io-faceboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D1" (at 4.826 0) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 5.33) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D1.8mm_W1.8mm_H2.4mm_Horizontal_O1.27mm_Z1.6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D1.8mm_W1.8mm_H2.4mm_Horizontal_O1.27mm_Z1.6mm" (layer "F.Cu")
    (at 103.378 73.406)
    (descr "LED, ,  diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm, 2 pins")
    (tags "LED   diameter 1.8mm size 1.8x2.4mm^2 z-position of LED center 1.6mm 2 pins")
    (property "Sheetfile" "vgaterm-io-faceboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D2" (at -2.286 0) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 5.33) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D2-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D1.8mm_W1.8mm_H2.4mm_Horizontal_O1.27mm_Z1.6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 83.058 68.326 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "vgaterm-io-faceboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 2.54 0 180) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 1 "Net-(D1-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 10 "/S_{0}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 102.616 70.104 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "vgaterm-io-faceboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 2.54 -0.254 180) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 3 "Net-(D2-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 11 "/S_{1}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Horizontal" (layer "F.Cu")
    (at 112.268 73.603 -90)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "vgaterm-io-faceboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at -2.483 0 -180) (layer "F.SilkS"))
    (fp_text value "Conn_01x02" (at 4.385 4.81 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.77 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "/RXI_{0}") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "/TXI_{0}") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical" (layer "B.Cu")
    (at 105.41 70.104)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (property "Sheetfile" "vgaterm-io-faceboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J4" (at 2.54 0) (layer "B.SilkS"))
    (fp_text value "Conn_01x04" (at 0 -10.39) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -3.81 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "/S_{1}") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "/TXI_{0}") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "/RXI_{0}") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical" (layer "B.Cu")
    (at 80.01 70.104)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (property "Sheetfile" "vgaterm-io-faceboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3" (at 2.286 -7.366) (layer "B.SilkS"))
    (fp_text value "Conn_01x04" (at 0 -10.39) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -3.81 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "VCC") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "/D+") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "/D-") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "/S_{0}") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 91.186 80.01) (end 82.042 80.01)
    (layer "Edge.Cuts"))
  (gr_line (start 76.962 62.23) (end 78.232 60.96)
    (layer "Edge.Cuts"))
  (gr_line (start 114.554 62.23) (end 113.284 60.96)
    (layer "Edge.Cuts"))
  (gr_line (start 82.042 80.01) (end 82.042 78.74)
    (layer "Edge.Cuts"))
  (gr_line (start 91.186 78.74) (end 91.694 77.978)
    (layer "Edge.Cuts"))
  (gr_line (start 81.534 77.978) (end 82.042 78.74)
    (layer "Edge.Cuts"))
  (gr_line (start 81.534 77.978) (end 77.724 77.978)
    (layer "Edge.Cuts"))
  (gr_line (start 77.724 77.978) (end 76.962 77.216)
    (layer "Edge.Cuts"))
  (gr_line (start 114.554 62.23) (end 114.554 76.708)
    (layer "Edge.Cuts"))
  (gr_line (start 76.962 77.216) (end 76.962 62.23)
    (layer "Edge.Cuts"))
  (gr_line (start 113.538 77.978) (end 114.554 76.708)
    (layer "Edge.Cuts"))
  (gr_line (start 91.186 78.74) (end 91.186 80.01)
    (layer "Edge.Cuts"))
  (gr_line (start 113.538 77.978) (end 91.694 77.978)
    (layer "Edge.Cuts"))
  (gr_line (start 78.232 60.96) (end 113.284 60.96)
    (layer "Edge.Cuts"))
  (gr_text "A1" (at 108.204 64.516) (layer "F.SilkS"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 103.378 73.406) (xy 78.486 73.406))
    (height 10.414)
    (gr_text "24.8920 mm" (at 90.932 61.842) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 2) (net_name "VCC") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 66.294 81.28)
        (xy 127.762 81.28)
        (xy 127.762 52.578)
        (xy 66.294 52.578)
      )
    )
  )
  (zone (net 9) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 66.04 81.28)
        (xy 127.762 81.28)
        (xy 127.254 52.578)
        (xy 65.786 52.578)
      )
    )
  )
)
