(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~86~ubuntu19.10.1)
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 64)
    (zones 0)
    (modules 12)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.27)
    (trace_clearance 0.2032)
    (zone_clearance 0.4064)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8128)
    (via_drill 0.4064)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.8128 0.4064)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J2-Pad2)")
  (net 3 +5V)
  (net 4 "Net-(JP1-Pad1)")
  (net 5 "Net-(JP1-Pad2)")
  (net 6 "Net-(JP2-Pad1)")
  (net 7 "Net-(JP4-Pad1)")
  (net 8 "Net-(Q1-Pad1)")
  (net 9 +3V3)
  (net 10 "Net-(U1-Pad7)")
  (net 11 "Net-(U1-Pad6)")
  (net 12 "Net-(U1-Pad5)")
  (net 13 "Net-(U1-Pad12)")
  (net 14 "Net-(U1-Pad4)")
  (net 15 "Net-(U1-Pad3)")
  (net 16 "Net-(U1-Pad2)")
  (net 17 "Net-(U1-Pad15)")
  (net 18 "Net-(U1-Pad1)")
  (net 19 "Net-(U1-Pad16)")
  (net 20 "Net-(JP3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.2032)
    (via_dia 0.8128)
    (via_drill 0.4064)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(JP2-Pad1)")
    (add_net "Net-(JP3-Pad1)")
    (add_net "Net-(JP4-Pad1)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
  )
  (net_class Thicc ""
    (clearance 0.254)
    (trace_width 0.762)
    (via_dia 0.8128)
    (via_drill 0.4064)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net "Net-(JP1-Pad1)")
  )
  (module duck:jumper_smd_nc (layer F.Cu) (tedit 5EF2C4F0)
    (at 99.314 92.456 270)
    (fp_text reference JP3 (at 0 2.794 90) (layer F.SilkS) hide)
    (fp_text value D4 (at 0 -2.54 90) (layer F.Fab))
    (pad 1 smd rect (at -0.635 0 270) (size 1 1.7) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(JP3-Pad1)"))
    (pad 2 smd rect (at 0.635 0 270) (size 1 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
  )
  (module Jumpers:SMT-JUMPER_2_NC_TRACE_SILK (layer F.Cu) (tedit 5EF2C482)
    (at 109.22 95.25 270)
    (attr smd)
    (fp_text reference JP2 (at 0 -1.524 270) (layer F.SilkS) hide)
    (fp_text value D4 (at -1.778 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.508 0 270) (size 0.635 1.27) (layers F.Cu F.Mask)
      (net 6 "Net-(JP2-Pad1)") (solder_mask_margin 0.1016))
    (pad 2 smd rect (at 0.508 0 270) (size 0.635 1.27) (layers F.Cu F.Mask)
      (net 5 "Net-(JP1-Pad2)") (solder_mask_margin 0.1016))
  )
  (module Jumpers:SMT-JUMPER_2_NO_SILK (layer F.Cu) (tedit 200000)
    (at 114.3 95.25 270)
    (attr smd)
    (fp_text reference JP1 (at 0 -1.524 90) (layer F.SilkS) hide)
    (fp_text value D1 (at -1.778 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.4064 0 270) (size 0.635 1.27) (layers F.Cu F.Mask)
      (net 4 "Net-(JP1-Pad1)") (solder_mask_margin 0.1016))
    (pad 2 smd rect (at 0.4064 0 270) (size 0.635 1.27) (layers F.Cu F.Mask)
      (net 5 "Net-(JP1-Pad2)") (solder_mask_margin 0.1016))
  )
  (module Jumpers:SMT-JUMPER_2_NO_SILK (layer F.Cu) (tedit 200000)
    (at 111.76 95.25 270)
    (attr smd)
    (fp_text reference JP4 (at 0 -1.524 90) (layer F.SilkS) hide)
    (fp_text value D2 (at -1.778 0 180) (layer F.SilkS))
    (pad 2 smd rect (at 0.4064 0 270) (size 0.635 1.27) (layers F.Cu F.Mask)
      (net 5 "Net-(JP1-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.4064 0 270) (size 0.635 1.27) (layers F.Cu F.Mask)
      (net 7 "Net-(JP4-Pad1)") (solder_mask_margin 0.1016))
  )
  (module digikey-footprints:SOT-23-3 (layer F.Cu) (tedit 5D28A5E3)
    (at 107.188 108.458 90)
    (attr smd)
    (fp_text reference Q1 (at -1.524 -2.794 90) (layer F.SilkS))
    (fp_text value DMG2302U (at 0.025 3.25 90) (layer F.Fab))
    (fp_text user %R (at -0.125 0.15 90) (layer F.Fab))
    (pad 3 smd rect (at 1.05 0 90) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J2-Pad2)") (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 0.95 90) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(JP1-Pad2)") (solder_mask_margin 0.07))
    (pad 1 smd rect (at -1.05 -0.95 90) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(Q1-Pad1)") (solder_mask_margin 0.07))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 100.33 109.22)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -2.032 -1.7 90) (layer F.SilkS))
    (fp_text value R (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(JP1-Pad2)"))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 103.886 104.822 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -2.968 0 180) (layer F.SilkS))
    (fp_text value R (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(Q1-Pad1)"))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 107.442 103.806 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -2.968 0 180) (layer F.SilkS))
    (fp_text value R (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SOT-23-6 (layer F.Cu) (tedit 5D28A5EB)
    (at 100.33 104.14)
    (attr smd)
    (fp_text reference U2 (at 0.025 -3.048) (layer F.SilkS))
    (fp_text value SN74LVC1T45DBV (at -0.025 3.575) (layer F.Fab))
    (fp_text user %R (at 0.025 0) (layer F.Fab))
    (pad 3 smd rect (at 0.95 1.35) (size 0.55 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(JP1-Pad2)"))
    (pad 2 smd rect (at 0 1.35) (size 0.55 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.95 1.35) (size 0.55 1) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V3))
    (pad 4 smd rect (at 0.95 -1.35) (size 0.55 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J2-Pad2)"))
    (pad 5 smd rect (at 0 -1.35) (size 0.55 1) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V3))
    (pad 6 smd rect (at -0.95 -1.35) (size 0.55 1) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
  )
  (module Connectors:PINHEAD1-2 (layer F.Cu) (tedit 0)
    (at 99.568 95.504 270)
    (fp_text reference J1 (at 1.27 -3.9 90) (layer F.SilkS) hide)
    (fp_text value PWR (at 1.27 3.81 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
  )
  (module Connectors:PINHEAD1-3 (layer F.Cu) (tedit 0)
    (at 114.3 107.95 90)
    (fp_text reference J2 (at -0.254 -2.286 90) (layer F.SilkS))
    (fp_text value LED (at 2.54 3.81 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad2)"))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module duck:wemos-d1-mini-no-keepout (layer B.Cu) (tedit 5EF2B67E)
    (at 107.385001 101.157025)
    (fp_text reference U1 (at -19.3 0 -90) (layer B.SilkS))
    (fp_text value WeMos_D1_mini (at 0 0) (layer B.Fab))
    (pad 8 thru_hole circle (at -8.89 11.43) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 +3V3))
    (pad 9 thru_hole circle (at -8.89 -11.43) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(JP3-Pad1)"))
    (pad 7 thru_hole circle (at -6.35 11.43) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(U1-Pad7)"))
    (pad 10 thru_hole circle (at -6.35 -11.43) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at -3.81 11.43 270) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(U1-Pad6)"))
    (pad 11 thru_hole circle (at -3.81 -11.43) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(JP2-Pad1)"))
    (pad 5 thru_hole circle (at -1.27 11.43) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(U1-Pad5)"))
    (pad 12 thru_hole circle (at -1.27 -11.43) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad12)"))
    (pad 4 thru_hole circle (at 1.27 11.43) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(U1-Pad4)"))
    (pad 13 thru_hole circle (at 1.27 -11.43) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(JP4-Pad1)"))
    (pad 3 thru_hole circle (at 3.81 11.43) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "Net-(U1-Pad3)"))
    (pad 14 thru_hole circle (at 3.81 -11.43) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "Net-(JP1-Pad1)"))
    (pad 2 thru_hole circle (at 6.35 11.43) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "Net-(U1-Pad2)"))
    (pad 15 thru_hole circle (at 6.35 -11.43) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(U1-Pad15)"))
    (pad 1 thru_hole circle (at 8.89 11.43) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "Net-(U1-Pad1)"))
    (pad 16 thru_hole circle (at 8.89 -11.43) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "Net-(U1-Pad16)"))
    (model ${KIPRJMOD}/3dshapes/wemos_d1_mini.3dshapes/d1_mini_shield.wrl
      (offset (xyz -17.89999973116897 -12.79999980776329 8.39999987384466))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 180 90))
    )
    (model ${KIPRJMOD}/3dshapes/wemos_d1_mini.3dshapes/SLW-108-01-G-S.wrl
      (offset (xyz 0 -11.39999982878918 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 0))
    )
    (model ${KIPRJMOD}/3dshapes/wemos_d1_mini.3dshapes/SLW-108-01-G-S.wrl
      (offset (xyz 0 11.39999982878918 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 0))
    )
    (model ${KIPRJMOD}/3dshapes/wemos_d1_mini.3dshapes/TSW-108-05-G-S.wrl
      (offset (xyz 0 -11.39999982878918 7.299999890364999))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 90 0 0))
    )
    (model ${KIPRJMOD}/3dshapes/wemos_d1_mini.3dshapes/TSW-108-05-G-S.wrl
      (offset (xyz 0 11.39999982878918 7.299999890364999))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 90 0 0))
    )
  )
  (gr_line (start 97.155 88.392) (end 117.729 88.392) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97.155 113.919) (end 97.155 88.392) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 117.729 113.919) (end 97.155 113.919) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 117.729 88.392) (end 117.729 113.919) (layer Edge.Cuts) (width 0.05))
  (gr_text 74LVC1T45 (at 98.044 103.378 90) (layer F.SilkS))
  (gr_text "Populate U2 -OR-\nQ1, R1, R2, R3" (at 109.982 98.806) (layer B.SilkS))
  (gr_text 2020-06-23 (at 112.268 94.234) (layer B.SilkS))
  (gr_text "ESP8266 LED SHIELD" (at 109.22 92.456) (layer B.SilkS))
  (gr_text 3V3 (at 98.552 111.252) (layer F.SilkS))
  (gr_text "pwr\nfeed" (at 101.6 92.202) (layer F.SilkS))
  (gr_text GND (at 105.156 98.552) (layer F.SilkS))
  (gr_text 5V (at 104.14 94.488) (layer F.SilkS))
  (gr_text GND (at 114.554 110.236) (layer F.SilkS))
  (gr_text 5V (at 114.3 100.584) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4064))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.4064) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 118.11 114.3) (xy 96.52 114.3) (xy 96.52 87.63) (xy 118.11 87.63)
      )
    )
  )
)
