(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 29)
    (no_connects 0)
    (area 111.684999 51.740999 140.537001 93.293001)
    (thickness 1.6)
    (drawings 13)
    (tracks 54)
    (zones 0)
    (modules 11)
    (nets 23)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad2)")
  (net 2 "Net-(J1-Pad3)")
  (net 3 "Net-(J1-Pad4)")
  (net 4 "Net-(J2-Pad2)")
  (net 5 "Net-(J2-Pad3)")
  (net 6 "Net-(J2-Pad4)")
  (net 7 "Net-(J3-Pad2)")
  (net 8 "Net-(J3-Pad3)")
  (net 9 "Net-(J3-Pad4)")
  (net 10 "Net-(J4-Pad2)")
  (net 11 "Net-(J4-Pad3)")
  (net 12 "Net-(J4-Pad4)")
  (net 13 "Net-(J5-Pad2)")
  (net 14 "Net-(J5-Pad3)")
  (net 15 "Net-(J6-Pad2)")
  (net 16 "Net-(J6-Pad3)")
  (net 17 "Net-(J5-Pad4)")
  (net 18 "Net-(J6-Pad4)")
  (net 19 "Net-(J7-Pad2)")
  (net 20 "Net-(J7-Pad4)")
  (net 21 "Net-(J7-Pad3)")
  (net 22 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J5-Pad4)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(J6-Pad4)")
    (add_net "Net-(J7-Pad2)")
    (add_net "Net-(J7-Pad3)")
    (add_net "Net-(J7-Pad4)")
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5A650960)
    (at 126.238 81.026)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_Pad (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Connectors_JST:JST_EH_B04B-EH-A_04x2.50mm_Straight (layer F.Cu) (tedit 5A6509A6)
    (at 138.43 54.864 270)
    (descr "JST EH series connector, B04B-EH-A, 2.50mm pitch, top entry")
    (tags "connector jst eh top vertical straight")
    (fp_text reference J1 (at 3.75 -3 270) (layer F.SilkS) hide)
    (fp_text value Conn_01x04 (at 3.75 3.5 270) (layer F.Fab))
    (fp_text user %R (at 3.75 -3 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 GND))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 5 0 270) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at 7.5 0 270) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad4)"))
    (model Connectors_JST.3dshapes/JST_EH_B04B-EH-A_04x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_EH_B04B-EH-A_04x2.50mm_Straight (layer F.Cu) (tedit 5A650980)
    (at 138.43 68.834 270)
    (descr "JST EH series connector, B04B-EH-A, 2.50mm pitch, top entry")
    (tags "connector jst eh top vertical straight")
    (fp_text reference J2 (at 3.75 -3 270) (layer F.SilkS) hide)
    (fp_text value Conn_01x04 (at 3.75 3.5 270) (layer F.Fab))
    (fp_text user %R (at 3.75 -3 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 GND))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad2)"))
    (pad 3 thru_hole circle (at 5 0 270) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad3)"))
    (pad 4 thru_hole circle (at 7.5 0 270) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad4)"))
    (model Connectors_JST.3dshapes/JST_EH_B04B-EH-A_04x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_EH_B04B-EH-A_04x2.50mm_Straight (layer F.Cu) (tedit 5A650974)
    (at 138.43 82.804 270)
    (descr "JST EH series connector, B04B-EH-A, 2.50mm pitch, top entry")
    (tags "connector jst eh top vertical straight")
    (fp_text reference J3 (at 3.75 -3 270) (layer F.SilkS) hide)
    (fp_text value Conn_01x04 (at 3.75 3.5 270) (layer F.Fab))
    (fp_text user %R (at 3.75 -3 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 GND))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad2)"))
    (pad 3 thru_hole circle (at 5 0 270) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(J3-Pad3)"))
    (pad 4 thru_hole circle (at 7.5 0 270) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(J3-Pad4)"))
    (model Connectors_JST.3dshapes/JST_EH_B04B-EH-A_04x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_EH_B04B-EH-A_04x2.50mm_Straight (layer F.Cu) (tedit 5A650997)
    (at 114.554 54.864 270)
    (descr "JST EH series connector, B04B-EH-A, 2.50mm pitch, top entry")
    (tags "connector jst eh top vertical straight")
    (fp_text reference J4 (at 3.75 -3 270) (layer F.SilkS) hide)
    (fp_text value Conn_01x04 (at 3.75 3.5 270) (layer F.Fab))
    (fp_text user %R (at 3.75 -3 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 GND))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(J4-Pad2)"))
    (pad 3 thru_hole circle (at 5 0 270) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 "Net-(J4-Pad3)"))
    (pad 4 thru_hole circle (at 7.5 0 270) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(J4-Pad4)"))
    (model Connectors_JST.3dshapes/JST_EH_B04B-EH-A_04x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_EH_B04B-EH-A_04x2.50mm_Straight (layer F.Cu) (tedit 5A65098E)
    (at 114.554 68.834 270)
    (descr "JST EH series connector, B04B-EH-A, 2.50mm pitch, top entry")
    (tags "connector jst eh top vertical straight")
    (fp_text reference J5 (at 3.75 -3 270) (layer F.SilkS) hide)
    (fp_text value Conn_01x04 (at 3.75 3.5 270) (layer F.Fab))
    (fp_text user %R (at 3.75 -3 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 GND))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 "Net-(J5-Pad2)"))
    (pad 3 thru_hole circle (at 5 0 270) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(J5-Pad3)"))
    (pad 4 thru_hole circle (at 7.5 0 270) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 "Net-(J5-Pad4)"))
    (model Connectors_JST.3dshapes/JST_EH_B04B-EH-A_04x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_EH_B04B-EH-A_04x2.50mm_Straight (layer F.Cu) (tedit 5A650968)
    (at 114.554 82.804 270)
    (descr "JST EH series connector, B04B-EH-A, 2.50mm pitch, top entry")
    (tags "connector jst eh top vertical straight")
    (fp_text reference J6 (at 3.75 -3 270) (layer F.SilkS) hide)
    (fp_text value Conn_01x04 (at 3.75 3.5 270) (layer F.Fab))
    (fp_text user %R (at 3.75 -3 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 GND))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(J6-Pad2)"))
    (pad 3 thru_hole circle (at 5 0 270) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(J6-Pad3)"))
    (pad 4 thru_hole circle (at 7.5 0 270) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 "Net-(J6-Pad4)"))
    (model Connectors_JST.3dshapes/JST_EH_B04B-EH-A_04x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_EH_B04B-EH-A_04x2.50mm_Straight (layer F.Cu) (tedit 5A65096F)
    (at 130.048 90.932 180)
    (descr "JST EH series connector, B04B-EH-A, 2.50mm pitch, top entry")
    (tags "connector jst eh top vertical straight")
    (fp_text reference J7 (at 3.75 -3 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x04 (at 3.75 3.5 180) (layer F.Fab))
    (fp_text user %R (at 3.75 -3 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 GND))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 19 "Net-(J7-Pad2)"))
    (pad 3 thru_hole circle (at 5 0 180) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 "Net-(J7-Pad3)"))
    (pad 4 thru_hole circle (at 7.5 0 180) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 20 "Net-(J7-Pad4)"))
    (model Connectors_JST.3dshapes/JST_EH_B04B-EH-A_04x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module moshozenfootprints:Moshozen (layer B.Cu) (tedit 0)
    (at 126.238 70.866 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (module teensy:Teensy30_31_32_LC_edited (layer F.Cu) (tedit 5A650987)
    (at 126.238 69.596 270)
    (fp_text reference U1 (at 0 -10.16 270) (layer F.SilkS) hide)
    (fp_text value Teensy-LC (at 0 10.16 270) (layer F.Fab))
    (pad 17 thru_hole circle (at 16.51 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 18 thru_hole circle (at 16.51 -2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 19 thru_hole circle (at 16.51 -5.08 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(J7-Pad2)"))
    (pad 20 thru_hole circle (at 16.51 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 16 thru_hole circle (at 16.51 2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 15 thru_hole circle (at 16.51 5.08 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole circle (at 16.51 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(J7-Pad4)"))
    (pad 21 thru_hole circle (at 13.97 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 22 thru_hole circle (at 11.43 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J3-Pad4)"))
    (pad 23 thru_hole circle (at 8.89 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J3-Pad3)"))
    (pad 24 thru_hole circle (at 6.35 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J3-Pad2)"))
    (pad 25 thru_hole circle (at 3.81 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J2-Pad4)"))
    (pad 26 thru_hole circle (at 1.27 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J2-Pad3)"))
    (pad 27 thru_hole circle (at -1.27 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J2-Pad2)"))
    (pad 28 thru_hole circle (at -3.81 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J1-Pad4)"))
    (pad 29 thru_hole circle (at -6.35 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(J1-Pad3)"))
    (pad 30 thru_hole circle (at -8.89 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(J1-Pad2)"))
    (pad 31 thru_hole circle (at -11.43 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 32 thru_hole circle (at -13.97 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 22 GND))
    (pad 33 thru_hole circle (at -16.51 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole circle (at 13.97 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J7-Pad3)"))
    (pad 12 thru_hole circle (at 11.43 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(J6-Pad4)"))
    (pad 11 thru_hole circle (at 8.89 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J6-Pad3)"))
    (pad 10 thru_hole circle (at 6.35 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J6-Pad2)"))
    (pad 9 thru_hole circle (at 3.81 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole circle (at 1.27 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole circle (at -1.27 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J5-Pad4)"))
    (pad 6 thru_hole circle (at -3.81 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J5-Pad3)"))
    (pad 5 thru_hole circle (at -6.35 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J5-Pad2)"))
    (pad 4 thru_hole circle (at -8.89 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J4-Pad4)"))
    (pad 3 thru_hole circle (at -11.43 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J4-Pad3)"))
    (pad 2 thru_hole circle (at -13.97 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J4-Pad2)"))
    (pad 1 thru_hole rect (at -16.51 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 22 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5A65099E)
    (at 126.238 60.706)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_Pad (at 0 4.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_text "12 11 26" (at 124.968 88.392 180) (layer B.SilkS))
  (gr_text "2  1  0" (at 116.586 59.944 270) (layer B.SilkS))
  (gr_text "5  4  3" (at 116.586 73.914 270) (layer B.SilkS))
  (gr_text "10 9  8" (at 116.586 87.884 270) (layer B.SilkS))
  (gr_text "15 16 17" (at 136.398 87.884 270) (layer B.SilkS))
  (gr_text "18 19 20" (at 136.398 73.66 270) (layer B.SilkS))
  (gr_text "21 22 23" (at 136.398 59.944 270) (layer B.SilkS))
  (gr_text v2.0 (at 131.572 54.356 270) (layer B.SilkS))
  (gr_text github.com/mtrudel/teensyhid (at 121.412 70.612 270) (layer B.SilkS))
  (gr_line (start 111.76 93.218) (end 111.76 51.816) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.462 93.218) (end 111.76 93.218) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.462 51.816) (end 140.462 93.218) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.76 51.816) (end 140.462 51.816) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 22) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.462 93.218) (xy 111.76 93.218) (xy 111.76 51.816) (xy 140.462 51.816)
      )
    )
  )
  (zone (net 22) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.76 51.816) (xy 140.716 51.816) (xy 140.462 93.218) (xy 111.76 93.218) (xy 111.76 52.07)
      )
    )
  )
)
